(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 66)
    (no_connects 0)
    (area 79.934999 118.034999 97.865001 148.665001)
    (thickness 1.6)
    (drawings 58)
    (tracks 229)
    (zones 0)
    (modules 17)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.0254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6096)
    (via_drill 0.3048)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.07)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x210fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers2/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 TCK)
  (net 4 TMS)
  (net 5 TDI)
  (net 6 TDO)
  (net 7 PB4C/CS)
  (net 8 PL9B)
  (net 9 PL9A)
  (net 10 PB9B)
  (net 11 PB9A)
  (net 12 PB6D/MISO)
  (net 13 PB6C/SCLK)
  (net 14 PB11A)
  (net 15 PB11B)
  (net 16 PB20C/SN)
  (net 17 PB20D/MOSI)
  (net 18 PR5D)
  (net 19 PR5C)
  (net 20 PT17D/DONE)
  (net 21 PT15D/PROGRAMN)
  (net 22 PT15C/JTAGENB)
  (net 23 PT12D/SDA)
  (net 24 PT12C/SCL)
  (net 25 EXT3v3)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net PB11A)
    (add_net PB11B)
    (add_net PB20C/SN)
    (add_net PB20D/MOSI)
    (add_net PB4C/CS)
    (add_net PB6C/SCLK)
    (add_net PB6D/MISO)
    (add_net PB9A)
    (add_net PB9B)
    (add_net PL9A)
    (add_net PL9B)
    (add_net PR5C)
    (add_net PR5D)
    (add_net PT12C/SCL)
    (add_net PT12D/SDA)
    (add_net PT15C/JTAGENB)
    (add_net PT15D/PROGRAMN)
    (add_net PT17D/DONE)
    (add_net TCK)
    (add_net TDI)
    (add_net TDO)
    (add_net TMS)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net EXT3v3)
    (add_net GND)
  )
  (module 32QFN (layer F.Cu) (tedit 592B3A1F)
    (at 88.9 132.9055 180)
    (attr smd)
    (fp_text reference U1 (at 0 -1.7145 180) (layer F.Fab))
    (fp_text value LCMXO2-1200HC-4SG32C (at 0 1.27 180) (layer F.Fab))
    (pad 32 smd oval (at -1.75 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 5 TDI) (solder_mask_margin 0.07))
    (pad 31 smd oval (at -1.25 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 30 smd oval (at -0.75 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 3 TCK) (solder_mask_margin 0.07))
    (pad 29 smd oval (at -0.25 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 4 TMS) (solder_mask_margin 0.07))
    (pad 28 smd oval (at 0.25 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 24 PT12C/SCL) (solder_mask_margin 0.07))
    (pad 27 smd oval (at 0.75 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 23 PT12D/SDA) (solder_mask_margin 0.07))
    (pad 26 smd oval (at 1.25 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 22 PT15C/JTAGENB) (solder_mask_margin 0.07))
    (pad 25 smd oval (at 1.75 -2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 21 PT15D/PROGRAMN) (solder_mask_margin 0.07))
    (pad 24 smd oval (at 2.5 -1.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 23 smd oval (at 2.5 -1.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 20 PT17D/DONE) (solder_mask_margin 0.07))
    (pad 22 smd oval (at 2.5 -0.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 21 smd oval (at 2.5 -0.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 19 PR5C) (solder_mask_margin 0.07))
    (pad 20 smd oval (at 2.5 0.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 18 PR5D) (solder_mask_margin 0.07))
    (pad 19 smd oval (at 2.5 0.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 18 smd oval (at 2.5 1.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 17 smd oval (at 2.5 1.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 17 PB20D/MOSI) (solder_mask_margin 0.07))
    (pad 16 smd oval (at 1.75 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 16 PB20C/SN) (solder_mask_margin 0.07))
    (pad 15 smd oval (at 1.25 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 14 smd oval (at 0.75 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 15 PB11B) (solder_mask_margin 0.07))
    (pad 13 smd oval (at 0.25 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 14 PB11A) (solder_mask_margin 0.07))
    (pad 12 smd oval (at -0.25 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 10 PB9B) (solder_mask_margin 0.07))
    (pad 11 smd oval (at -0.75 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 11 PB9A) (solder_mask_margin 0.07))
    (pad 10 smd oval (at -1.25 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 12 PB6D/MISO) (solder_mask_margin 0.07))
    (pad 9 smd oval (at -1.75 2.5 270) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 13 PB6C/SCLK) (solder_mask_margin 0.07))
    (pad 8 smd oval (at -2.5 1.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 7 PB4C/CS) (solder_mask_margin 0.07))
    (pad 7 smd oval (at -2.5 1.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 6 smd oval (at -2.5 0.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 5 smd oval (at -2.5 0.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 8 PL9B) (solder_mask_margin 0.07))
    (pad 4 smd oval (at -2.5 -0.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 9 PL9A) (solder_mask_margin 0.07))
    (pad 3 smd oval (at -2.5 -0.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 2 smd oval (at -2.5 -1.25 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3) (solder_mask_margin 0.07))
    (pad 1 smd oval (at -2.5 -1.75 180) (size 0.7 0.24) (layers F.Cu F.Paste F.Mask)
      (net 6 TDO) (solder_mask_margin 0.07))
    (pad 33 smd rect (at -0.7 -0.7 180) (size 1.17 1.17) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 0.7 0.7 180) (size 1.17 1.17) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at 0.7 -0.7 180) (size 1.17 1.17) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 33 smd rect (at -0.7 0.7 180) (size 1.17 1.17) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5962A474)
    (at 96.52 119.38)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 0 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 EXT3v3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 PB9B))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 PB9A))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 PB6D/MISO))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 PB6C/SCLK))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 PB4C/CS))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 PL9B))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 PL9A))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 TMS))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 TCK))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 TDI))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 TDO))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5962A48E)
    (at 83.82 147.32 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X05 (at 0 12.49 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 TMS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 TCK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 TDI))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 TDO))
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5914076C)
    (at 81.28 119.38)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 0 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 PB11A))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 PB11B))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 PB20C/SN))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 PB20D/MOSI))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 PR5D))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 PR5C))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 PT17D/DONE))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 PT15D/PROGRAMN))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 PT15C/JTAGENB))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 PT12D/SDA))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 PT12C/SCL))
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 59140720)
    (at 88.9 121.285 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -1.27 0.127 180) (layer F.Fab))
    (fp_text value 1uF (at 0.01778 0.00508 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 EXT3v3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 591406E9)
    (at 83.693 130.8735 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.3335 -0.127 90) (layer F.Fab))
    (fp_text value 100nF (at 0 0.02032 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 placed (layer F.Cu) (tedit 59110B6D)
    (at 86.36 128.778 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at -0.04064 -0.04572 180) (layer F.Fab))
    (fp_text user %R (at -1.26238 -0.0254 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59110B84)
    (at 92.6592 130.8735 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0.04318 0 90) (layer F.Fab))
    (fp_text user %R (at 1.3589 -0.00254 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59110B8F)
    (at 94.0562 130.8735 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0.02286 0.0127 90) (layer F.Fab))
    (fp_text user %R (at 1.4097 0.0762 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59140649)
    (at 92.71 134.9375 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -1.5875 0 270) (layer F.Fab))
    (fp_text value 10nF (at -0.01016 -0.0381 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5914066D)
    (at 91.8845 138.684)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.3335 0) (layer F.Fab))
    (fp_text value 4.7k (at -0.0635 0.0127) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 TCK))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59110B3A)
    (at 88.9 119.8245 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at -0.02286 -0.0254 180) (layer F.Fab))
    (fp_text user %R (at -1.2827 -0.01778 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 EXT3v3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59110B45)
    (at 88.9 122.7455 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at -0.00254 -0.02286 180) (layer F.Fab))
    (fp_text user %R (at -1.27 0.0635 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 EXT3v3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59110B79)
    (at 85.09 130.8735 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0.04318 0.01016 90) (layer F.Fab))
    (fp_text user %R (at 1.3081 0.01524 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 591406C1)
    (at 91.8845 137.2235)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 1.3335 -0.0635) (layer F.Fab))
    (fp_text value 100nF (at 0.06858 0.01778) (layer F.Fab))
    (fp_text user %R (at 1.3335 -0.0635) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5914069B)
    (at 85.09 135.636 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -1.27 0 270) (layer F.Fab) hide)
    (fp_text value 10nF (at -0.00254 -0.01016 270) (layer F.Fab))
    (fp_text user %R (at -1.27 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors_SMD:L_0603 (layer F.Cu) (tedit 59140711)
    (at 89.662 124.841 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 0.762 90) (layer F.Fab))
    (fp_text value bead (at 0.03048 -0.00508 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 EXT3v3))
    (model Inductors_SMD.3dshapes\L_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text SCL/11 (at 82.9945 145.542) (layer B.SilkS))
  (gr_text SDA/10 (at 82.55 144.018) (layer B.SilkS))
  (gr_text JTGNB/9 (at 82.55 142.24) (layer B.SilkS))
  (gr_text PGMN/8 (at 82.55 139.7) (layer B.SilkS))
  (gr_text DONE/7 (at 82.55 137.16) (layer B.SilkS))
  (gr_text 6 (at 82.55 134.62) (layer B.SilkS))
  (gr_text 5 (at 82.55 132.08) (layer B.SilkS))
  (gr_text MOSI/4 (at 82.55 129.54) (layer B.SilkS))
  (gr_text SN/3 (at 82.55 127) (layer B.SilkS))
  (gr_text 2 (at 82.55 124.46) (layer B.SilkS))
  (gr_text 1 (at 82.55 121.92) (layer B.SilkS))
  (gr_text GND (at 82.55 119.38) (layer B.SilkS))
  (gr_text 12/TDO (at 94.869 145.542) (layer B.SilkS))
  (gr_text 13/TDI (at 95.25 144.018) (layer B.SilkS))
  (gr_text 14/TCK (at 95.25 142.24) (layer B.SilkS))
  (gr_text 15/TMS (at 95.25 139.7) (layer B.SilkS))
  (gr_text 16 (at 95.25 137.16) (layer B.SilkS))
  (gr_text 17 (at 95.25 134.62) (layer B.SilkS))
  (gr_text 18/CS (at 95.25 132.08) (layer B.SilkS))
  (gr_text 19/SCLK (at 95.25 129.54) (layer B.SilkS))
  (gr_text 20/MISO (at 95.25 127) (layer B.SilkS))
  (gr_text 21 (at 95.25 124.46) (layer B.SilkS))
  (gr_text 22 (at 95.25 121.92) (layer B.SilkS))
  (gr_text 3.3v (at 95.25 119.38) (layer B.SilkS))
  (gr_text Ax (at 88.138 138.43) (layer F.SilkS))
  (gr_text TinyFPGA (at 88.65 141.5) (layer F.SilkS))
  (gr_text 22 (at 95.25 121.92) (layer F.SilkS))
  (gr_text 21 (at 95.25 124.46) (layer F.SilkS))
  (gr_text 20 (at 95.25 127) (layer F.SilkS))
  (gr_text 19 (at 95.25 129.032) (layer F.SilkS))
  (gr_text 18 (at 95.25 132.842) (layer F.SilkS))
  (gr_text 17 (at 95.25 134.62) (layer F.SilkS))
  (gr_text 16 (at 95.25 137.16) (layer F.SilkS))
  (gr_text 15 (at 95.25 139.7) (layer F.SilkS))
  (gr_text 14 (at 95.25 141.986) (layer F.SilkS))
  (gr_text 3.3v (at 95.25 119.38) (layer F.SilkS))
  (gr_text TDO (at 93.98 145.796 90) (layer F.SilkS))
  (gr_text GND (at 91.44 145.796 90) (layer F.SilkS))
  (gr_text TDI (at 88.9 145.796 90) (layer F.SilkS))
  (gr_text TCK (at 86.36 145.796 90) (layer F.SilkS))
  (gr_text TMS (at 83.82 145.796 90) (layer F.SilkS))
  (gr_text 9 (at 82.55 141.986) (layer F.SilkS))
  (gr_text 8 (at 82.55 139.7) (layer F.SilkS))
  (gr_text 7 (at 82.55 137.16) (layer F.SilkS))
  (gr_text 6 (at 82.55 134.62) (layer F.SilkS))
  (gr_text 5 (at 82.55 132.715) (layer F.SilkS))
  (gr_text 4 (at 82.55 129.032) (layer F.SilkS))
  (gr_text 3 (at 82.55 127) (layer F.SilkS))
  (gr_text 2 (at 82.55 124.46) (layer F.SilkS))
  (gr_text 1 (at 82.55 121.92) (layer F.SilkS))
  (gr_text GND (at 82.55 119.38) (layer F.SilkS))
  (gr_line (start 80.01 148.59) (end 80.01 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 148.59) (end 80.01 148.59) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 118.11) (end 97.79 148.59) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.01 118.11) (end 97.79 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.55 118.364) (xy 95.25 118.364) (xy 95.25 146.05) (xy 82.55 146.05)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.0254))
    (min_thickness 0.0254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.41 131.42) (xy 90.39 131.42) (xy 90.39 134.4) (xy 87.41 134.4)
      )
    )
  )
)
