(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(A1-Pad1)")
  (net 2 "unconnected-(A1-Pad2)")
  (net 3 "unconnected-(A1-Pad3)")
  (net 4 "GND")
  (net 5 "Net-(A1-Pad5)")
  (net 6 "Net-(A1-Pad6)")
  (net 7 "Net-(A1-Pad7)")
  (net 8 "Net-(A1-Pad8)")
  (net 9 "Net-(A1-Pad9)")
  (net 10 "Net-(A1-Pad11)")
  (net 11 "Net-(A1-Pad12)")
  (net 12 "Net-(A1-Pad13)")
  (net 13 "Net-(A1-Pad15)")
  (net 14 "Net-(A1-Pad16)")
  (net 15 "unconnected-(A1-Pad17)")
  (net 16 "unconnected-(A1-Pad18)")
  (net 17 "unconnected-(A1-Pad19)")
  (net 18 "unconnected-(A1-Pad20)")
  (net 19 "unconnected-(A1-Pad21)")
  (net 20 "Net-(A1-Pad22)")
  (net 21 "Net-(A1-Pad23)")
  (net 22 "Net-(A1-Pad24)")
  (net 23 "Net-(A1-Pad25)")
  (net 24 "unconnected-(A1-Pad28)")
  (net 25 "Net-(A1-Pad30)")
  (net 26 "Net-(C1-Pad2)")
  (net 27 "Net-(C12-Pad1)")
  (net 28 "Net-(C13-Pad1)")
  (net 29 "Net-(J1-Pad1)")
  (net 30 "Net-(R4-Pad1)")
  (net 31 "unconnected-(U4-Pad4)")
  (net 32 "unconnected-(U5-Pad4)")
  (net 33 "unconnected-(U6-Pad4)")
  (net 34 "Net-(J1-Pad2)")
  (net 35 "Net-(R5-Pad1)")
  (net 36 "Net-(R6-Pad1)")
  (net 37 "Net-(A1-Pad14)")
  (net 38 "Net-(J1-Pad3)")
  (net 39 "Net-(J1-Pad5)")
  (net 40 "Net-(J1-Pad4)")
  (net 41 "Net-(J1-Pad6)")
  (net 42 "Net-(J1-Pad7)")
  (net 43 "Net-(R20-Pad1)")
  (net 44 "Net-(R21-Pad1)")
  (net 45 "Net-(R22-Pad1)")
  (net 46 "Net-(R23-Pad1)")
  (net 47 "Net-(R24-Pad1)")
  (net 48 "Net-(R25-Pad1)")
  (net 49 "Net-(R26-Pad1)")
  (net 50 "Net-(R27-Pad1)")
  (net 51 "Net-(R28-Pad1)")
  (net 52 "Net-(R29-Pad1)")
  (net 53 "Net-(R30-Pad1)")
  (net 54 "Net-(R31-Pad1)")
  (net 55 "Net-(R32-Pad1)")
  (net 56 "Net-(R33-Pad1)")
  (net 57 "Net-(R34-Pad1)")
  (net 58 "Net-(R35-Pad1)")
  (net 59 "Net-(R36-Pad1)")
  (net 60 "Net-(J1-Pad8)")
  (net 61 "Net-(J1-Pad9)")
  (net 62 "Net-(J1-Pad10)")
  (net 63 "Net-(J1-Pad11)")
  (net 64 "unconnected-(J1-Pad12)")
  (net 65 "unconnected-(J1-Pad13)")
  (net 66 "Net-(J1-Pad14)")
  (net 67 "Net-(J1-Pad15)")
  (net 68 "Net-(J1-Pad16)")
  (net 69 "Net-(J1-Pad17)")
  (net 70 "Net-(J1-Pad19)")
  (net 71 "Net-(J1-Pad20)")
  (net 72 "Net-(J1-Pad21)")
  (net 73 "Net-(J1-Pad22)")
  (net 74 "Net-(J1-Pad23)")
  (net 75 "unconnected-(J1-Pad24)")
  (net 76 "unconnected-(J1-Pad25)")
  (net 77 "Net-(R1-Pad1)")
  (net 78 "Net-(R2-Pad1)")
  (net 79 "Net-(U10-Pad2)")
  (net 80 "Net-(R3-Pad1)")
  (net 81 "Net-(R9-Pad1)")
  (net 82 "Net-(R10-Pad1)")
  (net 83 "Net-(R11-Pad1)")
  (net 84 "Net-(R12-Pad1)")
  (net 85 "Net-(R13-Pad1)")
  (net 86 "Net-(R14-Pad1)")
  (net 87 "Net-(R15-Pad1)")
  (net 88 "Net-(R16-Pad1)")
  (net 89 "Net-(R17-Pad1)")
  (net 90 "Net-(U12-Pad2)")
  (net 91 "Net-(R18-Pad1)")
  (net 92 "Net-(R19-Pad1)")
  (net 93 "Net-(R37-Pad2)")
  (net 94 "Net-(R38-Pad2)")
  (net 95 "unconnected-(U13-Pad4)")
  (net 96 "unconnected-(U15-Pad4)")
  (net 97 "unconnected-(U16-Pad4)")
  (net 98 "unconnected-(U17-Pad4)")
  (net 99 "unconnected-(U18-Pad4)")
  (net 100 "unconnected-(U19-Pad4)")
  (net 101 "unconnected-(U20-Pad4)")
  (net 102 "unconnected-(U21-Pad4)")
  (net 103 "unconnected-(U22-Pad4)")
  (net 104 "unconnected-(U23-Pad4)")
  (net 105 "unconnected-(U24-Pad4)")
  (net 106 "unconnected-(U25-Pad4)")
  (net 107 "unconnected-(U26-Pad4)")
  (net 108 "unconnected-(U27-Pad4)")
  (net 109 "unconnected-(U28-Pad4)")
  (net 110 "unconnected-(U29-Pad4)")
  (net 111 "unconnected-(U30-Pad4)")
  (net 112 "Net-(A1-Pad27)")
  (net 113 "Net-(R39-Pad2)")
  (net 114 "Net-(R40-Pad2)")
  (net 115 "Net-(R41-Pad2)")
  (net 116 "Net-(R42-Pad2)")
  (net 117 "Net-(R43-Pad2)")
  (net 118 "Net-(R44-Pad2)")
  (net 119 "Net-(R45-Pad2)")
  (net 120 "Net-(A1-Pad26)")
  (net 121 "Net-(R7-Pad1)")
  (net 122 "Net-(A1-Pad10)")
  (net 123 "unconnected-(U14-Pad4)")
  (net 124 "Net-(R55-Pad1)")
  (net 125 "Net-(R58-Pad1)")
  (net 126 "Net-(J1-Pad18)")
  (net 127 "Net-(U11-Pad2)")
  (net 128 "unconnected-(U1-Pad4)")
  (net 129 "Net-(U1-Pad2)")
  (net 130 "Net-(U2-Pad2)")
  (net 131 "unconnected-(U3-Pad4)")
  (net 132 "unconnected-(U2-Pad4)")
  (net 133 "Net-(U3-Pad2)")
  (net 134 "Net-(U37-Pad2)")
  (net 135 "unconnected-(U31-Pad4)")
  (net 136 "unconnected-(U32-Pad4)")
  (net 137 "Net-(U38-Pad5)")
  (net 138 "Net-(R8-Pad1)")
  (net 139 "Net-(U38-Pad7)")
  (net 140 "unconnected-(U7-Pad4)")
  (net 141 "Net-(U38-Pad4)")
  (net 142 "unconnected-(U8-Pad4)")
  (net 143 "Net-(U38-Pad2)")
  (net 144 "unconnected-(U9-Pad4)")
  (net 145 "unconnected-(U10-Pad4)")
  (net 146 "unconnected-(U11-Pad4)")
  (net 147 "unconnected-(U12-Pad4)")
  (net 148 "Net-(U39-Pad5)")
  (net 149 "Net-(U13-Pad2)")
  (net 150 "Net-(U14-Pad2)")
  (net 151 "Net-(U15-Pad2)")
  (net 152 "Net-(U16-Pad2)")
  (net 153 "Net-(U17-Pad2)")
  (net 154 "Net-(U18-Pad2)")
  (net 155 "Net-(U19-Pad2)")
  (net 156 "Net-(U20-Pad2)")
  (net 157 "Net-(U21-Pad2)")
  (net 158 "Net-(U22-Pad2)")
  (net 159 "Net-(U23-Pad2)")
  (net 160 "Net-(U25-Pad2)")
  (net 161 "Net-(U26-Pad2)")
  (net 162 "Net-(U27-Pad2)")
  (net 163 "Net-(U28-Pad2)")
  (net 164 "Net-(U29-Pad2)")
  (net 165 "Net-(U30-Pad2)")
  (net 166 "Net-(U31-Pad2)")
  (net 167 "Net-(U32-Pad2)")
  (net 168 "Net-(U33-Pad2)")
  (net 169 "unconnected-(U33-Pad4)")
  (net 170 "Net-(U34-Pad2)")
  (net 171 "unconnected-(U34-Pad4)")
  (net 172 "Net-(U35-Pad2)")
  (net 173 "unconnected-(U35-Pad4)")
  (net 174 "Net-(U36-Pad2)")
  (net 175 "unconnected-(U36-Pad4)")
  (net 176 "unconnected-(U37-Pad9)")
  (net 177 "unconnected-(U37-Pad10)")
  (net 178 "unconnected-(U37-Pad15)")
  (net 179 "unconnected-(U37-Pad16)")
  (net 180 "unconnected-(U38-Pad9)")
  (net 181 "unconnected-(U38-Pad10)")
  (net 182 "unconnected-(U38-Pad15)")
  (net 183 "unconnected-(U38-Pad16)")
  (net 184 "unconnected-(U39-Pad9)")
  (net 185 "unconnected-(U39-Pad10)")
  (net 186 "unconnected-(U39-Pad15)")
  (net 187 "unconnected-(U39-Pad16)")
  (net 188 "unconnected-(U40-Pad9)")
  (net 189 "unconnected-(U40-Pad10)")
  (net 190 "unconnected-(U40-Pad15)")
  (net 191 "unconnected-(U40-Pad16)")
  (net 192 "unconnected-(U41-Pad9)")
  (net 193 "unconnected-(U41-Pad10)")
  (net 194 "unconnected-(U41-Pad15)")
  (net 195 "unconnected-(U41-Pad16)")
  (net 196 "unconnected-(U42-Pad9)")
  (net 197 "unconnected-(U42-Pad10)")
  (net 198 "unconnected-(U42-Pad15)")
  (net 199 "unconnected-(U42-Pad16)")
  (net 200 "unconnected-(U43-Pad9)")
  (net 201 "unconnected-(U43-Pad10)")
  (net 202 "unconnected-(U43-Pad15)")
  (net 203 "unconnected-(U43-Pad16)")
  (net 204 "unconnected-(U44-Pad9)")
  (net 205 "unconnected-(U44-Pad10)")
  (net 206 "unconnected-(U44-Pad15)")
  (net 207 "unconnected-(U44-Pad16)")
  (net 208 "unconnected-(U45-Pad9)")
  (net 209 "unconnected-(U45-Pad10)")
  (net 210 "unconnected-(U45-Pad15)")
  (net 211 "unconnected-(U45-Pad16)")
  (net 212 "Net-(J5-Pad1)")
  (net 213 "Net-(U24-Pad2)")
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 147.32 72.39)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers F&B.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 123.19 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R34" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "Net-(R34-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(J1-Pad23)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.27 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V18" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 74 "Net-(J1-Pad23)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 63 "Net-(J1-Pad11)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 75.565 125.997699 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R42" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(R42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 85.09 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U24" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(R24-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "Net-(U24-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(J1-Pad20)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "unconnected-(U24-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 213 "Net-(U24-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 69.85 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(R20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J1-Pad19)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.07 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V8" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 39 "Net-(J1-Pad5)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 126 "Net-(J1-Pad18)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.785 95.25 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R56" (at 0 1.905) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 107.64 78.4225 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U38" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "Net-(U38-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(R38-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "Net-(U38-Pad4)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(U38-Pad5)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(R38-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(U38-Pad7)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(A1-Pad6)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 180 "unconnected-(U38-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "unconnected-(U38-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 182 "unconnected-(U38-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 183 "unconnected-(U38-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 95.25 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R57" (at 0 -1.905) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 75.565 131.077699 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 50.165 128.537699 -90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U40" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "Net-(U16-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(R40-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(U15-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "Net-(U13-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(R40-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(U14-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(A1-Pad8)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 188 "unconnected-(U40-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 189 "unconnected-(U40-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 190 "unconnected-(U40-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 191 "unconnected-(U40-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.815 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J1-Pad15)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 45.085 131.077699 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0.14058 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 126.055 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "Net-(R2-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(U2-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(J1-Pad14)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "unconnected-(U2-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(U2-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 95.885 128.537699 -90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U43" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 163 "Net-(U28-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(R43-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "Net-(U27-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 160 "Net-(U25-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(R43-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "Net-(U26-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(A1-Pad11)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 200 "unconnected-(U43-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 201 "unconnected-(U43-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 202 "unconnected-(U43-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 203 "unconnected-(U43-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 127 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U35" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(R35-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "Net-(U35-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(J1-Pad23)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "unconnected-(U35-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "Net-(U35-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 58.42 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U17" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Net-(R17-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "Net-(U17-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(J1-Pad18)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "unconnected-(U17-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "Net-(U17-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.195 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(R8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.435 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_GH_BM03B-GHS-TBT_1x03-1MP_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 133.985 73.66)
    (descr "JST GH series connector, BM03B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST GH side entry")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 5.08 -1.27) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Female" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.25 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 0 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 1.25 1.95) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "MP" smd roundrect (at -3.1 -1.4) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect (at 3.1 -1.4) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM03B-GHS-TBT_1x03-1MP_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.85 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 1.715 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(R19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.57 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(R32-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J1-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.45 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V7" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 69 "Net-(J1-Pad17)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 39 "Net-(J1-Pad5)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.38 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(R33-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(J1-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R52" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(A1-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 100.33 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U28" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(R28-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "Net-(U28-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(J1-Pad9)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "unconnected-(U28-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "Net-(U28-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.14 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R29" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R29-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J1-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.625 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R47" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(A1-Pad12)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.03 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V16" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 73 "Net-(J1-Pad22)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 62 "Net-(J1-Pad10)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 119.38 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U33" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(R33-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "Net-(U33-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(J1-Pad10)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "unconnected-(U33-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "Net-(U33-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 42.545 95.25 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0.14058 -1.34 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 110.815 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U6" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(R6-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Net-(U38-Pad7)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(J1-Pad15)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(U6-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Net-(U38-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.66 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(R21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(J1-Pad19)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-223_ST_LIT:SOT-223_ST_LIT" (layer "F.Cu")
    (tedit 0)
    (at 38.735 100.33 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U47" (at 3.82 -3.175 90) (layer "F.SilkS"))
    (fp_text value "LT3088EST-PBF" (at -4.445 -0.635 180) (layer "F.SilkS"))
    (fp_text user "*" (at 0 0 90) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2987 3.4925 90) (size 0.889 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(C13-Pad1)") (pinfunction "SET") (pintype "input"))
    (pad "2" smd rect (at 0 3.4925 90) (size 0.889 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(A1-Pad25)") (pinfunction "OUT") (pintype "output"))
    (pad "3" smd rect (at 2.2987 3.4925 90) (size 0.889 1.016) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "Net-(A1-Pad27)") (pinfunction "IN") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 71.12 96.52)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R58" (at -0.559999 -1.43) (layer "F.SilkS"))
    (fp_text value "0.1" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(R58-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.9 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(J1-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.785 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R51" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(A1-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.81 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R36" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R36-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(J1-Pad11)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 62.865 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R53" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(A1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 103.195 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U8" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Net-(R8-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "Net-(U38-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J1-Pad3)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "unconnected-(U8-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "Net-(U38-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 114.625 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(R5-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(U38-Pad5)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(J1-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(U5-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "Net-(U38-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.76 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "Net-(R31-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(J1-Pad22)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.285 125.997699 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R45" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(R45-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 125.997699 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R41" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(R41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.79 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V14" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 72 "Net-(J1-Pad21)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 61 "Net-(J1-Pad9)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 142.374669 86.245 90)
    (descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 47.1mm mounting-hole-offset 47.1mm")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -16.62 -3.7 90) (layer "F.SilkS"))
    (fp_text value "DB25_Female_MountingHoles" (at -16.62 15.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -16.62 11.265 90) (layer "F.Fab"))
    (pad "0" thru_hole circle locked (at 6.93 0.3 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "PAD") (pintype "passive"))
    (pad "0" thru_hole circle locked (at -40.17 0.3 90) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "PAD") (pintype "passive"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.77 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.54 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -8.31 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at -11.08 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at -13.85 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at -16.62 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at -19.39 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at -22.16 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J1-Pad9)") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at -24.93 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J1-Pad10)") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle locked (at -27.7 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J1-Pad11)") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle locked (at -30.47 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 64 "unconnected-(J1-Pad12)") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle locked (at -33.24 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 65 "unconnected-(J1-Pad13)") (pinfunction "13") (pintype "passive"))
    (pad "14" thru_hole circle locked (at -1.385 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J1-Pad14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle locked (at -4.155 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J1-Pad15)") (pinfunction "P15") (pintype "passive"))
    (pad "16" thru_hole circle locked (at -6.925 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J1-Pad16)") (pinfunction "P16") (pintype "passive"))
    (pad "17" thru_hole circle locked (at -9.695 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad17)") (pinfunction "P17") (pintype "passive"))
    (pad "18" thru_hole circle locked (at -12.465 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(J1-Pad18)") (pinfunction "P18") (pintype "passive"))
    (pad "19" thru_hole circle locked (at -15.235 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J1-Pad19)") (pinfunction "P19") (pintype "passive"))
    (pad "20" thru_hole circle locked (at -18.005 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J1-Pad20)") (pinfunction "P20") (pintype "passive"))
    (pad "21" thru_hole circle locked (at -20.775 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(J1-Pad21)") (pinfunction "P21") (pintype "passive"))
    (pad "22" thru_hole circle locked (at -23.545 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(J1-Pad22)") (pinfunction "P22") (pintype "passive"))
    (pad "23" thru_hole circle locked (at -26.315 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(J1-Pad23)") (pinfunction "P23") (pintype "passive"))
    (pad "24" thru_hole circle locked (at -29.085 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 75 "unconnected-(J1-Pad24)") (pinfunction "P24") (pintype "passive"))
    (pad "25" thru_hole circle locked (at -31.855 2.84 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 76 "unconnected-(J1-Pad25)") (pinfunction "P25") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-25_Female_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 130.81 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U36" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(R36-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "Net-(U36-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(J1-Pad11)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "unconnected-(U36-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "Net-(U36-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 45.085 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R46" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(A1-Pad13)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 107.95 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U30" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(R30-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "Net-(U30-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(J1-Pad22)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "unconnected-(U30-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "Net-(U30-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.96 80.9625 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R37" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(R37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.045 125.997699 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R44" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(R44-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.33 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(R28-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(J1-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 112.72 75.8825 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 88.9 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U25" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(R25-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "Net-(U25-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(J1-Pad8)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "unconnected-(U25-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "Net-(U25-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 111.76 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U31" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(R31-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "Net-(U31-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(J1-Pad22)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "unconnected-(U31-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "Net-(U31-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 87.955 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U12" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(R12-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(U12-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(J1-Pad4)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "unconnected-(U12-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "Net-(U12-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 96.52 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(J1-Pad21)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.95 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R30" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(R30-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(J1-Pad22)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 43.18 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J1-Pad17)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.17 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V13" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 60 "Net-(J1-Pad8)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 72 "Net-(J1-Pad21)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 112.72 80.9625 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R38" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(R38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 81.28 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U23" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(R23-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(U23-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(J1-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "unconnected-(U23-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(U23-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 122.88 78.4225 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U37" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(U37-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(R37-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(U3-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(U1-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(R37-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "Net-(U2-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(A1-Pad5)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 176 "unconnected-(U37-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 177 "unconnected-(U37-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 178 "unconnected-(U37-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 179 "unconnected-(U37-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.595 91.1225 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 29 "Net-(J1-Pad1)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 66 "Net-(J1-Pad14)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 122.245 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(R3-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Net-(U3-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(J1-Pad14)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "unconnected-(U3-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "Net-(U3-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 35.56 117.475 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.68 180) (layer "F.SilkS"))
    (fp_text value "100u" (at 0 1.68 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.09 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 1.705 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(R24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(J1-Pad20)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 77.47 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(R22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J1-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 69.85 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U20" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(R20-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "Net-(U20-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(J1-Pad19)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(U20-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "Net-(U20-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 71.12 104.14 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -0.14058 1.759999 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.285 131.077699 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.865 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.74538 -0.022324 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 77.47 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U22" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(R22-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "Net-(U22-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(J1-Pad7)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "unconnected-(U22-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "Net-(U22-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.28 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "Net-(R23-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(J1-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.005 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(J1-Pad15)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 38.735 110.49)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R60" (at 0 1.905) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 46.99 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U14" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "Net-(R14-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(U14-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(J1-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "unconnected-(U14-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(U14-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 59.69 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V9" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 126 "Net-(J1-Pad18)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 41 "Net-(J1-Pad6)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 118.435 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "Net-(R4-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(U37-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(J1-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(U4-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(U37-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 62.23 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U18" (at 0 -0.635) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.508 -0.127) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "Net-(R18-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "Net-(U18-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(J1-Pad6)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "unconnected-(U18-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "Net-(U18-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Connector_JST:JST_GH_BM03B-GHS-TBT_1x03-1MP_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 5B78AD87)
    (at 133.985 132.08 180)
    (descr "JST GH series connector, BM03B-GHS-TBT (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST GH side entry")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at -5.08 -0.635 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Female" (at 0 4 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.25 1.95 180) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 0 1.95 180) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 1.25 1.95 180) (size 0.6 1.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "MP" smd roundrect (at 3.1 -1.4 180) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "MP" smd roundrect (at -3.1 -1.4 180) (size 1 2.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM03B-GHS-TBT_1x03-1MP_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.705 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R49" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(A1-Pad10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 35.56 133.35)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers F&B.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.625 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(J1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.045 131.077699 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 126.365 128.537699 -90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U45" (at -2.807699 -3.81 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 174 "Net-(U36-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(R45-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 172 "Net-(U35-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 168 "Net-(U33-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(R45-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 170 "Net-(U34-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(A1-Pad13)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 208 "unconnected-(U45-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 209 "unconnected-(U45-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 210 "unconnected-(U45-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "unconnected-(U45-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 62.23 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(R18-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "Net-(J1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.61 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(R16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(J1-Pad18)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.495 91.1225 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V6" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 68 "Net-(J1-Pad16)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 40 "Net-(J1-Pad4)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 35.56 113.665 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.68 180) (layer "F.SilkS"))
    (fp_text value "100u" (at 0 1.68 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 92.4 78.4225 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U39" (at 0 -3.45 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(U12-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(R39-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(U11-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "Net-(U39-Pad5)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(R39-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(U10-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(A1-Pad7)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 184 "unconnected-(U39-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 185 "unconnected-(U39-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 186 "unconnected-(U39-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 187 "unconnected-(U39-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 115.57 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U32" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(R32-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "Net-(U32-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(J1-Pad10)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "unconnected-(U32-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "Net-(U32-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 74.93 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V11" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 70 "Net-(J1-Pad19)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 42 "Net-(J1-Pad7)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 123.19 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U34" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(R34-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "Net-(U34-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(J1-Pad23)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "unconnected-(U34-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "Net-(U34-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 67.945 99.695 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R55" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "100" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(R55-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "Net-(A1-Pad26)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99.385 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(R9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(J1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 50.855899 120.678999 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U15" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.028999 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(R15-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(U15-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(J1-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "unconnected-(U15-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(U15-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 55.245 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R50" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(A1-Pad9)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 43.18 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U13" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(R13-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(U13-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(J1-Pad17)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "unconnected-(U13-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(U13-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.65 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V17" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 62 "Net-(J1-Pad10)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 74 "Net-(J1-Pad23)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.355 91.1225 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 34 "Net-(J1-Pad2)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 67 "Net-(J1-Pad15)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 66.04 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U19" (at 0 -0.635) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.635 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "Net-(R19-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(U19-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(J1-Pad6)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "unconnected-(U19-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(U19-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.805 125.997699 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(R43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.575 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J1-Pad16)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 73.66 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U21" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(R21-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "Net-(U21-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(J1-Pad19)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "unconnected-(U21-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "Net-(U21-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 129.865 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(R1-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(U1-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(J1-Pad1)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "unconnected-(U1-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(U1-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "D22012_B_NKK:D22012_B_NKK" (layer "F.Cu")
    (tedit 0)
    (at 50.165 78.74 180)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 12.065 -4.421774) (layer "F.SilkS") hide)
    (fp_text value "D22018B" (at 0 -4.421774) (layer "F.SilkS") hide)
    (fp_text user "*" (at -0.635 -1.905) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad25)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 5.08 0 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask)
      (net 125 "Net-(R58-Pad1)") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 10.16 0 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask)
      (net 212 "Net-(J5-Pad1)") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at -2.54 -2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle (at 12.7 -2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "6" thru_hole circle (at -2.54 2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "7" thru_hole circle (at 12.7 2.54 180) (size 1.4986 1.4986) (drill 0.9906) (layers *.Cu *.Mask))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 80.645 128.537699 -90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U42" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 213 "Net-(U24-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(R42-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 159 "Net-(U23-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 157 "Net-(U21-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(R42-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "Net-(U22-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(A1-Pad10)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 196 "unconnected-(U42-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 197 "unconnected-(U42-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 198 "unconnected-(U42-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 199 "unconnected-(U42-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.245 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J1-Pad14)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 91.765 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U11" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(R11-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(U11-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(J1-Pad16)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 146 "unconnected-(U11-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 127 "Net-(U11-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.805 131.077699 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 65.405 128.537699 -90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U41" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 156 "Net-(U20-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(R41-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(U19-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "Net-(U17-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(R41-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "Net-(U18-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(A1-Pad9)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 192 "unconnected-(U41-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 193 "unconnected-(U41-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 194 "unconnected-(U41-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 195 "unconnected-(U41-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 147.32 133.35)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers F&B.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.71 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(R26-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(J1-Pad21)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.48 75.8825 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.405 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R54" (at -2.54 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(A1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:BNC_Amphenol_B6252HB-NPP3G-50_Horizontal" (layer "F.Cu")
    (tedit 5C13907B)
    (at 76.835 81.915)
    (descr "http://www.farnell.com/datasheets/612848.pdf")
    (tags "BNC Amphenol Horizontal")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 4) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial_Power" (at 0 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 212 "Net-(J5-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at -5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 -5.08) (size 3.5 7) (drill 2.01) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0) (size 1.6 2.5) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/BNC_Amphenol_B6252HB-NPP3G-50_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.48 81.1525 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R39" (at -0.19 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(R39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DCK0006A_N:DCK0006A_N" (layer "F.Cu")
    (tedit 0)
    (at 71.12 99.695 180)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U46" (at 0.635 -1.905) (layer "F.SilkS"))
    (fp_text value "INA213AIDCKT" (at -6.985 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0 0) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user ".Designator" (at -0.0508 -0.6604 90) (layer "Cmts.User"))
    (fp_text user ".Designator" (at -0.0508 -0.6604 90) (layer "F.Fab"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.124999 -0.650001 270) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "REF") (pintype "input"))
    (pad "2" smd rect (at -1.124999 0 270) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -1.124999 0.649999 270) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "Net-(A1-Pad27)") (pinfunction "V+") (pintype "power_in"))
    (pad "4" smd rect (at 1.125002 0.649999 270) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "Net-(R58-Pad1)") (pinfunction "IN+") (pintype "input"))
    (pad "5" smd rect (at 1.125002 0 270) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(C1-Pad2)") (pinfunction "IN-") (pintype "input"))
    (pad "6" smd rect (at 1.125002 -0.650001 270) (size 0.399999 0.850001) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "Net-(R55-Pad1)") (pinfunction "OUT") (pintype "output"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 82.55 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V12" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 42 "Net-(J1-Pad7)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 71 "Net-(J1-Pad20)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.41 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V15" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 61 "Net-(J1-Pad9)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 73 "Net-(J1-Pad22)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 45.085 125.807699 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R40" (at -0.19 -1.905 90) (layer "F.SilkS"))
    (fp_text value "0.5" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(R40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50.8 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 111.125 128.537699 -90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U44" (at 0 -3.81 90) (layer "F.SilkS"))
    (fp_text value "DRV8847SPWR" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(A1-Pad22)") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 167 "Net-(U32-Pad2)") (pinfunction "OUT1") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(R44-Pad2)") (pinfunction "ISEN12") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 166 "Net-(U31-Pad2)") (pinfunction "OUT2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "Net-(U29-Pad2)") (pinfunction "OUT4") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(R44-Pad2)") (pinfunction "ISEN34") (pintype "passive"))
    (pad "7" smd roundrect (at -2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 165 "Net-(U30-Pad2)") (pinfunction "OUT3") (pintype "output"))
    (pad "8" smd roundrect (at -2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(A1-Pad12)") (pinfunction "~{FAULT}") (pintype "open_collector"))
    (pad "9" smd roundrect (at 2.8625 2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 204 "unconnected-(U44-Pad9)") (pinfunction "IN3") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 205 "unconnected-(U44-Pad10)") (pinfunction "IN4") (pintype "input"))
    (pad "11" smd roundrect (at 2.8625 0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(A1-Pad24)") (pinfunction "SCL") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pinfunction "VM") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.8625 -0.325 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.8625 -0.975 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(A1-Pad23)") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2.8625 -1.625 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 206 "unconnected-(U44-Pad15)") (pinfunction "IN2") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 270) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 207 "unconnected-(U44-Pad16)") (pinfunction "IN1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 95.575 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U10" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(R10-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(U10-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(J1-Pad16)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "unconnected-(U10-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(U10-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.765 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(J1-Pad16)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.735 91.1225 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V4" (at -0.235 -1.715) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 67 "Net-(J1-Pad15)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 38 "Net-(J1-Pad3)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.96 75.8825 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 1.5875 -1.595 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.975 91.1225 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V2" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 66 "Net-(J1-Pad14)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 34 "Net-(J1-Pad2)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 54.61 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U16" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.030398 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(R16-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(U16-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "Net-(J1-Pad18)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "unconnected-(U16-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(U16-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 58.42 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(R17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(J1-Pad18)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R35" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(R35-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(J1-Pad23)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 107.005 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U7" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "Net-(R7-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "Net-(U38-Pad4)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(J1-Pad15)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "unconnected-(U7-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "Net-(U38-Pad4)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.115 91.1225 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V5" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 38 "Net-(J1-Pad3)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 68 "Net-(J1-Pad16)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 131.077699 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -0.14058 1.905 90) (layer "F.SilkS"))
    (fp_text value "0.1u" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 42.1 110.49)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R59" (at 0 1.905) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(A1-Pad14)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 35.56 72.39)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2_DIN965_Pad" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 4 "GND"))
  )
  (footprint "Connector_BarrelJack:BarrelJack_CUI_PJ-063AH_Horizontal" (layer "F.Cu")
    (tedit 5B0886BD)
    (at 62.23 82.335 180)
    (descr "Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf")
    (tags "barrel jack cui dc power")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -6.985 0.42) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial_Power" (at 0 13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 9 180) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 180) (size 4 2) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad30)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 6 180) (size 3.3 2) (drill oval 2.3 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "MP" thru_hole oval (at 4.5 7 180) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad "MP" thru_hole oval (at -4.5 7 180) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 104.14 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U29" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(R29-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "Net-(U29-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(J1-Pad9)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 110 "unconnected-(U29-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "Net-(U29-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.955 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(J1-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 46.99 117.742699 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(R14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(J1-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.055 89.2175)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.905 0 90) (layer "F.SilkS"))
    (fp_text value "50" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(J1-Pad14)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_DIP_SPSTx02_Slide_9.78x7.26mm_W7.62mm_P2.54mm" (layer "F.Cu")
    (tedit 5A4E1404)
    (at 81.3225 97.785)
    (descr "2x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x7.26mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.81 -3.42) (layer "F.SilkS"))
    (fp_text value "SW_DIP_x02" (at 3.81 5.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.27 1.27 90) (layer "F.Fab"))
    (fp_text user "on" (at 5.365 -1.4975) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad16)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad15)") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx02_Slide_9.78x7.26mm_W7.62mm_P2.54mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50.165 104.14 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R48" (at -2.54 0 180) (layer "F.SilkS"))
    (fp_text value "1k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(A1-Pad27)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(A1-Pad11)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 96.52 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U27" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(R27-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "Net-(U27-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(J1-Pad21)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "unconnected-(U27-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "Net-(U27-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 67.31 115.837699)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "V10" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "VC080505A150DP" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 41 "Net-(J1-Pad6)") (pintype "bidirectional"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 70 "Net-(J1-Pad19)") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 99.385 86.0425 -90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U9" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at 0.508 1.016) (layer "F.SilkS"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(R9-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "Net-(U39-Pad5)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(J1-Pad3)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(U9-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 270) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "Net-(U39-Pad5)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "SOT-753_1P6X2P9_ONS:SOT-753_1P6X2P9_ONS" (layer "F.Cu")
    (tedit 0)
    (at 92.71 120.917699 90)
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U26" (at 0.254 -0.508) (layer "F.SilkS"))
    (fp_text value "SBE805-TL-E" (at -0.254 0) (layer "F.SilkS"))
    (fp_text user "*" (at -0.367301 1.016) (layer "F.SilkS"))
    (fp_text user "0.102in/2.591mm" (at 0 -3.8608 90) (layer "Cmts.User"))
    (fp_text user "0.036in/0.903mm" (at -1.2954 3.8608 90) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0 90) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at -4.3434 0 90) (layer "Cmts.User"))
    (fp_text user "0.016in/0.406mm" (at 4.3434 -0.95 90) (layer "Cmts.User"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (fp_text user "*" (at -0.5461 -1.4072 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(R26-Pad1)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "2" smd rect (at 1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "Net-(U26-Pad2)") (pinfunction "CATHODE") (pintype "unspecified"))
    (pad "3" smd rect (at -1.2954 -0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(J1-Pad21)") (pinfunction "ANODE") (pintype "unspecified"))
    (pad "4" smd rect (at -1.2954 0 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "unconnected-(U26-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect (at -1.2954 0.950001 90) (size 0.903199 0.4064) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "Net-(U26-Pad2)") (pinfunction "ANODE") (pintype "unspecified"))
  )
  (footprint "Module:Arduino_Nano" (layer "B.Cu")
    (tedit 58ACAF70)
    (at 75.565 107.315 90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (property "Sheetfile" "RF_control_board_v4.1.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A1" (at 0 5.08) (layer "B.SilkS"))
    (fp_text value "Arduino_Nano_v3.x" (at 8.89 -19.05) (layer "B.Fab"))
    (fp_text user "USB" (at 7.62 -35.56 270 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 7.614999 -9.035001) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "unconnected-(A1-Pad1)") (pinfunction "D1/TX") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "unconnected-(A1-Pad2)") (pinfunction "D0/RX") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "unconnected-(A1-Pad3)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad5)") (pinfunction "D2") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad6)") (pinfunction "D3") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 0 -15.24 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad7)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 0 -17.78 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad8)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 -20.32 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad9)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at 0 -22.86 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(A1-Pad10)") (pinfunction "D7") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 -25.4 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad11)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 0 -27.94 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad12)") (pinfunction "D9") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 0 -30.48 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad13)") (pinfunction "D10") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 0 -33.02 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(A1-Pad14)") (pinfunction "D11") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at 0 -35.56 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad15)") (pinfunction "D12") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 15.24 -35.56 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad16)") (pinfunction "D13") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 15.24 -33.02 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(A1-Pad17)") (pinfunction "3V3") (pintype "power_out"))
    (pad "18" thru_hole oval (at 15.24 -30.48 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(A1-Pad18)") (pinfunction "AREF") (pintype "input"))
    (pad "19" thru_hole oval (at 15.24 -27.94 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(A1-Pad19)") (pinfunction "A0") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at 15.24 -25.4 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(A1-Pad20)") (pinfunction "A1") (pintype "bidirectional"))
    (pad "21" thru_hole oval (at 15.24 -22.86 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(A1-Pad21)") (pinfunction "A2") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 15.24 -20.32 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad22)") (pinfunction "A3") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 15.24 -17.78 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad23)") (pinfunction "A4") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 15.24 -15.24 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad24)") (pinfunction "A5") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 15.24 -12.7 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad25)") (pinfunction "A6") (pintype "bidirectional"))
    (pad "26" thru_hole oval (at 15.24 -10.16 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(A1-Pad26)") (pinfunction "A7") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 15.24 -7.62 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(A1-Pad27)") (pinfunction "+5V") (pintype "power_out"))
    (pad "28" thru_hole oval (at 15.24 -5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(A1-Pad28)") (pinfunction "~{RESET}") (pintype "input"))
    (pad "29" thru_hole oval (at 15.24 -2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "30" thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad30)") (pinfunction "VIN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 150.495 69.215) (end 32.385 136.525) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "DRV chips require\n>2.6 V to operate" (at 45.085 86.36) (layer "F.SilkS"))
  (gr_text "GND" (at 132.715 79.375 90) (layer "F.SilkS"))
  (gr_text "SDA" (at 133.985 79.375 90) (layer "F.SilkS"))
  (gr_text "MOUNT ARDUINO\nON REVERSE" (at 55.88 99.06) (layer "F.SilkS"))
  (gr_text "SCL" (at 135.255 79.375 90) (layer "F.SilkS"))
  (gr_text "bit 1" (at 86.995 97.79) (layer "F.SilkS"))
  (gr_text "SDA" (at 133.985 126.365 90) (layer "F.SilkS"))
  (gr_text "GND" (at 135.255 126.365 90) (layer "F.SilkS"))
  (gr_text "ARD" (at 40.64 73.66) (layer "F.SilkS"))
  (gr_text "Operate warm\nwithout varistors" (at 67.945 111.125) (layer "F.SilkS"))
  (gr_text "bit 0" (at 86.995 100.33) (layer "F.SilkS"))
  (gr_text "SCL" (at 132.715 126.365 90) (layer "F.SilkS"))
  (gr_text "SLAC National Accelerator Laboratory\nRF switch control board \nv4.2 - 08/11/2023\nTaj Dyson (tdyson@stanford.edu)" (at 112.395 102.87) (layer "F.SilkS"))
  (gr_text "EXT" (at 50.8 73.66) (layer "F.SilkS"))
  (zone (net 4) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.227612 70.474086)
        (xy 149.225724 135.277594)
        (xy 33.654858 135.279001)
        (xy 33.656746 70.498719)
      )
    )
  )
)
