(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 15)
    (no_connects 0)
    (area 142.519399 100.253799 153.035001 117.195601)
    (thickness 1.6)
    (drawings 12)
    (tracks 66)
    (zones 0)
    (modules 12)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (34 B.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.3048)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(P2-Pad1)")
  (net 4 "Net-(P6-Pad1)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R3-Pad2)")
  (net 7 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.635)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U1-Pad5)")
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5DE173DF)
    (at 150.4188 101.2952 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -10.0711 -2.1336 180) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5DE0C183)
    (at 149.1869 111.7346)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 8.8011 -4.8006 90) (layer F.SilkS) hide)
    (fp_text value TLC555 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 3 "Net-(P2-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 6 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 7 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 3 "Net-(P2-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5DE17443)
    (at 146.4691 107.188)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 12.7889 6.7564) (layer F.SilkS) hide)
    (fp_text value - (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5DE1742C)
    (at 151.8539 104.2797)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 11.5189 -4.6736) (layer F.SilkS) hide)
    (fp_text value + (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5DE17449)
    (at 151.8158 116.0272)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 10.2489 8.0264) (layer F.SilkS) hide)
    (fp_text value O (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(P6-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5DE17446)
    (at 144.018 115.697)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 12.7889 -0.8636) (layer F.SilkS) hide)
    (fp_text value C (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(P2-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5DE17432)
    (at 144.018 101.727)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 12.7889 1.6764) (layer F.SilkS) hide)
    (fp_text value C (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(P2-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5DE1743A)
    (at 144.018 108.712)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 12.7889 4.2164) (layer F.SilkS) hide)
    (fp_text value G (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5DE1743E)
    (at 150.5966 107.2007 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -8.8011 -5.9436 180) (layer F.SilkS) hide)
    (fp_text value .1 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5DE1742F)
    (at 147.7772 104.1654 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -11.3411 1.6764 180) (layer F.SilkS) hide)
    (fp_text value 22K (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 3 "Net-(P2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5DE17436)
    (at 147.7645 116.1161 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -11.3411 5.4864 180) (layer F.SilkS) hide)
    (fp_text value 1K (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 4 "Net-(P6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Mask)
      (net 6 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Symbol_6.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 147.574 103.886 270)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0 270) (layer B.Fab) hide)
  )
  (gr_text "cap2pi\nmincepi" (at 148.082 111.76 90) (layer B.SilkS))
  (gr_text OUT (at 150.31 114.96) (layer F.SilkS))
  (gr_text 3v3 (at 150.368 102.87) (layer F.SilkS))
  (gr_text GND (at 145.034 105.918) (layer F.SilkS))
  (gr_text 102 (at 146.44 114.92) (layer F.SilkS))
  (gr_text 104 (at 150.622 105.664) (layer F.SilkS))
  (gr_text 223 (at 144.272 104.267) (layer F.SilkS))
  (gr_text 105 (at 146.939 101.346) (layer F.SilkS))
  (gr_line (start 142.6464 117.0686) (end 142.6464 100.3808) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 152.908 117.0686) (end 142.6464 117.0686) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 152.908 100.3808) (end 152.908 117.0686) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 142.6464 100.3808) (end 152.908 100.3808) (angle 90) (layer Edge.Cuts) (width 0.254))
)
