(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 48)
    (no_connects 0)
    (area 71.184699 41.809599 98.309501 84.885601)
    (thickness 1.6)
    (drawings 11)
    (tracks 297)
    (zones 0)
    (modules 16)
    (nets 44)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(8MHz1-Pad1)")
  (net 4 "Net-(8MHz1-Pad2)")
  (net 5 "Net-(ANT1-Pad1)")
  (net 6 /B0)
  (net 7 /B2)
  (net 8 /B3)
  (net 9 /B4)
  (net 10 /MISO)
  (net 11 /SCK)
  (net 12 /MOSI)
  (net 13 /RST)
  (net 14 /CS)
  (net 15 "Net-(U1-Pad12)")
  (net 16 "Net-(U1-Pad8)")
  (net 17 "Net-(U1-Pad6)")
  (net 18 "Net-(U1-Pad5)")
  (net 19 "Net-(U1-Pad4)")
  (net 20 "Net-(U1-Pad3)")
  (net 21 "Net-(U1-Pad2)")
  (net 22 /IRQ)
  (net 23 "Net-(U1-Pad18)")
  (net 24 "Net-(U1-Pad19)")
  (net 25 "Net-(U1-Pad20)")
  (net 26 "Net-(U2-Pad16)")
  (net 27 /D6)
  (net 28 "Net-(U2-Pad12)")
  (net 29 "Net-(U2-Pad11)")
  (net 30 "Net-(U2-Pad7)")
  (net 31 "Net-(U2-Pad6)")
  (net 32 "Net-(U1-Pad21)")
  (net 33 "Net-(U1-Pad22)")
  (net 34 "Net-(U1-Pad25)")
  (net 35 "Net-(U1-Pad33)")
  (net 36 "Net-(U1-Pad36)")
  (net 37 "Net-(U1-Pad37)")
  (net 38 "Net-(U1-Pad38)")
  (net 39 "Net-(U1-Pad39)")
  (net 40 "Net-(U1-Pad40)")
  (net 41 "Net-(U1-Pad41)")
  (net 42 "Net-(U1-Pad42)")
  (net 43 "Net-(U1-Pad31)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /B0)
    (add_net /B2)
    (add_net /B3)
    (add_net /B4)
    (add_net /CS)
    (add_net /D6)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(8MHz1-Pad1)")
    (add_net "Net-(8MHz1-Pad2)")
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad33)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net VCC)
  )
  (module BATTCOM_20MM_PTH (layer Top) (tedit 0)
    (at 84.7217 52.9336)
    (fp_text reference BAT1 (at -6.985 -0.635) (layer F.SilkS))
    (fp_text value BATTERY (at -6.985 0.635) (layer F.SilkS))
    (pad 1 thru_hole oval (at -10.5 0 90) (size 5.5626 2.7813) (drill 1.8542) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 10.5 0 90) (size 5.5626 2.7813) (drill 1.8542) (layers *.Cu *.Mask))
    (pad 2 smd rect (at 0 0) (size 4.064 4.064) (layers Top F.Paste F.Mask)
      (net 1 GND))
  )
  (module 2X3 (layer Bottom) (tedit 0)
    (at 90.424 80.01 90)
    (fp_text reference JP1 (at -1.27 4.445 90) (layer B.SilkS))
    (fp_text value AVR_PRG (at -1.27 -3.175 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6256 1.6256) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /MISO))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.6256 1.6256) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.6256 1.6256) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /SCK))
    (pad 4 thru_hole circle (at 2.54 2.54 90) (size 1.6256 1.6256) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.6256 1.6256) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /RST))
    (pad 6 thru_hole circle (at 5.08 2.54 90) (size 1.6256 1.6256) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module BUTTON-CONDUCTIVE (layer Bottom) (tedit 0)
    (at 84.7471 58.0644 180)
    (fp_text reference B0 (at -0.889 3.048 180) (layer B.SilkS))
    (fp_text value BUTTON-CONDUCTIVESMD (at -1.016 -3.429 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.54 2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 6 /B0))
    (pad 2 smd rect (at 2.54 -2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
  )
  (module BUTTON-CONDUCTIVE (layer Bottom) (tedit 0)
    (at 76.8731 65.9384 180)
    (fp_text reference B3 (at -0.889 3.048 180) (layer B.SilkS))
    (fp_text value BUTTON-CONDUCTIVESMD (at -1.016 -3.429 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.54 2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 8 /B3))
    (pad 2 smd rect (at 2.54 -2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
  )
  (module BUTTON-CONDUCTIVE (layer Bottom) (tedit 0)
    (at 92.6211 65.9384 180)
    (fp_text reference B2 (at -0.889 3.048 180) (layer B.SilkS))
    (fp_text value BUTTON-CONDUCTIVESMD (at -1.016 -3.429 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.54 2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 7 /B2))
    (pad 2 smd rect (at 2.54 -2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
  )
  (module BUTTON-CONDUCTIVE (layer Bottom) (tedit 0)
    (at 84.7471 65.9384 180)
    (fp_text reference B4 (at -0.889 3.048 180) (layer B.SilkS))
    (fp_text value BUTTON-CONDUCTIVESMD (at -1.016 -3.429 180) (layer B.SilkS))
    (pad 1 smd rect (at 2.54 2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 9 /B4))
    (pad 2 smd rect (at 2.54 -2.54 180) (size 0.2032 0.2032) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
  )
  (module Crystals:Crystal_SMD_0603_2Pads_obsolete (layer Top) (tedit 0)
    (at 74.676 82.55 180)
    (descr "Crystal, Quarz, SMD, 0603, 2 Pads, Obsolete!, NOT for new designs!,")
    (tags "Crystal Quarz SMD 0603 2 Pads")
    (attr smd)
    (fp_text reference 8MHz1 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value CRYSTAL_2 (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -2.25044 0 180) (size 1.6002 2.4003) (layers Top F.Paste F.Mask)
      (net 3 "Net-(8MHz1-Pad1)"))
    (pad 2 smd rect (at 2.25044 0 180) (size 1.6002 2.4003) (layers Top F.Paste F.Mask)
      (net 4 "Net-(8MHz1-Pad2)"))
  )
  (module open-project:1PIN_S_SMD (layer Bottom) (tedit 514E2455)
    (at 86.106 69.342)
    (descr "1 pin SMD")
    (tags DEV)
    (fp_text reference ANT1 (at -0.01 1.52) (layer B.SilkS) hide)
    (fp_text value ANT (at -0.01 -1.73) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers Bottom B.Paste B.SilkS B.Mask)
      (net 5 "Net-(ANT1-Pad1)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 541A9B4D)
    (at 74.676 80.01 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value CAP (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 3 "Net-(8MHz1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 541A9B4D)
    (at 73.152 77.978)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9) (layer F.SilkS))
    (fp_text value CAP (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 4 "Net-(8MHz1-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 541A9B4D)
    (at 73.152 75.692 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 541A9B4D)
    (at 73.406 69.596 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 541A9B4D)
    (at 73.406 71.374 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer Top) (tedit 541A9B4D)
    (at 78.232 77.47)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers Top F.Paste F.Mask)
      (net 14 /CS))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer Bottom) (tedit 54130A77)
    (at 79.502 77.724 180)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 7.45 180) (layer B.SilkS))
    (fp_text value ATmega32U4 (at 0 -7.45 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -5.7 4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 22 /IRQ))
    (pad 2 smd rect (at -5.7 3.2 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 21 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -5.7 2.4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 20 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -5.7 1.6 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 19 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -5.7 0.8 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 18 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -5.7 0 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 17 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -5.7 -0.8 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 2 VCC))
    (pad 8 smd rect (at -5.7 -1.6 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 16 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -5.7 -2.4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 11 /SCK))
    (pad 10 smd rect (at -5.7 -3.2 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 12 /MOSI))
    (pad 11 smd rect (at -5.7 -4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 10 /MISO))
    (pad 12 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 15 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 13 /RST))
    (pad 14 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 2 VCC))
    (pad 15 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(8MHz1-Pad2)"))
    (pad 17 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(8MHz1-Pad1)"))
    (pad 18 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 23 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 24 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 25 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 32 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 33 "Net-(U1-Pad22)"))
    (pad 23 smd rect (at 5.7 -4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 5.7 -3.2 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 2 VCC))
    (pad 25 smd rect (at 5.7 -2.4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 34 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 5.7 -1.6 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 6 /B0))
    (pad 27 smd rect (at 5.7 -0.8 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 27 /D6))
    (pad 28 smd rect (at 5.7 0 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 14 /CS))
    (pad 29 smd rect (at 5.7 0.8 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 9 /B4))
    (pad 30 smd rect (at 5.7 1.6 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 7 /B2))
    (pad 31 smd rect (at 5.7 2.4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 43 "Net-(U1-Pad31)"))
    (pad 32 smd rect (at 5.7 3.2 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 8 /B3))
    (pad 33 smd rect (at 5.7 4 180) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 35 "Net-(U1-Pad33)"))
    (pad 34 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 2 VCC))
    (pad 35 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 36 "Net-(U1-Pad36)"))
    (pad 37 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 37 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 38 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 39 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 40 "Net-(U1-Pad40)"))
    (pad 41 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 41 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 42 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers Bottom B.Paste B.Mask)
      (net 2 VCC))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RFM95W-868S2:XCVR_RFM95W-868S2 (layer Top) (tedit 0)
    (at 89.662 76.454 180)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U2 (at -5.06 -9.485 180) (layer F.SilkS))
    (fp_text value RFM95W-868S2 (at -4.275 9.465 180) (layer F.SilkS))
    (pad 1 smd rect (at -7.4 -7 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 2 smd rect (at -7.4 -5 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 10 /MISO) (solder_mask_margin 0.2))
    (pad 3 smd rect (at -7.4 -3 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 12 /MOSI) (solder_mask_margin 0.2))
    (pad 4 smd rect (at -7.4 -1 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 11 /SCK) (solder_mask_margin 0.2))
    (pad 5 smd rect (at -7.4 1 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 14 /CS) (solder_mask_margin 0.2))
    (pad 6 smd rect (at -7.4 3 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 31 "Net-(U2-Pad6)") (solder_mask_margin 0.2))
    (pad 7 smd rect (at -7.4 5 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 30 "Net-(U2-Pad7)") (solder_mask_margin 0.2))
    (pad 8 smd rect (at -7.4 7 180) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 9 smd rect (at 7.4 7) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 5 "Net-(ANT1-Pad1)") (solder_mask_margin 0.2))
    (pad 10 smd rect (at 7.4 5) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 11 smd rect (at 7.4 3) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 29 "Net-(U2-Pad11)") (solder_mask_margin 0.2))
    (pad 12 smd rect (at 7.4 1) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 28 "Net-(U2-Pad12)") (solder_mask_margin 0.2))
    (pad 13 smd rect (at 7.4 -1) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.2))
    (pad 14 smd rect (at 7.4 -3) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 22 /IRQ) (solder_mask_margin 0.2))
    (pad 15 smd rect (at 7.4 -5) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 27 /D6) (solder_mask_margin 0.2))
    (pad 16 smd rect (at 7.4 -7) (size 1.95 1.05) (layers Top F.Paste F.Mask)
      (net 26 "Net-(U2-Pad16)") (solder_mask_margin 0.2))
  )
  (gr_text "RFM95 LoraWAN Keyfob\nBrandon Byrne\nRev 0\n1/7/2017" (at 84.836 50.8) (layer B.SilkS))
  (gr_arc (start 71.2597 59.7408) (end 71.2597 58.547) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 98.2345 59.7408) (end 98.2345 60.9346) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.8891 41.8846) (end 71.2597 48.514) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.6051 41.8846) (end 98.2345 48.514) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.8891 41.8846) (end 91.6051 41.8846) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.2345 48.514) (end 98.2345 58.547) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.2345 60.9346) (end 98.2345 84.8106) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.2345 84.8106) (end 71.2597 84.8106) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.2597 48.514) (end 71.2597 58.547) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 71.2597 84.8106) (end 71.2597 60.9346) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69.85 40.894) (xy 96.266 40.386) (xy 107.188 86.614) (xy 76.454 94.488) (xy 62.23 80.772)
        (xy 65.532 42.418) (xy 69.85 40.894)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67.564 40.132) (xy 101.854 39.878) (xy 109.474 90.424) (xy 70.358 98.552) (xy 60.96 75.438)
        (xy 67.564 40.132)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.946 64.262) (xy 77.724 64.262) (xy 78.74 66.294) (xy 77.216 67.564) (xy 75.692 67.056)
        (xy 75.184 65.532) (xy 75.946 64.262)
      )
    )
  )
)
