(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~88~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 124)
    (zones 0)
    (modules 22)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.000001)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (user_via 0.4572 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 41.275 63.627)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(D1-Pad2)")
  (net 4 /SCL)
  (net 5 /SDA)
  (net 6 /INT2)
  (net 7 /INT1)
  (net 8 /SA0)
  (net 9 "Net-(U1-Pad11)")
  (net 10 "Net-(U1-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /INT1)
    (add_net /INT2)
    (add_net /SA0)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net VCC)
  )
  (module hardware:bunny-01 (layer B.Cu) (tedit 0)
    (at 53.721 63.119 180)
    (fp_text reference Ref** (at 0 0) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 0) (layer B.SilkS) hide)
  )
  (module hardware:ISM330DHCX (layer F.Cu) (tedit 0)
    (at 50.546 56.007)
    (fp_text reference Ref** (at 0 0) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 0) (layer F.SilkS) hide)
  )
  (module "hardware:ISM330DHCX Stemma interrupts" locked (layer F.Cu) (tedit 0)
    (at 51.562 68.199)
    (fp_text reference Ref** (at 0 0) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 0) (layer F.SilkS) hide)
  )
  (module hardware:Batería locked (layer F.Cu) (tedit 0)
    (at 43.942 69.342)
    (fp_text reference Ref** (at 0 0) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 0) (layer F.SilkS) hide)
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 52.705 59.944)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (fp_text user ΩY (at 0.508 1.27) (layer F.SilkS))
    (fp_text user ΩR (at -1.524 -1.778) (layer F.SilkS))
    (fp_text user ΩP (at 2.032 -1.016) (layer F.SilkS))
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 46.609 59.944)
    (fp_text reference "" (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (fp_text user Z (at 0.254 1.27) (layer F.SilkS))
    (fp_text user X (at 2.032 -1.016) (layer F.SilkS))
    (fp_text user Y (at -1.016 -1.778) (layer F.SilkS))
  )
  (module ISM330DHCXTR:PQFN50P250X300X86-14N (layer F.Cu) (tedit 6325F494)
    (at 48.895 63.627)
    (fp_text reference U1 (at 0.032 -2.4064) (layer F.Fab))
    (fp_text value ISM330DHCXTR (at 6.5344 2.4064) (layer F.Fab))
    (pad 14 smd roundrect (at -0.5 -0.91 270) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 5 /SDA))
    (pad 13 smd roundrect (at 0 -0.91 270) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 4 /SCL))
    (pad 12 smd roundrect (at 0.5 -0.91 270) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 2 VCC))
    (pad 11 smd roundrect (at 1.16 -0.75 180) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 9 "Net-(U1-Pad11)"))
    (pad 10 smd roundrect (at 1.16 -0.25 180) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 10 "Net-(U1-Pad10)"))
    (pad 9 smd roundrect (at 1.16 0.25 180) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 6 /INT2))
    (pad 8 smd roundrect (at 1.16 0.75 180) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 2 VCC))
    (pad 7 smd roundrect (at 0.5 0.91 90) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 1 GND))
    (pad 6 smd roundrect (at 0 0.91 90) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 1 GND))
    (pad 5 smd roundrect (at -0.5 0.91 90) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 2 VCC))
    (pad 4 smd roundrect (at -1.16 0.75) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 7 /INT1))
    (pad 3 smd roundrect (at -1.16 0.25) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 1 GND))
    (pad 2 smd roundrect (at -1.16 -0.25) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.16 -0.75) (size 0.61 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.09)
      (net 8 /SA0))
    (model ${KIPRJMOD}/kicad-library/ISM330DHCXTR/ISM330DHCXTR.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 6325F2F6)
    (at 43.307 70.993 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.Fab))
    (fp_text value Conn_01x04_Male (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /INT2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /INT1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 51.435 63.627 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.43 90) (layer F.Fab))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 48.895 65.913)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.Fab))
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 38.735 57.277)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference H4 (at 0 -2.75) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at -0.7112 -4.3688) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "SM04B-SRSS-TB(LF)(SN):JST_SM04B-SRSS-TB(LF)(SN)" locked (layer F.Cu) (tedit 62488FD6)
    (at 41.275 63.627 270)
    (fp_text reference J2 (at -0.545095 -1.767685 90) (layer F.Fab))
    (fp_text value "SM04B-SRSS-TB(LF)(SN)" (at 12.17039 5.74055 90) (layer F.Fab))
    (pad 4 smd rect (at 1.5 0 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 3 smd rect (at 0.5 0 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /SDA))
    (pad 2 smd rect (at -0.5 0 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -1.5 0 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S1 smd rect (at -2.8 3.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S2 smd rect (at 2.8 3.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model "${KIPRJMOD}/kicad-library/SM04B-SRSS-TB(LF)(SN)/SM04B-SRSS-TB_LF__SN_.step"
      (offset (xyz 0 -0.5 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "SM04B-SRSS-TB(LF)(SN):JST_SM04B-SRSS-TB(LF)(SN)" locked (layer F.Cu) (tedit 62488FD6)
    (at 56.515 63.627 90)
    (fp_text reference J1 (at -0.545095 -1.767685 90) (layer F.Fab))
    (fp_text value "SM04B-SRSS-TB(LF)(SN)" (at 12.17039 5.74055 90) (layer F.Fab))
    (pad 4 smd rect (at 1.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 3 smd rect (at 0.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /SDA))
    (pad 2 smd rect (at -0.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -1.5 0 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S1 smd rect (at -2.8 3.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad S2 smd rect (at 2.8 3.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model "${KIPRJMOD}/kicad-library/SM04B-SRSS-TB(LF)(SN)/SM04B-SRSS-TB_LF__SN_.step"
      (offset (xyz 0 -0.5 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 44.323 65.659 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.Fab))
    (fp_text value PU (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /SDA))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 44.323 67.183 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.43) (layer F.Fab))
    (fp_text value PU (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /SCL))
    (pad 1 smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745321)
    (at 42.291 57.277 270)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 90) (layer F.Fab))
    (fp_text value SolderJumper_3_Bridged12 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0 270) (size 1 1.5) (layers F.Cu F.Mask)
      (net 8 /SA0))
    (pad 3 smd custom (at 1.3 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 52.705 66.675)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.68) (layer F.Fab))
    (fp_text value 10uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 59.055 69.977)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference H3 (at 0 -2.75) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at 3.8862 4.4958) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 38.735 69.977)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference H2 (at 0 -2.75) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at 1.9812 4.3688) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_ISO7380_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 59.055 57.277 90)
    (descr "Mounting Hole 2.2mm, M2, ISO7380")
    (tags "mounting hole 2.2mm m2 iso7380")
    (attr virtual)
    (fp_text reference H1 (at 0 -2.75 90) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at 4.2926 4.699 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 3.5 3.5) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 53.975 70.231 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -1.8796 0.0254 180) (layer F.Fab) hide)
    (fp_text value ? (at 1.7272 0.2286 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 55.753 70.231 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D1 (at -2.2352 0.1016 180) (layer F.Fab) hide)
    (fp_text value LED (at -2.2098 0.0508 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "François\nGervais" (at 40.767 56.769) (layer B.SilkS))
  (gr_text v1.0.0 (at 44.323 68.961) (layer B.SilkS))
  (gr_arc (start 59.055 57.277) (end 61.595 57.277) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 61.595 69.977) (end 61.595 57.277) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38.735 69.977) (end 36.195 69.977) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 36.195 57.277) (end 36.195 69.977) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 59.055 54.737) (end 38.735 54.737) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 59.055 69.977) (end 59.055 72.517) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 38.735 72.517) (end 59.055 72.517) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38.735 57.277) (end 38.735 54.737) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 61.722 72.644) (xy 36.068 72.644) (xy 36.068 54.61) (xy 61.722 54.61)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer In2.Cu) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.304) (thermal_bridge_width 0.304))
    (polygon
      (pts
        (xy 61.722 72.644) (xy 36.068 72.644) (xy 36.068 54.61) (xy 61.722 54.61)
      )
    )
  )
)
