(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 359)
    (no_connects 0)
    (area 107.463829 42.696129 175.076371 132.558671)
    (thickness 1.6)
    (drawings 19)
    (tracks 2088)
    (zones 0)
    (modules 101)
    (nets 139)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.27)
    (user_trace_width 0.1524)
    (user_trace_width 0.508)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.00254)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEEFFF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory plots))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 +5V)
  (net 3 SYS_5V)
  (net 4 GND)
  (net 5 +1V2)
  (net 6 PMOD1_A1)
  (net 7 PMOD1_B1)
  (net 8 PMOD1_A2)
  (net 9 PMOD1_B2)
  (net 10 PMOD1_A3)
  (net 11 PMOD1_B3)
  (net 12 PMOD1_A4)
  (net 13 PMOD1_B4)
  (net 14 PMOD2_A1)
  (net 15 PMOD2_B1)
  (net 16 PMOD2_A2)
  (net 17 PMOD2_B2)
  (net 18 PMOD2_A3)
  (net 19 PMOD2_B3)
  (net 20 PMOD2_A4)
  (net 21 PMOD2_B4)
  (net 22 GPMC_AD6)
  (net 23 GPMC_AD7)
  (net 24 GPMC_AD2)
  (net 25 GPMC_AD3)
  (net 26 GPMC_ADVN)
  (net 27 GPMC_OEN)
  (net 28 GPMC_BE0N)
  (net 29 GPMC_WEIN)
  (net 30 GPMC_AD13)
  (net 31 GPMC_AD12)
  (net 32 GPMC_AD9)
  (net 33 GPMC_AD10)
  (net 34 GPMC_AD15)
  (net 35 GPMC_AD14)
  (net 36 GPMC_AD11)
  (net 37 GPMC_CLK)
  (net 38 GPMC_AD8)
  (net 39 GPMC_CSN1)
  (net 40 GPMC_AD5)
  (net 41 GPMC_AD4)
  (net 42 GPMC_AD1)
  (net 43 GPMC_AD0)
  (net 44 BB_CFG_SCL)
  (net 45 BB_CFG_SDA)
  (net 46 BB_IRQ_FPGA_TO_ARM)
  (net 47 BB_IRQ_ARM_TO_FPGA)
  (net 48 SPI_SS)
  (net 49 SPI_MISO)
  (net 50 SPI_MOSI)
  (net 51 SPI_SCK)
  (net 52 "Net-(D5-Pad1)")
  (net 53 OSC_OUT)
  (net 54 "Net-(R11-Pad2)")
  (net 55 GROVE1_IO0)
  (net 56 GROVE1_IO1)
  (net 57 GROVE2_IO0)
  (net 58 GROVE2_IO1)
  (net 59 GROVE3_IO0)
  (net 60 GROVE3_IO1)
  (net 61 GROVE4_IO0)
  (net 62 GROVE4_IO1)
  (net 63 "Net-(U1-Pad133)")
  (net 64 ICE40_CDONE)
  (net 65 ICE40_CRESET)
  (net 66 USER_BTN0)
  (net 67 USER_BTN1)
  (net 68 SDRAM_D7)
  (net 69 SDRAM_D6)
  (net 70 SDRAM_D5)
  (net 71 SDRAM_D4)
  (net 72 SDRAM_D3)
  (net 73 SDRAM_D2)
  (net 74 SDRAM_D1)
  (net 75 SDRAM_D0)
  (net 76 SDRAM_A0)
  (net 77 SDRAM_A1)
  (net 78 SDRAM_A2)
  (net 79 SDRAM_A3)
  (net 80 SDRAM_A4)
  (net 81 SDRAM_A5)
  (net 82 SDRAM_A6)
  (net 83 SDRAM_A7)
  (net 84 SDRAM_A8)
  (net 85 SDRAM_A9)
  (net 86 SDRAM_A10)
  (net 87 SDRAM_A11)
  (net 88 SDRAM_A12)
  (net 89 SDRAM_BA0)
  (net 90 SDRAM_BA1)
  (net 91 USER_LED3)
  (net 92 USER_LED2)
  (net 93 USER_LED1)
  (net 94 USER_LED0)
  (net 95 "Net-(R18-Pad2)")
  (net 96 "Net-(R22-Pad1)")
  (net 97 "Net-(C44-Pad1)")
  (net 98 "Net-(C45-Pad1)")
  (net 99 SDRAM_WE)
  (net 100 SDRAM_CAS)
  (net 101 SDRAM_RAS)
  (net 102 SDRAM_CS)
  (net 103 SDRAM_CKE)
  (net 104 SDRAM_CLK)
  (net 105 SDRAM_DQM)
  (net 106 PMOD3_A1)
  (net 107 PMOD3_B1)
  (net 108 PMOD3_A2)
  (net 109 PMOD3_B2)
  (net 110 PMOD3_A3)
  (net 111 PMOD3_B3)
  (net 112 PMOD3_A4)
  (net 113 PMOD3_B4)
  (net 114 PMOD4_A1)
  (net 115 PMOD4_B1)
  (net 116 PMOD4_A2)
  (net 117 PMOD4_B2)
  (net 118 PMOD4_A3)
  (net 119 PMOD4_B3)
  (net 120 PMOD4_A4)
  (net 121 PMOD4_B4)
  (net 122 "Net-(R3-Pad1)")
  (net 123 USER_SW1)
  (net 124 USER_SW0)
  (net 125 BB_CDONE)
  (net 126 BB_CRESET)
  (net 127 "Net-(C1-Pad1)")
  (net 128 "Net-(C1-Pad2)")
  (net 129 "Net-(C2-Pad1)")
  (net 130 "Net-(C2-Pad2)")
  (net 131 "Net-(D1-Pad1)")
  (net 132 "Net-(D2-Pad1)")
  (net 133 "Net-(D3-Pad1)")
  (net 134 "Net-(D4-Pad1)")
  (net 135 "Net-(R10-Pad2)")
  (net 136 "Net-(R12-Pad2)")
  (net 137 "Net-(R17-Pad2)")
  (net 138 "Net-(R21-Pad1)")
  (net_class Default "To jest domyślna klasa połączeń."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V2)
    (add_net +3V3)
    (add_net +5V)
    (add_net BB_CDONE)
    (add_net BB_CFG_SCL)
    (add_net BB_CFG_SDA)
    (add_net BB_CRESET)
    (add_net BB_IRQ_ARM_TO_FPGA)
    (add_net BB_IRQ_FPGA_TO_ARM)
    (add_net GND)
    (add_net GPMC_AD0)
    (add_net GPMC_AD1)
    (add_net GPMC_AD10)
    (add_net GPMC_AD11)
    (add_net GPMC_AD12)
    (add_net GPMC_AD13)
    (add_net GPMC_AD14)
    (add_net GPMC_AD15)
    (add_net GPMC_AD2)
    (add_net GPMC_AD3)
    (add_net GPMC_AD4)
    (add_net GPMC_AD5)
    (add_net GPMC_AD6)
    (add_net GPMC_AD7)
    (add_net GPMC_AD8)
    (add_net GPMC_AD9)
    (add_net GPMC_ADVN)
    (add_net GPMC_BE0N)
    (add_net GPMC_CLK)
    (add_net GPMC_CSN1)
    (add_net GPMC_OEN)
    (add_net GPMC_WEIN)
    (add_net GROVE1_IO0)
    (add_net GROVE1_IO1)
    (add_net GROVE2_IO0)
    (add_net GROVE2_IO1)
    (add_net GROVE3_IO0)
    (add_net GROVE3_IO1)
    (add_net GROVE4_IO0)
    (add_net GROVE4_IO1)
    (add_net ICE40_CDONE)
    (add_net ICE40_CRESET)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C44-Pad1)")
    (add_net "Net-(C45-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad133)")
    (add_net OSC_OUT)
    (add_net PMOD1_A1)
    (add_net PMOD1_A2)
    (add_net PMOD1_A3)
    (add_net PMOD1_A4)
    (add_net PMOD1_B1)
    (add_net PMOD1_B2)
    (add_net PMOD1_B3)
    (add_net PMOD1_B4)
    (add_net PMOD2_A1)
    (add_net PMOD2_A2)
    (add_net PMOD2_A3)
    (add_net PMOD2_A4)
    (add_net PMOD2_B1)
    (add_net PMOD2_B2)
    (add_net PMOD2_B3)
    (add_net PMOD2_B4)
    (add_net PMOD3_A1)
    (add_net PMOD3_A2)
    (add_net PMOD3_A3)
    (add_net PMOD3_A4)
    (add_net PMOD3_B1)
    (add_net PMOD3_B2)
    (add_net PMOD3_B3)
    (add_net PMOD3_B4)
    (add_net PMOD4_A1)
    (add_net PMOD4_A2)
    (add_net PMOD4_A3)
    (add_net PMOD4_A4)
    (add_net PMOD4_B1)
    (add_net PMOD4_B2)
    (add_net PMOD4_B3)
    (add_net PMOD4_B4)
    (add_net SDRAM_A0)
    (add_net SDRAM_A1)
    (add_net SDRAM_A10)
    (add_net SDRAM_A11)
    (add_net SDRAM_A12)
    (add_net SDRAM_A2)
    (add_net SDRAM_A3)
    (add_net SDRAM_A4)
    (add_net SDRAM_A5)
    (add_net SDRAM_A6)
    (add_net SDRAM_A7)
    (add_net SDRAM_A8)
    (add_net SDRAM_A9)
    (add_net SDRAM_BA0)
    (add_net SDRAM_BA1)
    (add_net SDRAM_CAS)
    (add_net SDRAM_CKE)
    (add_net SDRAM_CLK)
    (add_net SDRAM_CS)
    (add_net SDRAM_D0)
    (add_net SDRAM_D1)
    (add_net SDRAM_D2)
    (add_net SDRAM_D3)
    (add_net SDRAM_D4)
    (add_net SDRAM_D5)
    (add_net SDRAM_D6)
    (add_net SDRAM_D7)
    (add_net SDRAM_DQM)
    (add_net SDRAM_RAS)
    (add_net SDRAM_WE)
    (add_net SPI_MISO)
    (add_net SPI_MOSI)
    (add_net SPI_SCK)
    (add_net SPI_SS)
    (add_net SYS_5V)
    (add_net USER_BTN0)
    (add_net USER_BTN1)
    (add_net USER_LED0)
    (add_net USER_LED1)
    (add_net USER_LED2)
    (add_net USER_LED3)
    (add_net USER_SW0)
    (add_net USER_SW1)
  )
  (module Housings_QFP:TQFP-144_20x20mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 144.808 80.545 270)
    (descr "P/PG-TQFP-144-2, -3, -7 (see MAXIM 21-0087.PDF and 90-0144.PDF)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at -10.795 -11.176 360) (layer F.SilkS))
    (fp_text value iCE40-HX4K-TQ144 (at 0 12.275 270) (layer F.Fab))
    (pad 1 smd rect (at -10.55 -8.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 GPMC_AD10))
    (pad 2 smd rect (at -10.55 -8.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 GPMC_AD9))
    (pad 3 smd rect (at -10.55 -7.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 GPMC_AD13))
    (pad 4 smd rect (at -10.55 -7.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 114 PMOD4_A1))
    (pad 5 smd rect (at -10.55 -6.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 6 smd rect (at -10.55 -6.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -10.55 -5.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 115 PMOD4_B1))
    (pad 8 smd rect (at -10.55 -5.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 116 PMOD4_A2))
    (pad 9 smd rect (at -10.55 -4.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 117 PMOD4_B2))
    (pad 10 smd rect (at -10.55 -4.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 118 PMOD4_A3))
    (pad 11 smd rect (at -10.55 -3.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 120 PMOD4_A4))
    (pad 12 smd rect (at -10.55 -3.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 121 PMOD4_B4))
    (pad 13 smd rect (at -10.55 -2.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 14 smd rect (at -10.55 -2.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 15 smd rect (at -10.55 -1.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 119 PMOD4_B3))
    (pad 16 smd rect (at -10.55 -1.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 GPMC_AD12))
    (pad 17 smd rect (at -10.55 -0.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 GPMC_BE0N))
    (pad 18 smd rect (at -10.55 -0.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 GPMC_WEIN))
    (pad 19 smd rect (at -10.55 0.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 GPMC_ADVN))
    (pad 20 smd rect (at -10.55 0.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 GPMC_OEN))
    (pad 21 smd rect (at -10.55 1.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 GPMC_AD2))
    (pad 22 smd rect (at -10.55 1.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 GPMC_AD3))
    (pad 23 smd rect (at -10.55 2.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 GPMC_AD6))
    (pad 24 smd rect (at -10.55 2.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 GPMC_AD7))
    (pad 25 smd rect (at -10.55 3.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 USER_BTN0))
    (pad 26 smd rect (at -10.55 3.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 USER_BTN1))
    (pad 27 smd rect (at -10.55 4.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 28 smd rect (at -10.55 4.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 94 USER_LED0))
    (pad 29 smd rect (at -10.55 5.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 93 USER_LED1))
    (pad 30 smd rect (at -10.55 5.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 31 smd rect (at -10.55 6.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 92 USER_LED2))
    (pad 32 smd rect (at -10.55 6.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 91 USER_LED3))
    (pad 33 smd rect (at -10.55 7.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 124 USER_SW0))
    (pad 34 smd rect (at -10.55 7.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 123 USER_SW1))
    (pad 35 smd rect (at -10.55 8.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad133)"))
    (pad 36 smd rect (at -10.55 8.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad133)"))
    (pad 37 smd rect (at -8.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 PMOD1_B1))
    (pad 38 smd rect (at -8.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 PMOD1_A1))
    (pad 39 smd rect (at -7.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 PMOD1_B2))
    (pad 40 smd rect (at -7.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 41 smd rect (at -6.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 PMOD1_A2))
    (pad 42 smd rect (at -6.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 PMOD1_B3))
    (pad 43 smd rect (at -5.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 PMOD1_A3))
    (pad 44 smd rect (at -5.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 PMOD1_B4))
    (pad 45 smd rect (at -4.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 PMOD1_A4))
    (pad 46 smd rect (at -4.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 47 smd rect (at -3.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 PMOD2_B1))
    (pad 48 smd rect (at -3.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 PMOD2_A1))
    (pad 49 smd rect (at -2.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 PMOD2_B2))
    (pad 50 smd rect (at -2.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad133)"))
    (pad 51 smd rect (at -1.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad133)"))
    (pad 52 smd rect (at -1.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 PMOD2_A2))
    (pad 53 smd rect (at -0.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(C2-Pad1)"))
    (pad 54 smd rect (at -0.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(C2-Pad2)"))
    (pad 55 smd rect (at 0.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 PMOD2_B3))
    (pad 56 smd rect (at 0.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 PMOD2_A3))
    (pad 57 smd rect (at 1.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 58 smd rect (at 1.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad133)"))
    (pad 59 smd rect (at 2.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 60 smd rect (at 2.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 PMOD2_B4))
    (pad 61 smd rect (at 3.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 OSC_OUT))
    (pad 62 smd rect (at 3.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 PMOD2_A4))
    (pad 63 smd rect (at 4.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 BB_IRQ_FPGA_TO_ARM))
    (pad 64 smd rect (at 4.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 BB_IRQ_ARM_TO_FPGA))
    (pad 65 smd rect (at 5.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 ICE40_CDONE))
    (pad 66 smd rect (at 5.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 ICE40_CRESET))
    (pad 67 smd rect (at 6.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 SPI_MISO))
    (pad 68 smd rect (at 6.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 SPI_MOSI))
    (pad 69 smd rect (at 7.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 70 smd rect (at 7.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 SPI_SCK))
    (pad 71 smd rect (at 8.25 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 SPI_SS))
    (pad 72 smd rect (at 8.75 10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 73 smd rect (at 10.55 8.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 GROVE1_IO1))
    (pad 74 smd rect (at 10.55 8.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 GROVE1_IO0))
    (pad 75 smd rect (at 10.55 7.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 GROVE2_IO1))
    (pad 76 smd rect (at 10.55 7.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 GROVE2_IO0))
    (pad 77 smd rect (at 10.55 6.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad133)"))
    (pad 78 smd rect (at 10.55 6.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 SDRAM_D7))
    (pad 79 smd rect (at 10.55 5.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 SDRAM_D6))
    (pad 80 smd rect (at 10.55 5.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 SDRAM_D5))
    (pad 81 smd rect (at 10.55 4.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 SDRAM_A4))
    (pad 82 smd rect (at 10.55 4.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 84 SDRAM_A8))
    (pad 83 smd rect (at 10.55 3.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 81 SDRAM_A5))
    (pad 84 smd rect (at 10.55 3.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 85 SDRAM_A9))
    (pad 85 smd rect (at 10.55 2.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 87 SDRAM_A11))
    (pad 86 smd rect (at 10.55 2.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 87 smd rect (at 10.55 1.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 88 SDRAM_A12))
    (pad 88 smd rect (at 10.55 1.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 103 SDRAM_CKE))
    (pad 89 smd rect (at 10.55 0.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 90 smd rect (at 10.55 0.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 82 SDRAM_A6))
    (pad 91 smd rect (at 10.55 -0.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 83 SDRAM_A7))
    (pad 92 smd rect (at 10.55 -0.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 93 smd rect (at 10.55 -1.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 104 SDRAM_CLK))
    (pad 94 smd rect (at 10.55 -1.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 105 SDRAM_DQM))
    (pad 95 smd rect (at 10.55 -2.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 SDRAM_D4))
    (pad 96 smd rect (at 10.55 -2.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 SDRAM_D0))
    (pad 97 smd rect (at 10.55 -3.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 SDRAM_D1))
    (pad 98 smd rect (at 10.55 -3.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 SDRAM_D2))
    (pad 99 smd rect (at 10.55 -4.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 SDRAM_D3))
    (pad 100 smd rect (at 10.55 -4.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 101 smd rect (at 10.55 -5.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 SDRAM_A3))
    (pad 102 smd rect (at 10.55 -5.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 GROVE3_IO1))
    (pad 103 smd rect (at 10.55 -6.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 104 smd rect (at 10.55 -6.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 GROVE3_IO0))
    (pad 105 smd rect (at 10.55 -7.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 GROVE4_IO1))
    (pad 106 smd rect (at 10.55 -7.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 GROVE4_IO0))
    (pad 107 smd rect (at 10.55 -8.25 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 106 PMOD3_A1))
    (pad 108 smd rect (at 10.55 -8.75 270) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D5-Pad1)"))
    (pad 109 smd rect (at 8.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 110 smd rect (at 8.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 107 PMOD3_B1))
    (pad 111 smd rect (at 7.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 112 smd rect (at 7.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 108 PMOD3_A2))
    (pad 113 smd rect (at 6.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 109 PMOD3_B2))
    (pad 114 smd rect (at 6.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 110 PMOD3_A3))
    (pad 115 smd rect (at 5.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 111 PMOD3_B3))
    (pad 116 smd rect (at 5.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 SDRAM_A2))
    (pad 117 smd rect (at 4.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 SDRAM_A1))
    (pad 118 smd rect (at 4.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 SDRAM_A0))
    (pad 119 smd rect (at 3.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 86 SDRAM_A10))
    (pad 120 smd rect (at 3.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 SDRAM_BA1))
    (pad 121 smd rect (at 2.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 89 SDRAM_BA0))
    (pad 122 smd rect (at 2.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 102 SDRAM_CS))
    (pad 123 smd rect (at 1.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 124 smd rect (at 1.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 101 SDRAM_RAS))
    (pad 125 smd rect (at 0.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 100 SDRAM_CAS))
    (pad 126 smd rect (at 0.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(C1-Pad2)"))
    (pad 127 smd rect (at -0.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(C1-Pad1)"))
    (pad 128 smd rect (at -0.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 99 SDRAM_WE))
    (pad 129 smd rect (at -1.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 112 PMOD3_A4))
    (pad 130 smd rect (at -1.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 113 PMOD3_B4))
    (pad 131 smd rect (at -2.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 132 smd rect (at -2.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 133 smd rect (at -3.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad133)"))
    (pad 134 smd rect (at -3.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 GPMC_AD0))
    (pad 135 smd rect (at -4.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 GPMC_AD4))
    (pad 136 smd rect (at -4.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 GPMC_AD1))
    (pad 137 smd rect (at -5.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 GPMC_CSN1))
    (pad 138 smd rect (at -5.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 GPMC_AD5))
    (pad 139 smd rect (at -6.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 GPMC_AD8))
    (pad 140 smd rect (at -6.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 141 smd rect (at -7.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 GPMC_AD11))
    (pad 142 smd rect (at -7.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 GPMC_CLK))
    (pad 143 smd rect (at -8.25 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 GPMC_AD15))
    (pad 144 smd rect (at -8.75 -10.55) (size 1.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 GPMC_AD14))
    (model Housings_QFP.3dshapes/TQFP-144_20x20mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP_1:TSOPII-54_10.16x22.22mm-Pitch0.8mm (layer F.Cu) (tedit 55BAC4E8)
    (at 144.4932 107.09056 180)
    (descr "TSOPII-54: Plastic Thin Small Outline Package; 54 leads; body width 10.16mm; (see 128m-as4c4m32s-tsopii.pdf and http://www.infineon.com/cms/packages/SMD_-_Surface_Mounted_Devices/P-PG-TSOPII/P-TSOPII-54-1.html)")
    (tags "TSOPII 0.8")
    (fp_text reference U6 (at -4.318 -11.938 180) (layer F.SilkS))
    (fp_text value MT48LC32M8A2P (at 0 12 180) (layer F.Fab))
    (pad 28 smd rect (at 5.53 10.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -5.53 -10.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -5.53 -9.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 75 SDRAM_D0))
    (pad 3 smd rect (at -5.53 -8.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -5.53 -8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -5.53 -7.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 74 SDRAM_D1))
    (pad 6 smd rect (at -5.53 -6.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 7 smd rect (at -5.53 -5.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -5.53 -4.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 73 SDRAM_D2))
    (pad 9 smd rect (at -5.53 -4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 10 smd rect (at -5.53 -3.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -5.53 -2.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 72 SDRAM_D3))
    (pad 12 smd rect (at -5.53 -1.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 13 smd rect (at -5.53 -0.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -5.53 0 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 15 smd rect (at -5.53 0.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -5.53 1.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 99 SDRAM_WE))
    (pad 17 smd rect (at -5.53 2.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 100 SDRAM_CAS))
    (pad 18 smd rect (at -5.53 3.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 101 SDRAM_RAS))
    (pad 19 smd rect (at -5.53 4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 102 SDRAM_CS))
    (pad 20 smd rect (at -5.53 4.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 89 SDRAM_BA0))
    (pad 21 smd rect (at -5.53 5.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 90 SDRAM_BA1))
    (pad 22 smd rect (at -5.53 6.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 86 SDRAM_A10))
    (pad 23 smd rect (at -5.53 7.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 76 SDRAM_A0))
    (pad 24 smd rect (at -5.53 8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 77 SDRAM_A1))
    (pad 25 smd rect (at -5.53 8.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 78 SDRAM_A2))
    (pad 26 smd rect (at -5.53 9.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 79 SDRAM_A3))
    (pad 27 smd rect (at -5.53 10.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 29 smd rect (at 5.53 9.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 80 SDRAM_A4))
    (pad 30 smd rect (at 5.53 8.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 81 SDRAM_A5))
    (pad 31 smd rect (at 5.53 8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 82 SDRAM_A6))
    (pad 32 smd rect (at 5.53 7.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 83 SDRAM_A7))
    (pad 33 smd rect (at 5.53 6.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 84 SDRAM_A8))
    (pad 34 smd rect (at 5.53 5.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 85 SDRAM_A9))
    (pad 35 smd rect (at 5.53 4.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 87 SDRAM_A11))
    (pad 36 smd rect (at 5.53 4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 88 SDRAM_A12))
    (pad 37 smd rect (at 5.53 3.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 103 SDRAM_CKE))
    (pad 38 smd rect (at 5.53 2.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 104 SDRAM_CLK))
    (pad 39 smd rect (at 5.53 1.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 105 SDRAM_DQM))
    (pad 40 smd rect (at 5.53 0.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 5.53 0 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 42 smd rect (at 5.53 -0.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd rect (at 5.53 -1.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 44 smd rect (at 5.53 -2.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 71 SDRAM_D4))
    (pad 45 smd rect (at 5.53 -3.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 46 smd rect (at 5.53 -4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 47 smd rect (at 5.53 -4.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 70 SDRAM_D5))
    (pad 48 smd rect (at 5.53 -5.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 49 smd rect (at 5.53 -6.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 50 smd rect (at 5.53 -7.2 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 69 SDRAM_D6))
    (pad 51 smd rect (at 5.53 -8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask))
    (pad 52 smd rect (at 5.53 -8.8 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 53 smd rect (at 5.53 -9.6 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 68 SDRAM_D7))
    (pad 54 smd rect (at 5.53 -10.4 180) (size 0.9 0.56) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Housings_SSOP.3dshapes/TSOPII-54_10.16x22.22mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_BeagleBone_Black:Socket_BeagleBone_Black (layer F.Cu) (tedit 58E563E4)
    (at 116.3701 62.3824)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 1.2319 -2.3114) (layer F.SilkS))
    (fp_text value BeagleBone_Black_Header (at -3.27914 8.39216 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 SYS_5V))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 SYS_5V))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 BB_CFG_SCL))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 BB_CFG_SDA))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 125 BB_CDONE))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 BB_IRQ_FPGA_TO_ARM))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 126 BB_CRESET))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 BB_IRQ_ARM_TO_FPGA))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 SPI_SS))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 SPI_MISO))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 SPI_MOSI))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 SPI_SCK))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model ${KIPRJMOD}/Socket_BeagleBone_Black.3dshapes/Socket_BeagleBone_Black.wrl
      (at (xyz 0.05 -1.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_BeagleBone_Black:Socket_BeagleBone_Black (layer F.Cu) (tedit 58E560DC)
    (at 164.6301 62.3824)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 1.2319 -2.4384) (layer F.SilkS))
    (fp_text value BeagleBone_Black_Header (at 5.25526 8.7376 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 GPMC_AD6))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 GPMC_AD7))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 GPMC_AD2))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 GPMC_AD3))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 GPMC_ADVN))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 GPMC_OEN))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 GPMC_BE0N))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 GPMC_WEIN))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 GPMC_AD13))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 GPMC_AD12))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 GPMC_AD9))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 GPMC_AD10))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 GPMC_AD15))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 GPMC_AD14))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 GPMC_AD11))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 GPMC_CLK))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 GPMC_AD8))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 GPMC_CSN1))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 GPMC_AD5))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 GPMC_AD4))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 GPMC_AD1))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 GPMC_AD0))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model ${KIPRJMOD}/Socket_BeagleBone_Black.3dshapes/Socket_BeagleBone_Black.wrl
      (at (xyz 0.05 -1.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF8708)
    (at 131.49 90.78 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C36 (at -0.07 -1.34 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F0DB44)
    (at 131.8 108.08 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C40 (at 0.1 1.32 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F09052)
    (at 155.77 60.53 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -0.02 1.4 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 SYS_5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F0900D)
    (at 159.04 60.47 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 1.52 450) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F3DA24)
    (at 160.64 60.47 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0.06 -1.43 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.7 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F3DA8F)
    (at 168.95 58.34 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at -0.16 1.51 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58E55FD8)
    (at 126.401 86.465 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C21 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.258 83.63 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.552 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F3D37B)
    (at 130.56 81.07 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.38 0.03 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF9032)
    (at 158.27 82.106 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.45 -0.014 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F3D378)
    (at 130.55 79.48 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.43 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF8A95)
    (at 152.99 68.15)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0.03 -1.35) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF8A99)
    (at 150.04 68.14 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.12 1.34 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 134.9 66.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -0.012 -1.524 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF8E49)
    (at 136.61 66.61 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -1.9446 -0.1612 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F3D2A6)
    (at 130.57 76.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 2.82 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F3D2A0)
    (at 130.57 77.96 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 2.81 -0.02 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 130.636 84.256 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 130.636 82.732 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 140.15 93.9 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F0C811)
    (at 141.69 93.9 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0.02 -1.35 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF9C7A)
    (at 157.78988 93.61424 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at -0.06 1.486 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 150.142 93.868 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.258 86.678)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 3.036 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.258 85.154)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C23 (at 3.048 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.05 77.26)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C24 (at 3.036 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.05 78.87)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at 3.048 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 140.0048 66.62 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF8E45)
    (at 138.31 66.61 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at -1.95 0.83 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 130.62 71.6 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 130.61 73.11 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 3.0639 -0.0039 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 147.094 93.88 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F0C80C)
    (at 145.57 93.88 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 0.03 1.21 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.29 89.242)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C33 (at 3.048 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 158.29 90.766)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 3.048 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 152.6092 117.50456)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 0.012 1.524) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 152.6092 107.09056)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C37 (at 0.012 1.524) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EF9BBD)
    (at 152.43 96.96)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C38 (at -0.03 1.48) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 152.6092 115.72656)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C39 (at 0.012 -1.524) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 152.6092 110.90056)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C41 (at 0.012 1.524) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F0CDD5)
    (at 137.5 109.44 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C42 (at 0 1.33 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58F0CDB5)
    (at 137.43 114.32 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C43 (at 0.07 1.32 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 110.744 63.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R21 (at 2.101 0 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 113.284 63.5 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R22 (at 2.032 0 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R22-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 114.5109 51.3038 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at -2.1336 0 180) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 114.5109 49.6528 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at -2.1336 0 180) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 114.5109 48.0018 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -2.1336 0 180) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 114.5617 46.3508 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at -2.1336 0 180) (layer F.SilkS))
    (fp_text value 240 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F3D135)
    (at 131.14 85.71 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at -0.27452 -1.26976 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 OSC_OUT))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EF9030)
    (at 157.78 80.63 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -2.9 0 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EFF32D)
    (at 126.2 81.07)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -2.2646 -0.0436) (layer F.SilkS))
    (fp_text value 100 (at 0 1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58CE4E7E)
    (at 156.97 54.25 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.09694 3.10588 180) (layer F.SilkS))
    (fp_text value MCP1826S-3302E/DB (at -5.29336 -0.381 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 SYS_5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIJ-8_5.3x5.3mm_Pitch1.27mm (layer F.Cu) (tedit 58F0DBAB)
    (at 125.483 110.282)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at -3.903 -3.582) (layer F.SilkS))
    (fp_text value M25PX32-VMW (at 0 3.68) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 48 SPI_SS))
    (pad 2 smd rect (at -3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 49 SPI_MISO))
    (pad 3 smd rect (at -3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(R12-Pad2)"))
    (pad 4 smd rect (at -3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 5 smd rect (at 3.65 1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 50 SPI_MOSI))
    (pad 6 smd rect (at 3.65 0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 51 SPI_SCK))
    (pad 7 smd rect (at 3.65 -0.635) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R11-Pad2)"))
    (pad 8 smd rect (at 3.65 -1.905) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIJ-8_5.3x5.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58CE4E7E)
    (at 164.27 54.27 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 3.06106 3.15664 180) (layer F.SilkS))
    (fp_text value MCP1826S-1202E/DB (at -5.35432 -0.12152 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +1V2))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58E567B4)
    (at 120.65 48.895 270)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.667 450) (layer F.SilkS))
    (fp_text value USER_BTN0 (at 0.2286 1.7526 270) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(R17-Pad2)"))
    (pad 1 smd rect (at -2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58E563C2)
    (at 126.238 48.895 270)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0.033 -2.667 450) (layer F.SilkS))
    (fp_text value USER_BTN1 (at 0.55 2.65 270) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R18-Pad2)"))
    (pad 1 smd rect (at -2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58F09193)
    (at 131.81584 48.895 270)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW3 (at -0.025 -2.814 450) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 ICE40_CRESET))
    (pad 1 smd rect (at -2.7 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R3-Pad1)"))
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23-6 (layer F.Cu) (tedit 53DE8DE3)
    (at 129.01 61.33)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U7 (at 0.019 2.361) (layer F.SilkS))
    (fp_text value SN74LVC2G14 (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C44-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(C45-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 67 USER_BTN1))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 66 USER_BTN0))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-8_4.4x3mm_Pitch0.65mm (layer F.Cu) (tedit 58F3C6D4)
    (at 123.663 96.666 90)
    (descr "8-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at -5.524 -0.963 90) (layer F.SilkS))
    (fp_text value AT24CS32-XHM (at 0 2.55 90) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at -2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 5 smd rect (at 2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 BB_CFG_SDA))
    (pad 6 smd rect (at 2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 BB_CFG_SCL))
    (pad 7 smd rect (at 2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 8 smd rect (at 2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-8_4.4x3mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 58F11058)
    (at 128.56 104.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 1.25 -2.45 90) (layer F.SilkS))
    (fp_text value JUMPER (at 1.7018 2.60096 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 125 BB_CDONE))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 ICE40_CDONE))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x01 (layer F.Cu) (tedit 58F11053)
    (at 132.19 104.2 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 1.06 2.49 270) (layer F.SilkS))
    (fp_text value JUMPER (at 1.20904 2.35712 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 126 BB_CRESET))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 ICE40_CRESET))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x01.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_2x06 (layer F.Cu) (tedit 0)
    (at 111.81712 77.597 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -2.80416 0.0508 270) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 6.30936 -2.30632 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 PMOD1_A1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 PMOD1_B1))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 PMOD1_A2))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 PMOD1_B2))
    (pad 5 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 PMOD1_A3))
    (pad 6 thru_hole oval (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 PMOD1_B3))
    (pad 7 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 PMOD1_A4))
    (pad 8 thru_hole oval (at 7.62 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 PMOD1_B4))
    (pad 9 thru_hole oval (at 10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 10 thru_hole oval (at 10.16 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 11 thru_hole oval (at 12.7 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 12 thru_hole oval (at 12.7 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_2x06 (layer F.Cu) (tedit 58E58DD8)
    (at 111.81712 100.457 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at -3.00736 0.0508 270) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 6.31444 -2.30632 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 PMOD2_A1))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 PMOD2_B1))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 PMOD2_A2))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 PMOD2_B2))
    (pad 5 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 PMOD2_A3))
    (pad 6 thru_hole oval (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 PMOD2_B3))
    (pad 7 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 PMOD2_A4))
    (pad 8 thru_hole oval (at 7.62 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 PMOD2_B4))
    (pad 9 thru_hole oval (at 10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 10 thru_hole oval (at 10.16 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 11 thru_hole oval (at 12.7 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 12 thru_hole oval (at 12.7 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 55BDE255)
    (at 111.7296 51.3038 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 91 USER_LED3))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(D4-Pad1)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 55BDE255)
    (at 111.7296 49.6528 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 92 USER_LED2))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(D3-Pad1)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 55BDE255)
    (at 111.7296 48.0018 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 93 USER_LED1))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(D2-Pad1)"))
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 55BDE255)
    (at 111.7296 46.3508 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value BLUE (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 94 USER_LED0))
    (pad 1 smd rect (at -0.7493 0) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(D1-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58EFB629)
    (at 123.28 91.09)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at 0.03 -1.48 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 132.6 61.47)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C46 (at 0 1.524) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F0DB34)
    (at 131.32 109.68 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at -2.33 0 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F0DBD4)
    (at 124.03 114.43 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at -2.36 0 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(R12-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EFB744)
    (at 125.43 114.42 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at -2.402 0.024 90) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 SPI_SS))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F0DB39)
    (at 131.32 111.08 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at -2.33 -0.1 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 SPI_SCK))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F10F8B)
    (at 126.58 94.184 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at -2.8076 -0.0246 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 BB_CFG_SDA))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F10F89)
    (at 126.58 95.708 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at -2.7822 0.0008 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 BB_CFG_SCL))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 122.751 54.451)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 2.54 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(R17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EF8AD5)
    (at 128.847 54.451)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 2.403 0.049) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R18-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5415CBB8)
    (at 122.751 55.848 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(R17-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C44-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EF8AD7)
    (at 128.847 55.848 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R20 (at -2.353 -0.022 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(R18-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(C45-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F1105B)
    (at 131.08 98.82 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at -0.014 -1.3048 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 65 ICE40_CRESET))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F1105E)
    (at 127.49 98.84 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at -0.0086 -1.3388 270) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 64 ICE40_CDONE))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E55F2A)
    (at 129.98 118.43 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R23 (at -2.4 0.05 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 GROVE1_IO1))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E5614F)
    (at 133.15 118.43 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R24 (at -2.4 0.05 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 GROVE2_IO1))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58E55F28)
    (at 131.72 118.43 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R25 (at -2.413 0.03048 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 GROVE1_IO0))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58F0CF84)
    (at 134.874 118.4402 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R26 (at -2.48 0.01 450) (layer F.SilkS))
    (fp_text value 10k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 GROVE2_IO0))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58EF8AEB)
    (at 133.38 54.77 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -0.01 -1.37 270) (layer F.SilkS))
    (fp_text value 100 (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 122.751 57.372)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C44 (at 3.048 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(C44-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 128.847 57.372)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C45 (at 3.048 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(C45-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer F.Cu) (tedit 58EF9C76)
    (at 156.01188 93.61424 270)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D5 (at -0.188 1.456 270) (layer F.SilkS))
    (fp_text value CDBU0520 (at 0.4699 -0.628671 270) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.85 0 270) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module Socket_Strips:Socket_Strip_Angled_2x06 (layer F.Cu) (tedit 58E56286)
    (at 170.81712 113.157 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at -3 0 90) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -2.6 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 107 PMOD3_B1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 106 PMOD3_A1))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 109 PMOD3_B2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 108 PMOD3_A2))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 111 PMOD3_B3))
    (pad 6 thru_hole oval (at 5.08 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 110 PMOD3_A3))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 113 PMOD3_B4))
    (pad 8 thru_hole oval (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 112 PMOD3_A4))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole oval (at 10.16 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 11 thru_hole oval (at 12.7 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 12 thru_hole oval (at 12.7 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Angled_2x06 (layer F.Cu) (tedit 58E562FC)
    (at 170.81712 90.297 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at -2.8956 -0.00212 90) (layer F.SilkS))
    (fp_text value CONN_02X06 (at 0 -2.6 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 114 PMOD4_A1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 115 PMOD4_B1))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 116 PMOD4_A2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 117 PMOD4_B2))
    (pad 5 thru_hole oval (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 118 PMOD4_A3))
    (pad 6 thru_hole oval (at 5.08 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 119 PMOD4_B3))
    (pad 7 thru_hole oval (at 7.62 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 120 PMOD4_A4))
    (pad 8 thru_hole oval (at 7.62 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 121 PMOD4_B4))
    (pad 9 thru_hole oval (at 10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole oval (at 10.16 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 11 thru_hole oval (at 12.7 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 12 thru_hole oval (at 12.7 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Angled_2x06.wrl
      (at (xyz 0.25 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module BeagleWire_elements_package:2_DIP_SWITCH (layer F.Cu) (tedit 58E5678D)
    (at 112.014 57.277)
    (fp_text reference SW4 (at -3.556 0 90) (layer F.SilkS))
    (fp_text value SW_DIP_x02 (at 0 -1.3) (layer F.Fab))
    (pad 1 smd rect (at -1.27 3.49) (size 1.52 2.16) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at 1.27 3.49) (size 1.52 2.16) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R22-Pad1)"))
    (pad 3 smd rect (at 1.27 -3.49) (size 1.52 2.16) (layers F.Cu F.Paste F.Mask)
      (net 123 USER_SW1))
    (pad 4 smd rect (at -1.27 -3.49) (size 1.52 2.16) (layers F.Cu F.Paste F.Mask)
      (net 124 USER_SW0))
  )
  (module BeagleWire_elements_package:ASDMB-100.000MHZ-XY-T (layer F.Cu) (tedit 58F11041)
    (at 128.687 86.505)
    (fp_text reference Y1 (at -0.002 2.03) (layer F.SilkS))
    (fp_text value ASDMB-100.000MHZ-XY-T (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.825 0.775) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.825 0.775) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 0.825 -0.775) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(R10-Pad2)"))
    (pad 4 smd rect (at -0.825 -0.775) (size 0.65 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module Sensors:Grove_SMD_Connector (layer F.Cu) (tedit 55FABB2A)
    (at 121.732 122.14)
    (attr smd)
    (fp_text reference GR1 (at -5.15036 -1.03726) (layer F.SilkS))
    (fp_text value Grove (at 0.1 -3.35) (layer F.Fab))
    (pad 4 smd rect (at -3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 56 GROVE1_IO1))
    (pad 1 smd rect (at 3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 55 GROVE1_IO0))
    (pad 6 smd rect (at -5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  )
  (module Sensors:Grove_SMD_Connector (layer F.Cu) (tedit 55FABB2A)
    (at 134.813 122.14)
    (attr smd)
    (fp_text reference GR2 (at -5.25276 -1.0709) (layer F.SilkS))
    (fp_text value Grove (at 0.1 -3.35) (layer F.Fab))
    (pad 4 smd rect (at -3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 58 GROVE2_IO1))
    (pad 1 smd rect (at 3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 57 GROVE2_IO0))
    (pad 6 smd rect (at -5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  )
  (module Sensors:Grove_SMD_Connector (layer F.Cu) (tedit 55FABB2A)
    (at 147.894 122.14)
    (attr smd)
    (fp_text reference GR3 (at -5.42294 -1.00232) (layer F.SilkS))
    (fp_text value Grove (at 0.1 -3.35) (layer F.Fab))
    (pad 4 smd rect (at -3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 60 GROVE3_IO1))
    (pad 1 smd rect (at 3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 59 GROVE3_IO0))
    (pad 6 smd rect (at -5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  )
  (module Sensors:Grove_SMD_Connector (layer F.Cu) (tedit 55FABB2A)
    (at 160.975 122.14)
    (attr smd)
    (fp_text reference GR4 (at -5.3442 -0.982) (layer F.SilkS))
    (fp_text value Grove (at 0.1 -3.35) (layer F.Fab))
    (pad 4 smd rect (at -3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 62 GROVE4_IO1))
    (pad 1 smd rect (at 3 -0.1) (size 1.01 2.74) (layers F.Cu F.Paste F.Mask)
      (net 61 GROVE4_IO0))
    (pad 6 smd rect (at -5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 5.4 7.4) (size 1.5 3) (layers F.Cu F.Paste F.Mask))
  )
  (gr_text "iCE40 FPGA Cape" (at 159.4866 107.315 90) (layer F.SilkS))
  (gr_text "m_w\npmezydlo\n" (at 171.4754 66.4464 90) (layer F.SilkS))
  (gr_text RST (at 131.7244 44.24172) (layer F.SilkS))
  (gr_text USR1 (at 126.34468 44.2214) (layer F.SilkS))
  (gr_text USR0 (at 120.523 44.196) (layer F.SilkS))
  (gr_text "Rev. 0  2017" (at 161.8234 107.315 90) (layer F.SilkS))
  (gr_text BeagleWire (at 156.2862 107.2134 90) (layer F.SilkS))
  (gr_arc (start 120.1651 119.8574) (end 120.1651 132.5574) (angle 90) (layer Edge.Cuts) (width 0.00254))
  (gr_arc (start 162.3751 119.8574) (end 175.0751 119.8574) (angle 90) (layer Edge.Cuts) (width 0.00254))
  (gr_arc (start 113.8151 49.0474) (end 107.4651 49.0474) (angle 90) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 135.4201 42.6974) (end 113.8151 42.6974) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 135.4201 64.2874) (end 135.4201 42.6974) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 153.2001 64.2874) (end 135.4201 64.2874) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 153.2001 49.6824) (end 153.2001 64.2874) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 175.0751 49.6824) (end 153.2001 49.6824) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 175.0751 119.8574) (end 175.0751 49.6824) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 120.1651 132.5574) (end 162.3751 132.5574) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 107.4651 49.0474) (end 107.4651 119.8574) (layer Edge.Cuts) (width 0.00254))
  (zone (net 1) (net_name +3V3) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.97 137.49) (xy 187.97 38.43) (xy 93.99 38.43) (xy 93.99 140.03) (xy 187.97 140.03)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.97 140.03) (xy 187.97 38.43) (xy 93.99 38.43) (xy 93.99 140.03)
      )
    )
  )
)
