(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 91)
    (no_connects 0)
    (area 137.424999 91.424999 162.575001 108.575001)
    (thickness 1.6002)
    (drawings 23)
    (tracks 415)
    (zones 0)
    (modules 36)
    (nets 37)
  )
  (page USLetter)
  (title_block
    (title "Power Switch")
    (date 2017-04-29)
    (rev 1.0)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.508)
    (user_trace_width 0.71)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1.27 0.508)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.13)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF79)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D4-Pad2)")
  (net 6 "Net-(D5-Pad2)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad3)")
  (net 9 "Net-(J2-Pad1)")
  (net 10 "Net-(R1-Pad2)")
  (net 11 "Net-(R2-Pad2)")
  (net 12 "Net-(R3-Pad2)")
  (net 13 "Net-(R4-Pad2)")
  (net 14 "Net-(R5-Pad2)")
  (net 15 "Net-(U1-Pad3)")
  (net 16 "Net-(U1-Pad4)")
  (net 17 "Net-(U1-Pad10)")
  (net 18 "Net-(U1-Pad11)")
  (net 19 "Net-(U1-Pad12)")
  (net 20 "Net-(U1-Pad13)")
  (net 21 "Net-(U1-Pad14)")
  (net 22 "Net-(U2-Pad5)")
  (net 23 "Net-(U2-Pad6)")
  (net 24 "Net-(J3-Pad3)")
  (net 25 "Net-(J3-Pad4)")
  (net 26 "Net-(J4-Pad3)")
  (net 27 "Net-(J4-Pad4)")
  (net 28 "Net-(C1-Pad1)")
  (net 29 "Net-(C2-Pad1)")
  (net 30 +3V3)
  (net 31 +5V)
  (net 32 "Net-(C4-Pad2)")
  (net 33 "Net-(R7-Pad2)")
  (net 34 "Net-(J6-Pad1)")
  (net 35 "Net-(J7-Pad1)")
  (net 36 "Net-(R8-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
  )
  (module local:MIC-5353 (layer F.Cu) (tedit 5938A6DB)
    (at 140.1 106.2 90)
    (fp_text reference U3 (at -1.6 0 180) (layer F.SilkS))
    (fp_text value MIC5353-3.3YMT-TR (at 1.6 0 180) (layer F.Fab))
    (pad 6 smd rect (at -0.5 -0.71 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -0.5 0.71 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at 0 -0.71 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 0.71 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.5 -0.71 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (pad 3 smd rect (at 0.5 0.71 90) (size 0.3 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 0 0 90) (size 1.4 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module LEDs:LED_0402 (layer B.Cu) (tedit 59965AB7)
    (at 160.75 105.8 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -1.3 0 450) (layer B.SilkS))
    (fp_text value LED (at 0 -1.4 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 599791B3)
    (at 151 100 90)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at -4.25 -3.75 90) (layer F.SilkS))
    (fp_text value STM32F303CC (at 0 6 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (pad 2 smd rect (at -4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C4-Pad2)"))
    (pad 8 smd rect (at -4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (pad 10 smd rect (at -4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at -2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad13)"))
    (pad 15 smd rect (at -1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad12)"))
    (pad 16 smd rect (at -1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad10)"))
    (pad 17 smd rect (at -0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad11)"))
    (pad 18 smd rect (at -0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (pad 19 smd rect (at 0.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (pad 20 smd rect (at 0.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (pad 21 smd rect (at 1.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad3)"))
    (pad 22 smd rect (at 1.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad4)"))
    (pad 23 smd rect (at 2.25 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 2.75 4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (pad 25 smd rect (at 4.35 2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 4.35 2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.35 1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 4.35 1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 4.35 0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R8-Pad2)"))
    (pad 30 smd rect (at 4.35 0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J4-Pad3)"))
    (pad 31 smd rect (at 4.35 -0.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad4)"))
    (pad 32 smd rect (at 4.35 -0.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (pad 33 smd rect (at 4.35 -1.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad2)"))
    (pad 34 smd rect (at 4.35 -1.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J6-Pad1)"))
    (pad 35 smd rect (at 4.35 -2.25 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 90) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (pad 37 smd rect (at 2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J7-Pad1)"))
    (pad 38 smd rect (at 2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd rect (at -0.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at -0.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R7-Pad2)"))
    (pad 45 smd rect (at -1.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 46 smd rect (at -1.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 47 smd rect (at -2.25 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 48 smd rect (at -2.75 -4.35 180) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:RFM22 (layer B.Cu) (tedit 528A8C3A)
    (at 156 92 180)
    (fp_text reference U1 (at 11.6 -1.3 180) (layer B.SilkS))
    (fp_text value RFM22 (at 11.8 -15 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.5 -1 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -0.5 -3 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.5 -5 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -0.5 -7 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -0.5 -9 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 +3V3))
    (pad 6 smd rect (at -0.5 -11 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U1-Pad4)"))
    (pad 7 smd rect (at -0.5 -13 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad3)"))
    (pad 8 smd rect (at -0.5 -15 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 16.5 -1 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 16.5 -3 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 16.5 -5 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 16.5 -7 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 16.5 -9 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 16.5 -11 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 16.5 -13 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 16.5 -15 180) (size 3 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module local:USB_Micro-B-SMD (layer F.Cu) (tedit 599791BD)
    (at 138.5522 96.80112 270)
    (descr http://portal.fciconnect.com/Comergent/fci/drawing/10118192.pdf)
    (tags "USB Micro 10118192")
    (fp_text reference J1 (at 0.44888 -5.5478 270) (layer F.SilkS))
    (fp_text value USB_OTG (at -0.05112 0.0522 270) (layer F.SilkS))
    (pad 6 smd rect (at -1.19888 -1.4478 270) (size 1.89738 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at 1.19888 -1.4478 270) (size 1.89992 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at 3.79984 -1.4478 270) (size 1.79578 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -3.0988 -3.99796 270) (size 2.0955 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 smd rect (at -1.29794 -4.12496 270) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -0.6477 -4.12496 270) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0 -4.12496 270) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.6477 -4.12496 270) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.29794 -4.12496 270) (size 0.39878 1.3462) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.0988 -3.99796 270) (size 2.0955 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 6 smd rect (at -3.79984 -1.4478 270) (size 1.79578 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module local:SOT-723 (layer F.Cu) (tedit 59965FAD)
    (at 140.8 104.2)
    (fp_text reference D1 (at -1.05 -0.2 90) (layer F.SilkS))
    (fp_text value NSR30CM3 (at 2.2 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.4 -0.49) (size 0.27 0.52) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 0 0.49) (size 0.36 0.52) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at 0.4 -0.49) (size 0.27 0.52) (layers F.Cu F.Paste F.Mask)
      (net 31 +5V))
  )
  (module LEDs:LED_0402 (layer B.Cu) (tedit 59965B37)
    (at 160.75 104.4 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -1.35 0 450) (layer B.SilkS))
    (fp_text value LED (at 0 -1.4 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer B.Cu) (tedit 59965AD2)
    (at 160.75 103 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -1.35 0 270) (layer B.SilkS))
    (fp_text value LED (at 0 -1.4 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0402 (layer B.Cu) (tedit 59965AC9)
    (at 160.75 107.2 180)
    (descr "LED 0402 smd package")
    (tags "LED led 0402 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -1.35 0 270) (layer B.SilkS))
    (fp_text value LED (at 0 -1.4 180) (layer B.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module local:U.FL-COAX (layer B.Cu) (tedit 0)
    (at 160.7 94.3)
    (attr smd)
    (fp_text reference J2 (at -1.85 1.85) (layer B.SilkS))
    (fp_text value CONN_COAXIAL (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.5 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0 1.5) (size 2.2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -1.5) (size 2.2 1) (layers B.Cu B.Paste B.Mask))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59965FF4)
    (at 146.1 93.4)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.4 0) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59965FD2)
    (at 146.1 94.4)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -1.4 0) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 59965ABF)
    (at 160.6 101.15 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 1.1 0 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 59965D4C)
    (at 160.6 100.15 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 1.1 0 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 59965B4B)
    (at 160.6 99.15 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 1.1 -0.05 270) (layer B.SilkS))
    (fp_text value R (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer B.Cu) (tedit 59965B67)
    (at 158.7 106.7 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at -1.2 0 180) (layer B.SilkS))
    (fp_text value R (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled (layer F.Cu) (tedit 5997919D)
    (at 159.55 103.9 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J3 (at 2.5 -2.1 90) (layer F.SilkS))
    (fp_text value CONN_01X04_MALE (at 0 4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 31 +5V))
    (pad 3 smd rect (at 0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J3-Pad4)"))
    (pad "" smd rect (at -2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors_JST:JST_SH_SM04B-SRSS-TB_04x1.00mm_Angled (layer F.Cu) (tedit 599791A8)
    (at 159.55 95.9 90)
    (descr http://www.jst-mfg.com/product/pdf/eng/eSH.pdf)
    (tags "connector jst sh")
    (attr smd)
    (fp_text reference J4 (at 2.45 -2.15 90) (layer F.SilkS))
    (fp_text value CONN_01X04_MALE (at 0 4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 31 +5V))
    (pad 3 smd rect (at 0.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J4-Pad3)"))
    (pad 4 smd rect (at 1.5 -1.9375 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad4)"))
    (pad "" smd rect (at -2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.8 1.9375 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59965FE3)
    (at 140.1 107.7 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at -1.5 -0.35 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59965FC9)
    (at 138.4 106.9 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 1.35 -0.2 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59965FDB)
    (at 138.4 104.7 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 1.55 0.05 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local:CERALOCK-CSTE_G_A (layer F.Cu) (tedit 5996566A)
    (at 150.4 106.7 180)
    (fp_text reference Y1 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value Ceralock (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0 180) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad6)"))
    (pad 2 smd rect (at 0 0 180) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.2 0 180) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad5)"))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59979195)
    (at 152.9 106.9 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -1.05 0.8 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59979186)
    (at 155.4 105.2 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0.05 0.85 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5997918D)
    (at 155.4 106.1 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 -0.9 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5997917A)
    (at 146.1 95.4)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at -1.6 0) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59979171)
    (at 155.3 95.7 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at -1.35 0.05 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59979169)
    (at 146.1 96.3)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at -1.55 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 59979161)
    (at 147.9 106.9 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -0.9 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59979149)
    (at 144.3 104.4 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0.5 0.9 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_B3U-1000P (layer F.Cu) (tedit 599A3634)
    (at 144 106.7)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 1.85 -1.9) (layer F.SilkS))
    (fp_text value SW_Push (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at 1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 +3V3))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3U-1000P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 59985C5E)
    (at 153 92.6)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J5 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01_MALE (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 32 "Net-(C4-Pad2)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 59985C69)
    (at 150.9 92.6)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J6 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01_MALE (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 34 "Net-(J6-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 59985C89)
    (at 148.8 92.6)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J7 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01_MALE (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 35 "Net-(J7-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 59985C8E)
    (at 155.1 92.6)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J8 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value CONN_01X01_MALE (at 0 2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 59985CA3)
    (at 146.1 92.4)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at -1.4 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text Pwr (at 159.5 107.6 90) (layer B.SilkS))
  (gr_text Tx (at 159.4 105.75 90) (layer B.SilkS))
  (gr_text Rx (at 159.4 104.4 90) (layer B.SilkS))
  (gr_text Link (at 159.35 103.05 90) (layer B.SilkS))
  (gr_text "LPLink Nano V1.0" (at 145.4 100.3 90) (layer F.SilkS))
  (gr_text Boot (at 142.4 104.65) (layer F.SilkS))
  (gr_text +5 (at 156.35 104.5 90) (layer F.SilkS))
  (gr_text Tx (at 156.35 103.45 90) (layer F.SilkS))
  (gr_text Rx (at 156.4 102.4 90) (layer F.SilkS))
  (gr_text GND (at 156.4 97.7 90) (layer F.SilkS))
  (gr_text +5 (at 156.35 96.45 90) (layer F.SilkS))
  (gr_text Tx (at 156.3 95.4 90) (layer F.SilkS))
  (gr_text Rx (at 156.3 94.4 90) (layer F.SilkS))
  (gr_text Flexi (at 158.15 107.55) (layer F.SilkS))
  (gr_text Main (at 158.5 92.25) (layer F.SilkS))
  (gr_arc (start 138.5 92.5) (end 137.5 92.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.5 92.5) (end 161.5 91.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.5 107.5) (end 162.5 107.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.5 107.5) (end 138.5 108.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.5 108.5) (end 161.5 108.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.5 91.5) (end 161.5 91.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.5 92.5) (end 162.5 107.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.5 92.5) (end 137.5 107.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 137.5 91.5) (xy 162.5 91.5) (xy 162.5 108.5) (xy 137.5 108.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 137.5 91.5) (xy 162.5 91.5) (xy 162.5 108.5) (xy 137.5 108.5)
      )
    )
  )
)
