(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 27)
    (no_connects 0)
    (area 130.785 78.664999 168.983001 104.215001)
    (thickness 1.6)
    (drawings 27)
    (tracks 105)
    (zones 0)
    (modules 5)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.498348)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 137.16 101.6)
    (visible_elements 7FFCFE09)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /ERR)
  (net 2 /COS1M)
  (net 3 /OUT5)
  (net 4 /OUT6)
  (net 5 /OUT7)
  (net 6 /+12V)
  (net 7 /CS)
  (net 8 /SCLK)
  (net 9 /SIN1P)
  (net 10 /SIN1M)
  (net 11 /GND)
  (net 12 /COS1P)
  (net 13 /DIN)
  (net 14 /COS2M)
  (net 15 /COS2P)
  (net 16 /SIN2M)
  (net 17 /SIN2P)
  (net 18 /+5V)
  (net 19 /RSTB)
  (net 20 "Net-(U1-Pad8)")
  (net 21 "Net-(U1-Pad5)")
  (net 22 "Net-(U1-Pad1)")
  (net 23 "Net-(U6-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+12V)
    (add_net /+5V)
    (add_net /COS1M)
    (add_net /COS1P)
    (add_net /COS2M)
    (add_net /COS2P)
    (add_net /CS)
    (add_net /DIN)
    (add_net /ERR)
    (add_net /GND)
    (add_net /OUT5)
    (add_net /OUT6)
    (add_net /OUT7)
    (add_net /RSTB)
    (add_net /SCLK)
    (add_net /SIN1M)
    (add_net /SIN1P)
    (add_net /SIN2M)
    (add_net /SIN2P)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U6-Pad10)")
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 134.62 99.06 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R2 (at 7.62 -2.86 90) (layer F.SilkS))
    (fp_text value 10k (at 7.62 2.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 /+5V))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /ERR))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MLX10407 (layer F.Cu) (tedit 5AA92CB6)
    (at 145.288 90.17)
    (fp_text reference U6 (at 0 1.5) (layer F.SilkS))
    (fp_text value MLX10407 (at 0 -1.5) (layer F.Fab))
    (pad 6 smd rect (at -0.635 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /COS1M))
    (pad 7 smd rect (at 0.635 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /OUT5))
    (pad 8 smd rect (at 1.905 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /OUT6))
    (pad 9 smd rect (at 3.175 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /OUT7))
    (pad 10 smd rect (at 4.445 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U6-Pad10)"))
    (pad 11 smd rect (at 5.715 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS))
    (pad 12 smd rect (at 6.985 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCLK))
    (pad 1 smd rect (at -6.985 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /+12V))
    (pad 2 smd rect (at -5.715 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /SIN1P))
    (pad 3 smd rect (at -4.445 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /SIN1M))
    (pad 4 smd rect (at -3.175 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /GND))
    (pad 5 smd rect (at -1.905 4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /COS1P))
    (pad 13 smd rect (at 6.985 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /DIN))
    (pad 14 smd rect (at 5.715 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /GND))
    (pad 15 smd rect (at 4.445 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /RSTB))
    (pad 16 smd rect (at 3.175 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /ERR))
    (pad 17 smd rect (at 1.905 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /GND))
    (pad 18 smd rect (at 0.635 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad8)"))
    (pad 19 smd rect (at -0.635 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad5)"))
    (pad 20 smd rect (at -1.905 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 14 /COS2M))
    (pad 21 smd rect (at -3.175 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /COS2P))
    (pad 22 smd rect (at -4.445 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /GND))
    (pad 23 smd rect (at -5.715 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 16 /SIN2M))
    (pad 24 smd rect (at -6.985 -4.4) (size 0.8 2.4) (layers F.Cu F.Paste F.Mask)
      (net 17 /SIN2P))
  )
  (module footprints:10P_PIN_HEADER (layer F.Cu) (tedit 5AA936D8)
    (at 148.59 101.6)
    (fp_text reference J1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x10_Male (at 0 -5.08) (layer F.Fab))
    (pad 1 thru_hole oval (at -11.43 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /GND))
    (pad 2 thru_hole oval (at -8.89 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /+5V))
    (pad 3 thru_hole oval (at -6.35 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 /+12V))
    (pad 4 thru_hole oval (at -3.81 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 /SIN1P))
    (pad 5 thru_hole oval (at -1.27 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 /SIN1M))
    (pad 6 thru_hole oval (at 1.27 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 /COS1P))
    (pad 7 thru_hole oval (at 3.81 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /COS1M))
    (pad 8 thru_hole oval (at 6.35 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 /OUT5))
    (pad 9 thru_hole oval (at 8.89 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 /OUT6))
    (pad 10 thru_hole oval (at 11.43 0) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 /OUT7))
  )
  (module footprints:10P_PIN_HEADER (layer F.Cu) (tedit 5AA936D8)
    (at 148.59 81.28 180)
    (fp_text reference J2 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x10_Male (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -11.43 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /CS))
    (pad 2 thru_hole oval (at -8.89 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /SCLK))
    (pad 3 thru_hole oval (at -6.35 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /DIN))
    (pad 4 thru_hole oval (at -3.81 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /RSTB))
    (pad 5 thru_hole oval (at -1.27 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 /ERR))
    (pad 6 thru_hole oval (at 1.27 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 /COS2M))
    (pad 7 thru_hole oval (at 3.81 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /COS2P))
    (pad 8 thru_hole oval (at 6.35 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /SIN2M))
    (pad 9 thru_hole oval (at 8.89 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /SIN2P))
    (pad 10 thru_hole oval (at 11.43 0 180) (size 1.524 3.048) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /GND))
  )
  (module footprints:ACH-8_000MHZ-EK (layer F.Cu) (tedit 5AA94353)
    (at 161.29 91.44 90)
    (fp_text reference U1 (at 0.508 0 90) (layer F.SilkS))
    (fp_text value ACH-8_000MHZ-EK (at 0 -7.62 90) (layer F.Fab))
    (pad 8 thru_hole circle (at -2.54 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad8)"))
    (pad 5 thru_hole circle (at 2.54 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at 2.54 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 /GND))
    (pad 1 thru_hole circle (at -2.54 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad1)"))
  )
  (gr_text DIN (at 154.94 83.439) (layer F.SilkS))
  (gr_text RSTB (at 152.4 83.439) (layer F.SilkS))
  (gr_text ERR (at 149.86 83.439) (layer F.SilkS))
  (gr_text C2M (at 147.32 83.439) (layer F.SilkS))
  (gr_text C2P (at 144.907 83.439) (layer F.SilkS))
  (gr_text S2M (at 142.24 83.439) (layer F.SilkS))
  (gr_text CS (at 162.052 81.28) (layer F.SilkS))
  (gr_text SCLK (at 157.861 83.566) (layer F.SilkS))
  (gr_text S2P (at 139.7 83.439) (layer F.SilkS))
  (gr_text 7 (at 160.02 99.06 90) (layer F.SilkS))
  (gr_text 6 (at 157.48 99.06 90) (layer F.SilkS))
  (gr_text 5 (at 154.94 99.06 90) (layer F.SilkS))
  (gr_text C1M (at 152.4 98.552 90) (layer F.SilkS))
  (gr_text C1P (at 149.86 98.552 90) (layer F.SilkS))
  (gr_text S1M (at 147.32 98.552 90) (layer F.SilkS))
  (gr_text S1P (at 144.78 98.552 90) (layer F.SilkS))
  (gr_text +12 (at 142.24 98.552 90) (layer F.SilkS))
  (gr_text +5 (at 139.7 98.806 90) (layer F.SilkS))
  (gr_text GND (at 137.16 98.552 90) (layer F.SilkS))
  (gr_text GND (at 134.874 81.026) (layer F.SilkS))
  (gr_line (start 167.64 104.14) (end 132.08 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 78.74) (end 167.64 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 78.74) (end 167.64 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 78.74) (end 132.08 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "MLX10407 Breakout\nN Piscitello\nWIT SAE\n2018-03 V1" (at 147.32 90.17) (layer B.SilkS))
  (gr_text ACH-8.000MHZ-EK (at 161.29 96.52) (layer F.SilkS))
  (gr_text 10k (at 134.62 91.44 90) (layer F.SilkS))
  (zone (net 11) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 78.74) (xy 167.64 78.74) (xy 167.64 104.14) (xy 132.08 104.14) (xy 132.08 99.06)
      )
    )
  )
  (zone (net 11) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 78.74) (xy 167.64 78.74) (xy 167.64 104.14) (xy 132.08 104.14)
      )
    )
  )
)
