<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="60.96" x2="60.96" y2="60.96" width="0.0254" layer="20"/>
<wire x1="60.96" y1="60.96" x2="60.96" y2="2.54" width="0.0254" layer="20"/>
<wire x1="60.96" y1="2.54" x2="2.54" y2="2.54" width="0.0254" layer="20"/>
<wire x1="2.54" y1="2.54" x2="2.54" y2="60.96" width="0.0254" layer="20"/>
<text>+12V </text>
<text>GND</text>
<text>AIR_LCDuino rev 0.1</text>
<text>RV-Builders Products</text>
<text>1</text>
<text>1</text>
</plain>
<libraries>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="PEC12_INCREMENTAL_ENCODER">
<description>Incremental Encoder with switch</description>
</package>
<package name="LED-5MM">
</package>
<package name="M1X2">
</package>
<package name="R603">
</package>
<package name="PTC0805">
<description>0805 fuse</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0805">
</package>
<package name="0603">
</package>
<package name="RESONATOR-SMD">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="EIA7343">
</package>
<package name="EIA3216">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
<package name="1X08">
</package>
</packages>
</library>
<library name="wifi_WX">
<packages>
<package name="DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 369C-01&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM317M-D.PDF</description>
</package>
</packages>
</library>
<library name="1AA_Stofer">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SW1" library="dp_devices" package="PEC12_INCREMENTAL_ENCODER" value="ENCODER_SW1-PEC12">
<attribute name="NAME"/>
</element>
<element name="LCD" library="pinhead" package="2X07" value="LCD"/>
<element name="LED1" library="dp_devices" package="LED-5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="dp_devices" package="M1X2" value="12V input">
<attribute name="NAME"/>
</element>
<element name="LED2" library="dp_devices" package="LED-5MM" value=""/>
<element name="R1" library="dp_devices" package="R603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="dp_devices" package="R603" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="dp_devices" package="R603" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="dp_devices" package="R603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="dp_devices" package="R603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R6" library="dp_devices" package="R603" value="">
<attribute name="NAME"/>
</element>
<element name="R7" library="dp_devices" package="R603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="dp_devices" package="R603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="0603" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun" package="RESONATOR-SMD" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="TQFP32-08" value="ATMEGA328P-AU(R)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="SparkFun" package="EIA7343" value="10uF">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun" package="1X06" value="5V UART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X06" value="1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="dp_devices" package="R603" value="120">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X08" value="1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="wifi_WX" package="DPACK" value="78M05">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="dp_devices" package="R603" value="14K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="dp_devices" package="R603" value="6.8K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="1AA_Stofer" package="SOT23-5" value="TC10553.3V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="dp_devices" package="PTC0805" value=""/>
<element name="LCD-BL" library="1AA_Stofer" package="1X02" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="C13" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="C19" pad="C"/>
<contactref element="JP2" pad="6"/>
<contactref element="J1" pad="1"/>
<contactref element="LCD" pad="1"/>
<contactref element="LCD" pad="5"/>
<contactref element="Q1" pad="2"/>
<contactref element="SW1" pad="C"/>
<contactref element="JP4" pad="6"/>
<contactref element="JP2" pad="5"/>
<contactref element="R10" pad="1"/>
<contactref element="JP3" pad="8"/>
<contactref element="LED1" pad="K"/>
<contactref element="LED2" pad="K"/>
<contactref element="U3" pad="4"/>
<contactref element="R12" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="C"/>
<contactref element="C8" pad="2"/>
<contactref element="SW1" pad="P2"/>
<contactref element="U1" pad="3"/>
<contactref element="C9" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="LCD-BL" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R2" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="R3" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$16">
</signal>
<signal name="AREF">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="R9" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="TXO">
<contactref element="U1" pad="31"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="A5_PC5_SCL">
<contactref element="U1" pad="28"/>
<contactref element="R8" pad="2"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="A4_PC4_SDA">
<contactref element="U1" pad="27"/>
<contactref element="R7" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="Q1" pad="3"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="RXI">
<contactref element="U1" pad="30"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="12V_INPUT">
<contactref element="C19" pad="A"/>
<contactref element="U3" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="D3_PD3(INT1)">
<contactref element="U1" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="SW1" pad="P1"/>
</signal>
<signal name="D4_PD4">
<contactref element="U1" pad="2"/>
<contactref element="LCD" pad="13"/>
</signal>
<signal name="D5_PD5">
<contactref element="U1" pad="9"/>
<contactref element="LCD" pad="14"/>
</signal>
<signal name="D6_PD6">
<contactref element="U1" pad="10"/>
<contactref element="LCD" pad="11"/>
</signal>
<signal name="D7_PD7">
<contactref element="U1" pad="11"/>
<contactref element="LCD" pad="12"/>
</signal>
<signal name="D9_PB1">
<contactref element="LCD" pad="4"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="D8_PB0">
<contactref element="LCD" pad="6"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="D10_PB2">
<contactref element="U1" pad="14"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LCD" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="D12_PB4_MISO">
<contactref element="U1" pad="16"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="D11_PB3_MOSI">
<contactref element="U1" pad="15"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="A0_PC0">
<contactref element="U1" pad="23"/>
<contactref element="R4" pad="2"/>
<contactref element="SW1" pad="B"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="C2" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="A"/>
<contactref element="R9" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="LCD" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="LCD-BL" pad="2"/>
</signal>
<signal name="A1_PC1">
<contactref element="U1" pad="24"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="ADC6">
<contactref element="U1" pad="19"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="ADC7">
<contactref element="U1" pad="22"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="A2_PC2">
<contactref element="U1" pad="25"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="D13_PB5_SCK">
<contactref element="U1" pad="17"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$1">
</signal>
<signal name="N$10">
</signal>
<signal name="V3_3V">
<contactref element="JP4" pad="5"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="A"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="A3_PC3">
<contactref element="U1" pad="26"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="D2_PD2(INT0)">
<contactref element="R1" pad="1"/>
<contactref element="SW1" pad="A"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
