(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-RK)")
  (net 2 "Net-(D1-GK)")
  (net 3 "Net-(D1-BK)")
  (net 4 "/B")
  (net 5 "/G")
  (net 6 "/R")
  (net 7 "GND")
  (footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief" (layer "F.Cu")
    (at 135.224 94.742 90)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.1sqmm strain-relief")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J3" (at -1.524 3.206 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 7.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 6 90) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.6 1.6) (drill 0.6) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.15625)
      (net 6 "/R") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief" (layer "F.Cu")
    (at 132.334 93.218 180)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.1sqmm strain-relief")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J2" (at -1.524 3.048) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 7.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 6 180) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.6 1.6) (drill 0.6) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.15625)
      (net 5 "/G") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_Avago_PLCC6_3x2.8mm" (layer "F.Cu")
    (at 138.43 90.678 180)
    (descr "https://docs.broadcom.com/docs/AV02-3793EN")
    (tags "LED Avago PLCC-6 ASMT-YTB7-0AA02")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RGB LED, 6 pin package")
    (property "ki_keywords" "LED RGB diode")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "LED_RGB" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.475 -0.9 180) (size 2.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(D1-RK)") (pinfunction "RK") (pintype "passive"))
    (pad "2" smd rect (at -1.475 0 180) (size 2.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(D1-GK)") (pinfunction "GK") (pintype "passive"))
    (pad "3" smd rect (at -1.475 0.9 180) (size 2.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(D1-BK)") (pinfunction "BK") (pintype "passive"))
    (pad "4" smd rect (at 1.475 0.9 180) (size 2.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/B") (pinfunction "BA") (pintype "passive"))
    (pad "5" smd rect (at 1.475 0 180) (size 2.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/G") (pinfunction "GA") (pintype "passive"))
    (pad "6" smd rect (at 1.475 -0.9 180) (size 2.3 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/R") (pinfunction "RA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_Avago_PLCC6_3x2.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief" (layer "F.Cu")
    (at 144.272 87.376)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.1sqmm strain-relief")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J4" (at -1.778 2.794) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 7.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 6) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.6 1.6) (drill 0.6) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.15625)
      (net 7 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief" (layer "F.Cu")
    (at 135.382 86.106 90)
    (descr "Soldered wire connection with feed through strain relief, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.1sqmm strain-relief")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr exclude_from_pos_files)
    (fp_text reference "J1" (at 1.524 3.048 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 7.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 6 90) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.6 1.6) (drill 0.6) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.15625)
      (net 4 "/B") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm_Relief.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 138.43 86.122 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -3.032 0 90) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 3 "Net-(D1-BK)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 138.43 95.25 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at -3.048 0 90) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 1 "Net-(D1-RK)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "B.Cu")
    (at 144.272 90.351)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "rgb_led.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.794 0.073) (layer "B.SilkS"))
    (fp_text value "R" (at 0 -1.65) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 2 "Net-(D1-GK)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.208333)
      (net 7 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 133.858 83.82) (end 143.51 83.82)
    (layer "Edge.Cuts"))
  (gr_arc (start 143.51 83.82) (mid 145.665261 84.712739) (end 146.558 86.868)
    (layer "Edge.Cuts"))
  (gr_arc (start 133.858 97.282) (mid 131.70274 96.389261) (end 130.810001 94.234001)
    (layer "Edge.Cuts"))
  (gr_line (start 130.81 86.868) (end 130.810001 94.234001)
    (layer "Edge.Cuts"))
  (gr_arc (start 146.558 94.234) (mid 145.665261 96.38926) (end 143.510001 97.281999)
    (layer "Edge.Cuts"))
  (gr_line (start 146.558 94.234) (end 146.558 86.868)
    (layer "Edge.Cuts"))
  (gr_line (start 133.858 97.282) (end 143.510001 97.281999)
    (layer "Edge.Cuts"))
  (gr_arc (start 130.81 86.868) (mid 131.702739 84.712739) (end 133.858 83.82)
    (layer "Edge.Cuts"))
  (zone (net 7) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 128.27 98.552)
        (xy 148.336 98.806)
        (xy 148.336 80.772)
        (xy 127 81.026)
      )
    )
  )
)
