(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 125)
    (zones 0)
    (modules 37)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.635)
    (via_min_drill 0.3048)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 164.084 105.664)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(R1-Pad2)")
  (net 3 VCC)
  (net 4 "Net-(C1-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 "Net-(C10-Pad1)")
  (net 7 "Net-(R4-Pad1)")
  (net 8 "Net-(R16-Pad1)")
  (net 9 "Net-(R16-Pad2)")
  (net 10 "Net-(R17-Pad1)")
  (net 11 "Net-(R17-Pad2)")
  (net 12 "Net-(R18-Pad1)")
  (net 13 "Net-(R18-Pad2)")
  (net 14 "Net-(R19-Pad1)")
  (net 15 "Net-(R19-Pad2)")
  (net 16 "Net-(TP3-Pad1)")
  (net 17 "Net-(U1-Pad2)")
  (net 18 "Net-(C3-Pad2)")
  (net 19 "Net-(C3-Pad1)")
  (net 20 "Net-(C4-Pad1)")
  (net 21 "Net-(C7-Pad1)")
  (net 22 "Net-(C8-Pad1)")
  (net 23 "Net-(R3-Pad1)")
  (net 24 "Net-(U3-Pad1)")
  (net 25 "Net-(U3-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(TP3-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad5)")
    (add_net VCC)
  )
  (module t_misc:NC7SZ14L6X (layer F.Cu) (tedit 5FF4966E)
    (at 136.398 98.806)
    (fp_text reference U3 (at 0 1.524) (layer F.SilkS))
    (fp_text value NC7SZ14L6X (at 2.286 9.144) (layer F.Fab))
    (pad 1 smd rect (at -0.35 -0.325) (size 0.2 0.52) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U3-Pad1)"))
    (pad 6 smd rect (at -0.35 0.325) (size 0.2 0.52) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (pad 5 smd rect (at 0 0.325) (size 0.2 0.52) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U3-Pad5)"))
    (pad 4 smd rect (at 0.35 0.325) (size 0.2 0.52) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad1)"))
    (pad 3 smd rect (at 0.35 -0.325) (size 0.2 0.52) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -0.325) (size 0.2 0.52) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C3-Pad2)"))
  )
  (module t_misc:4_Pad_OSC (layer F.Cu) (tedit 5FDA88B3)
    (at 134.462 98.317 90)
    (fp_text reference X1 (at 1.289 -0.858 270) (layer F.SilkS))
    (fp_text value ABLNO (at 6.623 -21.94 270) (layer F.Fab))
    (pad 4 smd trapezoid (at 2.1 -1.65 90) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 3 smd trapezoid (at 0.4 -1.65 90) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C3-Pad1)"))
    (pad 2 smd trapezoid (at 0.4 -0.35 90) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd custom (at 2.1 -0.35 90) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
  )
  (module t_misc:TDFN_2x1.3 (layer F.Cu) (tedit 5FD2A643)
    (at 148.717 93.091)
    (fp_text reference U2 (at -0.635 -1.651) (layer F.SilkS))
    (fp_text value PL611s-02DFN (at -34.163 -9.017) (layer F.Fab))
    (pad 6 smd custom (at -0.4 -0.88) (size 0.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R18-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 5 smd custom (at 0 -0.88) (size 0.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 4 smd custom (at 0.4 -0.88) (size 0.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R19-Pad1)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 3 smd custom (at 0.4 0.88) (size 0.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 2 smd custom (at 0 0.88) (size 0.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R17-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 1 smd custom (at -0.4 0.88) (size 0.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R16-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
      ))
    (pad 7 smd rect (at 0 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module ul_74LVC1G74DC:74LVC1G74DC (layer F.Cu) (tedit 0)
    (at 140.208 94.869)
    (fp_text reference U1 (at 0 -2.159) (layer F.SilkS))
    (fp_text value 74LVC1G74DC (at 2.032 11.557) (layer F.SilkS) hide)
    (fp_text user * (at -0.8128 -0.9779) (layer F.Fab))
    (fp_text user * (at -1.6002 -1.397) (layer F.SilkS))
    (fp_text user 0.048in/1.219mm (at -1.3462 3.4671) (layer Dwgs.User))
    (fp_text user 0.106in/2.692mm (at 0 -3.4671) (layer Dwgs.User))
    (fp_text user 0.011in/0.279mm (at 4.3942 -0.75) (layer Dwgs.User))
    (fp_text user 0.02in/0.5mm (at -4.3942 -0.5) (layer Dwgs.User))
    (fp_text user * (at -0.8128 -0.9779) (layer F.Fab))
    (fp_text user * (at -1.6002 -1.397) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 8 smd rect (at 1.3462 -0.750001) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C7-Pad1)"))
    (pad 7 smd rect (at 1.3462 -0.25) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C7-Pad1)"))
    (pad 6 smd rect (at 1.3462 0.25) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C7-Pad1)"))
    (pad 5 smd rect (at 1.3462 0.750001) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R4-Pad1)"))
    (pad 4 smd rect (at -1.3462 0.750001) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.3462 0.25) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at -1.3462 -0.25) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -1.3462 -0.750001) (size 1.2192 0.2794) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(TP3-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 141.224 89.154)
    (fp_text reference TP26 (at 1.524 -1.27) (layer F.SilkS))
    (fp_text value TestPoint (at -1.905 -9.525) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 136.144 86.614)
    (fp_text reference TP25 (at 0 -1.524) (layer F.SilkS))
    (fp_text value TestPoint (at -5.08 -8.89) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 153.797 93.726)
    (fp_text reference TP22 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 14.732 -4.572) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(R19-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5FF48C47)
    (at 153.797 98.806)
    (fp_text reference TP21 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 14.732 -5.842) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(R18-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 136.144 89.154)
    (fp_text reference TP20 (at -1.524 -1.27) (layer F.SilkS))
    (fp_text value TestPoint (at -13.97 -9.525) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C1-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 153.797 96.266)
    (fp_text reference TP19 (at -2.032 0.127) (layer F.SilkS))
    (fp_text value TestPoint (at 14.732 -5.207) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(R17-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 143.764 99.06)
    (fp_text reference TP18 (at 0.0381 1.5875) (layer F.SilkS))
    (fp_text value TestPoint (at 2.032 9.906) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(R16-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5FF4973A)
    (at 138.684 99.06 180)
    (fp_text reference TP17 (at 0 -1.524) (layer F.SilkS))
    (fp_text value TestPoint (at -0.254 -9.906) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 141.224 86.614)
    (fp_text reference TP15 (at 0 -1.524) (layer F.SilkS))
    (fp_text value TestPoint (at -1.905 -8.89) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5FF48F94)
    (at 134.112 92.075 270)
    (fp_text reference TP14 (at -1.651 1.778 180) (layer F.SilkS))
    (fp_text value TestPoint (at -0.381 17.78 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(R1-Pad2)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 141.224 99.06)
    (fp_text reference TP4 (at 0 1.524) (layer F.SilkS))
    (fp_text value TestPoint (at -9.144 9.906) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(C8-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 137.795 91.948 180)
    (fp_text reference TP3 (at 1.397 1.016) (layer F.SilkS))
    (fp_text value TestPoint (at 15.875 10.16) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(TP3-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5BAD3C2A)
    (at 138.684 89.154)
    (fp_text reference TP2 (at -1.27 -1.27) (layer F.SilkS))
    (fp_text value TestPoint (at -7.62 -9.525) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(C7-Pad1)"))
  )
  (module t_misc:TP60 (layer F.Cu) (tedit 5FF4836F)
    (at 138.684 86.614)
    (fp_text reference TP1 (at 0 -1.524) (layer F.SilkS))
    (fp_text value TestPoint (at -16.51 -8.89) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 150.5077 92.2147 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R19 (at 0 1.0287) (layer F.SilkS))
    (fp_text value R_Small (at -11.0363 6.2357) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R19-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5FF48B6A)
    (at 146.8628 92.7569 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R18 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value R_Small (at 13.1279 8.3312 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R18-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R18-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 149.352 95.631)
    (descr "SMT capacitor, 0402")
    (fp_text reference R17 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value R_Small (at 4.572 8.128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R17-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R17-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 148.8655 97.4344)
    (descr "SMT capacitor, 0402")
    (fp_text reference R16 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value R_Small (at 4.4235 5.0546) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R16-Pad1)"))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R16-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5FF48D6C)
    (at 144.187 95.631 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R4 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value R_Small (at -7.451 17.399) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 135.763 96.901 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R3 (at 1.397 -0.127 180) (layer F.SilkS))
    (fp_text value R_Small_US (at -1.143 40.767 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C3-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 135.382 94.234 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R2 (at 0 1.016) (layer F.SilkS))
    (fp_text value R_Small_US (at 23.876 -1.778) (layer F.SilkS) hide)
    (fp_text user %R (at 2.54 -13.97) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5FF48E8A)
    (at 132.969 94.234 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference R1 (at 0 1.016) (layer F.SilkS))
    (fp_text value R_Small_US (at 21.209 8.128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(R1-Pad2)"))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:fb_0603 (layer F.Cu) (tedit 5C15628F)
    (at 146.7231 90.0557)
    (descr "SMT resistor, 0603")
    (fp_text reference FB3 (at 0 -1.05) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 -12.3317) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at 0.8 0) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/FB_0603.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:fb_0603 (layer F.Cu) (tedit 5C15628F)
    (at 128.651 97.752 90)
    (descr "SMT resistor, 0603")
    (fp_text reference FB1 (at 0 -1.05 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at -1.054 -17.145 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.381 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at 0.8 0 90) (size 0.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/FB_0603.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 149.2631 90.0557 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C10 (at -0.0889 0.9017) (layer F.SilkS))
    (fp_text value C_Small (at -12.2809 3.4417) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5FF48D99)
    (at 146.473 95.631 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C8 (at 0 -1.016) (layer F.SilkS))
    (fp_text value C_Small (at 8.551 -14.097) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C8-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 144.145 93.98 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C7 (at 0 -1.016) (layer F.SilkS))
    (fp_text value C_Small (at -7.493 14.478) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C7-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5FF48E95)
    (at 130.175 96.816 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C6 (at 1.566 -0.127 180) (layer F.SilkS))
    (fp_text value C_Small (at -2.498 -19.685 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5FF48CCD)
    (at 144.145 90.593 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C5 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value C_Small (at 10.964 11.684 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5FF48DA2)
    (at 131.022 98.806 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C4 (at 0 -1.016) (layer F.SilkS))
    (fp_text value C_Small (at 19.516 -5.588) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5FF49140)
    (at 133.435 99.06 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C3 (at 0 -1.016) (layer F.SilkS))
    (fp_text value C_Small (at 20.659 -0.508) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C3-Pad2)"))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C3-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 131.445 96.774 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 1.524 0.127 180) (layer F.SilkS))
    (fp_text value C_Small (at -2.032 -19.685 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5FF48EFD)
    (at 130.302 94.234)
    (descr "SMT capacitor, 0402")
    (fp_text reference C1 (at 0 -1.016) (layer F.SilkS))
    (fp_text value C_Small (at -17.78 -7.366) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Clock Generator Test Board\nJanuary 7th, 2021" (at 136.144 94.869) (layer B.SilkS))
  (gr_line (start 157.099 84.074) (end 157.099 101.219) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.349 84.074) (end 157.099 84.074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.349 101.219) (end 125.349 84.074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.099 101.219) (end 125.349 101.219) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.464 100.584) (xy 125.984 100.584) (xy 125.984 84.709) (xy 156.464 84.709)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.464 100.584) (xy 125.984 100.584) (xy 125.984 84.709) (xy 156.464 84.709)
      )
    )
  )
)
