(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 11)
    (no_connects 0)
    (area 112.954999 54.656666 146.125001 96.595001)
    (thickness 1.6)
    (drawings 5)
    (tracks 17)
    (zones 0)
    (modules 5)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.81 2.54)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 116.84 66.04)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(RV1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(RV1-Pad3)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(RV1-Pad1)")
    (add_net "Net-(RV1-Pad3)")
  )
  (module KICAD_Libraries:Trimmer_Resistor_multiturn (layer F.Cu) (tedit 59BB0ED9)
    (at 128.905 91.44)
    (fp_text reference POT (at -3.81 1.27) (layer F.SilkS))
    (fp_text value 100 (at 8.89 -29.21) (layer F.Fab) hide)
    (pad 1 smd rect (at 2.54 -1.27) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(RV1-Pad1)"))
    (pad 2 smd rect (at 0 1.27) (size 1.524 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.54 -1.27) (size 3.048 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(RV1-Pad3)"))
  )
  (module KICAD_Libraries:SBL-1MHT (layer F.Cu) (tedit 59BB0F09)
    (at 127.635 76.835)
    (fp_text reference SBL-1 (at 10.795 -9.525) (layer F.SilkS))
    (fp_text value SBL-1 (at 1.905 -15.24) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.81 -7.62) (size 5.08 3.048) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 3.81 -7.62) (size 4.064 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.81 -2.54) (size 4.064 3.048) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 4 smd rect (at 3.81 -2.54) (size 4.064 3.048) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 5 smd rect (at -3.81 2.54) (size 4.064 3.048) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(RV1-Pad3)"))
    (pad 6 smd rect (at 3.81 2.54) (size 4.064 3.048) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(RV1-Pad1)"))
    (pad 7 smd rect (at -3.81 7.62) (size 4.064 3.048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 3.81 7.62) (size 4.064 3.048) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad1)"))
  )
  (module WEA-RF:Manhattan2Pad (layer F.Cu) (tedit 59BB0E53)
    (at 117.475 71.755)
    (fp_text reference RF (at 2.54 -5.08) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 3.81 -10.16) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.54) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0 2.54) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module WEA-RF:Manhattan2Pad (layer F.Cu) (tedit 59BB0E5F)
    (at 139.065 74.295 90)
    (fp_text reference IF (at -3.175 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 14.605 -5.715 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.54 90) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 0 2.54 90) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module WEA-RF:Manhattan2Pad (layer F.Cu) (tedit 59BBF967)
    (at 139.065 84.455 90)
    (fp_text reference LO (at -3.175 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 24.765 -3.81 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -2.54 90) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 0 2.54 90) (size 3.81 2.54) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_text "WEA 2017" (at 139.065 93.98) (layer F.SilkS))
  (gr_line (start 113.03 96.52) (end 113.03 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 96.52) (end 113.03 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 63.5) (end 146.05 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 63.5) (end 146.05 63.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 64.77) (xy 144.78 64.77) (xy 144.78 95.25) (xy 114.3 95.25)
      )
    )
  )
)
