(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 118)
    (zones 0)
    (modules 4)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.225)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (user_trace_width 1.5)
    (user_trace_width 1.75)
    (user_trace_width 2)
    (user_trace_width 2.5)
    (user_trace_width 3)
    (user_trace_width 4)
    (user_trace_width 5)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.254)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 "Net-(J1-Pad36)")
  (net 4 "Net-(J1-Pad37)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad37)")
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 104.14 112.268)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 1.86) (layer B.SilkS))
    (fp_text value 21K (at 2.54 -1.86) (layer B.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad37)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad36)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_TE-Connectivity:TE_1761469-1 (layer B.Cu) (tedit 0)
    (at 141.3 104.6 180)
    (fp_text reference J1 (at -38.6874 6.4519) (layer B.SilkS))
    (fp_text value 1761469-1 (at -45.2 -6.4) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -39.37 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at -36.83 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 3 thru_hole circle (at -34.29 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 4 thru_hole circle (at -31.75 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 5 thru_hole circle (at -29.21 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 6 thru_hole circle (at -26.67 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 7 thru_hole circle (at -24.13 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 8 thru_hole circle (at -21.59 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 9 thru_hole circle (at -19.05 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 10 thru_hole circle (at -16.51 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 11 thru_hole circle (at -13.97 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 12 thru_hole circle (at -11.43 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 13 thru_hole circle (at -8.89 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 14 thru_hole circle (at -6.35 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole circle (at -3.81 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole circle (at -1.27 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 17 thru_hole circle (at 1.27 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole circle (at 3.81 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 19 thru_hole circle (at 6.35 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 20 thru_hole circle (at 8.89 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole circle (at 11.43 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole circle (at 13.97 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 23 thru_hole circle (at 16.51 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 24 thru_hole circle (at 19.05 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 25 thru_hole circle (at 21.59 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 26 thru_hole circle (at 24.13 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 27 thru_hole circle (at 26.67 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at 29.21 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at 31.75 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at 34.29 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at 36.83 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at 39.37 -2.42 180) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at 39.37 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 34 thru_hole circle (at 36.83 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 34.29 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at 31.75 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad36)"))
    (pad 37 thru_hole circle (at 29.21 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad37)"))
    (pad 38 thru_hole circle (at 26.67 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at 24.13 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 40 thru_hole circle (at 21.59 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 41 thru_hole circle (at 19.05 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 42 thru_hole circle (at 16.51 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 43 thru_hole circle (at 13.97 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 44 thru_hole circle (at 11.43 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 45 thru_hole circle (at 8.89 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 46 thru_hole circle (at 6.35 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 47 thru_hole circle (at 3.81 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 48 thru_hole circle (at 1.27 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 49 thru_hole circle (at -1.27 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 50 thru_hole circle (at -3.81 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 51 thru_hole circle (at -6.35 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 52 thru_hole circle (at -8.89 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 53 thru_hole circle (at -11.43 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 54 thru_hole circle (at -13.97 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 55 thru_hole circle (at -16.51 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 56 thru_hole circle (at -19.05 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 57 thru_hole circle (at -21.59 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 58 thru_hole circle (at -24.13 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 59 thru_hole circle (at -26.67 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 60 thru_hole circle (at -29.21 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 61 thru_hole circle (at -31.75 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 62 thru_hole circle (at -34.29 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 63 thru_hole circle (at -36.83 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 64 thru_hole circle (at -39.37 2.42) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 +12V))
  )
  (module Connector_TE-Connectivity:6_position_6.35mm_header (layer B.Cu) (tedit 5E669147)
    (at 179.324 122.428 180)
    (fp_text reference J2 (at 0.2 -5.6) (layer B.SilkS))
    (fp_text value +12v (at -2.625 -11.05) (layer B.Fab))
    (pad 6 thru_hole oval (at 31.75 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 5 thru_hole oval (at 25.4 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 4 thru_hole oval (at 19.05 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 3 thru_hole oval (at 12.7 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 6.35 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole oval (at 0 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 +12V))
  )
  (module Connector_TE-Connectivity:6_position_6.35mm_header (layer B.Cu) (tedit 5E669147)
    (at 134.874 122.428 180)
    (fp_text reference J3 (at 0 -4.8) (layer B.SilkS))
    (fp_text value GND (at -2.625 -11.05) (layer B.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 6.35 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 12.7 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 19.05 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 25.4 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 31.75 0 180) (size 2 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text "Mount components on other side" (at 147.066 104.394) (layer F.SilkS))
  (gr_text "Mount components on other side" (at 141.732 128.016) (layer F.SilkS))
  (gr_text "-  -  -  -  -  -  -  -  -  -  -  " (at 117.856 117.094) (layer B.SilkS))
  (gr_text "+  +  +  +  +  +  +  +  +  +  +  +  +  " (at 162.56 116.694) (layer B.SilkS))
  (gr_text "Designed by Trevor Raty\nBased on JBoards design by Jeremy McElroy" (at 125.476 114.046) (layer F.SilkS))
  (gr_text "75a - 900w MAX Total\n30a - 360w MAX/Connection" (at 147.066 113.538) (layer F.SilkS))
  (gr_text +12v (at 178.816 113.538) (layer B.SilkS))
  (gr_text GND (at 132.842 113.284) (layer B.SilkS))
  (gr_line (start 100 130) (end 182.6 130) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 100) (end 182.6 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 182.6 130) (end 182.6 100) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 100 100) (end 100 130) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.75) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 148.59 108.966) (xy 141.986 117.856) (xy 139.954 129.54) (xy 100.33 129.794) (xy 100.33 116.078)
        (xy 110.236 116.078) (xy 115.824 109.474) (xy 115.824 100.076) (xy 148.59 100.076)
      )
    )
  )
  (zone (net 1) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.75) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 182.372 129.54) (xy 141.986 129.54) (xy 142.748 117.856) (xy 149.098 108.966) (xy 149.098 100.076)
        (xy 182.118 100.076)
      )
    )
  )
  (zone (net 1) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.75) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 182.372 129.54) (xy 141.986 129.54) (xy 142.748 117.856) (xy 149.098 108.966) (xy 149.098 100.076)
        (xy 182.118 100.076)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.75) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 148.59 108.966) (xy 141.986 117.856) (xy 139.954 129.54) (xy 100.33 129.794) (xy 100.33 116.078)
        (xy 110.236 116.078) (xy 115.824 109.474) (xy 115.824 100.076) (xy 148.59 100.076)
      )
    )
  )
)
