<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.58" y2="0" width="0" layer="20"/>
<wire x1="101.58" y1="0" x2="101.58" y2="106.35" width="0" layer="20"/>
<wire x1="101.58" y1="106.35" x2="0" y2="106.35" width="0" layer="20"/>
<wire x1="0" y1="106.35" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="DB9">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="SWITCH-SPDT">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
<package name="XBEE-SILK">
</package>
<package name="TRIM_POT_PTH">
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED_BARGAPH_10">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="D-7.5">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="DO41-7.6">
<description>&lt;b&gt;DO41&lt;/b&gt; 7.6mm x 2mm&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
</package>
</packages>
</library>
<library name="traco_thl_tel_series">
<packages>
<package name="TEL_5_SERIES">
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MSTBV9">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
<package name="MSTBV10">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitor-wima">
<packages>
<package name="C7.5B3">
<description>&lt;B&gt;MKS3&lt;/B&gt;, 10 x 3 mm, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DIL08-ROUND">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TO92-INLINE">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="LCD1602">
</package>
</packages>
</library>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO126AV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.3 mm</description>
</package>
</packages>
</library>
<library name="resistor-net">
<description>&lt;b&gt;Generic Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RN-11">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
<package name="RN-5">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lsta">
<packages>
<package name="FE07-2W">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rc-master">
<description>&lt;b&gt;R/C MASTER! - v1.07 (07/03/2007)&lt;/b&gt;&lt;p&gt;
&lt;p&gt;This library is a collection of SMD and through hole resistors and capacitors by various manufacturers. Some of these include types from Panasonic, Kemet, BC Components and others. Many of the packages were adapted from &lt;b&gt;rcl.lbr&lt;/b&gt; and &lt;b&gt;cap-pan40.lbr&lt;/b&gt; and have been renamed and grouped in a more logical form.&lt;/p&gt;&lt;p&gt;Silkscreen elements are a minimum of 8 mils in width with larger components using 10 mil widths. Most of the SMD components have text sizes of 0 .04" and thru-hole components are 0.05" in size.  A text ratio of 14 is used in both cases. Where practical, the elements are aligned on a 12.5 mil or 6.25 mil grid depending on the pad size and spacing.&lt;/p&gt;
&lt;p&gt;&lt;h4&gt;All capacitors are grouped by the following naming conventions:&lt;/h4&gt;&lt;/p&gt;
&lt;table width="380" border="1" bordercolor="#000000"&gt;
  &lt;tr&gt; 
    &lt;td width="81" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Prefix&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
    &lt;td width="289" bgcolor="#33CCFF"&gt;&lt;div align="center"&gt;&lt;strong&gt;Description&lt;/strong&gt;&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CBP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Bipolar Electrolytic Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CCA_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Chip Cap Array Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;CP_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Polarized Electrolytic/Tantalum Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;C_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Non-Polarized Film / Chip Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;FB_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Ferrite Bead Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;L_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Simple Chip Inductors&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
  &lt;tr&gt; 
    &lt;td&gt;&lt;div align="center"&gt;R_&lt;/div&gt;&lt;/td&gt;
    &lt;td&gt;&lt;div align="center"&gt;Resistor Types&lt;/div&gt;&lt;/td&gt;
  &lt;/tr&gt;
&lt;/table&gt;
&lt;p&gt;
&lt;p&gt;&lt;author&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;Copyright (C) 2007, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;
&lt;/author&gt;</description>
<packages>
<package name="CGOLD-SD-H">
<description>&lt;b&gt;GOLD CAP&lt;/b&gt; - Panasonic&lt;p&gt;
SD Series, Horizontal mount</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ISP" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="IC7" library="SparkFun" package="DIL16" value="MAX202"/>
<element name="IC8" library="SparkFun" package="DIL08" value="SN75LBC184P"/>
<element name="R25" library="SparkFun" package="AXIAL-0.4" value="1K-1%"/>
<element name="R26" library="SparkFun" package="AXIAL-0.4" value="1K-1%"/>
<element name="R18" library="SparkFun" package="AXIAL-0.4" value="10K-1%"/>
<element name="C24" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C22" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C11" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C10" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C9" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C18" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="X3" library="SparkFun" package="DB9" value=""/>
<element name="PRG" library="SparkFun" package="SWITCH-SPDT" value=""/>
<element name="C23" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C26" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C20" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="C19" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="LED1" library="SparkFun" package="LED3MM" value="RED"/>
<element name="R17" library="SparkFun" package="AXIAL-0.4" value="390R-1%"/>
<element name="C8" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="Y2" library="SparkFun" package="HC49US" value="16MHz"/>
<element name="C13" library="SparkFun" package="CAP-PTH-SMALL2" value="22pF"/>
<element name="C12" library="SparkFun" package="CAP-PTH-SMALL2" value="22pF"/>
<element name="DISP1" library="adafruit" package="LCD1602" value="HD44780LCD-1602"/>
<element name="IC6" library="atmel" package="DIL40" value="MEGA32-P">
<attribute name="OC_NEWARK" value="51P1794"/>
<attribute name="MPN" value="ATMEGA32-16PU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1661729"/>
</element>
<element name="XB1" library="SparkFun" package="XBEE-SILK" value="XBEE-1B2"/>
<element name="R20" library="SparkFun" package="AXIAL-0.4" value="22R"/>
<element name="R21" library="SparkFun" package="TRIM_POT_PTH" value="TRIMPOTPTH"/>
<element name="C17" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="IC9" library="SparkFun" package="DIL08" value="SN75LBC184P"/>
<element name="R27" library="SparkFun" package="AXIAL-0.4" value="1K-1%"/>
<element name="C25" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="D1" library="diode" package="D-7.5" value="1N4007"/>
<element name="C2" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="IC1" library="traco_thl_tel_series" package="TEL_5_SERIES" value="TEL5"/>
<element name="C5" library="SparkFun" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="X1" library="con-phoenix-508" package="MSTBV9" value="MSTBV9"/>
<element name="C1" library="capacitor-wima" package="C7.5B3" value="2,2nF/250V"/>
<element name="R22" library="SparkFun" package="AXIAL-0.4" value="1K-1%"/>
<element name="R23" library="SparkFun" package="AXIAL-0.4" value="1K"/>
<element name="R24" library="SparkFun" package="AXIAL-0.4" value="1K"/>
<element name="IC4" library="adafruit" package="DIL08-ROUND" value="DS1337"/>
<element name="Y1" library="SparkFun" package="TC26H" value="32,768kHz"/>
<element name="IC5" library="atmel" package="DIL08" value="AT24CP">
<attribute name="OC_NEWARK" value="03P2044"/>
<attribute name="MPN" value="AT24C1024BW-SH-B"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1362646"/>
</element>
<element name="C14" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="OK1" library="optocoupler" package="DIL16" value="PC847">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707735"/>
</element>
<element name="Q1" library="transistor-power" package="TO126AV" value="BD680"/>
<element name="R3" library="SparkFun" package="AXIAL-0.4" value="2K21"/>
<element name="D2" library="diode" package="D-7.5" value="1N4007"/>
<element name="Q2" library="transistor-power" package="TO126AV" value="BD680"/>
<element name="R4" library="SparkFun" package="AXIAL-0.4" value="2K21"/>
<element name="D3" library="diode" package="D-7.5" value="1N4007"/>
<element name="Q3" library="transistor-power" package="TO126AV" value="BD680"/>
<element name="Q4" library="transistor-power" package="TO126AV" value="BD680"/>
<element name="R5" library="SparkFun" package="AXIAL-0.4" value="2K21"/>
<element name="R6" library="SparkFun" package="AXIAL-0.4" value="2K21"/>
<element name="D4" library="diode" package="D-7.5" value="1N4007"/>
<element name="D5" library="diode" package="D-7.5" value="1N4007"/>
<element name="X2" library="con-phoenix-508" package="MSTBV10" value="MSTBV10">
<attribute name="OC_NEWARK" value="69R9844"/>
<attribute name="MPN" value="MSTBV 2,5/10-GF-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792798"/>
</element>
<element name="OK2" library="optocoupler" package="DIL16" value="PC847">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9707735"/>
</element>
<element name="S1" library="SparkFun" package="TACTILE-PTH" value="PTS645"/>
<element name="S2" library="SparkFun" package="TACTILE-PTH" value="PTS645"/>
<element name="S3" library="SparkFun" package="TACTILE-PTH" value="PTS645"/>
<element name="S4" library="SparkFun" package="TACTILE-PTH" value="PTS645"/>
<element name="RN2" library="resistor-net" package="RN-11" value="470R">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="L1" library="SparkFun" package="LED_BARGAPH_10" value="YE"/>
<element name="RN4" library="resistor-net" package="RN-5" value="4K7">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN3" library="resistor-net" package="RN-5" value="110K">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R28" library="SparkFun" package="AXIAL-0.4" value="2K21"/>
<element name="R29" library="SparkFun" package="AXIAL-0.4" value="2K21"/>
<element name="J1" library="con-lsta" package="FE07-2W" value="EXP">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RN1" library="resistor-net" package="RN-5" value="4K7">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="H1" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H2" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H3" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="H4" library="holes" package="3,0" value="MOUNT-HOLE3.0"/>
<element name="IC3" library="adafruit" package="TO92-INLINE" value="MCP1702-3302E/TO"/>
<element name="D10" library="diode" package="DO41-7.6" value="1N5817"/>
<element name="D11" library="diode" package="DO41-7.6" value="1N5817"/>
<element name="C15" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="R19" library="SparkFun" package="AXIAL-0.4" value="1K-1%"/>
<element name="C16" library="rc-master" package="CGOLD-SD-H" value="1F/5V"/>
<element name="C6" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
<element name="R7" library="SparkFun" package="AXIAL-0.4" value="10K-1%"/>
<element name="R1" library="SparkFun" package="AXIAL-0.4" value="49R9-1%"/>
<element name="R9" library="SparkFun" package="AXIAL-0.4" value="10K-1%"/>
<element name="R11" library="SparkFun" package="AXIAL-0.4" value="1K-1%"/>
<element name="R15" library="SparkFun" package="AXIAL-0.4" value="12K7-1%"/>
<element name="IC2" library="linear" package="DIL08" value="MCP6232-E/SN"/>
<element name="C3" library="SparkFun" package="CAP-PTH-SMALL2" value="10nF"/>
<element name="JP1" library="SparkFun" package="1X02" value=""/>
<element name="JP4" library="SparkFun" package="1X02" value=""/>
<element name="JP3" library="SparkFun" package="1X02" value=""/>
<element name="JP8" library="SparkFun" package="1X02" value=""/>
<element name="R16" library="SparkFun" package="AXIAL-0.4" value="49K9-1%"/>
<element name="D6" library="diode" package="DO41-7.6" value="1N5817"/>
<element name="D7" library="diode" package="DO41-7.6" value="1N5817"/>
<element name="C7" library="SparkFun" package="CAP-PTH-SMALL2" value="100nF"/>
</elements>
<signals>
<signal name="N$6">
<contactref element="R25" pad="P$2"/>
<contactref element="IC7" pad="12"/>
</signal>
<signal name="PD0">
<contactref element="R25" pad="P$1"/>
<contactref element="R26" pad="P$1"/>
<contactref element="IC6" pad="14"/>
</signal>
<signal name="PD1">
<contactref element="IC7" pad="11"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC6" pad="15"/>
</signal>
<signal name="N$12">
<contactref element="C11" pad="1"/>
<contactref element="IC6" pad="32"/>
</signal>
<signal name="GND">
<contactref element="C22" pad="2"/>
<contactref element="IC7" pad="15"/>
<contactref element="C24" pad="2"/>
<contactref element="IC8" pad="5"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="ISP" pad="6"/>
<contactref element="C26" pad="1"/>
<contactref element="X3" pad="5"/>
<contactref element="R17" pad="P$1"/>
<contactref element="C8" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC6" pad="31"/>
<contactref element="IC6" pad="11"/>
<contactref element="DISP1" pad="16"/>
<contactref element="R21" pad="3"/>
<contactref element="DISP1" pad="5"/>
<contactref element="C17" pad="2"/>
<contactref element="DISP1" pad="1"/>
<contactref element="C25" pad="2"/>
<contactref element="IC9" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="16"/>
<contactref element="C1" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="XB1" pad="10"/>
<contactref element="R24" pad="P$1"/>
<contactref element="C14" pad="2"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC5" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC4" pad="4"/>
<contactref element="RN2" pad="1"/>
<contactref element="RN4" pad="1"/>
<contactref element="J1" pad="14"/>
<contactref element="X1" pad="9"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="-"/>
<contactref element="D7" pad="A"/>
<contactref element="C3" pad="2"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="R16" pad="P$2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C7" pad="2"/>
<contactref element="X1" pad="5"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="C24" pad="1"/>
<contactref element="IC8" pad="8"/>
<contactref element="C22" pad="1"/>
<contactref element="IC7" pad="16"/>
<contactref element="C23" pad="2"/>
<contactref element="ISP" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="R18" pad="P$1"/>
<contactref element="X3" pad="6"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="IC6" pad="30"/>
<contactref element="IC6" pad="10"/>
<contactref element="R21" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="DISP1" pad="2"/>
<contactref element="R20" pad="P$1"/>
<contactref element="C25" pad="1"/>
<contactref element="IC9" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="14"/>
<contactref element="C5" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="OK2" pad="16"/>
<contactref element="OK2" pad="14"/>
<contactref element="OK2" pad="12"/>
<contactref element="OK2" pad="10"/>
<contactref element="RN3" pad="1"/>
<contactref element="R28" pad="P$1"/>
<contactref element="R29" pad="P$1"/>
<contactref element="J1" pad="13"/>
<contactref element="D11" pad="A"/>
<contactref element="D6" pad="C"/>
<contactref element="IC2" pad="8"/>
<contactref element="C7" pad="1"/>
<contactref element="X1" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="IC7" pad="9"/>
<contactref element="PRG" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="C18" pad="2"/>
<contactref element="PRG" pad="2"/>
</signal>
<signal name="PD5">
<contactref element="IC8" pad="2"/>
<contactref element="IC8" pad="3"/>
<contactref element="IC6" pad="19"/>
</signal>
<signal name="N$15">
<contactref element="IC7" pad="2"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="IC7" pad="6"/>
<contactref element="C26" pad="2"/>
</signal>
<signal name="N$42">
<contactref element="IC8" pad="7"/>
<contactref element="X3" pad="3"/>
</signal>
<signal name="N$44">
<contactref element="IC8" pad="6"/>
<contactref element="X3" pad="8"/>
</signal>
<signal name="N$45">
<contactref element="X3" pad="9"/>
<contactref element="IC7" pad="8"/>
</signal>
<signal name="N$46">
<contactref element="IC7" pad="13"/>
<contactref element="X3" pad="7"/>
</signal>
<signal name="N$48">
<contactref element="IC7" pad="14"/>
<contactref element="X3" pad="2"/>
</signal>
<signal name="N$49">
<contactref element="IC7" pad="7"/>
<contactref element="X3" pad="4"/>
</signal>
<signal name="N$47">
<contactref element="IC7" pad="4"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="IC7" pad="1"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="C19" pad="2"/>
<contactref element="IC7" pad="3"/>
</signal>
<signal name="N$52">
<contactref element="C20" pad="2"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="N$74">
<contactref element="LED1" pad="K"/>
<contactref element="R17" pad="P$2"/>
</signal>
<signal name="N$27">
<contactref element="C12" pad="2"/>
<contactref element="IC6" pad="12"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="3"/>
<contactref element="IC6" pad="8"/>
<contactref element="J1" pad="10"/>
<contactref element="L1" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="1"/>
<contactref element="IC6" pad="7"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$1">
<contactref element="ISP" pad="5"/>
<contactref element="R18" pad="P$2"/>
<contactref element="IC6" pad="9"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="IC6" pad="6"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="DISP1" pad="15"/>
<contactref element="R20" pad="P$2"/>
</signal>
<signal name="N$14">
<contactref element="R21" pad="2"/>
<contactref element="DISP1" pad="3"/>
</signal>
<signal name="PC2">
<contactref element="DISP1" pad="14"/>
<contactref element="IC6" pad="24"/>
<contactref element="S1" pad="3"/>
<contactref element="RN3" pad="2"/>
</signal>
<signal name="PC3">
<contactref element="IC6" pad="25"/>
<contactref element="DISP1" pad="13"/>
<contactref element="S2" pad="3"/>
<contactref element="RN3" pad="3"/>
</signal>
<signal name="PC4">
<contactref element="IC6" pad="26"/>
<contactref element="DISP1" pad="12"/>
<contactref element="S3" pad="3"/>
<contactref element="RN3" pad="4"/>
</signal>
<signal name="PC5">
<contactref element="IC6" pad="27"/>
<contactref element="DISP1" pad="11"/>
<contactref element="S4" pad="3"/>
<contactref element="RN3" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="R26" pad="P$2"/>
<contactref element="IC8" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="IC6" pad="23"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC4" pad="5"/>
<contactref element="J1" pad="6"/>
<contactref element="R28" pad="P$2"/>
</signal>
<signal name="SCL">
<contactref element="IC6" pad="22"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC4" pad="6"/>
<contactref element="J1" pad="5"/>
<contactref element="R29" pad="P$2"/>
</signal>
<signal name="PD3">
<contactref element="IC9" pad="4"/>
<contactref element="IC6" pad="17"/>
<contactref element="R23" pad="P$1"/>
</signal>
<signal name="PD6">
<contactref element="IC9" pad="2"/>
<contactref element="IC9" pad="3"/>
<contactref element="IC6" pad="20"/>
</signal>
<signal name="N$28">
<contactref element="R27" pad="P$2"/>
<contactref element="IC9" pad="1"/>
</signal>
<signal name="PD2">
<contactref element="IC6" pad="16"/>
<contactref element="R27" pad="P$1"/>
<contactref element="R22" pad="P$1"/>
</signal>
<signal name="AI7">
<contactref element="IC6" pad="33"/>
<contactref element="OK2" pad="15"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="AI6">
<contactref element="IC6" pad="34"/>
<contactref element="OK2" pad="13"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="AI5">
<contactref element="IC6" pad="35"/>
<contactref element="OK2" pad="11"/>
<contactref element="L1" pad="3"/>
</signal>
<signal name="AI4">
<contactref element="IC6" pad="36"/>
<contactref element="OK2" pad="9"/>
<contactref element="L1" pad="4"/>
</signal>
<signal name="AI3">
<contactref element="IC6" pad="37"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="AI2">
<contactref element="IC6" pad="38"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="AI1">
<contactref element="IC6" pad="39"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="AI0">
<contactref element="IC6" pad="40"/>
<contactref element="IC2" pad="1"/>
<contactref element="R15" pad="P$1"/>
</signal>
<signal name="PD4">
<contactref element="IC6" pad="18"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="PC6">
<contactref element="IC6" pad="28"/>
<contactref element="DISP1" pad="6"/>
</signal>
<signal name="PC7">
<contactref element="DISP1" pad="4"/>
<contactref element="IC6" pad="29"/>
</signal>
<signal name="N$97">
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="22"/>
<contactref element="IC1" pad="23"/>
</signal>
<signal name="N$76">
<contactref element="IC1" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$73">
<contactref element="D1" pad="A"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$77">
<contactref element="C1" pad="2"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="XB1" pad="3"/>
<contactref element="R23" pad="P$2"/>
<contactref element="R24" pad="P$2"/>
</signal>
<signal name="N$53">
<contactref element="XB1" pad="2"/>
<contactref element="R22" pad="P$2"/>
</signal>
<signal name="RSSI">
<contactref element="XB1" pad="6"/>
<contactref element="L1" pad="10"/>
</signal>
<signal name="PB3">
<contactref element="IC6" pad="4"/>
<contactref element="OK1" pad="7"/>
</signal>
<signal name="PB2">
<contactref element="IC6" pad="3"/>
<contactref element="OK1" pad="5"/>
</signal>
<signal name="PB1">
<contactref element="IC6" pad="2"/>
<contactref element="OK1" pad="3"/>
</signal>
<signal name="PB0">
<contactref element="IC6" pad="1"/>
<contactref element="OK1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC4" pad="2"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC4" pad="1"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC6" pad="13"/>
<contactref element="Y2" pad="2"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="PB4">
<contactref element="IC6" pad="5"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="N$75">
<contactref element="Q1" pad="B"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$79">
<contactref element="OK1" pad="16"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$80">
<contactref element="Q1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$81">
<contactref element="Q2" pad="B"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="N$83">
<contactref element="Q2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="N$82">
<contactref element="R4" pad="P$2"/>
<contactref element="OK1" pad="14"/>
</signal>
<signal name="N$84">
<contactref element="R5" pad="P$2"/>
<contactref element="OK1" pad="12"/>
</signal>
<signal name="N$85">
<contactref element="R6" pad="P$2"/>
<contactref element="OK1" pad="10"/>
</signal>
<signal name="N$86">
<contactref element="Q4" pad="B"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$87">
<contactref element="Q3" pad="B"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$88">
<contactref element="D5" pad="C"/>
<contactref element="Q4" pad="C"/>
<contactref element="X2" pad="5"/>
</signal>
<signal name="N$89">
<contactref element="D4" pad="C"/>
<contactref element="Q3" pad="C"/>
<contactref element="X2" pad="4"/>
</signal>
<signal name="L24">
<contactref element="Q1" pad="E"/>
<contactref element="Q2" pad="E"/>
<contactref element="Q3" pad="E"/>
<contactref element="Q4" pad="E"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="OK2" pad="7"/>
<contactref element="X2" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="OK2" pad="5"/>
<contactref element="X2" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="OK2" pad="3"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="N$20">
<contactref element="OK2" pad="1"/>
<contactref element="X2" pad="9"/>
</signal>
<signal name="M1">
<contactref element="OK1" pad="13"/>
<contactref element="OK1" pad="11"/>
<contactref element="OK1" pad="9"/>
<contactref element="D3" pad="A"/>
<contactref element="D5" pad="A"/>
<contactref element="RN1" pad="1"/>
<contactref element="X2" pad="10"/>
<contactref element="OK1" pad="15"/>
<contactref element="D2" pad="A"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="RN2" pad="11"/>
<contactref element="L1" pad="20"/>
</signal>
<signal name="N$29">
<contactref element="RN2" pad="10"/>
<contactref element="L1" pad="19"/>
</signal>
<signal name="N$34">
<contactref element="RN2" pad="9"/>
<contactref element="L1" pad="18"/>
</signal>
<signal name="N$35">
<contactref element="RN2" pad="8"/>
<contactref element="L1" pad="17"/>
</signal>
<signal name="N$36">
<contactref element="RN2" pad="7"/>
<contactref element="L1" pad="16"/>
</signal>
<signal name="N$37">
<contactref element="RN2" pad="6"/>
<contactref element="L1" pad="15"/>
</signal>
<signal name="N$38">
<contactref element="RN2" pad="5"/>
<contactref element="L1" pad="14"/>
</signal>
<signal name="N$39">
<contactref element="RN2" pad="4"/>
<contactref element="L1" pad="13"/>
</signal>
<signal name="N$40">
<contactref element="RN2" pad="3"/>
<contactref element="L1" pad="12"/>
</signal>
<signal name="N$41">
<contactref element="RN2" pad="2"/>
<contactref element="L1" pad="11"/>
</signal>
<signal name="PB0L">
<contactref element="OK1" pad="2"/>
<contactref element="L1" pad="8"/>
</signal>
<signal name="PB1L">
<contactref element="OK1" pad="4"/>
<contactref element="L1" pad="7"/>
</signal>
<signal name="PB2L">
<contactref element="OK1" pad="6"/>
<contactref element="L1" pad="6"/>
</signal>
<signal name="PB3L">
<contactref element="OK1" pad="8"/>
<contactref element="L1" pad="5"/>
</signal>
<signal name="N$43">
<contactref element="S1" pad="1"/>
<contactref element="RN4" pad="2"/>
</signal>
<signal name="N$54">
<contactref element="S2" pad="1"/>
<contactref element="RN4" pad="3"/>
</signal>
<signal name="N$55">
<contactref element="S3" pad="1"/>
<contactref element="RN4" pad="4"/>
</signal>
<signal name="N$56">
<contactref element="S4" pad="1"/>
<contactref element="RN4" pad="5"/>
</signal>
<signal name="PWM1">
<contactref element="J1" pad="4"/>
<contactref element="IC6" pad="21"/>
</signal>
<signal name="N$9">
<contactref element="RN1" pad="5"/>
<contactref element="OK2" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="OK2" pad="8"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="OK2" pad="6"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="OK2" pad="4"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="RTN">
<contactref element="X1" pad="8"/>
<contactref element="IC9" pad="6"/>
</signal>
<signal name="RTP">
<contactref element="X1" pad="7"/>
<contactref element="IC9" pad="7"/>
</signal>
<signal name="N$23">
<contactref element="D10" pad="A"/>
<contactref element="D11" pad="C"/>
<contactref element="R19" pad="P$2"/>
</signal>
<signal name="N$25">
<contactref element="D10" pad="C"/>
<contactref element="C15" pad="1"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="N$26">
<contactref element="R19" pad="P$1"/>
<contactref element="C16" pad="+"/>
</signal>
<signal name="3.3V">
<contactref element="IC3" pad="3"/>
<contactref element="C6" pad="1"/>
<contactref element="XB1" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="IC2" pad="2"/>
<contactref element="JP8" pad="1"/>
<contactref element="R15" pad="P$2"/>
</signal>
<signal name="N$66">
<contactref element="R7" pad="P$2"/>
<contactref element="R11" pad="P$2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$70">
<contactref element="JP1" pad="2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$111">
<contactref element="JP4" pad="2"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$107">
<contactref element="JP8" pad="2"/>
<contactref element="R16" pad="P$1"/>
</signal>
<signal name="AA">
<contactref element="JP1" pad="1"/>
<contactref element="R7" pad="P$1"/>
<contactref element="JP3" pad="1"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="D6" pad="A"/>
<contactref element="D7" pad="C"/>
<contactref element="IC2" pad="3"/>
<contactref element="R11" pad="P$1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
