<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.1">
<drawing>
<board>
<plain>
<hole x="4" y="4" drill="3.2"/>
<hole x="4" y="32" drill="3.2"/>
<hole x="36" y="32" drill="3.2"/>
<hole x="36" y="4" drill="3.2"/>
<text>Y&lt;-</text>
<text>-&gt;X</text>
<text>Y&lt;-</text>
<text>-&gt;X</text>
<text>-&gt;Y</text>
<text>-&gt;Y</text>
<text>-&gt;X</text>
<text>-&gt;X</text>
<text>SVIS
10/19/18</text>
<text>SVIS
10/19/18</text>
<text>SVIS
10/19/18</text>
<text>SVIS
10/19/18</text>
<wire x1="0" y1="0" x2="0" y2="36" width="0.254" layer="20"/>
<wire x1="0" y1="36" x2="40" y2="36" width="0.254" layer="20"/>
<wire x1="40" y1="36" x2="40" y2="0" width="0.254" layer="20"/>
<wire x1="40" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="svis">
<packages>
<package name="QFN50P400X400X95-25N">
</package>
<package name="SM09B-SRSS-TB">
</package>
</packages>
</library>
<library name="teensy">
<packages>
<package name="TEENSY_3.0-3.2&amp;LC_DIL">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ICM20689" library="svis" package="QFN50P400X400X95-25N" value="ICM-20689">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" 6-Axis Drone/Vr/Iot Solution _Pi "/>
<attribute name="MF" value="TDK-InvenSense"/>
<attribute name="MP" value="ICM-20689"/>
<attribute name="PACKAGE" value="QFN-24 InvenSense"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="CAM1" library="svis" package="SM09B-SRSS-TB" value="SM09B-SRSS-TB">
<attribute name="NAME"/>
</element>
<element name="TEENSY" library="teensy" package="TEENSY_3.0-3.2&amp;LC_DIL" value="TEENSY_3.0_DIL">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07857"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0603" value="2.2uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-07888"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="0.47uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0603" value="10nF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="CAM2" library="svis" package="SM09B-SRSS-TB" value="SM09B-SRSS-TB">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="TEENSY" pad="GND"/>
<contactref element="TEENSY" pad="AGND"/>
<contactref element="ICM20689" pad="11"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="ICM20689" pad="9"/>
<contactref element="CAM1" pad="4"/>
<contactref element="CAM1" pad="2"/>
<contactref element="CAM1" pad="6"/>
<contactref element="CAM2" pad="2"/>
<contactref element="CAM2" pad="4"/>
<contactref element="CAM2" pad="6"/>
<contactref element="ICM20689" pad="25"/>
<contactref element="ICM20689" pad="18"/>
<contactref element="CAM2" pad="9"/>
<contactref element="CAM1" pad="9"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="TEENSY" pad="3.3V"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="ICM20689" pad="8"/>
<contactref element="C4" pad="2"/>
<contactref element="ICM20689" pad="22"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="ICM20689" pad="13"/>
</signal>
<signal name="VIN">
<contactref element="TEENSY" pad="VIN"/>
</signal>
<signal name="IMU_SDA">
<contactref element="ICM20689" pad="24"/>
<contactref element="TEENSY" pad="18/A4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="IMU_SCL">
<contactref element="ICM20689" pad="23"/>
<contactref element="TEENSY" pad="19/A5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C1" pad="1"/>
<contactref element="ICM20689" pad="10"/>
</signal>
<signal name="IMU_INT">
<contactref element="ICM20689" pad="12"/>
<contactref element="TEENSY" pad="20/A6"/>
</signal>
<signal name="CAM1_TX">
<contactref element="CAM1" pad="8"/>
<contactref element="TEENSY" pad="0"/>
</signal>
<signal name="CAM1_RX">
<contactref element="CAM1" pad="7"/>
<contactref element="TEENSY" pad="1"/>
</signal>
<signal name="CAM1_STROBE">
<contactref element="CAM1" pad="5"/>
<contactref element="TEENSY" pad="4"/>
</signal>
<signal name="CAM1_TRIGGER">
<contactref element="CAM1" pad="3"/>
<contactref element="TEENSY" pad="2"/>
</signal>
<signal name="CAM1_IO">
<contactref element="CAM1" pad="1"/>
<contactref element="TEENSY" pad="3"/>
</signal>
<signal name="CAM2_TX">
<contactref element="CAM2" pad="8"/>
<contactref element="TEENSY" pad="9"/>
</signal>
<signal name="CAM2_RX">
<contactref element="CAM2" pad="7"/>
<contactref element="TEENSY" pad="10"/>
</signal>
<signal name="CAM2_TRIGGER">
<contactref element="CAM2" pad="3"/>
<contactref element="TEENSY" pad="6"/>
</signal>
<signal name="CAM2_IO">
<contactref element="CAM2" pad="1"/>
<contactref element="TEENSY" pad="7"/>
</signal>
<signal name="CAM2_STROBE">
<contactref element="CAM2" pad="5"/>
<contactref element="TEENSY" pad="8"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
