<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<circle x="13.97" y="11.43" radius="9.525" width="0.1524" layer="20"/>
<circle x="13.97" y="11.43" radius="6.35" width="0.1524" layer="20"/>
<hole x="13.97" y="11.43" drill="12.7"/>
<text>©2023 BrainOnDrugs
Effects </text>
<text>LED Indicator
Washer PCB v1.0</text>
<text>+9v</text>
<text>GND</text>
</plain>
<libraries>
<library name="PulseOximeterECG_AU">
<description>Generated from &lt;b&gt;PulseOximeterECG_AU.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="supply pins">
<packages>
<package name="AB9V">
<description>&lt;B&gt;9-V BATTERY CLIP&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED2" library="PulseOximeterECG_AU" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="PulseOximeterECG_AU" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="PulseOximeterECG_AU" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07856"/>
<attribute name="VALUE"/>
</element>
<element name="V1" library="supply pins" package="AB9V" value=""/>
</elements>
<signals>
<signal name="+9V">
<contactref element="LED2" pad="A"/>
<contactref element="V1" pad="+"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="LED4" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="AGND">
<contactref element="R1" pad="1"/>
<contactref element="V1" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
