(kicad_pcb (version 20171130) (host pcbnew 5.1.4+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 254)
    (zones 0)
    (modules 5)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.3)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (aux_axis_origin 102 84)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "export/"))
  )
  (net 0 "")
  (net 1 3V3)
  (net 2 GND)
  (net 3 CS)
  (net 4 HOLD)
  (net 5 MISO)
  (net 6 SCK)
  (net 7 WP)
  (net 8 MOSI)
  (net 9 GENIO1)
  (net 10 GENIO2)
  (net 11 GENIO3)
  (net 12 GENIO4)
  (net 13 GENIO5)
  (net 14 GENIO6)
  (net 15 GENIO7)
  (net 16 GENIO8)
  (net 17 GENIO9)
  (net 18 GENIO10)
  (net 19 GENIO11)
  (net 20 GENIO12)
  (net 21 GENIO13)
  (net 22 GENIO14)
  (net 23 GENIO15)
  (net 24 GENIO16)
  (net 25 GENIO17)
  (net 26 GENIO18)
  (net 27 GENIO19)
  (net 28 GENIO20)
  (net 29 GENIO21)
  (net 30 GENIO22)
  (net 31 GENIO23)
  (net 32 GENIO24)
  (net 33 GENIO25)
  (net 34 GENIO26)
  (net 35 GENIO27)
  (net 36 GENIO28)
  (net 37 GENIO29)
  (net 38 GENIO30)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3V3)
    (add_net CS)
    (add_net GENIO1)
    (add_net GENIO10)
    (add_net GENIO11)
    (add_net GENIO12)
    (add_net GENIO13)
    (add_net GENIO14)
    (add_net GENIO15)
    (add_net GENIO16)
    (add_net GENIO17)
    (add_net GENIO18)
    (add_net GENIO19)
    (add_net GENIO2)
    (add_net GENIO20)
    (add_net GENIO21)
    (add_net GENIO22)
    (add_net GENIO23)
    (add_net GENIO24)
    (add_net GENIO25)
    (add_net GENIO26)
    (add_net GENIO27)
    (add_net GENIO28)
    (add_net GENIO29)
    (add_net GENIO3)
    (add_net GENIO30)
    (add_net GENIO4)
    (add_net GENIO5)
    (add_net GENIO6)
    (add_net GENIO7)
    (add_net GENIO8)
    (add_net GENIO9)
    (add_net GND)
    (add_net HOLD)
    (add_net MISO)
    (add_net MOSI)
    (add_net SCK)
    (add_net WP)
  )
  (module Package_SO:TSOP-II-54_22.2x10.16mm_P0.8mm (layer F.Cu) (tedit 5B589EC7)
    (at 123 60.25 90)
    (descr "54-lead TSOP typ II package")
    (tags "TSOPII TSOP2")
    (attr smd)
    (fp_text reference U2 (at 0 -12.5 90) (layer F.SilkS))
    (fp_text value TSOP-II-54-x8 (at 0 12.5 90) (layer F.Fab))
    (fp_text user %R (at -0.606 0.88 90) (layer F.Fab))
    (pad 54 smd rect (at 5.75 -10.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 53 smd rect (at 5.75 -9.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 24 GENIO16))
    (pad 52 smd rect (at 5.75 -8.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 51 smd rect (at 5.75 -8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 50 smd rect (at 5.75 -7.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 25 GENIO17))
    (pad 49 smd rect (at 5.75 -6.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 48 smd rect (at 5.75 -5.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 47 smd rect (at 5.75 -4.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 26 GENIO18))
    (pad 46 smd rect (at 5.75 -4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 45 smd rect (at 5.75 -3.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 44 smd rect (at 5.75 -2.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 27 GENIO19))
    (pad 43 smd rect (at 5.75 -1.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 42 smd rect (at 5.75 -0.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 5.75 0 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 40 smd rect (at 5.75 0.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 5.75 1.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 28 GENIO20))
    (pad 38 smd rect (at 5.75 2.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 29 GENIO21))
    (pad 37 smd rect (at 5.75 3.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 30 GENIO22))
    (pad 36 smd rect (at 5.75 4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 31 GENIO23))
    (pad 35 smd rect (at 5.75 4.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 32 GENIO24))
    (pad 34 smd rect (at 5.75 5.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 33 GENIO25))
    (pad 33 smd rect (at 5.75 6.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 34 GENIO26))
    (pad 32 smd rect (at 5.75 7.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 35 GENIO27))
    (pad 31 smd rect (at 5.75 8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 36 GENIO28))
    (pad 30 smd rect (at 5.75 8.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 37 GENIO29))
    (pad 29 smd rect (at 5.75 9.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 38 GENIO30))
    (pad 28 smd rect (at 5.75 10.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 27 smd rect (at -5.75 10.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 26 smd rect (at -5.75 9.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 23 GENIO15))
    (pad 25 smd rect (at -5.75 8.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 22 GENIO14))
    (pad 24 smd rect (at -5.75 8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 21 GENIO13))
    (pad 23 smd rect (at -5.75 7.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 20 GENIO12))
    (pad 22 smd rect (at -5.75 6.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 19 GENIO11))
    (pad 21 smd rect (at -5.75 5.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 18 GENIO10))
    (pad 20 smd rect (at -5.75 4.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 17 GENIO9))
    (pad 19 smd rect (at -5.75 4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 16 GENIO8))
    (pad 18 smd rect (at -5.75 3.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 15 GENIO7))
    (pad 17 smd rect (at -5.75 2.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 14 GENIO6))
    (pad 16 smd rect (at -5.75 1.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 13 GENIO5))
    (pad 15 smd rect (at -5.75 0.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -5.75 0 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 13 smd rect (at -5.75 -0.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -5.75 -1.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -5.75 -2.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 12 GENIO4))
    (pad 10 smd rect (at -5.75 -3.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -5.75 -4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 8 smd rect (at -5.75 -4.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 11 GENIO3))
    (pad 7 smd rect (at -5.75 -5.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -5.75 -6.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -5.75 -7.2 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 10 GENIO2))
    (pad 4 smd rect (at -5.75 -8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.75 -8.8 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at -5.75 -9.6 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 9 GENIO1))
    (pad 1 smd rect (at -5.75 -10.4 90) (size 1.51 0.458) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-II-54_22.2x10.16mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module inv_hdr:PinHeader_2x20_P2.54mm_Horizontal_Mirrored (layer F.Cu) (tedit 5D72096D)
    (at 105.5 73.8 90)
    (descr "Through hole angled pin header, 2x20, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x20 2.54mm double row")
    (fp_text reference CON1 (at 2.2 -2.5 90) (layer F.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at -3.115 50.53 -90) (layer F.Fab))
    (fp_text user %R (at -2.77 24.13) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 CS))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 HOLD))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 MISO))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 SCK))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 WP))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 MOSI))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 GENIO1))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GENIO2))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GENIO3))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 GENIO4))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 GENIO5))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GENIO6))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GENIO7))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GENIO8))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GENIO9))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GENIO10))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 GENIO11))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 GENIO12))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 GENIO13))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 GENIO14))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 GENIO15))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 GENIO16))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 GENIO17))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 GENIO18))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 GENIO19))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 GENIO20))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 GENIO21))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GENIO22))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 GENIO23))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 GENIO24))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 GENIO25))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 GENIO26))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 GENIO27))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 GENIO28))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 GENIO29))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 GENIO30))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Horizontal.wrl
      (offset (xyz 2.54 -48.26 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 110.5 67.25 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -2.5 0 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at -0.04 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 105 57.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 2.232 -0.0565 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 3V3))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SSOP-8_5.25x5.24mm_P1.27mm (layer F.Cu) (tedit 5B9564B2)
    (at 106.25 63.25 90)
    (descr "SSOP, 8 Pin (http://www.fujitsu.com/ca/en/Images/MB85RS2MT-DS501-00023-1v0-E.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (attr smd)
    (fp_text reference U1 (at -2.7 -3.7 90) (layer F.SilkS))
    (fp_text value W25Q128JVSIQ (at 0 3.57 90) (layer F.Fab))
    (fp_text user %R (at -0.111 -0.447 90) (layer F.Fab))
    (pad 8 smd roundrect (at 3.6125 -1.905 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 3V3))
    (pad 7 smd roundrect (at 3.6125 -0.635 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 HOLD))
    (pad 6 smd roundrect (at 3.6125 0.635 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 SCK))
    (pad 5 smd roundrect (at 3.6125 1.905 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 MOSI))
    (pad 4 smd roundrect (at -3.6125 1.905 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 3 smd roundrect (at -3.6125 0.635 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 WP))
    (pad 2 smd roundrect (at -3.6125 -0.635 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 MISO))
    (pad 1 smd roundrect (at -3.6125 -1.905 90) (size 1.725 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 CS))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-8_5.25x5.24mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 156 52.75) (end 157.5 52.75) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.5 52.75) (end 103.5 51.25) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156 82.5) (end 156 84) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103.5 82.5) (end 102 82.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "SDRAM Cart Rev.B\nJacob Creedon\n@jacobcreedon" (at 146 61.5) (layer F.SilkS))
  (gr_line (start 157.5 52.75) (end 157.5 82.5) (layer Edge.Cuts) (width 0.05))
  (gr_text "3V3\nGND" (at 105.664 69.9135 90) (layer B.SilkS))
  (gr_line (start 103.5 51.25) (end 156 51.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102 82.5) (end 102 52.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156 84) (end 103.5 84) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102 84) (xy 102 51.25) (xy 157.5 51.25) (xy 157.5 84)
      )
    )
  )
)
