(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 710)
    (zones 0)
    (modules 54)
    (nets 135)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.152)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.9)
    (user_trace_width 1.2)
    (trace_clearance 0.152)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.152)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 8 8)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber"))
  )
  (net 0 "")
  (net 1 /+TMDS_CLK)
  (net 2 /-TMDS_0)
  (net 3 /+TMDS_0)
  (net 4 /-TMDS_1)
  (net 5 /+TMDS_1)
  (net 6 /-TMDS_2)
  (net 7 /+TMDS_2)
  (net 8 /-TMDS_CLK)
  (net 9 "Net-(J1-Pad13)")
  (net 10 "Net-(J1-Pad14)")
  (net 11 "Net-(J1-Pad15)")
  (net 12 "Net-(J1-Pad16)")
  (net 13 "Net-(J2-Pad3)")
  (net 14 /GND)
  (net 15 /+5)
  (net 16 "Net-(J2-Pad4)")
  (net 17 "Net-(J2-Pad2)")
  (net 18 /+3.3)
  (net 19 "Net-(U1-Pad3)")
  (net 20 "Net-(U1-Pad8)")
  (net 21 "Net-(U1-Pad9)")
  (net 22 "Net-(U1-Pad10)")
  (net 23 "Net-(U1-Pad14)")
  (net 24 /TMS)
  (net 25 /TCK)
  (net 26 /TDI)
  (net 27 /TDO)
  (net 28 "Net-(U1-Pad19)")
  (net 29 "Net-(U1-Pad21)")
  (net 30 "Net-(U1-Pad23)")
  (net 31 "Net-(U1-Pad25)")
  (net 32 "Net-(U1-Pad26)")
  (net 33 "Net-(U1-Pad31)")
  (net 34 "Net-(U1-Pad80)")
  (net 35 "Net-(U1-Pad81)")
  (net 36 "Net-(U1-Pad84)")
  (net 37 "Net-(U1-Pad85)")
  (net 38 "Net-(U1-Pad86)")
  (net 39 "Net-(U1-Pad87)")
  (net 40 /27CLK)
  (net 41 "Net-(U1-Pad89)")
  (net 42 "Net-(U1-Pad90)")
  (net 43 "Net-(U1-Pad91)")
  (net 44 "Net-(U1-Pad92)")
  (net 45 "Net-(U1-Pad94)")
  (net 46 "Net-(U1-Pad95)")
  (net 47 "Net-(U1-Pad97)")
  (net 48 "Net-(U1-Pad98)")
  (net 49 "Net-(U1-Pad99)")
  (net 50 "Net-(U1-Pad100)")
  (net 51 "Net-(U1-Pad101)")
  (net 52 "Net-(U1-Pad103)")
  (net 53 "Net-(U1-Pad105)")
  (net 54 "Net-(U1-Pad106)")
  (net 55 "Net-(U1-Pad112)")
  (net 56 "Net-(U1-Pad113)")
  (net 57 "Net-(U1-Pad114)")
  (net 58 "Net-(U1-Pad117)")
  (net 59 "Net-(U1-Pad123)")
  (net 60 "Net-(U1-Pad124)")
  (net 61 "Net-(U1-Pad125)")
  (net 62 "Net-(U1-Pad126)")
  (net 63 "Net-(U1-Pad127)")
  (net 64 "Net-(U1-Pad128)")
  (net 65 "Net-(U1-Pad129)")
  (net 66 "Net-(U1-Pad130)")
  (net 67 "Net-(U1-Pad134)")
  (net 68 "Net-(U1-Pad137)")
  (net 69 "Net-(U1-Pad138)")
  (net 70 "Net-(U1-Pad139)")
  (net 71 "Net-(U1-Pad140)")
  (net 72 "Net-(U1-Pad141)")
  (net 73 "Net-(J3-Pad6)")
  (net 74 "Net-(J3-Pad8)")
  (net 75 "Net-(J3-Pad7)")
  (net 76 "Net-(U1-Pad55)")
  (net 77 "Net-(U3-Pad6)")
  (net 78 "Net-(U3-Pad7)")
  (net 79 "Net-(U3-Pad8)")
  (net 80 "Net-(U3-Pad49)")
  (net 81 /HPD)
  (net 82 "Net-(R5-Pad2)")
  (net 83 "Net-(R6-Pad2)")
  (net 84 "Net-(R7-Pad1)")
  (net 85 /DE)
  (net 86 /HSYNC)
  (net 87 /VSYNC)
  (net 88 /SDA)
  (net 89 /SCL)
  (net 90 /DVI_CLK)
  (net 91 "Net-(U1-Pad88)")
  (net 92 /D23)
  (net 93 /D22)
  (net 94 /D21)
  (net 95 /D20)
  (net 96 /D19)
  (net 97 /D18)
  (net 98 /D17)
  (net 99 /D16)
  (net 100 /D15)
  (net 101 /D14)
  (net 102 /D13)
  (net 103 /D12)
  (net 104 /D11)
  (net 105 /D10)
  (net 106 /D9)
  (net 107 /D8)
  (net 108 /D7)
  (net 109 /D6)
  (net 110 /D5)
  (net 111 /D4)
  (net 112 /D3)
  (net 113 /D2)
  (net 114 /D1)
  (net 115 /D0)
  (net 116 /+3.3_DVI)
  (net 117 /SENSOR)
  (net 118 "Net-(R10-Pad2)")
  (net 119 "Net-(R11-Pad2)")
  (net 120 "Net-(R12-Pad2)")
  (net 121 "Net-(R13-Pad2)")
  (net 122 "Net-(R15-Pad2)")
  (net 123 /DVI_RST)
  (net 124 "Net-(SW1-Pad5)")
  (net 125 "Net-(SW1-Pad6)")
  (net 126 "Net-(SW1-Pad7)")
  (net 127 "Net-(SW1-Pad8)")
  (net 128 /A)
  (net 129 /C)
  (net 130 /B)
  (net 131 "Net-(D1-Pad1)")
  (net 132 "Net-(D1-Pad2)")
  (net 133 "Net-(U1-Pad28)")
  (net 134 "Net-(U1-Pad32)")
  (net_class Default "This is the default net class."
    (clearance 0.152)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3.3)
    (add_net /+3.3_DVI)
    (add_net /+5)
    (add_net /+TMDS_0)
    (add_net /+TMDS_1)
    (add_net /+TMDS_2)
    (add_net /+TMDS_CLK)
    (add_net /-TMDS_0)
    (add_net /-TMDS_1)
    (add_net /-TMDS_2)
    (add_net /-TMDS_CLK)
    (add_net /27CLK)
    (add_net /A)
    (add_net /B)
    (add_net /C)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D14)
    (add_net /D15)
    (add_net /D16)
    (add_net /D17)
    (add_net /D18)
    (add_net /D19)
    (add_net /D2)
    (add_net /D20)
    (add_net /D21)
    (add_net /D22)
    (add_net /D23)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /DE)
    (add_net /DVI_CLK)
    (add_net /DVI_RST)
    (add_net /GND)
    (add_net /HPD)
    (add_net /HSYNC)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SENSOR)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /VSYNC)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(SW1-Pad5)")
    (add_net "Net-(SW1-Pad6)")
    (add_net "Net-(SW1-Pad7)")
    (add_net "Net-(SW1-Pad8)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad100)")
    (add_net "Net-(U1-Pad101)")
    (add_net "Net-(U1-Pad103)")
    (add_net "Net-(U1-Pad105)")
    (add_net "Net-(U1-Pad106)")
    (add_net "Net-(U1-Pad112)")
    (add_net "Net-(U1-Pad113)")
    (add_net "Net-(U1-Pad114)")
    (add_net "Net-(U1-Pad117)")
    (add_net "Net-(U1-Pad123)")
    (add_net "Net-(U1-Pad124)")
    (add_net "Net-(U1-Pad125)")
    (add_net "Net-(U1-Pad126)")
    (add_net "Net-(U1-Pad127)")
    (add_net "Net-(U1-Pad128)")
    (add_net "Net-(U1-Pad129)")
    (add_net "Net-(U1-Pad130)")
    (add_net "Net-(U1-Pad134)")
    (add_net "Net-(U1-Pad137)")
    (add_net "Net-(U1-Pad138)")
    (add_net "Net-(U1-Pad139)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad140)")
    (add_net "Net-(U1-Pad141)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad80)")
    (add_net "Net-(U1-Pad81)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad86)")
    (add_net "Net-(U1-Pad87)")
    (add_net "Net-(U1-Pad88)")
    (add_net "Net-(U1-Pad89)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U1-Pad90)")
    (add_net "Net-(U1-Pad91)")
    (add_net "Net-(U1-Pad92)")
    (add_net "Net-(U1-Pad94)")
    (add_net "Net-(U1-Pad95)")
    (add_net "Net-(U1-Pad97)")
    (add_net "Net-(U1-Pad98)")
    (add_net "Net-(U1-Pad99)")
    (add_net "Net-(U3-Pad49)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
  )
  (module Housings_QFP:TQFP-64_1EP_10x10mm_Pitch0.5mm (layer F.Cu) (tedit 5C51CDE4)
    (at 119 91 90)
    (descr "64-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1 mm Body, 2.00 mm Footprint [TQFP] thermal pad")
    (tags "QFP 0.5 ")
    (attr smd)
    (fp_text reference U3 (at 0 -7.45 90) (layer F.SilkS))
    (fp_text value TFP410PAP (at -3.5 0.2 180) (layer F.Fab) hide)
    (fp_text user %R (at 7.5 -5.9 180) (layer F.Fab))
    (pad 65 thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 2.8) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 3 -3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 smd rect (at 0 0 270) (size 8 8) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 64 smd rect (at -3.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 63 smd rect (at -3.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 115 /D0))
    (pad 62 smd rect (at -2.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 114 /D1))
    (pad 61 smd rect (at -2.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 113 /D2))
    (pad 60 smd rect (at -1.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 112 /D3))
    (pad 59 smd rect (at -1.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 111 /D4))
    (pad 58 smd rect (at -0.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 110 /D5))
    (pad 57 smd rect (at -0.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 90 /DVI_CLK))
    (pad 56 smd rect (at 0.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 55 smd rect (at 0.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 109 /D6))
    (pad 54 smd rect (at 1.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 108 /D7))
    (pad 53 smd rect (at 1.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 107 /D8))
    (pad 52 smd rect (at 2.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 106 /D9))
    (pad 51 smd rect (at 2.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 105 /D10))
    (pad 50 smd rect (at 3.25 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 104 /D11))
    (pad 49 smd rect (at 3.75 -5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U3-Pad49)"))
    (pad 48 smd rect (at 5.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 47 smd rect (at 5.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 103 /D12))
    (pad 46 smd rect (at 5.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 102 /D13))
    (pad 45 smd rect (at 5.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 101 /D14))
    (pad 44 smd rect (at 5.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 100 /D15))
    (pad 43 smd rect (at 5.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 99 /D16))
    (pad 42 smd rect (at 5.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 98 /D17))
    (pad 41 smd rect (at 5.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 97 /D18))
    (pad 40 smd rect (at 5.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 /D19))
    (pad 39 smd rect (at 5.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 /D20))
    (pad 38 smd rect (at 5.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 /D21))
    (pad 37 smd rect (at 5.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 /D22))
    (pad 36 smd rect (at 5.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 92 /D23))
    (pad 35 smd rect (at 5.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 34 smd rect (at 5.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 33 smd rect (at 5.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 32 smd rect (at 3.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 31 smd rect (at 3.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /+TMDS_2))
    (pad 30 smd rect (at 2.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /-TMDS_2))
    (pad 29 smd rect (at 2.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 28 smd rect (at 1.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /+TMDS_1))
    (pad 27 smd rect (at 1.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /-TMDS_1))
    (pad 26 smd rect (at 0.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 25 smd rect (at 0.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /+TMDS_0))
    (pad 24 smd rect (at -0.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /-TMDS_0))
    (pad 23 smd rect (at -0.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 22 smd rect (at -1.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /+TMDS_CLK))
    (pad 21 smd rect (at -1.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /-TMDS_CLK))
    (pad 20 smd rect (at -2.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 19 smd rect (at -2.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R6-Pad2)"))
    (pad 18 smd rect (at -3.25 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 17 smd rect (at -3.75 5.7 180) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 16 smd rect (at -5.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 15 smd rect (at -5.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 /SCL))
    (pad 14 smd rect (at -5.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 88 /SDA))
    (pad 13 smd rect (at -5.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 123 /DVI_RST))
    (pad 12 smd rect (at -5.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 11 smd rect (at -5.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R7-Pad1)"))
    (pad 10 smd rect (at -5.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 9 smd rect (at -5.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R5-Pad2)"))
    (pad 8 smd rect (at -5.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(U3-Pad8)"))
    (pad 7 smd rect (at -5.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(U3-Pad7)"))
    (pad 6 smd rect (at -5.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(U3-Pad6)"))
    (pad 5 smd rect (at -5.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 87 /VSYNC))
    (pad 4 smd rect (at -5.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 86 /HSYNC))
    (pad 3 smd rect (at -5.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 2 smd rect (at -5.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 85 /DE))
    (pad 1 smd rect (at -5.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 65 thru_hole circle (at 3 -2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 3 -1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 3 0 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 3 1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 3 2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 3 3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -3 3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -3 2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 0 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 -1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 -2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 2 -3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 -3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 -3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 -3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 -3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -3 -3 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -3 -2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -3 -1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -3 0 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -3 1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 0 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 -1 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -2 -2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at -1 -2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 0 -2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 65 thru_hole circle (at 1 -2 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:HDMI_THRU (layer F.Cu) (tedit 5C51CC0B)
    (at 131.125 84.5 90)
    (fp_text reference J1 (at -7 -4 90) (layer F.SilkS))
    (fp_text value HDMI_A (at 0.875 6.725 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 4.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 7 /+TMDS_2))
    (pad 3 thru_hole circle (at 3.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 6 /-TMDS_2))
    (pad 5 thru_hole circle (at 2.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 7 thru_hole circle (at 1.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 3 /+TMDS_0))
    (pad 9 thru_hole circle (at 0.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 2 /-TMDS_0))
    (pad 11 thru_hole circle (at -0.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 13 thru_hole circle (at -1.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad13)"))
    (pad 15 thru_hole circle (at -2.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad15)"))
    (pad 17 thru_hole circle (at -3.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 19 thru_hole circle (at -4.5 0 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 81 /HPD))
    (pad 2 thru_hole circle (at 4 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 4 thru_hole circle (at 3 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 5 /+TMDS_1))
    (pad 6 thru_hole circle (at 2 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 4 /-TMDS_1))
    (pad 8 thru_hole circle (at 1 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 10 thru_hole circle (at 0 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 1 /+TMDS_CLK))
    (pad 12 thru_hole circle (at -1 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 8 /-TMDS_CLK))
    (pad 14 thru_hole circle (at -2 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad14)"))
    (pad 16 thru_hole circle (at -3 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad16)"))
    (pad 18 thru_hole circle (at -4 0.8 90) (size 0.75 0.75) (drill 0.45) (layers *.Cu *.Mask)
      (net 15 /+5))
    (pad SH thru_hole oval (at 7.25 0.4 90) (size 1.2 2.6) (drill oval 0.9 2.3) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad SH thru_hole oval (at -7.25 0.4 90) (size 1.2 2.6) (drill oval 0.9 2.3) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad SH thru_hole oval (at 7.25 6.34 90) (size 1.3 2.1) (drill oval 1 1.8) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad SH thru_hole oval (at -7.25 6.34 90) (size 1.3 2.1) (drill oval 1 1.8) (layers *.Cu *.Mask)
      (net 14 /GND))
  )
  (module digikey-footprints:USB_Mini_B_Female_548190519 (layer F.Cu) (tedit 5C3E27AF)
    (at 131.55 110.35 180)
    (fp_text reference J2 (at -6.35 0.95 180) (layer F.SilkS))
    (fp_text value USB_B_Mini (at -1.15 -3.35) (layer F.Fab))
    (fp_text user %R (at -5.7 -0.075 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 0 180) (size 1.65 1.1) (drill 0.7 (offset 0.275 0)) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad3)"))
    (pad 5 thru_hole oval (at 0 -1.6 180) (size 1.65 1.1) (drill 0.7 (offset 0.275 0)) (layers *.Cu *.Mask)
      (net 15 /+5))
    (pad 1 thru_hole oval (at 0 1.6 180) (size 1.65 1.1) (drill 0.7 (offset 0.275 0)) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 4 thru_hole oval (at -1.2 -0.8 180) (size 1.65 1.1) (drill 0.7 (offset -0.275 0)) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad4)"))
    (pad 2 thru_hole oval (at -1.2 0.8 180) (size 1.65 1.1) (drill 0.7 (offset -0.275 0)) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad2)"))
    (pad 6 thru_hole oval (at -5.05 -3.65 180) (size 2.7 1.7) (drill oval 1.9 0.7) (layers *.Cu *.Mask)
      (net 14 /GND))
    (pad 6 thru_hole oval (at -5.05 3.65 180) (size 2.7 1.7) (drill oval 1.9 0.7) (layers *.Cu *.Mask)
      (net 14 /GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E260F)
    (at 126.02 92.94 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value .1u (at 0 -0.06 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 116 /+3.3_DVI))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E2A16)
    (at 78.1 94.8)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 1.7) (layer F.SilkS))
    (fp_text value 10K (at 0 0.1 90) (layer F.Fab))
    (fp_text user %R (at 0 1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R13-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E29FA)
    (at 78.1 92.8)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -3.2 0.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at -3.2 0.1 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R12-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2509)
    (at 103.9 96.55)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 1.75) (layer B.SilkS))
    (fp_text value INDUCTOR (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 116 /+3.3_DVI))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C3E39F5)
    (at 75.92 102.77 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0.08 1.96 270) (layer B.SilkS))
    (fp_text value 10K (at -0.017678 0.017678 180) (layer B.Fab))
    (fp_text user %R (at 0.05 1.99 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 130 /B))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C3E3A29)
    (at 78.6 102.825 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -0.029999) (layer B.Fab))
    (fp_text user %R (at 0 1.670001 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 128 /A))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2627)
    (at 126.03 86.89 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value .1u (at -0.07 -0.01 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 116 /+3.3_DVI))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E2A2D)
    (at 78.15 87.3)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 10K (at 0 0.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E25F4)
    (at 125.89 96.43 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at -3.71 0.03 180) (layer B.SilkS))
    (fp_text value .1u (at -0.01 0.03 270) (layer B.Fab))
    (fp_text user %R (at -3.71 0.03 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 116 /+3.3_DVI))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C530087)
    (at 113.03 95.32 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 10u (at 0 -0.07) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 116 /+3.3_DVI))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E29D4)
    (at 78.15 89.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -3.25 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0.1 90) (layer F.Fab))
    (fp_text user %R (at -3.25 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E3082)
    (at 99 106 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 89 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C3E3CEA)
    (at 104 106)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7) (layer B.SilkS))
    (fp_text value 150 (at 0 0 -90) (layer B.Fab))
    (fp_text user %R (at 0 1.675) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 117 /SENSOR))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5C3E39BD)
    (at 70.9 102.825 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 10K (at 0.05 0.025 180) (layer B.Fab))
    (fp_text user %R (at 0 1.7 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 129 /C))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E257C)
    (at 117.62 97.83 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value .1u (at -0.07 -0.02 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 116 /+3.3_DVI))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E3CB0)
    (at 71.05 93.675 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1K (at -0.025 0 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.675) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-5MM (layer B.Cu) (tedit 5C3E3D16)
    (at 113.1376 100.975308 180)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference R2 (at -2.2874 0.125308 270) (layer B.SilkS))
    (fp_text value R_PHOTO (at 4.2626 1.725308 180) (layer B.Fab) hide)
    (fp_text user K (at 4.4876 2.450308 180) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 117 /SENSOR))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 14 /GND))
    (model LEDs.3dshapes/LED-5MM.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-5MM (layer F.Cu) (tedit 5570F7EA)
    (at 71.6 89.625 90)
    (descr "LED 5mm round vertical")
    (tags "LED 5mm round vertical")
    (fp_text reference D1 (at 5.35 0.025 180) (layer F.SilkS))
    (fp_text value LED (at 0.15 -1.975 90) (layer F.Fab))
    (fp_text user K (at -1.905 1.905 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.9 1.9) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E24E2)
    (at 94.21 101.97 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value .1u (at 0.03 -0.09) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E2814)
    (at 131.67 103.12 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 510 (at -0.03 -0.08 270) (layer F.Fab))
    (fp_text user %R (at -0.03 -1.68) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E283B)
    (at 128.84 100.28 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -3.36 -0.02 180) (layer F.SilkS))
    (fp_text value 5K (at -0.06 0.08 270) (layer F.Fab))
    (fp_text user %R (at -3.36 -0.02 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E28C1)
    (at 134.45 96.45 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 1k (at -0.05 -0.05) (layer F.Fab))
    (fp_text user %R (at 0 -1.65 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R5-Pad2)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 81 /HPD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2454)
    (at 83.33 89.11 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.43 0.01 180) (layer B.SilkS))
    (fp_text value .1u (at 0.13 0.01 270) (layer B.Fab))
    (fp_text user %R (at 3.53 0.01 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E28E6)
    (at 130.22 96.39 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.68 90) (layer F.SilkS))
    (fp_text value 10K (at 0 -0.02 180) (layer F.Fab))
    (fp_text user %R (at -0.01 1.68 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad16)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /+5))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E290A)
    (at 127.88 96.42 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -1.58 -1.48 90) (layer F.SilkS))
    (fp_text value 10K (at -0.08 0.02 180) (layer F.Fab))
    (fp_text user %R (at -1.58 -1.48 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /+5))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad15)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E289B)
    (at 118.16 101.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 2.2K (at 0 0.04) (layer F.Fab))
    (fp_text user %R (at 0 -1.66 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 116 /+3.3_DVI))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 123 /DVI_RST))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E287D)
    (at 123.24 100.3 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 1.46 -1.6 180) (layer F.SilkS))
    (fp_text value 2.2K (at 0.06 0 270) (layer F.Fab))
    (fp_text user %R (at 1.46 -1.6 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 88 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2485)
    (at 83.339999 91.7 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.539999 0.1 180) (layer B.SilkS))
    (fp_text value .1u (at 0.039999 0 270) (layer B.Fab))
    (fp_text user %R (at 3.539999 -0.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E24F4)
    (at 101.58 101.89 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value .1u (at 0.01 -0.02) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E24D2)
    (at 88.05 101.92 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value .1u (at 0.08 -0.05) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E251C)
    (at 101.4 87.09)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 1.75) (layer B.SilkS))
    (fp_text value .1u (at 0 0.01 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E24BF)
    (at 83.34 96.82 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 3.44 0.02 180) (layer B.SilkS))
    (fp_text value .1u (at 0.04 0.02 270) (layer B.Fab))
    (fp_text user %R (at 3.44 0.02 180) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3CFDF9)
    (at 122.25 108.24 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.36 -2.45 90) (layer B.SilkS))
    (fp_text value 10u (at 0 0) (layer B.Fab))
    (fp_text user %R (at -3.46 -2.45 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2 (layer F.Cu) (tedit 5C3CFE0A)
    (at 124.592782 106.349344 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0.750656 -2.007218) (layer F.SilkS))
    (fp_text value TC1264-3.3VDBTR (at -1.414214 2.12132) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 270) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /+5))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3CFFF5)
    (at 119.74 108.23 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -3.57 2.66 90) (layer B.SilkS))
    (fp_text value .1u (at 0.070711 -0.070711) (layer B.Fab))
    (fp_text user %R (at -3.47 2.56 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2446)
    (at 83.34 84.24 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 3.74 0.04 180) (layer B.SilkS))
    (fp_text value .1u (at 0.04 0.04 270) (layer B.Fab))
    (fp_text user %R (at 3.74 0.04 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E252B)
    (at 101.41 83.6)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 1.75) (layer B.SilkS))
    (fp_text value .1u (at 0 -0.1 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:SS-10-23NP-LE (layer F.Cu) (tedit 5C3E36A1)
    (at 78.5 99 270)
    (fp_text reference SW1 (at -0.875 9.325 270) (layer F.SilkS))
    (fp_text value SW_Coded (at 9.35 6.3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 /A))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 /B))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /+3.3))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 /C))
    (pad 5 thru_hole circle (at 7.62 7.62 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(SW1-Pad5)"))
    (pad 6 thru_hole circle (at 7.62 5.08 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(SW1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 2.54 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(SW1-Pad7)"))
    (pad 8 thru_hole circle (at 7.62 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(SW1-Pad8)"))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2539)
    (at 99.95 79.41 45)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 1.75 45) (layer B.SilkS))
    (fp_text value .1u (at 0.113137 0.098995 135) (layer B.Fab))
    (fp_text user %R (at 0 1.75 45) (layer B.Fab))
    (pad 1 smd rect (at -1.249999 0 45) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.249999 0 45) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2557)
    (at 87.91 78.75 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value .1u (at 0 0.09 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3E2546)
    (at 95.27 78.74 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value .1u (at 0.04 0.03 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /+3.3))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Altera:altera144_wcenterpad (layer F.Cu) (tedit 5C51CD85)
    (at 94.95 90.55 90)
    (attr smd)
    (fp_text reference U1 (at -10.4 -10.2 180) (layer F.SilkS))
    (fp_text value 10M02SCE144I7G (at 6.32 0.11 180) (layer F.Fab))
    (pad 1 smd rect (at -10.7 -8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 2 smd rect (at -10.7 -8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 3 smd rect (at -10.7 -7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -10.7 -7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 128 /A))
    (pad 5 smd rect (at -10.7 -6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 130 /B))
    (pad 6 smd rect (at -10.7 -6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 129 /C))
    (pad 7 smd rect (at -10.7 -5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 117 /SENSOR))
    (pad 8 smd rect (at -10.7 -5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at -10.7 -4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at -10.7 -4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at -10.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 12 smd rect (at -10.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 13 smd rect (at -10.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R15-Pad2)"))
    (pad 14 smd rect (at -10.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at -10.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /TMS))
    (pad 16 smd rect (at -10.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /TCK))
    (pad 17 smd rect (at -10.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /TDI))
    (pad 18 smd rect (at -10.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /TDO))
    (pad 19 smd rect (at -10.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at -10.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 21 smd rect (at -10.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at -10.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 23 smd rect (at -10.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at -10.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 89 /SCL))
    (pad 25 smd rect (at -10.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at -10.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad26)"))
    (pad 27 smd rect (at -10.7 4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /27CLK))
    (pad 28 smd rect (at -10.7 4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at -10.7 5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 30 smd rect (at -10.7 5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 31 smd rect (at -10.7 6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad31)"))
    (pad 32 smd rect (at -10.7 6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(U1-Pad32)"))
    (pad 33 smd rect (at -10.7 7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 90 /DVI_CLK))
    (pad 34 smd rect (at -10.7 7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 35 smd rect (at -10.7 8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 36 smd rect (at -10.7 8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 37 smd rect (at -8.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 38 smd rect (at -8.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 39 smd rect (at -7.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 88 /SDA))
    (pad 40 smd rect (at -7.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 123 /DVI_RST))
    (pad 41 smd rect (at -6.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 87 /VSYNC))
    (pad 42 smd rect (at -6.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 86 /HSYNC))
    (pad 43 smd rect (at -5.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 44 smd rect (at -5.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 85 /DE))
    (pad 45 smd rect (at -4.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 46 smd rect (at -4.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 115 /D0))
    (pad 47 smd rect (at -3.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 114 /D1))
    (pad 48 smd rect (at -3.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 113 /D2))
    (pad 49 smd rect (at -2.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 112 /D3))
    (pad 50 smd rect (at -2.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 111 /D4))
    (pad 51 smd rect (at -1.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 110 /D5))
    (pad 52 smd rect (at -1.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 109 /D6))
    (pad 53 smd rect (at -0.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 108 /D7))
    (pad 54 smd rect (at -0.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 107 /D8))
    (pad 55 smd rect (at 0.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(U1-Pad55)"))
    (pad 56 smd rect (at 0.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 57 smd rect (at 1.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 58 smd rect (at 1.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 59 smd rect (at 2.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 106 /D9))
    (pad 60 smd rect (at 2.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 105 /D10))
    (pad 61 smd rect (at 3.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 104 /D11))
    (pad 62 smd rect (at 3.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 103 /D12))
    (pad 63 smd rect (at 4.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 102 /D13))
    (pad 64 smd rect (at 4.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 65 smd rect (at 5.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 101 /D14))
    (pad 66 smd rect (at 5.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 67 smd rect (at 6.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 100 /D15))
    (pad 68 smd rect (at 6.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 99 /D16))
    (pad 69 smd rect (at 7.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 98 /D17))
    (pad 70 smd rect (at 7.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 97 /D18))
    (pad 71 smd rect (at 8.25 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 72 smd rect (at 8.75 10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 73 smd rect (at 10.7 8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 74 smd rect (at 10.7 8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 96 /D19))
    (pad 75 smd rect (at 10.7 7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 95 /D20))
    (pad 76 smd rect (at 10.7 7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 94 /D21))
    (pad 77 smd rect (at 10.7 6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 78 smd rect (at 10.7 6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 93 /D22))
    (pad 79 smd rect (at 10.7 5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 92 /D23))
    (pad 80 smd rect (at 10.7 5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U1-Pad80)"))
    (pad 81 smd rect (at 10.7 4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U1-Pad81)"))
    (pad 82 smd rect (at 10.7 4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 83 smd rect (at 10.7 3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 84 smd rect (at 10.7 3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U1-Pad84)"))
    (pad 85 smd rect (at 10.7 2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad85)"))
    (pad 86 smd rect (at 10.7 2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad86)"))
    (pad 87 smd rect (at 10.7 1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad87)"))
    (pad 88 smd rect (at 10.7 1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U1-Pad88)"))
    (pad 89 smd rect (at 10.7 0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad89)"))
    (pad 90 smd rect (at 10.7 0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad90)"))
    (pad 91 smd rect (at 10.7 -0.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad91)"))
    (pad 92 smd rect (at 10.7 -0.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad92)"))
    (pad 93 smd rect (at 10.7 -1.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 94 smd rect (at 10.7 -1.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad94)"))
    (pad 95 smd rect (at 10.7 -2.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad95)"))
    (pad 96 smd rect (at 10.7 -2.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 97 smd rect (at 10.7 -3.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad97)"))
    (pad 98 smd rect (at 10.7 -3.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U1-Pad98)"))
    (pad 99 smd rect (at 10.7 -4.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U1-Pad99)"))
    (pad 100 smd rect (at 10.7 -4.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U1-Pad100)"))
    (pad 101 smd rect (at 10.7 -5.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U1-Pad101)"))
    (pad 102 smd rect (at 10.7 -5.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 103 smd rect (at 10.7 -6.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U1-Pad103)"))
    (pad 104 smd rect (at 10.7 -6.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 105 smd rect (at 10.7 -7.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U1-Pad105)"))
    (pad 106 smd rect (at 10.7 -7.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U1-Pad106)"))
    (pad 107 smd rect (at 10.7 -8.25 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 108 smd rect (at 10.7 -8.75 90) (size 1.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 109 smd rect (at 8.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 110 smd rect (at 8.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 111 smd rect (at 7.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 112 smd rect (at 7.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U1-Pad112)"))
    (pad 113 smd rect (at 6.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U1-Pad113)"))
    (pad 114 smd rect (at 6.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U1-Pad114)"))
    (pad 115 smd rect (at 5.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(D1-Pad2)"))
    (pad 116 smd rect (at 5.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 117 smd rect (at 4.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U1-Pad117)"))
    (pad 118 smd rect (at 4.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 119 smd rect (at 3.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 120 smd rect (at 3.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(R11-Pad2)"))
    (pad 121 smd rect (at 2.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 122 smd rect (at 2.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(R10-Pad2)"))
    (pad 123 smd rect (at 1.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U1-Pad123)"))
    (pad 124 smd rect (at 1.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U1-Pad124)"))
    (pad 125 smd rect (at 0.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U1-Pad125)"))
    (pad 126 smd rect (at 0.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U1-Pad126)"))
    (pad 127 smd rect (at -0.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U1-Pad127)"))
    (pad 128 smd rect (at -0.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U1-Pad128)"))
    (pad 129 smd rect (at -1.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U1-Pad129)"))
    (pad 130 smd rect (at -1.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U1-Pad130)"))
    (pad 131 smd rect (at -2.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(R12-Pad2)"))
    (pad 132 smd rect (at -2.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 133 smd rect (at -3.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 134 smd rect (at -3.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U1-Pad134)"))
    (pad 135 smd rect (at -4.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(R13-Pad2)"))
    (pad 136 smd rect (at -4.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 137 smd rect (at -5.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U1-Pad137)"))
    (pad 138 smd rect (at -5.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U1-Pad138)"))
    (pad 139 smd rect (at -6.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U1-Pad139)"))
    (pad 140 smd rect (at -6.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U1-Pad140)"))
    (pad 141 smd rect (at -7.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U1-Pad141)"))
    (pad 142 smd rect (at -7.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 143 smd rect (at -8.25 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (pad 144 smd rect (at -8.75 -10.7 90) (size 0.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (pad 145 smd rect (at 0 0 90) (size 6.7 6.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -2 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -3 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at -1 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 2.8) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 0 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 1 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 -3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 3 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 3 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 0 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 -1 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (pad 145 thru_hole circle (at 2 -2 90) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 14 /GND) (zone_connect 2))
    (model ../../electronics/kicad/3d/smd_lqfp/tqfp-144.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5AB29A19)
    (at 123.75 78.525)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5C3CFE16)
    (at 128.75 109.99 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.09 -1.85 270) (layer B.SilkS))
    (fp_text value 10u (at 0.015722 -0.049497 180) (layer B.Fab))
    (fp_text user %R (at 0.09 -1.85 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 /+5))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E2999)
    (at 80 113 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 10K (at 0 0 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /TCK))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C3E2989)
    (at 80 111)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "Net-(R15-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /+3.3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:IDC_Header_Straight_10pins (layer F.Cu) (tedit 0)
    (at 88 113)
    (descr "10 pins through hole IDC header")
    (tags "IDC header socket VASCH")
    (fp_text reference J3 (at 5.08 -7.62) (layer F.SilkS))
    (fp_text value AVR-JTAG-10 (at 5.1 2.9) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /TCK))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /TDO))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /+3.3))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /TMS))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J3-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /TDI))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /GND))
  )
  (module Oscillators:Oscillator_DIP-8 (layer F.Cu) (tedit 58CD3344)
    (at 109 107 270)
    (descr "Oscillator, DIP8,http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
    (tags oscillator)
    (fp_text reference X1 (at -0.2 -2.7) (layer F.SilkS))
    (fp_text value CXO_DIP8 (at 2.1 -2.4) (layer F.Fab))
    (fp_text user %R (at 0.1 -2.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /+3.3))
    (pad 8 thru_hole circle (at 0 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /+3.3))
    (pad 5 thru_hole circle (at 7.62 -7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /27CLK))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /GND))
    (model ${KISYS3DMOD}/Oscillators.3dshapes/Oscillator_DIP-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5AB29A19)
    (at 124.85 114.475)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5AB29A19)
    (at 73 79)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
  )
  (module pads:2.3_hole_mount (layer F.Cu) (tedit 5AB29A19)
    (at 73 114)
    (fp_text reference "" (at 0 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 -0.5) (layer F.Fab))
    (pad "" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.3) (layers *.Cu *.Mask))
  )
  (gr_text "TIME SLEUTH 1.1" (at 109.5 86.5 90) (layer F.SilkS))
  (gr_line (start 67 75) (end 67 118) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139 75) (end 67 75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 139 118) (end 139 75) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 67 118) (end 139 118) (layer Edge.Cuts) (width 0.2))
  (zone (net 14) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 118) (xy 139 118) (xy 139 75) (xy 67 75)
      )
    )
  )
  (zone (net 14) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 118) (xy 139 118) (xy 139 75) (xy 67 75)
      )
    )
  )
)
