(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 95)
    (zones 0)
    (modules 10)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010ec_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../Desktop/untitled folder/"))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BB664A1)
    (at 54 52.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BB664A1)
    (at 54 141.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BB664A1)
    (at 108 141.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Matt (layer F.Cu) (tedit 5BB2E068)
    (at 76.2 102.8065)
    (descr "Terminal Block Phoenix PT-1,5-7-5.0-H, 7 pins, pitch 5mm, size 35x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-7-5.0-H pitch 5mm size 35x9mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference REF** (at 15 -5.06) (layer F.SilkS) hide)
    (fp_text value TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Matt (at 15 5.06) (layer B.Fab) hide)
    (fp_text user %R (at 15 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 10 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 15 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 20 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 25 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 30 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Mini-Fit_Jr_5566-20A_2x10_P4.20mm_Vertical (layer F.Cu) (tedit 5BB2D405)
    (at 58.42 102.8065 90)
    (descr "Molex Mini-Fit Jr. Power Connectors, old mpn/engineering number: 5566-20A, example for new mpn: 39-28-x20x, 10 Pins per row, Mounting:  (http://www.molex.com/pdm_docs/sd/039281043_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Mini-Fit_Jr side entry")
    (fp_text reference PicoPSU (at 18.9 -3.45 90) (layer F.SilkS))
    (fp_text value Molex_Mini-Fit_Jr_5566-20A_2x10_P4.20mm_Vertical (at 18.9 9.95 90) (layer F.Fab) hide)
    (fp_text user %R (at 18.9 -1.55 90) (layer F.Fab))
    (pad 20 thru_hole oval (at 37.8 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 33.6 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 29.4 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 25.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 21 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 16.8 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 12.6 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 8.4 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 4.2 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 5.5 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 37.8 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 33.6 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 29.4 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 25.2 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 21 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 16.8 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 12.6 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 8.4 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 4.2 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.7 3.3) (drill 1.4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Mini-Fit_Jr_5566-20A_2x10_P4.20mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-14_W7.62mm_Socket (layer F.Cu) (tedit 5BB2D3FA)
    (at 72.39 120.65 270)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference 74LS04 (at 3.81 -2.33 270) (layer F.SilkS))
    (fp_text value DIP-14_W7.62mm_Socket (at 3.81 17.57 270) (layer F.Fab) hide)
    (fp_text user 74LS04 (at 3.81 7.62) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 7.62 10.16 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 7.62 12.7 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 7.62 15.24 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5BB2D778)
    (at 64.77 113.03)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference 4.7K (at 3.81 -2.37) (layer F.SilkS))
    (fp_text value R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (at 3.81 2.37) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5BB2D75A)
    (at 59.01436 112.46866)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference Fan (at 0 -2.33) (layer F.SilkS))
    (fp_text value PinHeader_1x02_P2.54mm_Vertical (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Matt (layer F.Cu) (tedit 5BB2E068)
    (at 76.2 64.7065)
    (descr "Terminal Block Phoenix PT-1,5-7-5.0-H, 7 pins, pitch 5mm, size 35x9mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.mouser.com/ds/2/324/ItemDetail_1935161-922578.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-7-5.0-H pitch 5mm size 35x9mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference REF** (at 15 -5.06) (layer F.SilkS) hide)
    (fp_text value TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Matt (at 15 5.06) (layer B.Fab) hide)
    (fp_text user %R (at 15 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 10 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 15 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 20 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 25 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 30 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_PT-1,5-7-5.0-H_1x07_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 5BB664A1)
    (at 108 52.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm (at 0 3.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (gr_text "+5V SB" (at 106.2 68 90) (layer F.SilkS))
  (gr_text +5V (at 101.2 68 90) (layer F.SilkS))
  (gr_text +5V (at 96.2 68 90) (layer F.SilkS))
  (gr_text +5V (at 91.2 68 90) (layer F.SilkS))
  (gr_text +12V (at 86.2 68 90) (layer F.SilkS))
  (gr_text +12V (at 81.2 68 90) (layer F.SilkS))
  (gr_text PwrOn (at 106.2 100 90) (layer F.SilkS))
  (gr_text -12V (at 76.2 100 90) (layer F.SilkS))
  (gr_text +12V (at 81.2 100 90) (layer F.SilkS))
  (gr_text GND (at 86.2 100 90) (layer F.SilkS))
  (gr_text GND (at 91.2 100 90) (layer F.SilkS))
  (gr_text GND (at 96.2 100 90) (layer F.SilkS))
  (gr_text GND (at 101.2 100 90) (layer F.SilkS))
  (gr_line (start 111 50) (end 111 144) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 50) (end 50 144) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 144) (end 111 144) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 50) (end 111 50) (layer Edge.Cuts) (width 0.15))
)
