(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "unconnected-(A1-Pad3V3)")
  (net 2 "unconnected-(A1-Pad5V1)")
  (net 3 "unconnected-(A1-Pad5V2)")
  (net 4 "unconnected-(A1-Pad5V3)")
  (net 5 "unconnected-(A1-Pad5V4)")
  (net 6 "Net-(A1-PadA0)")
  (net 7 "Net-(A1-PadA1)")
  (net 8 "Net-(A1-PadA2)")
  (net 9 "Net-(A1-PadA3)")
  (net 10 "unconnected-(A1-PadA4)")
  (net 11 "unconnected-(A1-PadA5)")
  (net 12 "unconnected-(A1-PadA6)")
  (net 13 "unconnected-(A1-PadA7)")
  (net 14 "unconnected-(A1-PadA8)")
  (net 15 "unconnected-(A1-PadA9)")
  (net 16 "unconnected-(A1-PadA10)")
  (net 17 "unconnected-(A1-PadA11)")
  (net 18 "unconnected-(A1-PadA12)")
  (net 19 "unconnected-(A1-PadA13)")
  (net 20 "unconnected-(A1-PadA14)")
  (net 21 "unconnected-(A1-PadA15)")
  (net 22 "unconnected-(A1-PadAREF)")
  (net 23 "unconnected-(A1-PadD0)")
  (net 24 "unconnected-(A1-PadD1)")
  (net 25 "Net-(A1-PadD2)")
  (net 26 "Net-(A1-PadD3)")
  (net 27 "Net-(A1-PadD4)")
  (net 28 "Net-(A1-PadD5)")
  (net 29 "Net-(A1-PadD6)")
  (net 30 "Net-(A1-PadD7)")
  (net 31 "unconnected-(A1-PadD8)")
  (net 32 "unconnected-(A1-PadD9)")
  (net 33 "unconnected-(A1-PadD10)")
  (net 34 "unconnected-(A1-PadD11)")
  (net 35 "unconnected-(A1-PadD12)")
  (net 36 "unconnected-(A1-PadD13)")
  (net 37 "unconnected-(A1-PadD14)")
  (net 38 "unconnected-(A1-PadD15)")
  (net 39 "unconnected-(A1-PadD16)")
  (net 40 "unconnected-(A1-PadD17)")
  (net 41 "unconnected-(A1-PadD18)")
  (net 42 "unconnected-(A1-PadD19)")
  (net 43 "unconnected-(A1-PadD20)")
  (net 44 "unconnected-(A1-PadD21)")
  (net 45 "unconnected-(A1-PadD22)")
  (net 46 "unconnected-(A1-PadD23)")
  (net 47 "unconnected-(A1-PadD24)")
  (net 48 "unconnected-(A1-PadD25)")
  (net 49 "unconnected-(A1-PadD26)")
  (net 50 "unconnected-(A1-PadD27)")
  (net 51 "unconnected-(A1-PadD28)")
  (net 52 "unconnected-(A1-PadD29)")
  (net 53 "unconnected-(A1-PadD30)")
  (net 54 "unconnected-(A1-PadD31)")
  (net 55 "unconnected-(A1-PadD32)")
  (net 56 "unconnected-(A1-PadD33)")
  (net 57 "unconnected-(A1-PadD34)")
  (net 58 "unconnected-(A1-PadD35)")
  (net 59 "unconnected-(A1-PadD36)")
  (net 60 "unconnected-(A1-PadD37)")
  (net 61 "unconnected-(A1-PadD38)")
  (net 62 "unconnected-(A1-PadD39)")
  (net 63 "unconnected-(A1-PadD40)")
  (net 64 "unconnected-(A1-PadD41)")
  (net 65 "unconnected-(A1-PadD42)")
  (net 66 "unconnected-(A1-PadD43)")
  (net 67 "unconnected-(A1-PadD44)")
  (net 68 "unconnected-(A1-PadD45)")
  (net 69 "unconnected-(A1-PadD46)")
  (net 70 "unconnected-(A1-PadD47)")
  (net 71 "unconnected-(A1-PadD48)")
  (net 72 "unconnected-(A1-PadD49)")
  (net 73 "unconnected-(A1-PadD50)")
  (net 74 "unconnected-(A1-PadD51)")
  (net 75 "unconnected-(A1-PadD52)")
  (net 76 "unconnected-(A1-PadD53)")
  (net 77 "GND")
  (net 78 "unconnected-(A1-PadIORF)")
  (net 79 "unconnected-(A1-PadMISO)")
  (net 80 "unconnected-(A1-PadMOSI)")
  (net 81 "unconnected-(A1-PadRST1)")
  (net 82 "unconnected-(A1-PadRST2)")
  (net 83 "unconnected-(A1-PadSCK)")
  (net 84 "unconnected-(A1-PadSCL)")
  (net 85 "unconnected-(A1-PadSDA)")
  (net 86 "+12V")
  (net 87 "unconnected-(A1-PadGND4)")
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 153.7 69.5)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "D3" (at 8.3 5.8) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-PadD3)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 124.9 55.5)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "D7" (at 0 -7.4) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 "Net-(A1-PadD7)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Barrel Power Jack Adapter:PJ-102AH" (layer "F.Cu")
    (tedit 0)
    (at 108.865075 81.3 90)
    (descr "PJ-102AH")
    (tags "Connector")
    (property "Description" "DC POWER JACK")
    (property "Height" "")
    (property "Manufacturer_Name" "CUI Devices")
    (property "Manufacturer_Part_Number" "PJ-102AH")
    (property "Mouser Part Number" "490-PJ-102AH")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CUI-Devices/PJ-102AH?qs=WyjlAZoYn50Yq4CrVLCXLw%3D%3D")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 4.035 -6.411 90) (layer "F.SilkS"))
    (fp_text value "PJ-102AH" (at 4.035 -6.411 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.035 -6.411 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 4.3 3 90) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 86 "+12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 4.3 -3 90) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -0.4 0 90) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (model "PJ-102AH.stp"
      (offset (xyz 4.309999878 -2.78999992 6.579999825))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 153.7 55.5)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "D5" (at 0 -7.4) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-PadD5)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 124.9 83.8)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "A0" (at 0 7.8) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-PadA0)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Arduino:Arduino_Mega2560_R3_Shield" (layer "F.Cu")
    (tedit 5A8605D3)
    (at 99.419 96.769237)
    (descr "https://docs.arduino.cc/hardware/mega-2560")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "A1" (at 2.54 -54.356) (layer "B.SilkS"))
    (fp_text value "Arduino_Mega2560_R3_Shield" (at 27.305 -54.356) (layer "B.Fab"))
    (fp_text user "D0" (at 63.5 -48.895 unlocked) (layer "B.SilkS"))
    (fp_text user "." (at 62.484 -32.004) (layer "B.SilkS"))
    (fp_text user "." (at 62.484 -32.004) (layer "F.SilkS"))
    (fp_text user "D0" (at 63.5 -48.895 unlocked) (layer "F.SilkS"))
    (fp_text user "Barrel Jack" (at 5.065 -7.7981) (layer "B.Fab"))
    (fp_text user "USB" (at 1.535 -38.0986) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at 66.04 -7.62) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 13.97 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 90.17 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 96.52 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 66.04 -35.56) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 15.24 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "3V3" thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "unconnected-(A1-Pad3V3)") (pinfunction "3.3V") (pintype "power_out+no_connect"))
    (pad "5V1" thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "unconnected-(A1-Pad5V1)") (pinfunction "5V") (pintype "power_in+no_connect"))
    (pad "5V2" thru_hole oval (at 66.167 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "unconnected-(A1-Pad5V2)") (pinfunction "SPI_5V") (pintype "power_in+no_connect"))
    (pad "5V3" thru_hole oval (at 93.98 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "unconnected-(A1-Pad5V3)") (pinfunction "5V") (pintype "power_in+no_connect"))
    (pad "5V4" thru_hole oval (at 96.52 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "unconnected-(A1-Pad5V4)") (pinfunction "5V") (pintype "power_in+no_connect"))
    (pad "A0" thru_hole oval (at 50.8 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-PadA0)") (pinfunction "A0") (pintype "bidirectional"))
    (pad "A1" thru_hole oval (at 53.34 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-PadA1)") (pinfunction "A1") (pintype "bidirectional"))
    (pad "A2" thru_hole oval (at 55.88 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-PadA2)") (pinfunction "A2") (pintype "bidirectional"))
    (pad "A3" thru_hole oval (at 58.42 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-PadA3)") (pinfunction "A3") (pintype "bidirectional"))
    (pad "A4" thru_hole oval (at 60.96 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "unconnected-(A1-PadA4)") (pinfunction "A4") (pintype "bidirectional+no_connect"))
    (pad "A5" thru_hole oval (at 63.5 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "unconnected-(A1-PadA5)") (pinfunction "A5") (pintype "bidirectional+no_connect"))
    (pad "A6" thru_hole oval (at 66.04 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "unconnected-(A1-PadA6)") (pinfunction "A6") (pintype "bidirectional+no_connect"))
    (pad "A7" thru_hole oval (at 68.58 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "unconnected-(A1-PadA7)") (pinfunction "A7") (pintype "bidirectional+no_connect"))
    (pad "A8" thru_hole oval (at 73.66 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "unconnected-(A1-PadA8)") (pinfunction "A8") (pintype "bidirectional+no_connect"))
    (pad "A9" thru_hole oval (at 76.2 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "unconnected-(A1-PadA9)") (pinfunction "A9") (pintype "bidirectional+no_connect"))
    (pad "A10" thru_hole oval (at 78.74 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "unconnected-(A1-PadA10)") (pinfunction "A10") (pintype "bidirectional+no_connect"))
    (pad "A11" thru_hole oval (at 81.28 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "unconnected-(A1-PadA11)") (pinfunction "A11") (pintype "bidirectional+no_connect"))
    (pad "A12" thru_hole oval (at 83.82 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "unconnected-(A1-PadA12)") (pinfunction "A12") (pintype "bidirectional+no_connect"))
    (pad "A13" thru_hole oval (at 86.36 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "unconnected-(A1-PadA13)") (pinfunction "A13") (pintype "bidirectional+no_connect"))
    (pad "A14" thru_hole oval (at 88.9 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "unconnected-(A1-PadA14)") (pinfunction "A14") (pintype "bidirectional+no_connect"))
    (pad "A15" thru_hole oval (at 91.44 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "unconnected-(A1-PadA15)") (pinfunction "A15") (pintype "bidirectional+no_connect"))
    (pad "AREF" thru_hole oval (at 23.876 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "unconnected-(A1-PadAREF)") (pinfunction "AREF") (pintype "input+no_connect"))
    (pad "D0" thru_hole oval (at 63.5 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "unconnected-(A1-PadD0)") (pinfunction "D0/RX0") (pintype "bidirectional+no_connect"))
    (pad "D1" thru_hole oval (at 60.96 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "unconnected-(A1-PadD1)") (pinfunction "D1/TX0") (pintype "bidirectional+no_connect"))
    (pad "D2" thru_hole oval (at 58.42 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-PadD2)") (pinfunction "D2_INT0") (pintype "bidirectional"))
    (pad "D3" thru_hole oval (at 55.88 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-PadD3)") (pinfunction "D3_INT1") (pintype "bidirectional"))
    (pad "D4" thru_hole oval (at 53.34 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-PadD4)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "D5" thru_hole oval (at 50.8 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-PadD5)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "D6" thru_hole oval (at 48.26 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-PadD6)") (pinfunction "D6") (pintype "bidirectional"))
    (pad "D7" thru_hole oval (at 45.72 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(A1-PadD7)") (pinfunction "D7") (pintype "bidirectional"))
    (pad "D8" thru_hole oval (at 41.656 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "unconnected-(A1-PadD8)") (pinfunction "D8") (pintype "bidirectional+no_connect"))
    (pad "D9" thru_hole oval (at 39.116 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "unconnected-(A1-PadD9)") (pinfunction "D9") (pintype "bidirectional+no_connect"))
    (pad "D10" thru_hole oval (at 36.576 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "unconnected-(A1-PadD10)") (pinfunction "D10") (pintype "bidirectional+no_connect"))
    (pad "D11" thru_hole oval (at 34.036 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "unconnected-(A1-PadD11)") (pinfunction "D11") (pintype "bidirectional+no_connect"))
    (pad "D12" thru_hole oval (at 31.496 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "unconnected-(A1-PadD12)") (pinfunction "D12") (pintype "bidirectional+no_connect"))
    (pad "D13" thru_hole oval (at 28.956 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "unconnected-(A1-PadD13)") (pinfunction "D13") (pintype "bidirectional+no_connect"))
    (pad "D14" thru_hole oval (at 68.58 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "unconnected-(A1-PadD14)") (pinfunction "D14/TX3") (pintype "bidirectional+no_connect"))
    (pad "D15" thru_hole oval (at 71.12 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "unconnected-(A1-PadD15)") (pinfunction "D15/RX3") (pintype "bidirectional+no_connect"))
    (pad "D16" thru_hole oval (at 73.66 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "unconnected-(A1-PadD16)") (pinfunction "D16/TX2") (pintype "bidirectional+no_connect"))
    (pad "D17" thru_hole oval (at 76.2 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "unconnected-(A1-PadD17)") (pinfunction "D17/RX2") (pintype "bidirectional+no_connect"))
    (pad "D18" thru_hole oval (at 78.74 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "unconnected-(A1-PadD18)") (pinfunction "D18/TX1") (pintype "bidirectional+no_connect"))
    (pad "D19" thru_hole oval (at 81.28 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "unconnected-(A1-PadD19)") (pinfunction "D19/RX1") (pintype "bidirectional+no_connect"))
    (pad "D20" thru_hole oval (at 83.82 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "unconnected-(A1-PadD20)") (pinfunction "D20/SDA") (pintype "bidirectional+no_connect"))
    (pad "D21" thru_hole oval (at 86.36 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "unconnected-(A1-PadD21)") (pinfunction "D21/SCL") (pintype "bidirectional+no_connect"))
    (pad "D22" thru_hole oval (at 93.98 -48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "unconnected-(A1-PadD22)") (pinfunction "D22") (pintype "bidirectional+no_connect"))
    (pad "D23" thru_hole oval (at 96.52 -48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "unconnected-(A1-PadD23)") (pinfunction "D23") (pintype "bidirectional+no_connect"))
    (pad "D24" thru_hole oval (at 93.98 -45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "unconnected-(A1-PadD24)") (pinfunction "D24") (pintype "bidirectional+no_connect"))
    (pad "D25" thru_hole oval (at 96.52 -45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "unconnected-(A1-PadD25)") (pinfunction "D25") (pintype "bidirectional+no_connect"))
    (pad "D26" thru_hole oval (at 93.98 -43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "unconnected-(A1-PadD26)") (pinfunction "D26") (pintype "bidirectional+no_connect"))
    (pad "D27" thru_hole oval (at 96.52 -43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 "unconnected-(A1-PadD27)") (pinfunction "D27") (pintype "bidirectional+no_connect"))
    (pad "D28" thru_hole oval (at 93.98 -40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "unconnected-(A1-PadD28)") (pinfunction "D28") (pintype "bidirectional+no_connect"))
    (pad "D29" thru_hole oval (at 96.52 -40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 "unconnected-(A1-PadD29)") (pinfunction "D29") (pintype "bidirectional+no_connect"))
    (pad "D30" thru_hole oval (at 93.98 -38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 "unconnected-(A1-PadD30)") (pinfunction "D30") (pintype "bidirectional+no_connect"))
    (pad "D31" thru_hole oval (at 96.52 -38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "unconnected-(A1-PadD31)") (pinfunction "D31") (pintype "bidirectional+no_connect"))
    (pad "D32" thru_hole oval (at 93.98 -35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "unconnected-(A1-PadD32)") (pinfunction "D32") (pintype "bidirectional+no_connect"))
    (pad "D33" thru_hole oval (at 96.52 -35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "unconnected-(A1-PadD33)") (pinfunction "D33") (pintype "bidirectional+no_connect"))
    (pad "D34" thru_hole oval (at 93.98 -33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "unconnected-(A1-PadD34)") (pinfunction "D34") (pintype "bidirectional+no_connect"))
    (pad "D35" thru_hole oval (at 96.52 -33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "unconnected-(A1-PadD35)") (pinfunction "D35") (pintype "bidirectional+no_connect"))
    (pad "D36" thru_hole oval (at 93.98 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 "unconnected-(A1-PadD36)") (pinfunction "D36") (pintype "bidirectional+no_connect"))
    (pad "D37" thru_hole oval (at 96.52 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 "unconnected-(A1-PadD37)") (pinfunction "D37") (pintype "bidirectional+no_connect"))
    (pad "D38" thru_hole oval (at 93.98 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 "unconnected-(A1-PadD38)") (pinfunction "D38") (pintype "bidirectional+no_connect"))
    (pad "D39" thru_hole oval (at 96.52 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 "unconnected-(A1-PadD39)") (pinfunction "D39") (pintype "bidirectional+no_connect"))
    (pad "D40" thru_hole oval (at 93.98 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "unconnected-(A1-PadD40)") (pinfunction "D40") (pintype "bidirectional+no_connect"))
    (pad "D41" thru_hole oval (at 96.52 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "unconnected-(A1-PadD41)") (pinfunction "D41") (pintype "bidirectional+no_connect"))
    (pad "D42" thru_hole oval (at 93.98 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "unconnected-(A1-PadD42)") (pinfunction "D42") (pintype "bidirectional+no_connect"))
    (pad "D43" thru_hole oval (at 96.52 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "unconnected-(A1-PadD43)") (pinfunction "D43") (pintype "bidirectional+no_connect"))
    (pad "D44" thru_hole oval (at 93.98 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 "unconnected-(A1-PadD44)") (pinfunction "D44") (pintype "bidirectional+no_connect"))
    (pad "D45" thru_hole oval (at 96.52 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 "unconnected-(A1-PadD45)") (pinfunction "D45") (pintype "bidirectional+no_connect"))
    (pad "D46" thru_hole oval (at 93.98 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 "unconnected-(A1-PadD46)") (pinfunction "D46") (pintype "bidirectional+no_connect"))
    (pad "D47" thru_hole oval (at 96.52 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "unconnected-(A1-PadD47)") (pinfunction "D47") (pintype "bidirectional+no_connect"))
    (pad "D48" thru_hole oval (at 93.98 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 "unconnected-(A1-PadD48)") (pinfunction "D48") (pintype "bidirectional+no_connect"))
    (pad "D49" thru_hole oval (at 96.52 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "unconnected-(A1-PadD49)") (pinfunction "D49") (pintype "bidirectional+no_connect"))
    (pad "D50" thru_hole oval (at 93.98 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "unconnected-(A1-PadD50)") (pinfunction "D50_MISO") (pintype "bidirectional+no_connect"))
    (pad "D51" thru_hole oval (at 96.52 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "unconnected-(A1-PadD51)") (pinfunction "D51_MOSI") (pintype "bidirectional+no_connect"))
    (pad "D52" thru_hole oval (at 93.98 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "unconnected-(A1-PadD52)") (pinfunction "D52_SCK") (pintype "bidirectional+no_connect"))
    (pad "D53" thru_hole oval (at 96.52 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "unconnected-(A1-PadD53)") (pinfunction "D53_CS") (pintype "bidirectional+no_connect"))
    (pad "GND1" thru_hole rect (at 26.416 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND2" thru_hole rect (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND3" thru_hole rect (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND4" thru_hole rect (at 66.167 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "unconnected-(A1-PadGND4)") (pinfunction "SPI_GND") (pintype "power_in+no_connect"))
    (pad "GND5" thru_hole rect (at 93.98 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND6" thru_hole rect (at 96.52 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "IORF" thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "unconnected-(A1-PadIORF)") (pinfunction "IOREF") (pintype "output+no_connect"))
    (pad "MISO" thru_hole oval (at 63.627 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 "unconnected-(A1-PadMISO)") (pinfunction "SPI_MISO") (pintype "input+no_connect"))
    (pad "MOSI" thru_hole oval (at 66.167 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "unconnected-(A1-PadMOSI)") (pinfunction "SPI_MOSI") (pintype "output+no_connect"))
    (pad "RST1" thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "unconnected-(A1-PadRST1)") (pinfunction "RESET") (pintype "open_collector+no_connect"))
    (pad "RST2" thru_hole oval (at 63.627 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 "unconnected-(A1-PadRST2)") (pinfunction "SPI_RESET") (pintype "open_collector+no_connect"))
    (pad "SCK" thru_hole oval (at 63.627 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "unconnected-(A1-PadSCK)") (pinfunction "SPI_SCK") (pintype "output+no_connect"))
    (pad "SCL" thru_hole oval (at 18.796 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 "unconnected-(A1-PadSCL)") (pinfunction "SCL") (pintype "bidirectional+no_connect"))
    (pad "SDA" thru_hole oval (at 21.336 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 "unconnected-(A1-PadSDA)") (pinfunction "SDA") (pintype "bidirectional+no_connect"))
    (pad "VIN" thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 "+12V") (pinfunction "VIN") (pintype "power_in"))
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 153.6 83.8)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "A2" (at 0 7.7) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-PadA2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 139.2 55.5)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "D6" (at 0 -7.4) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-PadD6)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 177.2 83.7)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "A3" (at 0 7.7) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-PadA3)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 139.2 83.8)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "A1" (at 0 7.7) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-PadA1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 139.2 69.5)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "D4" (at -8.4 5.8) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(A1-PadD4)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CONNBNC001_vertical:CONBNC001" (layer "F.Cu")
    (tedit 0)
    (at 177.7 55.5)
    (descr "CONBNC001-2")
    (tags "Integrated Circuit")
    (property "Datasheet_1" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7FC-CONBNC001%7FA%7Fpdf%7FEnglish%7FENG_CD_C-CONBNC001_A.pdf%7FCONBNC001")
    (property "Footprint_1" "CONBNC001")
    (property "Height" "14.9")
    (property "Manufacturer_Name" "TE Connectivity / Linx Technologies")
    (property "Manufacturer_Part_Number" "CONBNC001")
    (property "Mouser Part Number" "712-CONBNC001")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TE-Connectivity-Linx-Technologies/CONBNC001?qs=doiCPypUmgHczHAGaJs8Lg%3D%3D")
    (property "Reference_1" "IC")
    (property "Sheetfile" "File: speckle_Edwin.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "CONBNC001")
    (attr through_hole)
    (fp_text reference "D2" (at 0.1 -7.4) (layer "F.SilkS"))
    (fp_text value "CONBNC001" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-PadD2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.15 3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.15 -3.15) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 77 "GND") (pinfunction "5") (pintype "passive"))
    (model "CONBNC001.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 98 41) (end 202.1 99.1) (layer "Edge.Cuts") (width 0.1) (fill none))
  (zone (net 77) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201 98)
        (xy 99 98)
        (xy 99 42)
        (xy 201 42)
      )
    )
  )
)
