(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 0)
    (no_connects 0)
    (area 49.386667 47.925 100.075001 62.325)
    (thickness 1.6)
    (drawings 48)
    (tracks 106)
    (zones 0)
    (modules 11)
    (nets 9)
  )
  (page A4)
  (title_block
    (title ProgrammerClip)
    (date 2017-03-21)
    (rev A)
    (comment 3 CC-BY-SA-NC)
    (comment 4 "PITIOT Mathieu")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.35)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.3)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.8)
    (via_min_drill 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.050000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory exports/))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net 5 "Net-(P1-Pad5)")
  (net 6 "Net-(P1-Pad6)")
  (net 7 "Net-(P1-Pad7)")
  (net 8 "Net-(P1-Pad8)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.3)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm (layer F.Cu) (tedit 58D2B68A)
    (at 53.25 51.2)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference P1 (at 1.25 9.7) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 1.27 9.95) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad8)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0DE)
    (at 96.75 51.2)
    (fp_text reference W1 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(P1-Pad1)"))
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0D6)
    (at 96.75 53.75)
    (fp_text reference W2 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -0.01) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(P1-Pad3)"))
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0CE)
    (at 96.75 56.28)
    (fp_text reference W3 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0CA)
    (at 96.75 58.82)
    (fp_text reference W4 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(P1-Pad7)"))
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0DB)
    (at 94.21 51.2)
    (fp_text reference W5 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad2)"))
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0D3)
    (at 96.75 53.74)
    (fp_text reference W6 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0CD)
    (at 94.21 56.28)
    (fp_text reference W7 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad6)"))
  )
  (module ehko:Pogo_pin_connect_1.02mm (layer F.Cu) (tedit 58D1A0C8)
    (at 94.21 58.82)
    (fp_text reference W8 (at 0 2) (layer F.SilkS) hide)
    (fp_text value 1P (at 0 -2.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad8)"))
  )
  (module ehko:Logo_silks_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 75 57.6)
    (descr "CC BY-NC-SA logo, 10x3.6mm, SilkS")
    (fp_text reference G*** (at 0.3 -1.4) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.3 0.5) (layer F.SilkS) hide)
  )
  (module ehko:Logo_silks_CC-BY-NC-SA_10x3.6mm (layer B.Cu) (tedit 0)
    (at 75 57.6 180)
    (descr "CC BY-NC-SA logo, 10x3.6mm, SilkS")
    (fp_text reference G*** (at 0.3 1.4 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.3 -0.5 180) (layer B.SilkS) hide)
  )
  (gr_text ehko.fr (at 75.1 54.7) (layer B.SilkS))
  (gr_text ehko.fr (at 75 54.7) (layer F.SilkS))
  (gr_text PgmClip-A (at 75.2 51.9) (layer B.SilkS))
  (gr_text PgmClip-A (at 75 51.9) (layer F.SilkS))
  (gr_line (start 87.8 59.8) (end 88.5 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.2 59.8) (end 87.8 59.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.5 60.5) (end 86.2 59.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.8 59.8) (end 76.5 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2 59.8) (end 75.8 59.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.5 60.5) (end 74.2 59.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.8 59.8) (end 64.5 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 62.2 59.8) (end 63.8 59.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.5 60.5) (end 62.2 59.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.8 50.2) (end 88.5 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 86.2 50.2) (end 87.8 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.5 49.5) (end 86.2 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.8 50.2) (end 76.5 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2 50.2) (end 75.8 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.5 49.5) (end 74.2 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.8 50.2) (end 64.5 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 62.2 50.2) (end 63.8 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.5 49.5) (end 62.2 50.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 64.5 49.5) (end 64.6 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "2 1\n4 3\n6 5\n8 7" (at 60.4 55.1) (layer F.SilkS))
  (gr_text "1 2\n3 4\n5 6\n7 8" (at 89.7 55.1) (layer F.SilkS))
  (gr_line (start 100 49.5) (end 98.8 48.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.6 49.5) (end 88.5 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.8 48.3) (end 90.6 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.6 60.5) (end 88.5 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.8 61.7) (end 90.6 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.8 61.7) (end 100 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.8 61.7) (end 91.8 61.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.4 60.5) (end 61.5 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.2 61.7) (end 59.4 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.2 61.7) (end 50 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.4 49.5) (end 61.5 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58.2 48.3) (end 59.4 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.2 48.3) (end 51.3 48.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 49.5) (end 51.2 48.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.5 60.5) (end 64.5 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.5 60.5) (end 76.5 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.5 49.5) (end 64.5 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.5 49.5) (end 76.5 49.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.2 61.7) (end 58.2 61.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 51.2 48.3) (end 58.2 48.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 98.8 48.3) (end 91.8 48.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50 49.5) (end 50 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 49.5) (end 100 60.5) (angle 90) (layer Edge.Cuts) (width 0.15))
)
