(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 25)
    (tracks 254)
    (zones 0)
    (modules 18)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 "Net-(J1-Pad6)")
  (net 3 GND)
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 +3V3)
  (net 8 "Net-(U2-PadD2)")
  (net 9 RX2)
  (net 10 TX2)
  (net 11 +5V)
  (net 12 "Net-(R1-Pad1)")
  (net 13 "Net-(U2-PadD27)")
  (net 14 "Net-(U2-PadD26)")
  (net 15 "Net-(D1-Pad1)")
  (net 16 "Net-(D2-Pad2)")
  (net 17 EN)
  (net 18 GPS_RX)
  (net 19 GPS_TX)
  (net 20 SCL)
  (net 21 SDA)
  (net 22 CS)
  (net 23 CLK)
  (net 24 MISO)
  (net 25 MOSI)
  (net 26 RST)
  (net 27 "Net-(R4-Pad1)")
  (net 28 "Net-(R5-Pad1)")
  (net 29 ESP-Wifi-Off)
  (net 30 ESP-Wifi-Mode)
  (net 31 EVO-Wifi-Off)
  (net 32 ESP-Restore-Defaults)
  (net 33 3OE)
  (net 34 4Y)
  (net 35 "Net-(U2-PadD4)")
  (net 36 "Net-(U2-PadD12)")
  (net 37 "Net-(U2-PadD14)")
  (net 38 "Net-(U2-PadD3)")
  (net 39 "Net-(U2-PadD1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3OE)
    (add_net 4Y)
    (add_net CLK)
    (add_net CS)
    (add_net EN)
    (add_net ESP-Restore-Defaults)
    (add_net ESP-Wifi-Mode)
    (add_net ESP-Wifi-Off)
    (add_net EVO-Wifi-Off)
    (add_net GPS_RX)
    (add_net GPS_TX)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(U2-PadD1)")
    (add_net "Net-(U2-PadD12)")
    (add_net "Net-(U2-PadD14)")
    (add_net "Net-(U2-PadD2)")
    (add_net "Net-(U2-PadD26)")
    (add_net "Net-(U2-PadD27)")
    (add_net "Net-(U2-PadD3)")
    (add_net "Net-(U2-PadD4)")
    (add_net RST)
    (add_net RX2)
    (add_net SCL)
    (add_net SDA)
    (add_net TX2)
  )
  (net_class 12V ""
    (clearance 0.4)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
  )
  (net_class 5V_3V3 ""
    (clearance 0.3)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 54.58 76.89)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference SPI (at 2.01 -4.77 90) (layer B.SilkS))
    (fp_text value SPI (at 0 -17.57) (layer B.Fab))
    (fp_text user %R (at 0 -7.62 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 CS))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 CLK))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 MISO))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 MOSI))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 RST))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 40.67 61.34 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 4K7 (at 3.83 0 90) (layer F.SilkS))
    (fp_text value 4K7 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 SDA))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP32DEVKIT1:ESP32-DEVKITV1 (layer F.Cu) (tedit 6035BED3)
    (at 50.8 80.391 90)
    (fp_text reference U2 (at -14.605 -15.875 90) (layer F.SilkS) hide)
    (fp_text value ESP32DEVKITV1 (at 0 0 90) (layer F.Fab))
    (fp_text user ESP32-DEVKITV1 (at 11.35 15.97 90) (layer F.Fab))
    (pad 3V3 thru_hole circle (at -16.52 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad GND@2 thru_hole circle (at -13.98 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad D15 thru_hole circle (at -11.44 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 31 EVO-Wifi-Off))
    (pad D2 thru_hole circle (at -8.9 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(U2-PadD2)"))
    (pad D4 thru_hole circle (at -6.36 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-PadD4)"))
    (pad D16 thru_hole circle (at -3.82 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 9 RX2))
    (pad D17 thru_hole circle (at -1.28 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 10 TX2))
    (pad D5 thru_hole circle (at 1.26 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 22 CS))
    (pad D18 thru_hole circle (at 3.8 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 23 CLK))
    (pad D19 thru_hole circle (at 6.34 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 24 MISO))
    (pad D21 thru_hole circle (at 8.88 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 21 SDA))
    (pad D3 thru_hole circle (at 11.42 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(U2-PadD3)"))
    (pad D1 thru_hole circle (at 13.96 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(U2-PadD1)"))
    (pad D22 thru_hole circle (at 16.5 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 20 SCL))
    (pad D23 thru_hole circle (at 19.04 12.27 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 25 MOSI))
    (pad VIN thru_hole circle (at -16.52 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad GND@1 thru_hole circle (at -13.98 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad D13 thru_hole circle (at -11.44 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 26 RST))
    (pad D12 thru_hole circle (at -8.9 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-PadD12)"))
    (pad D14 thru_hole circle (at -6.36 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-PadD14)"))
    (pad D27 thru_hole circle (at -3.82 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-PadD27)"))
    (pad D26 thru_hole circle (at -1.28 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-PadD26)"))
    (pad D25 thru_hole circle (at 1.26 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 19 GPS_TX))
    (pad D33 thru_hole circle (at 3.8 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 18 GPS_RX))
    (pad D32 thru_hole circle (at 6.34 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 33 3OE))
    (pad D35 thru_hole circle (at 8.88 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 34 4Y))
    (pad D34 thru_hole circle (at 11.42 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 32 ESP-Restore-Defaults))
    (pad D39 thru_hole circle (at 13.96 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 30 ESP-Wifi-Mode))
    (pad D36 thru_hole circle (at 16.5 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 29 ESP-Wifi-Off))
    (pad EN thru_hole circle (at 19.04 -13.135 90) (size 1.9304 1.9304) (drill 1) (layers *.Cu *.Mask)
      (net 17 EN))
    (model ${KIPRJMOD}/ESP32DEVKIT1/ESP-WROOM32.STEP
      (offset (xyz -15.75 -1 25))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Connector_RJ:RJ12_Amphenol_54601 (layer B.Cu) (tedit 5AE2E32D)
    (at 48.26 95.123 180)
    (descr "RJ12 connector  https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0082.pdf")
    (tags "RJ12 connector")
    (fp_text reference AUX (at 3.302 1.905) (layer B.SilkS))
    (fp_text value RJ12-AUX (at 3.54 -18.3) (layer B.Fab))
    (fp_text user %R (at 3.16 -7.76) (layer B.Fab))
    (pad "" np_thru_hole circle (at 8.25 -8.89 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad "" np_thru_hole circle (at -1.91 -8.89 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.52 1.52) (drill 0.76) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ12_Amphenol_54601.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 57.97 83.88 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 3.937 0 90) (layer F.SilkS))
    (fp_text value D (at 3.81 2.47 90) (layer F.Fab))
    (fp_text user %R (at 4.2 0 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CoolLick:Coollick (layer B.Cu) (tedit 604275F6)
    (at 45.0215 86.36 180)
    (descr "Converted using: svg2mod -i Coollick.svg -c -f .11")
    (tags svg2mod)
    (attr virtual)
    (fp_text reference svg2mod (at 0 4.71236) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -4.71236) (layer B.SilkS) hide)
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 49.911 82.677 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 50K (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 50K (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (offset (xyz 0 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SN74HC125N:DIP794W45P254L1969H508Q14 (layer F.Cu) (tedit 6035BDB3)
    (at 47.74 68.93 180)
    (fp_text reference U1 (at 0 -9.144) (layer F.SilkS))
    (fp_text value SN74HC125N (at 11.875 11.135) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.97 -7.62 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 10 TX2))
    (pad 2 thru_hole circle (at -3.97 -5.08 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at -3.97 -2.54 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 28 "Net-(R5-Pad1)"))
    (pad 4 thru_hole circle (at -3.97 0 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 5 thru_hole circle (at -3.97 2.54 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 6 thru_hole circle (at -3.97 5.08 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 9 RX2))
    (pad 7 thru_hole circle (at -3.97 7.62 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole circle (at 3.97 7.62 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 27 "Net-(R4-Pad1)"))
    (pad 9 thru_hole circle (at 3.97 5.08 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole circle (at 3.97 2.54 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 33 3OE))
    (pad 11 thru_hole circle (at 3.97 0 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 34 4Y))
    (pad 12 thru_hole circle (at 3.97 -2.54 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 27 "Net-(R4-Pad1)"))
    (pad 13 thru_hole circle (at 3.97 -5.08 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 14 thru_hole circle (at 3.97 -7.62 180) (size 1.17 1.17) (drill 0.77) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-14_W7.62mm.step
      (offset (xyz -3.75 7.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 54.23 91.43 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 4.064 0 90) (layer F.SilkS))
    (fp_text value D (at 2.794 0.635 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.SilkS))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 4.2 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 16 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 +5V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 58.64 80.96 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference BC (at 0 2.0955 270) (layer B.SilkS))
    (fp_text value BUCK (at 0 -7.41 90) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 40.259 82.677 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 330 (at 3.683 0 90) (layer F.SilkS))
    (fp_text value 330R (at 3.937 0.127 90) (layer F.Fab))
    (fp_text user %R (at -0.762 -8.509 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad6)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (offset (xyz 0 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 42.672 82.677 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 330 (at 3.683 0 90) (layer F.SilkS))
    (fp_text value 330R (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 6.35 -19.05 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (offset (xyz 0 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 45.085 82.677 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 330 (at 3.683 0 90) (layer F.SilkS))
    (fp_text value 330R (at 3.937 0.127 90) (layer F.Fab))
    (fp_text user %R (at 0.254 -22.733 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(R5-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (offset (xyz 0 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 47.498 82.677 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 50K (at 3.937 0 90) (layer F.SilkS))
    (fp_text value 50K (at 3.81 0 90) (layer F.Fab))
    (fp_text user %R (at 3.556 11.811 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (offset (xyz 0 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 40.67 79.04)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference GPS (at 2.03 -0.87 90) (layer B.SilkS))
    (fp_text value GPS (at 0 -9.95) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 -90) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GPS_RX))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 GPS_TX))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 57.74 61.3 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference I2C (at -2.02 -3.75 90) (layer B.SilkS))
    (fp_text value I2C (at 0 -9.95) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 SCL))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 60.26 68.94 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference 4K7 (at 3.47 0.09 90) (layer F.SilkS))
    (fp_text value 4K7 (at 3.81 1.92 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 SCL))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 61.7 105.06 90)
    (descr "Through hole straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.54mm double row")
    (fp_text reference SW (at 1.27 2.33 270) (layer B.SilkS))
    (fp_text value Conn_02x04_Odd_Even (at 1.27 -9.95 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -3.81) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 EVO-Wifi-Off))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 ESP-Wifi-Off))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 ESP-Wifi-Mode))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 ESP-Restore-Defaults))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 56.28 78.44 270) (layer F.SilkS))
  (gr_text 5v (at 52.87 79.24 270) (layer F.SilkS))
  (gr_text 12v (at 58.73 78.55 270) (layer F.SilkS))
  (gr_text "HomeBrew\nGPS+WiFi+BT" (at 55.3085 98.6155) (layer F.SilkS))
  (gr_text GND (at 43.18 96.266) (layer B.SilkS))
  (gr_text RX (at 46.99 98.806) (layer B.SilkS))
  (gr_text TX (at 44.45 98.806) (layer B.SilkS))
  (gr_text Select (at 41.91 98.806) (layer B.SilkS))
  (gr_text +12v (at 45.72 96.266) (layer B.SilkS))
  (gr_text 5v (at 52.82 78.82 270) (layer B.SilkS))
  (gr_text GND (at 56.24 78.23 270) (layer B.SilkS))
  (gr_text 12v (at 58.55 78.36 270) (layer B.SilkS))
  (gr_text 74HC125 (at 47.905 69.596 90) (layer F.SilkS))
  (gr_text "WiFi Reset" (at 53.42 97.46 280) (layer B.SilkS))
  (gr_text "WiFi Mode" (at 56.16 97.54 280) (layer B.SilkS))
  (gr_text "ESPWiFi On" (at 58.6 97.08 280) (layer B.SilkS))
  (gr_text "EVOWiFi Off" (at 60.88 96.89 280) (layer B.SilkS))
  (gr_line (start 36.195 59.436) (end 36.195 107.061) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.4525 59.436) (end 36.195 59.436) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.4525 107.061) (end 64.4525 59.436) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 36.195 107.061) (end 64.4525 107.061) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.4525 107.061) (xy 36.195 107.061) (xy 36.17125 60.07175) (xy 64.42875 60.00825)
      )
    )
  )
)
