(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 8)
    (zones 0)
    (modules 7)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (grid_origin 107.95 63.5)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 107.95 63.5)
    (fp_text reference D1 (at -1.5 3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad2)"))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 146.05 63.5 180)
    (fp_text reference D2 (at -1.4 -3 180) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0 180) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.425 0 180) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
  )
  (module AOR_custom:header_01x02 (layer F.Cu) (tedit 5C6B48DB)
    (at 114.935 67.945 90)
    (fp_text reference J1 (at -1.555 -1.985 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -0.5 90) (layer F.Fab))
    (fp_text user "" (at 0 1.778 90) (layer B.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 5V))
  )
  (module AOR_custom:header_01x02 (layer F.Cu) (tedit 5C6B48C9)
    (at 139.065 67.945 90)
    (fp_text reference J2 (at -1.555 1.885 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -0.5 90) (layer F.Fab))
    (fp_text user "" (at 0 1.778 90) (layer B.SilkS))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 5V))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 111.255 66.675 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 5V))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.875 66.675)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0.075 1.825) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 126.45 69)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "ACP3-X-LTE-PCB\nREV. A, 2-18-2019" (at 126.45 66.5) (layer F.SilkS))
  (gr_text GND (at 136.45 69.5) (layer F.SilkS))
  (gr_text GND (at 117.45 69.5) (layer F.SilkS))
  (gr_text 5V (at 136.45 66.5) (layer F.SilkS))
  (gr_text 5V (at 117.45 66.5) (layer F.SilkS))
  (gr_line (start 104.95 62) (end 104.95 70.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.95 62) (end 104.95 62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.95 65) (end 110.95 62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.95 65) (end 110.95 65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.95 62) (end 142.95 65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.95 62) (end 142.95 62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.95 70.5) (end 148.95 62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.95 70.5) (end 148.95 70.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.95 62) (xy 110.95 68.5) (xy 142.95 68.5) (xy 142.95 62) (xy 148.95 62)
        (xy 148.95 70.5) (xy 104.95 70.5) (xy 104.95 62)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104.95 62) (xy 110.95 62) (xy 110.95 65) (xy 142.95 65) (xy 142.95 62)
        (xy 148.95 62) (xy 148.95 70.5) (xy 104.95 70.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.95 65) (xy 110.95 62) (xy 104.95 62) (xy 104.95 65)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.95 65) (xy 148.95 65) (xy 148.95 62) (xy 142.95 62)
      )
    )
  )
  (zone (net 4) (net_name 5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.95 65) (xy 111.95 67.5) (xy 141.95 67.5) (xy 141.95 65)
      )
    )
  )
)
