(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1~bpo8+1)
  (general
    (links 116)
    (no_connects 0)
    (area 116.764999 86.284999 167.715001 106.755001)
    (thickness 1.6)
    (drawings 4)
    (tracks 138)
    (zones 0)
    (modules 85)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3302)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BT1-Pad1)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 +3V3)
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 "Net-(D3-Pad2)")
  (net 10 /pmod_connector/spi1_ss0)
  (net 11 /ds3234_circuit/32kHz)
  (net 12 /pmod_connector/gpio_mio9)
  (net 13 /ds3234_circuit/rst_n)
  (net 14 /pmod_connector/sp1_miso)
  (net 15 /pmod_connector/spi1_clk)
  (net 16 /pmod_connector/gpio_mio14)
  (net 17 /pmod_connector/gpio_mio15)
  (net 18 /pmod_connector/spi1_mosi)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.3302)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net /ds3234_circuit/32kHz)
    (add_net /ds3234_circuit/rst_n)
    (add_net /pmod_connector/gpio_mio14)
    (add_net /pmod_connector/gpio_mio15)
    (add_net /pmod_connector/gpio_mio9)
    (add_net /pmod_connector/sp1_miso)
    (add_net /pmod_connector/spi1_clk)
    (add_net /pmod_connector/spi1_mosi)
    (add_net /pmod_connector/spi1_ss0)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 166.37 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 166.37 105.41)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 144.78 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 158.496 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 154.94 94.234)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 150.368 94.742)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 150.368 97.028)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 150.368 98.298)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 150.368 99.568)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 150.368 100.838)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 137.16 93.218)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 134.62 93.218)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 132.08 93.218)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 150.368 92.202)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 154.94 97.79)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 154.94 100.33)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 154.94 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 150.368 102.108)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 142.24 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 132.08 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 129.54 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 129.54 93.218)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 139.7 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 137.16 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 134.62 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 132.08 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 129.54 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 139.7 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 137.16 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 134.62 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 132.08 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 129.54 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 127 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 119.38 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 124.46 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 121.92 104.14)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 121.92 101.6)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 121.92 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 119.38 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 124.46 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 121.92 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 121.92 93.98)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 121.92 91.44)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 119.38 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 121.92 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 124.46 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 127 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 129.54 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 132.08 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 134.62 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 137.16 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 139.7 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 144.78 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 146.05 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 147.32 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 165.1 93.98)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 165.1 91.44)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 162.56 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 156.718 88.9)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 153.67 91.44)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 154.94 101.6)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 160.02 101.6)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 165.1 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 160.02 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 162.56 101.6)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 165.1 101.6)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 162.56 99.06)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 162.56 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module batter_rec:MS920T-FL27E (layer B.Cu) (tedit 5A94C13E)
    (at 146.05 96.52 180)
    (fp_text reference BT1 (at -5.8 0 450) (layer B.SilkS))
    (fp_text value MS920T-FL27E (at -5.625 5.65 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 1 -1 180) (size 1.8 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1 1 180) (size 1.8 0.7) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(BT1-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5A937F88)
    (at 138.43 96.52 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BAS40-04 (at 0 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module soic:SOIC20 (layer F.Cu) (tedit 0)
    (at 152.4 96.52)
    (solder_paste_margin -0.0508)
    (attr smd)
    (fp_text reference IC1 (at 0 7.62) (layer F.SilkS))
    (fp_text value DS3234 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -4.685 -5.715) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 10 /pmod_connector/spi1_ss0))
    (pad 2 smd rect (at -4.685 -4.445) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -4.685 -3.175) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 11 /ds3234_circuit/32kHz))
    (pad 4 smd rect (at -4.685 -1.905) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 5 smd rect (at -4.685 -0.635) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 12 /pmod_connector/gpio_mio9))
    (pad 6 smd rect (at -4.685 0.635) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 13 /ds3234_circuit/rst_n))
    (pad 7 smd rect (at -4.685 1.905) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -4.685 3.175) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.685 4.445) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -4.685 5.715) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.685 5.715) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 4.685 4.445) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 4.685 3.175) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 4.685 1.905) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 4.685 0.635) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 4.685 -0.635) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 17 smd rect (at 4.685 -1.905) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 18 /pmod_connector/spi1_mosi))
    (pad 18 smd rect (at 4.685 -3.175) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 15 /pmod_connector/spi1_clk))
    (pad 19 smd rect (at 4.685 -4.445) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 14 /pmod_connector/sp1_miso))
    (pad 20 smd rect (at 4.685 -5.715) (size 1.98 0.53) (layers F.Cu F.Paste F.Mask)
      (net 15 /pmod_connector/spi1_clk))
  )
  (module batter_rec:PTS645SK43SMTR92LFS (layer F.Cu) (tedit 5A938360)
    (at 121.92 96.52 270)
    (fp_text reference SW1 (at 0.3 0 270) (layer F.SilkS))
    (fp_text value PTS645SK43SMTR92LFS (at 0.2 -4.2 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 4 2.3 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4 2.3 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4 -2.3 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /ds3234_circuit/rst_n))
    (pad 1 smd rect (at 4 -2.3 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /ds3234_circuit/rst_n))
  )
  (module batter_rec:PMOD (layer B.Cu) (tedit 5A93875C)
    (at 161.29 102.87)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference P1 (at 1.27 2.33) (layer B.SilkS))
    (fp_text value PMOD-Device-x2-Type-Generic-Alt (at 10.922 -15.494) (layer B.Fab) hide)
    (fp_text user %R (at 1.27 -6.35 90) (layer B.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /pmod_connector/spi1_ss0))
    (pad 7 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ds3234_circuit/32kHz))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /pmod_connector/spi1_mosi))
    (pad 8 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /pmod_connector/gpio_mio9))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /pmod_connector/sp1_miso))
    (pad 9 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /pmod_connector/gpio_mio14))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /pmod_connector/spi1_clk))
    (pad 10 thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /pmod_connector/gpio_mio15))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A94C24F)
    (at 145.669 93.218 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value C1608X7R1E104M080AA (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5A94C15F)
    (at 152.019 88.9 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.699 0.254 180) (layer F.SilkS))
    (fp_text value C3216X7R1V106M160AC (at 0 2 180) (layer F.Fab) hide)
    (fp_text user %R (at -4.191 0.254 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module batter_rec:GND-VIA (layer F.Cu) (tedit 5A94C9C0)
    (at 165.1 96.52)
    (fp_text reference REF** (at 0.1 1.9) (layer F.SilkS) hide)
    (fp_text value GND-VIA (at 0 -1.4) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A962F07)
    (at 133.35 101.6 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value "LG L29K-F2J1-24-Z" (at 0 1.55 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A962F5F)
    (at 133.35 91.44 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value "LS L29K-G1J2-1-Z" (at 0 1.55 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SuperSOT-3 (layer F.Cu) (tedit 5A962F0F)
    (at 139.7 101.6 180)
    (descr "3-pin SuperSOT package https://www.fairchildsemi.com/package-drawings/MA/MA03B.pdf")
    (tags "SuperSOT-3 SSOT-3")
    (attr smd)
    (fp_text reference Q1 (at 0 -2.35 180) (layer F.SilkS))
    (fp_text value FDN339AN (at 0 2.4 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /pmod_connector/gpio_mio14))
    (pad 2 smd rect (at -1.1 0.95 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SuperSOT-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SuperSOT-3 (layer F.Cu) (tedit 5A962F52)
    (at 139.7 91.44 180)
    (descr "3-pin SuperSOT package https://www.fairchildsemi.com/package-drawings/MA/MA03B.pdf")
    (tags "SuperSOT-3 SSOT-3")
    (attr smd)
    (fp_text reference Q2 (at 0 -2.35 180) (layer F.SilkS))
    (fp_text value FDN339AN (at 0 2.4 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /pmod_connector/gpio_mio15))
    (pad 2 smd rect (at -1.1 0.95 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.1 0 180) (size 1.4 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SuperSOT-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A962F77)
    (at 142.24 96.774 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 620 (at 0 1.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A962F67)
    (at 143.51 101.346 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /pmod_connector/gpio_mio9))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A962F19)
    (at 128.27 101.6)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 261 (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A962F72)
    (at 128.27 91.44)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 261 (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5A962F6D)
    (at 143.51 91.44 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /pmod_connector/spi1_ss0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 167.64 86.36) (end 116.84 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.64 106.68) (end 167.64 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.84 106.68) (end 167.64 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.84 86.36) (end 116.84 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.094 86.614) (xy 167.386 86.614) (xy 167.386 106.426) (xy 117.094 106.426)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.094 86.614) (xy 167.386 86.614) (xy 167.386 106.553) (xy 117.094 106.553)
      )
    )
  )
  (zone (net 5) (net_name +3V3) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.094 86.614) (xy 117.094 106.426) (xy 167.386 106.426) (xy 167.386 86.614)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.094 86.614) (xy 117.094 106.426) (xy 167.386 106.426) (xy 167.386 86.614)
      )
    )
  )
)
