(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 34)
    (no_connects 0)
    (area 126.310429 84.314 196.269572 125.336)
    (thickness 1.6)
    (drawings 5)
    (tracks 17)
    (zones 0)
    (modules 22)
    (nets 4)
  )
  (page A)
  (title_block
    (title "Positive Power Distributoin")
    (date 2017-02-21)
    (rev 1.0)
    (company "Rice University")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.524)
    (trace_clearance 0.381)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.7 3.7)
    (pad_drill 3.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 130.81 86.36)
    (grid_origin 130.81 86.36)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 V_OUT)
  (net_class Default "This is the default net class."
    (clearance 0.381)
    (trace_width 1.524)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
    (add_net V_OUT)
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD01C5)
    (at 161.29 118.11)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P9 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD01BB)
    (at 152.4 118.11)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P8 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD01B1)
    (at 143.51 118.11)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P7 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD01A8)
    (at 170.18 118.11)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P10 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD019D)
    (at 179.07 118.11)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P11 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD0192)
    (at 179.07 106.68)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P6 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD0188)
    (at 170.18 106.68)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P5 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD017C)
    (at 161.29 106.68)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P4 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD0173)
    (at 152.4 106.68)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P3 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD0167)
    (at 143.51 106.68)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P2 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value OUT (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_2pin_straight (layer F.Cu) (tedit 58AD013A)
    (at 134.62 106.68)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 2pin, straight,")
    (fp_text reference P1 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value IN (at 0 4.064) (layer F.SilkS))
    (fp_text user - (at 1.27 -3.81) (layer F.SilkS))
    (fp_text user + (at -1.27 -3.81) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 58ACF9E5)
    (at 144.78 96.52 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value CP1 (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58ACFAEA)
    (at 153.67 95.25 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value C (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 58ACFAEC)
    (at 175.26 95.25 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at -1.905 0 360) (layer F.SilkS))
    (fp_text value C (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 58ACFA20)
    (at 181.61 97.79)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value CP1 (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 58ACFAD2)
    (at 160.02 100.33)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 1N4004 (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 58ACFAED)
    (at 170.18 88.9 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1N4004 (at 5.08 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58ACFA03)
    (at 165.1 95.25)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U1 (at 0 -4.318) (layer F.SilkS))
    (fp_text value LM78xx (at 0 -2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 3 V_OUT))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 VCC))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 58AD0068)
    (at 187.96 90.17)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask)
      (clearance 2.54))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 58AD006C)
    (at 187.96 119.38)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask)
      (clearance 2.54))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 58AD0070)
    (at 134.62 119.38)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask)
      (clearance 2.54))
  )
  (module Mounting_Holes:MountingHole_3.7mm (layer F.Cu) (tedit 58AD0075)
    (at 134.62 90.17)
    (descr "Mounting Hole 3.7mm, no annular")
    (tags "mounting hole 3.7mm no annular")
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm (at 0 4.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.7 3.7) (drill 3.7) (layers *.Cu *.Mask)
      (clearance 2.54))
  )
  (gr_text "Positive Power Distribution\n2017/02/21" (at 189.23 104.775 90) (layer F.SilkS))
  (gr_line (start 130.81 86.36) (end 130.81 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 86.36) (end 130.81 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.77 123.19) (end 191.77 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 123.19) (end 191.77 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.524))
    (polygon
      (pts
        (xy 191.135 122.555) (xy 131.445 122.555) (xy 131.445 86.995) (xy 191.135 86.995)
      )
    )
  )
  (zone (net 3) (net_name V_OUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1.524))
    (polygon
      (pts
        (xy 182.245 121.285) (xy 140.335 121.285) (xy 140.335 103.505) (xy 182.245 103.505)
      )
    )
  )
)
