(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 271)
    (no_connects 0)
    (area 33.424999 28.674999 158.325001 100.825001)
    (thickness 1.6)
    (drawings 22)
    (tracks 1002)
    (zones 0)
    (modules 91)
    (nets 140)
  )
  (page USLetter)
  (title_block
    (date 2018-01-16)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.5)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 1.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(D201-Pad1)")
  (net 2 "Net-(D201-Pad2)")
  (net 3 "Net-(D202-Pad1)")
  (net 4 "Net-(D202-Pad2)")
  (net 5 "Net-(D203-Pad1)")
  (net 6 "Net-(D203-Pad2)")
  (net 7 "Net-(D204-Pad1)")
  (net 8 "Net-(D204-Pad2)")
  (net 9 "Net-(D205-Pad1)")
  (net 10 "Net-(D205-Pad2)")
  (net 11 "Net-(D206-Pad1)")
  (net 12 "Net-(D206-Pad2)")
  (net 13 "Net-(D207-Pad1)")
  (net 14 "Net-(D207-Pad2)")
  (net 15 "Net-(D208-Pad1)")
  (net 16 "Net-(D208-Pad2)")
  (net 17 "Net-(D209-Pad1)")
  (net 18 "Net-(D209-Pad2)")
  (net 19 "Net-(D210-Pad1)")
  (net 20 "Net-(D210-Pad2)")
  (net 21 "Net-(D211-Pad1)")
  (net 22 "Net-(D211-Pad2)")
  (net 23 "Net-(D212-Pad1)")
  (net 24 "Net-(D212-Pad2)")
  (net 25 "Net-(D213-Pad1)")
  (net 26 "Net-(D213-Pad2)")
  (net 27 "Net-(D214-Pad1)")
  (net 28 "Net-(D214-Pad2)")
  (net 29 "Net-(D215-Pad1)")
  (net 30 "Net-(D215-Pad2)")
  (net 31 "Net-(D216-Pad1)")
  (net 32 "Net-(D216-Pad2)")
  (net 33 "Net-(D301-Pad1)")
  (net 34 "Net-(D301-Pad2)")
  (net 35 "Net-(D302-Pad1)")
  (net 36 "Net-(D302-Pad2)")
  (net 37 "Net-(D303-Pad1)")
  (net 38 "Net-(D303-Pad2)")
  (net 39 "Net-(D304-Pad1)")
  (net 40 "Net-(D304-Pad2)")
  (net 41 "Net-(D305-Pad1)")
  (net 42 "Net-(D305-Pad2)")
  (net 43 "Net-(D306-Pad1)")
  (net 44 "Net-(D306-Pad2)")
  (net 45 "Net-(D307-Pad1)")
  (net 46 "Net-(D307-Pad2)")
  (net 47 "Net-(D308-Pad1)")
  (net 48 "Net-(D308-Pad2)")
  (net 49 "Net-(D309-Pad1)")
  (net 50 "Net-(D309-Pad2)")
  (net 51 "Net-(D310-Pad1)")
  (net 52 "Net-(D310-Pad2)")
  (net 53 "Net-(D311-Pad1)")
  (net 54 "Net-(D311-Pad2)")
  (net 55 "Net-(D312-Pad1)")
  (net 56 "Net-(D312-Pad2)")
  (net 57 "Net-(D313-Pad1)")
  (net 58 "Net-(D313-Pad2)")
  (net 59 "Net-(D314-Pad1)")
  (net 60 "Net-(D314-Pad2)")
  (net 61 "Net-(D315-Pad1)")
  (net 62 "Net-(D315-Pad2)")
  (net 63 "Net-(D316-Pad1)")
  (net 64 "Net-(D316-Pad2)")
  (net 65 "Net-(R201-Pad2)")
  (net 66 "Net-(R202-Pad2)")
  (net 67 "Net-(R203-Pad2)")
  (net 68 "Net-(R204-Pad2)")
  (net 69 "Net-(R205-Pad1)")
  (net 70 "Net-(R206-Pad1)")
  (net 71 "Net-(R207-Pad1)")
  (net 72 "Net-(R208-Pad1)")
  (net 73 "Net-(R209-Pad2)")
  (net 74 "Net-(R210-Pad2)")
  (net 75 "Net-(R211-Pad2)")
  (net 76 "Net-(R212-Pad2)")
  (net 77 "Net-(R213-Pad1)")
  (net 78 "Net-(R214-Pad1)")
  (net 79 "Net-(R215-Pad1)")
  (net 80 "Net-(R216-Pad1)")
  (net 81 "Net-(R301-Pad2)")
  (net 82 "Net-(R302-Pad2)")
  (net 83 "Net-(R303-Pad2)")
  (net 84 "Net-(R304-Pad2)")
  (net 85 "Net-(R305-Pad1)")
  (net 86 "Net-(R306-Pad1)")
  (net 87 "Net-(R307-Pad1)")
  (net 88 "Net-(R308-Pad1)")
  (net 89 "Net-(R309-Pad2)")
  (net 90 "Net-(R310-Pad2)")
  (net 91 "Net-(R311-Pad2)")
  (net 92 "Net-(R312-Pad2)")
  (net 93 "Net-(R313-Pad1)")
  (net 94 "Net-(R314-Pad1)")
  (net 95 "Net-(R315-Pad1)")
  (net 96 "Net-(R316-Pad1)")
  (net 97 /GND)
  (net 98 /24GND)
  (net 99 /SCL)
  (net 100 /~INT)
  (net 101 /SDA)
  (net 102 /~RESET)
  (net 103 /24V)
  (net 104 "Net-(D101-Pad1)")
  (net 105 /5G)
  (net 106 /5V)
  (net 107 /3.3V)
  (net 108 "Net-(M1-Pad2)")
  (net 109 "Net-(M1-Pad3)")
  (net 110 "Net-(M1-Pad4)")
  (net 111 "Net-(M1-Pad5)")
  (net 112 "Net-(M1-Pad7)")
  (net 113 "Net-(M1-Pad8)")
  (net 114 "Net-(M1-Pad9)")
  (net 115 "Net-(M1-Pad10)")
  (net 116 "Net-(M1-Pad17)")
  (net 117 "Net-(M1-Pad18)")
  (net 118 "Net-(M1-Pad19)")
  (net 119 "Net-(M1-Pad20)")
  (net 120 "Net-(M1-Pad22)")
  (net 121 "Net-(M1-Pad23)")
  (net 122 "Net-(M1-Pad24)")
  (net 123 "Net-(M1-Pad25)")
  (net 124 "Net-(M2-Pad2)")
  (net 125 "Net-(M2-Pad3)")
  (net 126 "Net-(M2-Pad4)")
  (net 127 "Net-(M2-Pad5)")
  (net 128 "Net-(M2-Pad7)")
  (net 129 "Net-(M2-Pad8)")
  (net 130 "Net-(M2-Pad9)")
  (net 131 "Net-(M2-Pad10)")
  (net 132 "Net-(M2-Pad17)")
  (net 133 "Net-(M2-Pad18)")
  (net 134 "Net-(M2-Pad19)")
  (net 135 "Net-(M2-Pad20)")
  (net 136 "Net-(M2-Pad22)")
  (net 137 "Net-(M2-Pad23)")
  (net 138 "Net-(M2-Pad24)")
  (net 139 "Net-(M2-Pad25)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /24GND)
    (add_net /24V)
    (add_net /3.3V)
    (add_net /5G)
    (add_net /5V)
    (add_net /GND)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /~INT)
    (add_net /~RESET)
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D201-Pad1)")
    (add_net "Net-(D201-Pad2)")
    (add_net "Net-(D202-Pad1)")
    (add_net "Net-(D202-Pad2)")
    (add_net "Net-(D203-Pad1)")
    (add_net "Net-(D203-Pad2)")
    (add_net "Net-(D204-Pad1)")
    (add_net "Net-(D204-Pad2)")
    (add_net "Net-(D205-Pad1)")
    (add_net "Net-(D205-Pad2)")
    (add_net "Net-(D206-Pad1)")
    (add_net "Net-(D206-Pad2)")
    (add_net "Net-(D207-Pad1)")
    (add_net "Net-(D207-Pad2)")
    (add_net "Net-(D208-Pad1)")
    (add_net "Net-(D208-Pad2)")
    (add_net "Net-(D209-Pad1)")
    (add_net "Net-(D209-Pad2)")
    (add_net "Net-(D210-Pad1)")
    (add_net "Net-(D210-Pad2)")
    (add_net "Net-(D211-Pad1)")
    (add_net "Net-(D211-Pad2)")
    (add_net "Net-(D212-Pad1)")
    (add_net "Net-(D212-Pad2)")
    (add_net "Net-(D213-Pad1)")
    (add_net "Net-(D213-Pad2)")
    (add_net "Net-(D214-Pad1)")
    (add_net "Net-(D214-Pad2)")
    (add_net "Net-(D215-Pad1)")
    (add_net "Net-(D215-Pad2)")
    (add_net "Net-(D216-Pad1)")
    (add_net "Net-(D216-Pad2)")
    (add_net "Net-(D301-Pad1)")
    (add_net "Net-(D301-Pad2)")
    (add_net "Net-(D302-Pad1)")
    (add_net "Net-(D302-Pad2)")
    (add_net "Net-(D303-Pad1)")
    (add_net "Net-(D303-Pad2)")
    (add_net "Net-(D304-Pad1)")
    (add_net "Net-(D304-Pad2)")
    (add_net "Net-(D305-Pad1)")
    (add_net "Net-(D305-Pad2)")
    (add_net "Net-(D306-Pad1)")
    (add_net "Net-(D306-Pad2)")
    (add_net "Net-(D307-Pad1)")
    (add_net "Net-(D307-Pad2)")
    (add_net "Net-(D308-Pad1)")
    (add_net "Net-(D308-Pad2)")
    (add_net "Net-(D309-Pad1)")
    (add_net "Net-(D309-Pad2)")
    (add_net "Net-(D310-Pad1)")
    (add_net "Net-(D310-Pad2)")
    (add_net "Net-(D311-Pad1)")
    (add_net "Net-(D311-Pad2)")
    (add_net "Net-(D312-Pad1)")
    (add_net "Net-(D312-Pad2)")
    (add_net "Net-(D313-Pad1)")
    (add_net "Net-(D313-Pad2)")
    (add_net "Net-(D314-Pad1)")
    (add_net "Net-(D314-Pad2)")
    (add_net "Net-(D315-Pad1)")
    (add_net "Net-(D315-Pad2)")
    (add_net "Net-(D316-Pad1)")
    (add_net "Net-(D316-Pad2)")
    (add_net "Net-(M1-Pad10)")
    (add_net "Net-(M1-Pad17)")
    (add_net "Net-(M1-Pad18)")
    (add_net "Net-(M1-Pad19)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad20)")
    (add_net "Net-(M1-Pad22)")
    (add_net "Net-(M1-Pad23)")
    (add_net "Net-(M1-Pad24)")
    (add_net "Net-(M1-Pad25)")
    (add_net "Net-(M1-Pad3)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M1-Pad5)")
    (add_net "Net-(M1-Pad7)")
    (add_net "Net-(M1-Pad8)")
    (add_net "Net-(M1-Pad9)")
    (add_net "Net-(M2-Pad10)")
    (add_net "Net-(M2-Pad17)")
    (add_net "Net-(M2-Pad18)")
    (add_net "Net-(M2-Pad19)")
    (add_net "Net-(M2-Pad2)")
    (add_net "Net-(M2-Pad20)")
    (add_net "Net-(M2-Pad22)")
    (add_net "Net-(M2-Pad23)")
    (add_net "Net-(M2-Pad24)")
    (add_net "Net-(M2-Pad25)")
    (add_net "Net-(M2-Pad3)")
    (add_net "Net-(M2-Pad4)")
    (add_net "Net-(M2-Pad5)")
    (add_net "Net-(M2-Pad7)")
    (add_net "Net-(M2-Pad8)")
    (add_net "Net-(M2-Pad9)")
    (add_net "Net-(R201-Pad2)")
    (add_net "Net-(R202-Pad2)")
    (add_net "Net-(R203-Pad2)")
    (add_net "Net-(R204-Pad2)")
    (add_net "Net-(R205-Pad1)")
    (add_net "Net-(R206-Pad1)")
    (add_net "Net-(R207-Pad1)")
    (add_net "Net-(R208-Pad1)")
    (add_net "Net-(R209-Pad2)")
    (add_net "Net-(R210-Pad2)")
    (add_net "Net-(R211-Pad2)")
    (add_net "Net-(R212-Pad2)")
    (add_net "Net-(R213-Pad1)")
    (add_net "Net-(R214-Pad1)")
    (add_net "Net-(R215-Pad1)")
    (add_net "Net-(R216-Pad1)")
    (add_net "Net-(R301-Pad2)")
    (add_net "Net-(R302-Pad2)")
    (add_net "Net-(R303-Pad2)")
    (add_net "Net-(R304-Pad2)")
    (add_net "Net-(R305-Pad1)")
    (add_net "Net-(R306-Pad1)")
    (add_net "Net-(R307-Pad1)")
    (add_net "Net-(R308-Pad1)")
    (add_net "Net-(R309-Pad2)")
    (add_net "Net-(R310-Pad2)")
    (add_net "Net-(R311-Pad2)")
    (add_net "Net-(R312-Pad2)")
    (add_net "Net-(R313-Pad1)")
    (add_net "Net-(R314-Pad1)")
    (add_net "Net-(R315-Pad1)")
    (add_net "Net-(R316-Pad1)")
  )
  (module w_conn_strip:vasch_strip_4x2 locked (layer F.Cu) (tedit 5AA80528)
    (at 142.875 87.63 270)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P102 (at 2.54 -5.715 270) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 270) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 105 /5G))
    (pad 7 thru_hole oval (at 3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 97 /GND))
    (pad 1 thru_hole rect (at -3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 107 /3.3V))
    (pad 2 thru_hole oval (at -3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 106 /5V))
    (pad 3 thru_hole oval (at -1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 99 /SCL))
    (pad 4 thru_hole oval (at -1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 100 /~INT))
    (pad 5 thru_hole oval (at 1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 101 /SDA))
    (pad 6 thru_hole oval (at 1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 102 /~RESET))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "0 My Pins:KF141V-09P" (layer F.Cu) (tedit 5AA804D4)
    (at 45.72 35.56)
    (fp_text reference J201 (at 0 7.62 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Female (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(D201-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(D201-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D202-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D202-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(D203-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(D203-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(D204-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(D204-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(D205-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(D205-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(D206-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(D206-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(D207-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(D207-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(D208-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(D208-Pad1)"))
  )
  (module "0 My Pins:KF141V-09P" (layer F.Cu) (tedit 5AA804DA)
    (at 72.39 35.56)
    (fp_text reference J202 (at 0 7.62 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Female (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(D209-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(D209-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(D210-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(D210-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(D211-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(D211-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(D212-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(D212-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(D213-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(D213-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(D214-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(D214-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(D215-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(D215-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(D216-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(D216-Pad1)"))
  )
  (module "0 My Mount:DIN-Mount-Clip" locked (layer F.Cu) (tedit 5A5E1BC9)
    (at 38.1 64.77)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value DIN-Mount-Clip (at -3.81 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "0 My Mount:DIN-Mount-Clip" locked (layer F.Cu) (tedit 5A5E1BBB)
    (at 153.67 64.77)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value DIN-Mount-Clip (at -3.81 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "0 My Pins:KF141V-09P" (layer F.Cu) (tedit 5AA804E1)
    (at 99.06 35.56)
    (fp_text reference J301 (at 0 7.62 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Female (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(D301-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(D301-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 "Net-(D302-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 "Net-(D302-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(D303-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 "Net-(D303-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 "Net-(D304-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 39 "Net-(D304-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 "Net-(D305-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 "Net-(D305-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 "Net-(D306-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 "Net-(D306-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "Net-(D307-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "Net-(D307-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "Net-(D308-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 47 "Net-(D308-Pad1)"))
  )
  (module "0 My Pins:KF141V-09P" (layer F.Cu) (tedit 5AA804E7)
    (at 125.73 35.56)
    (fp_text reference J302 (at 0 7.62 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Female (at 7.62 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "Net-(D309-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "Net-(D309-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "Net-(D310-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "Net-(D310-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 53 "Net-(D311-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 53 "Net-(D311-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 55 "Net-(D312-Pad1)"))
    (pad 5 thru_hole circle (at 10.16 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 55 "Net-(D312-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 57 "Net-(D313-Pad1)"))
    (pad 6 thru_hole circle (at 12.7 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 57 "Net-(D313-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 59 "Net-(D314-Pad1)"))
    (pad 7 thru_hole circle (at 15.24 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 59 "Net-(D314-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 61 "Net-(D315-Pad1)"))
    (pad 8 thru_hole circle (at 17.78 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 61 "Net-(D315-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 63 "Net-(D316-Pad1)"))
    (pad 9 thru_hole circle (at 20.32 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 63 "Net-(D316-Pad1)"))
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 37.465 63.5 90)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference LIC101 (at 0.3 -1.4 90) (layer F.SilkS) hide)
    (fp_text value CC-BY-NC-SA-icon (at 0.3 0.5 90) (layer F.SilkS) hide)
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 50.165 54.61 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R201 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(R201-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 50.165 59.69 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R202 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(R202-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 50.165 64.77 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R203 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(R203-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 50.165 69.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R204 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(R204-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 61.595 72.39 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R205 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(R205-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(M1-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 61.595 67.31 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R206 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(R206-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(M1-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 61.595 62.23 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R207 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(R207-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(M1-Pad9)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 61.595 57.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R208 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(R208-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(M1-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 76.835 54.61 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R209 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(R209-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 76.835 59.69 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R210 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(R210-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 76.835 64.77 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R211 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(R211-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 76.835 69.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R212 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(R212-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 88.265 72.39 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R213 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(R213-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(M1-Pad22)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 88.265 67.31 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R214 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(R214-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(M1-Pad23)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 88.265 62.23 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R215 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(R215-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(M1-Pad24)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 88.265 57.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R216 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 80 "Net-(R216-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 123 "Net-(M1-Pad25)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 103.505 54.61 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R301 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 81 "Net-(R301-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 103.505 59.69 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R302 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(R302-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 103.505 64.77 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R303 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(R303-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 5A5D2ED1)
    (at 103.505 69.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R304 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 0 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 84 "Net-(R304-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 114.935 72.39 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R305 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 85 "Net-(R305-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 128 "Net-(M2-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 114.935 67.31 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R306 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(R306-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 129 "Net-(M2-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 114.935 62.23 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R307 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(R307-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 130 "Net-(M2-Pad9)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 114.935 57.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R308 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(R308-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(M2-Pad10)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 130.175 54.61 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R309 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(R309-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 130.175 59.69 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R310 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 90 "Net-(R310-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 130.175 64.77 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R311 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 91 "Net-(R311-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 130.175 69.85 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R312 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 103 /24V))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(R312-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 141.605 72.39 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R313 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R313-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 136 "Net-(M2-Pad22)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 141.605 67.31 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R314 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(R314-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 137 "Net-(M2-Pad23)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 141.605 62.23 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R315 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(R315-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 138 "Net-(M2-Pad24)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer B.Cu) (tedit 58E0A804)
    (at 141.605 57.15 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R316 (at 0 1.85 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.95 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(R316-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers B.Cu B.Paste B.Mask)
      (net 139 "Net-(M2-Pad25)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_4x2 locked (layer F.Cu) (tedit 5AA8052B)
    (at 48.895 87.63 270)
    (descr "Box header 4x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference P101 (at 2.54 5.715 270) (layer F.SilkS))
    (fp_text value MY_CONN_I2C (at 0 5.7 270) (layer F.SilkS) hide)
    (pad 8 thru_hole oval (at 3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 105 /5G))
    (pad 7 thru_hole oval (at 3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 97 /GND))
    (pad 1 thru_hole rect (at -3.81 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 107 /3.3V))
    (pad 2 thru_hole oval (at -3.81 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 106 /5V))
    (pad 3 thru_hole oval (at -1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 99 /SCL))
    (pad 4 thru_hole oval (at -1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 100 /~INT))
    (pad 5 thru_hole oval (at 1.27 1.27 270) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 101 /SDA))
    (pad 6 thru_hole oval (at 1.27 -1.27 270) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 102 /~RESET))
    (model walter/conn_strip/vasch_strip_4x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A8B48F0)
    (at 37.465 92.075 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C101 (at 5.842 0 360) (layer F.SilkS))
    (fp_text value CP (at 1.25 4.46 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 /3.3V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer F.Cu) (tedit 0)
    (at 37.465 63.5 90)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference LIC201 (at 0.3 -1.4 90) (layer F.SilkS) hide)
    (fp_text value CC-BY-NC-SA-icon (at 0.3 0.5 90) (layer F.SilkS) hide)
  )
  (module w_logo:Logo_silk_CC-BY-NC-SA_10x3.6mm (layer B.Cu) (tedit 0)
    (at 37.465 63.5 270)
    (descr "CC BY-NC-SA logo, 10x3.6mm")
    (fp_text reference LIC301 (at 0.3 1.4 270) (layer B.SilkS) hide)
    (fp_text value CC-BY-NC-SA-icon (at 0.3 -0.5 270) (layer B.SilkS) hide)
  )
  (module "0 My Pins:KF141V-02P" (layer F.Cu) (tedit 5AA804F6)
    (at 38.1 35.56)
    (fp_text reference P103 (at 4.445 7.62 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 103 /24V))
  )
  (module "0 My Pins:KF141V-02P" (layer F.Cu) (tedit 0)
    (at 153.67 35.56)
    (fp_text reference P104 (at -5 3 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 98 /24GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 103 /24V))
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 46.355 54.61)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U201 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(R201-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D201-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(M1-Pad5)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(R202-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D202-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(M1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(R203-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D203-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(M1-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(R204-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D204-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(M1-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 65.405 72.39 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U202 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11 180) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(R205-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D208-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(R206-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D207-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(R207-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D206-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(R208-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D205-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 73.025 54.61)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U204 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(R209-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D209-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(M1-Pad20)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(R210-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(D210-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(M1-Pad19)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(R211-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(D211-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(M1-Pad18)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(R212-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(D212-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(M1-Pad17)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 92.075 72.39 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U205 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11 180) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(R213-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(D216-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(R214-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(D215-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(R215-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(D214-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(R216-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(D213-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 99.695 54.61)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U301 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(R301-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(D301-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(M2-Pad5)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(R302-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(D302-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(M2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(R303-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(D303-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(M2-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(R304-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(D304-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(M2-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 118.745 72.39 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U302 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11 180) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(R305-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(D308-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(R306-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(D307-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(R307-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(D306-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(R308-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(D305-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 126.365 54.61)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U304 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 "Net-(R309-Pad2)"))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(D309-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(M2-Pad20)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 "Net-(R310-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(D310-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(M2-Pad19)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 "Net-(R311-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(D311-Pad2)"))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 "Net-(M2-Pad18)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 "Net-(R312-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(D312-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(M2-Pad17)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 145.415 72.39 180)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U305 (at 3.81 -2.33 180) (layer F.SilkS))
    (fp_text value LTV-845 (at 3.81 20.11 180) (layer F.Fab))
    (fp_text user %R (at 3.81 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 "Net-(R313-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(D316-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 "Net-(R314-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(D315-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 "Net-(R315-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(D314-Pad2)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 "Net-(R316-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(D313-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 /24V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3B80)
    (at 95.885 65.405 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D101 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(D101-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 107 /3.3V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3CAD)
    (at 48.26 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D201 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D201-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D201-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3D02)
    (at 50.8 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D202 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D202-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D202-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3D28)
    (at 53.34 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D203 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D203-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D203-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3D31)
    (at 55.88 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D204 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D204-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D204-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3D3A)
    (at 58.42 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D205 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D205-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D205-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3D43)
    (at 60.96 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D206 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D206-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D206-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3D4C)
    (at 63.5 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D207 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D207-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D207-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3D4D)
    (at 66.04 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D208 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D208-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D208-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E04)
    (at 74.93 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D209 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D209-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D209-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E09)
    (at 77.47 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D210 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D210-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D210-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E0D)
    (at 80.01 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D211 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D211-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D211-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E16)
    (at 82.55 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D212 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D212-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D212-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E33)
    (at 85.09 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D213 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D213-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D213-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E3A)
    (at 87.63 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D214 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D214-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D214-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E40)
    (at 90.17 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D215 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D215-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D215-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E47)
    (at 92.71 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D216 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D216-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D216-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E7E)
    (at 101.6 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D301 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D301-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D301-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E83)
    (at 104.14 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D302 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D302-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D302-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E88)
    (at 106.68 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D303 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(D303-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(D303-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E8E)
    (at 109.22 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D304 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(D304-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(D304-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E92)
    (at 111.76 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D305 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D305-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D305-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E97)
    (at 114.3 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D306 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D306-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D306-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3E9C)
    (at 116.84 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D307 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D307-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D307-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3EA0)
    (at 119.38 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D308 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(D308-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D308-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3ED1)
    (at 128.27 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D309 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(D309-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(D309-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3ED5)
    (at 130.81 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D310 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(D310-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(D310-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3ED8)
    (at 133.35 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D311 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(D311-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(D311-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3EE0)
    (at 135.89 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D312 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(D312-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(D312-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3EE4)
    (at 138.43 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D313 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(D313-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(D313-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3EE9)
    (at 140.97 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D314 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(D314-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(D314-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3EED)
    (at 143.51 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D315 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(D315-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D315-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 5A5F3EF2)
    (at 146.05 46.99 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D316 (at -5.08 0 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(D316-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(D316-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5A8B48FB)
    (at 95.885 73.025 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R104 (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(D101-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 97 /GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "0 My SparkFun:SparkFun_SX1509_Alt" (layer F.Cu) (tedit 5AA8046C)
    (at 75.565 87.63 90)
    (fp_text reference M1 (at 0 16.51 90) (layer F.SilkS))
    (fp_text value SparkFun_SX1509_Alt (at 0 0 180) (layer F.SilkS))
    (fp_text user ~INT (at -6.35 -13.97 180) (layer F.SilkS))
    (fp_text user ~RST (at -3.81 -13.97 180) (layer F.SilkS))
    (fp_text user SCL (at 6.35 -13.97 180) (layer F.SilkS))
    (fp_text user SDA (at 3.81 -13.97 180) (layer F.SilkS))
    (fp_text user 3.3V (at 1.27 -13.716 180) (layer F.SilkS))
    (fp_text user GND (at -1.27 -13.97 180) (layer F.SilkS))
    (fp_text user GND (at 4.826 -11.43 90) (layer F.SilkS))
    (fp_text user 15 (at 5.08 -8.89 90) (layer F.SilkS))
    (fp_text user 14 (at 5.08 -6.35 90) (layer F.SilkS))
    (fp_text user 13 (at 5.08 -3.81 90) (layer F.SilkS))
    (fp_text user 12 (at 5.08 -1.27 90) (layer F.SilkS))
    (fp_text user VCC2 (at 3.81 1.27 90) (layer F.SilkS))
    (fp_text user 11 (at 5.08 3.81 90) (layer F.SilkS))
    (fp_text user 10 (at 5.08 6.35 90) (layer F.SilkS))
    (fp_text user 9 (at 5.08 8.89 90) (layer F.SilkS))
    (fp_text user 8 (at 5.08 11.43 90) (layer F.SilkS))
    (fp_text user GND (at -4.064 -11.43 90) (layer F.SilkS))
    (fp_text user 7 (at -5.08 11.43 90) (layer F.SilkS))
    (fp_text user 6 (at -5.08 8.89 90) (layer F.SilkS))
    (fp_text user 5 (at -5.08 6.35 90) (layer F.SilkS))
    (fp_text user 4 (at -5.08 3.81 90) (layer F.SilkS))
    (fp_text user VCC1 (at -3.81 1.27 90) (layer F.SilkS))
    (fp_text user 3 (at -5.08 -1.27 90) (layer F.SilkS))
    (fp_text user 2 (at -5.08 -3.81 90) (layer F.SilkS))
    (fp_text user 1 (at -5.08 -6.35 90) (layer F.SilkS))
    (fp_text user 0 (at -5.08 -8.89 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 -11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 2 thru_hole circle (at -7.62 -8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 108 "Net-(M1-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 109 "Net-(M1-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 110 "Net-(M1-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 111 "Net-(M1-Pad5)"))
    (pad 6 thru_hole circle (at -7.62 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 /3.3V))
    (pad 7 thru_hole circle (at -7.62 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 112 "Net-(M1-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 113 "Net-(M1-Pad8)"))
    (pad 9 thru_hole circle (at -7.62 8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 114 "Net-(M1-Pad9)"))
    (pad 10 thru_hole circle (at -7.62 11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 115 "Net-(M1-Pad10)"))
    (pad 17 thru_hole circle (at 7.62 11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 116 "Net-(M1-Pad17)"))
    (pad 18 thru_hole circle (at 7.62 8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 117 "Net-(M1-Pad18)"))
    (pad 19 thru_hole circle (at 7.62 6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 118 "Net-(M1-Pad19)"))
    (pad 20 thru_hole circle (at 7.62 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 119 "Net-(M1-Pad20)"))
    (pad 21 thru_hole circle (at 7.62 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 /3.3V))
    (pad 22 thru_hole circle (at 7.62 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 120 "Net-(M1-Pad22)"))
    (pad 23 thru_hole circle (at 7.62 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 121 "Net-(M1-Pad23)"))
    (pad 24 thru_hole circle (at 7.62 -6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 122 "Net-(M1-Pad24)"))
    (pad 25 thru_hole circle (at 7.62 -8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 123 "Net-(M1-Pad25)"))
    (pad 26 thru_hole circle (at 7.62 -11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 27 thru_hole circle (at 6.35 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 99 /SCL))
    (pad 28 thru_hole circle (at 3.81 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 101 /SDA))
    (pad 29 thru_hole circle (at 1.27 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 /3.3V))
    (pad 30 thru_hole circle (at -1.27 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 31 thru_hole circle (at -3.81 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 102 /~RESET))
    (pad 32 thru_hole circle (at -6.35 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 100 /~INT))
  )
  (module "0 My SparkFun:SparkFun_SX1509_Alt" (layer F.Cu) (tedit 5AA80472)
    (at 116.205 87.63 90)
    (fp_text reference M2 (at 0 16.51 90) (layer F.SilkS))
    (fp_text value SparkFun_SX1509_Alt (at 0 0 180) (layer F.SilkS))
    (fp_text user ~INT (at -6.35 -13.97 180) (layer F.SilkS))
    (fp_text user ~RST (at -3.81 -13.97 180) (layer F.SilkS))
    (fp_text user SCL (at 6.35 -13.97 180) (layer F.SilkS))
    (fp_text user SDA (at 3.81 -13.97 180) (layer F.SilkS))
    (fp_text user 3.3V (at 1.27 -13.716 180) (layer F.SilkS))
    (fp_text user GND (at -1.27 -13.97 180) (layer F.SilkS))
    (fp_text user GND (at 4.826 -11.43 90) (layer F.SilkS))
    (fp_text user 15 (at 5.08 -8.89 90) (layer F.SilkS))
    (fp_text user 14 (at 5.08 -6.35 90) (layer F.SilkS))
    (fp_text user 13 (at 5.08 -3.81 90) (layer F.SilkS))
    (fp_text user 12 (at 5.08 -1.27 90) (layer F.SilkS))
    (fp_text user VCC2 (at 3.81 1.27 90) (layer F.SilkS))
    (fp_text user 11 (at 5.08 3.81 90) (layer F.SilkS))
    (fp_text user 10 (at 5.08 6.35 90) (layer F.SilkS))
    (fp_text user 9 (at 5.08 8.89 90) (layer F.SilkS))
    (fp_text user 8 (at 5.08 11.43 90) (layer F.SilkS))
    (fp_text user GND (at -4.064 -11.43 90) (layer F.SilkS))
    (fp_text user 7 (at -5.08 11.43 90) (layer F.SilkS))
    (fp_text user 6 (at -5.08 8.89 90) (layer F.SilkS))
    (fp_text user 5 (at -5.08 6.35 90) (layer F.SilkS))
    (fp_text user 4 (at -5.08 3.81 90) (layer F.SilkS))
    (fp_text user VCC1 (at -3.81 1.27 90) (layer F.SilkS))
    (fp_text user 3 (at -5.08 -1.27 90) (layer F.SilkS))
    (fp_text user 2 (at -5.08 -3.81 90) (layer F.SilkS))
    (fp_text user 1 (at -5.08 -6.35 90) (layer F.SilkS))
    (fp_text user 0 (at -5.08 -8.89 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.62 -11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 2 thru_hole circle (at -7.62 -8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 124 "Net-(M2-Pad2)"))
    (pad 3 thru_hole circle (at -7.62 -6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 125 "Net-(M2-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 126 "Net-(M2-Pad4)"))
    (pad 5 thru_hole circle (at -7.62 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 127 "Net-(M2-Pad5)"))
    (pad 6 thru_hole circle (at -7.62 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 /3.3V))
    (pad 7 thru_hole circle (at -7.62 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 128 "Net-(M2-Pad7)"))
    (pad 8 thru_hole circle (at -7.62 6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 129 "Net-(M2-Pad8)"))
    (pad 9 thru_hole circle (at -7.62 8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 130 "Net-(M2-Pad9)"))
    (pad 10 thru_hole circle (at -7.62 11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 131 "Net-(M2-Pad10)"))
    (pad 17 thru_hole circle (at 7.62 11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 132 "Net-(M2-Pad17)"))
    (pad 18 thru_hole circle (at 7.62 8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 133 "Net-(M2-Pad18)"))
    (pad 19 thru_hole circle (at 7.62 6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 134 "Net-(M2-Pad19)"))
    (pad 20 thru_hole circle (at 7.62 3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 135 "Net-(M2-Pad20)"))
    (pad 21 thru_hole circle (at 7.62 1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 /3.3V))
    (pad 22 thru_hole circle (at 7.62 -1.27 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 136 "Net-(M2-Pad22)"))
    (pad 23 thru_hole circle (at 7.62 -3.81 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 137 "Net-(M2-Pad23)"))
    (pad 24 thru_hole circle (at 7.62 -6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 138 "Net-(M2-Pad24)"))
    (pad 25 thru_hole circle (at 7.62 -8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 139 "Net-(M2-Pad25)"))
    (pad 26 thru_hole circle (at 7.62 -11.43 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 27 thru_hole circle (at 6.35 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 99 /SCL))
    (pad 28 thru_hole circle (at 3.81 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 101 /SDA))
    (pad 29 thru_hole circle (at 1.27 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 107 /3.3V))
    (pad 30 thru_hole circle (at -1.27 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 97 /GND))
    (pad 31 thru_hole circle (at -3.81 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 102 /~RESET))
    (pad 32 thru_hole circle (at -6.35 -16.51 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 100 /~INT))
  )
  (module Symbols:KiCad-Logo2_8mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 95.885 46.99 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_8mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_line (start 34.25 100.75) (end 157.5 100.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.5 28.75) (end 34.25 28.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 124.75 (width 0.3) (layer Cmts.User)
    (gr_text "124.750 mm" (at 95.875 20.4) (layer Cmts.User))
    (feature1 (pts (xy 158.25 27) (xy 158.25 19.05)))
    (feature2 (pts (xy 33.5 27) (xy 33.5 19.05)))
    (crossbar (pts (xy 33.5 21.75) (xy 158.25 21.75)))
    (arrow1a (pts (xy 158.25 21.75) (xy 157.123496 22.336421)))
    (arrow1b (pts (xy 158.25 21.75) (xy 157.123496 21.163579)))
    (arrow2a (pts (xy 33.5 21.75) (xy 34.626504 22.336421)))
    (arrow2b (pts (xy 33.5 21.75) (xy 34.626504 21.163579)))
  )
  (gr_arc (start 157.5 100) (end 158.25 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 158.25 29.5) (end 158.25 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 33.5 29.5) (end 33.5 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157.5 29.5) (end 157.5 28.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 34.25 29.5) (end 33.5 29.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 34.25 100) (end 34.25 100.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 72 (width 0.3) (layer Cmts.User)
    (gr_text "72.000 mm" (at 26.4 64.75 90) (layer Cmts.User))
    (feature1 (pts (xy 31.75 28.75) (xy 25.05 28.75)))
    (feature2 (pts (xy 31.75 100.75) (xy 25.05 100.75)))
    (crossbar (pts (xy 27.75 100.75) (xy 27.75 28.75)))
    (arrow1a (pts (xy 27.75 28.75) (xy 28.336421 29.876504)))
    (arrow1b (pts (xy 27.75 28.75) (xy 27.163579 29.876504)))
    (arrow2a (pts (xy 27.75 100.75) (xy 28.336421 99.623496)))
    (arrow2b (pts (xy 27.75 100.75) (xy 27.163579 99.623496)))
  )
  (gr_text jeditekunum (at 153.035 97.79) (layer F.SilkS))
  (gr_text by (at 153.035 95.885) (layer F.SilkS))
  (gr_text v1 (at 156.21 64.77 90) (layer F.SilkS))
  (gr_text "SX1509\nIsolated 32" (at 151.765 64.77 90) (layer F.SilkS))
  (gr_text 24V (at 154.305 46.99) (layer F.SilkS))
  (gr_text + (at 156.21 44.45) (layer F.SilkS))
  (gr_text - (at 153.035 44.45) (layer F.SilkS))
  (gr_text 24V (at 38.735 46.99) (layer F.SilkS))
  (gr_text + (at 40.64 44.45) (layer F.SilkS))
  (gr_text - (at 38.1 44.45) (layer F.SilkS))
  (gr_text "I2C Bus" (at 136.525 92.71 90) (layer F.SilkS))
  (gr_text "I2C Bus" (at 55.245 92.71 90) (layer F.SilkS))
)
