(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~65~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 530)
    (tracks 477)
    (zones 0)
    (modules 64)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (1 In1.Cu mixed)
    (2 In2.Cu power)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.13)
    (user_trace_width 0.13)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.13)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.13)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.4)
    (via_drill 0.28)
    (via_min_size 0.36)
    (via_min_drill 0.26)
    (user_via 0.36 0.26)
    (user_via 0.5 0.4)
    (uvia_size 0.36)
    (uvia_drill 0.26)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 2.1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_fffffff9)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "SVG/"))
  )
  (net 0 "")
  (net 1 2V8)
  (net 2 GND)
  (net 3 "Net-(C5-Pad1)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 /VDD_IO)
  (net 6 /VAA)
  (net 7 "Net-(C15-Pad1)")
  (net 8 /135_VDD)
  (net 9 /VDD_PLL)
  (net 10 /TRIGGER)
  (net 11 /SDATA)
  (net 12 /SCLK)
  (net 13 /OE)
  (net 14 /VSYNC)
  (net 15 /FLASH)
  (net 16 /HSYNC)
  (net 17 /DCMI_D1)
  (net 18 /DCMI_D4)
  (net 19 /DCMI_D0)
  (net 20 /DCMI_D5)
  (net 21 /DCMI_D6)
  (net 22 /DCMI_D2)
  (net 23 /DCMI_D3)
  (net 24 /DCMI_D7)
  (net 25 /EXTCLK)
  (net 26 /PIXCLK)
  (net 27 /IM_RST)
  (net 28 "Net-(R2-Pad2)")
  (net 29 "Net-(R3-Pad2)")
  (net 30 "Net-(R4-Pad2)")
  (net 31 "Net-(R5-Pad2)")
  (net 32 "Net-(R6-Pad2)")
  (net 33 "Net-(R7-Pad2)")
  (net 34 "Net-(R8-Pad2)")
  (net 35 "Net-(R9-Pad2)")
  (net 36 "Net-(R10-Pad2)")
  (net 37 "Net-(R11-Pad2)")
  (net 38 /STANDBY)
  (net 39 /CH_GND)
  (net 40 "Net-(L1-Pad2)")
  (net 41 "Net-(J9-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.13)
    (trace_width 0.13)
    (via_dia 0.4)
    (via_drill 0.28)
    (uvia_dia 0.36)
    (uvia_drill 0.26)
    (add_net /135_VDD)
    (add_net /CH_GND)
    (add_net /DCMI_D0)
    (add_net /DCMI_D1)
    (add_net /DCMI_D2)
    (add_net /DCMI_D3)
    (add_net /DCMI_D4)
    (add_net /DCMI_D5)
    (add_net /DCMI_D6)
    (add_net /DCMI_D7)
    (add_net /EXTCLK)
    (add_net /FLASH)
    (add_net /HSYNC)
    (add_net /IM_RST)
    (add_net /OE)
    (add_net /PIXCLK)
    (add_net /SCLK)
    (add_net /SDATA)
    (add_net /STANDBY)
    (add_net /TRIGGER)
    (add_net /VAA)
    (add_net /VDD_IO)
    (add_net /VDD_PLL)
    (add_net /VSYNC)
    (add_net 2V8)
    (add_net GND)
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(J9-Pad17)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
  )
  (module CustomParts:SAMTEC_FT5-15-01-K-RA-TR (layer F.Cu) (tedit 5CA6D872)
    (at 59.2 47.15 180)
    (attr smd)
    (fp_text reference J9 (at -4.96 -4.035 180) (layer F.SilkS) hide)
    (fp_text value FT5-30 (at 8.5 -3.6 180) (layer F.SilkS) hide)
    (pad P4 thru_hole circle (at 6.5 -1.02) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad P2 thru_hole circle (at -6.5 1.23 180) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad P3 thru_hole circle (at 6.5 1.23) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad P1 thru_hole circle (at -6.5 -1.02 180) (size 1.1 1.1) (drill 0.71) (layers *.Cu *.Mask))
    (pad Hole np_thru_hole circle (at 7.75 0.1 180) (size 1.45 1.45) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
    (pad Hole np_thru_hole circle (at -7.75 0.1 180) (size 1.45 1.45) (drill 1.45) (layers *.Cu *.Mask F.SilkS))
    (pad 30 smd rect (at 3.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 29 smd rect (at 3.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 28 smd rect (at 3 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /EXTCLK))
    (pad 27 smd rect (at 3 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 26 /PIXCLK))
    (pad 26 smd rect (at 2.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 2.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 16 /HSYNC))
    (pad 24 smd rect (at 2 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /DCMI_D0))
    (pad 23 smd rect (at 2 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 14 /VSYNC))
    (pad 22 smd rect (at 1.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /DCMI_D1))
    (pad 21 smd rect (at 1.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 1 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 24 /DCMI_D7))
    (pad 19 smd rect (at 1 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 15 /FLASH))
    (pad 18 smd rect (at 0.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /DCMI_D6))
    (pad 17 smd rect (at 0.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J9-Pad17)"))
    (pad 16 smd rect (at 0 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /DCMI_D4))
    (pad 15 smd rect (at 0 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 27 /IM_RST))
    (pad 14 smd rect (at -0.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 22 /DCMI_D2))
    (pad 13 smd rect (at -0.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -1 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 23 /DCMI_D3))
    (pad 11 smd rect (at -1 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at -1.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /DCMI_D5))
    (pad 9 smd rect (at -1.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 10 /TRIGGER))
    (pad 6 smd rect (at -2.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /SDATA))
    (pad 5 smd rect (at -2.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 13 /OE))
    (pad 4 smd rect (at -3 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCLK))
    (pad 3 smd rect (at -3 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.5 0.69 180) (size 0.3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 1 smd rect (at -3.5 -0.7355 180) (size 0.3 1.089) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/FT5-15-01-L-RA-K-TR.stp
      (offset (xyz 0 6.21 0.38))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 64.5 38.25)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 42.75 46)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29DFB)
    (at 39 27.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J11 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 39 /CH_GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29DF8)
    (at 25.5 39.117)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J12 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 39 /CH_GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29E01)
    (at 74.5 39.117)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J13 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 39 /CH_GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5CA29DFE)
    (at 61 27.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference J14 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 39 /CH_GND))
  )
  (module CustomParts:LensM12_Alum (layer B.Cu) (tedit 5CA3E29F)
    (at 50 37)
    (fp_text reference U3 (at -7.5 8.4) (layer B.SilkS) hide)
    (fp_text value LensM12 (at -6.7 10) (layer B.Fab) hide)
    (pad "" thru_hole circle (at -11 0) (size 3.8 3.8) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 11 0) (size 3.8 3.8) (drill 2.1) (layers *.Cu *.Mask)
      (clearance 0.1))
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousing.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousingScrew.step
      (offset (xyz 11 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
    (model /home/forrest/Documents/KiCad_Folder/KiCad/3D_Models/CameraHousingScrew.step
      (offset (xyz -11 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 47.6 47.2)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 62.5 39.55)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 65.25 33)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 63.3 33.5)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 40.2 42.8)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 35.95 32.15)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 38.25 47.75)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 35.65 36.35)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module CustomParts:IBGA63_9x9 (layer B.Cu) (tedit 5ADE0811)
    (at 50 37 180)
    (fp_text reference U5 (at -1.9 5.5 180) (layer B.SilkS) hide)
    (fp_text value AR0135 (at 4.8 2.5 180) (layer B.Fab) hide)
    (pad 64 smd circle (at 3.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 /IM_RST))
    (pad 63 smd circle (at 2.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 62 smd circle (at 1.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 2 smd circle (at -2.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd circle (at -1.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd circle (at -0.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd circle (at 0.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd circle (at 1.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 7 smd circle (at 2.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 8 smd circle (at 3.5 3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 38 /STANDBY))
    (pad 9 smd circle (at -3.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 /VDD_PLL))
    (pad 10 smd circle (at -2.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd circle (at -1.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd circle (at -0.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd circle (at 0.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd circle (at 1.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 15 smd circle (at 2.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 16 smd circle (at 3.5 2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 17 smd circle (at -3.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 /EXTCLK))
    (pad 18 smd circle (at -2.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd circle (at -1.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd circle (at -0.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd circle (at 0.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd circle (at 1.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 23 smd circle (at 2.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 24 smd circle (at 3.5 1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 25 smd circle (at -3.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(R11-Pad2)"))
    (pad 26 smd circle (at -2.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 /SCLK))
    (pad 27 smd circle (at -1.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /SDATA))
    (pad 28 smd circle (at -0.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 29 smd circle (at 0.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 30 smd circle (at 1.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /135_VDD))
    (pad 31 smd circle (at 2.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 32 smd circle (at 3.5 0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /VAA))
    (pad 33 smd circle (at -3.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 16 /HSYNC))
    (pad 34 smd circle (at -2.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 14 /VSYNC))
    (pad 35 smd circle (at -1.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 /PIXCLK))
    (pad 36 smd circle (at -0.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 15 /FLASH))
    (pad 37 smd circle (at 0.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 38 smd circle (at 1.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 39 smd circle (at 2.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 40 smd circle (at 3.5 -0.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 41 smd circle (at -3.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 18 /DCMI_D4))
    (pad 42 smd circle (at -2.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 /DCMI_D5))
    (pad 43 smd circle (at -1.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /DCMI_D6))
    (pad 44 smd circle (at -0.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 /DCMI_D7))
    (pad 45 smd circle (at 0.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 46 smd circle (at 1.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 47 smd circle (at 2.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 48 smd circle (at 3.5 -1.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 49 smd circle (at -3.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /DCMI_D0))
    (pad 50 smd circle (at -2.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 17 /DCMI_D1))
    (pad 51 smd circle (at -1.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /DCMI_D2))
    (pad 52 smd circle (at -0.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /DCMI_D3))
    (pad 53 smd circle (at 0.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 54 smd circle (at 1.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /VDD_IO))
    (pad 55 smd circle (at 2.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /TRIGGER))
    (pad 56 smd circle (at 3.5 -2.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 /OE))
    (pad 57 smd circle (at -3.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 58 smd circle (at -2.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 59 smd circle (at -1.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 60 smd circle (at -0.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 61 smd circle (at 0.5 -3.5 180) (size 0.55 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C9032B8)
    (at 51.75 31.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032C9)
    (at 50.25 31.5 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902F12)
    (at 44.525 35.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032BD)
    (at 53.925 31.475 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 10nF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032CD)
    (at 49.25 31.5 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C90333D)
    (at 48.5 42.45 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /VDD_IO))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902EE0)
    (at 44.525 36.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902EE3)
    (at 44.525 34.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C903340)
    (at 47.5 42.45 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /VDD_IO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902EBB)
    (at 33.2 39.6)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 22uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(C15-Pad1)"))
    (pad 2 smd roundrect (at 0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032B3)
    (at 48.25 31.5 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C29 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /135_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902ECB)
    (at 40.15 40.7 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C30 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902EC9)
    (at 38.15 41.15 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C32 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 /VAA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C9032AB)
    (at 47.25 31.5 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C33 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /135_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902EBE)
    (at 33.25 33.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C34 (at 0 -1.65 180) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /135_VDD))
    (pad 2 smd roundrect (at 0.85 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C90334A)
    (at 58 34 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C35 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /VDD_PLL))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C903350)
    (at 60.25 33.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C36 (at 0 -1.65) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 /VDD_PLL))
    (pad 2 smd roundrect (at 0.85 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5C902ED5)
    (at 40.25 45.45 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C38 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /VDD_IO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C902ED2)
    (at 38.25 45.45 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C39 (at 0 -1.65 270) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.85 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 5 /VDD_IO))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902EC1)
    (at 35.65 41.65 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032D2)
    (at 45 39.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032D6)
    (at 45 40.6)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903304)
    (at 54 38.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903323)
    (at 54 36.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032E5)
    (at 54 40.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032DC)
    (at 49.5 42.45 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032DF)
    (at 50.5 42.45 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R8-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C90331F)
    (at 54 37.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(R9-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032E9)
    (at 54 39.5 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C90333B)
    (at 56.5 36.95 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C90334D)
    (at 53.65 27.75 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /CH_GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902ECE)
    (at 36.25 44.45)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 4.7 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(L1-Pad2)"))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /VDD_IO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902EB8)
    (at 32.75 41.15 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 -1.17 180) (layer F.SilkS) hide)
    (fp_text value 10 (at 0 1.17 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C15-Pad1)"))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C902EC4)
    (at 36.15 40.15)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0 -1.17) (layer F.SilkS) hide)
    (fp_text value 4.7 (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VAA))
    (pad 1 smd roundrect (at -0.48 0) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903344)
    (at 64 41.1 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 1.5k (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /SDATA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C903347)
    (at 64 43.1 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.17 90) (layer F.SilkS) hide)
    (fp_text value 1.5k (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /SCLK))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 2V8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5C9032B1)
    (at 45.25 31.5 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /STANDBY))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_LGA:LGA-24L_3x3.5mm_P0.43mm (layer F.Cu) (tedit 5C9032C0)
    (at 50 37)
    (descr "LGA 24L 3x3.5mm Pitch 0.43mm")
    (tags "LGA 24L 3x3.5mm Pitch 0.43mm")
    (attr smd)
    (fp_text reference U1 (at 0 -2.7) (layer F.SilkS) hide)
    (fp_text value LSM9DS1 (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 -2.7) (layer F.Fab))
    (pad 1 smd rect (at -1.505 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 2 smd rect (at -1.475 -0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 12 /SCLK))
    (pad 17 smd rect (at 1.475 -0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.475 -0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 1.475 -0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -1.475 0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 11 /SDATA))
    (pad 15 smd rect (at 1.475 0.215) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -1.475 0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R2-Pad2)"))
    (pad 14 smd rect (at 1.475 0.645) (size 0.35 0.23) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at -1.075 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 23 smd rect (at -0.645 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 22 smd rect (at -0.215 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 2V8))
    (pad 21 smd rect (at 0.215 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 20 smd rect (at 0.645 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 1.075 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 1.505 -1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.505 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R3-Pad2)"))
    (pad 7 smd rect (at -1.075 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R7-Pad2)"))
    (pad 8 smd rect (at -0.645 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R8-Pad2)"))
    (pad 9 smd rect (at -0.215 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R6-Pad2)"))
    (pad 10 smd rect (at 0.215 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R10-Pad2)"))
    (pad 11 smd rect (at 0.645 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R4-Pad2)"))
    (pad 12 smd rect (at 1.075 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R9-Pad2)"))
    (pad 13 smd rect (at 1.505 1.225) (size 0.23 0.35) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-24L_3x3.5mm_P0.43mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 33.05 36.6 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at -3 0 270) (layer F.SilkS) hide)
    (fp_text value MCP1700-1802 (at 3 -3 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /135_VDD))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C95634C)
    (at 66.6 35.28)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 2V8))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /SDATA))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SCLK))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric (layer F.Cu) (tedit 5C9E48D4)
    (at 35.675 38.525 270)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0 -1.17 270) (layer F.SilkS) hide)
    (fp_text value Ferrite_Bead (at 0 1.17 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /VDD_PLL))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.6 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48E4)
    (at 44.4 27.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -1.43 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /CH_GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48EC)
    (at 70 34.8 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.43 180) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /CH_GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48E1)
    (at 30.05 41.6)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /CH_GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5C9E48E8)
    (at 55.35 27.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 -1.43 270) (layer F.SilkS) hide)
    (fp_text value .1uF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /CH_GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomParts:GND_Via (layer F.Cu) (tedit 5C9E4E4A)
    (at 30.7 39.35)
    (fp_text reference REF** (at 1.6 -0.2) (layer F.SilkS) hide)
    (fp_text value GND_Via (at 1.5 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.635 0.635) (drill 0.508) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module TestPoint:TestPoint_Pad_1.0x1.0mm (layer B.Cu) (tedit 5CA28B09)
    (at 59.05 47.8 180)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 1.448 180) (layer B.SilkS) hide)
    (fp_text value Test_Point (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.45 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1 1) (layers B.Cu B.Mask)
      (net 41 "Net-(J9-Pad17)"))
  )
  (gr_line (start 74 24.5) (end 26 24.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 29.5) (end 74 24.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 29.75) (end 79 29.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79 42.5) (end 79 29.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69 42.5) (end 79 42.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69 49.5) (end 69 42.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31 49.5) (end 69 49.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 31 42.5) (end 31 49.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 21 42.5) (end 31 42.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 21 29.5) (end 21 42.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 26 24.5) (end 21 29.5) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 21 26.5) (xy 19 26.5) (xy 19 24.5) (xy 79 24.5) (xy 79 49.5)
        (xy 21 49.5)
      )
    )
  )
  (zone (net 1) (net_name 2V8) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 29.5) (xy 19 29.5) (xy 19 27.5) (xy 21 27.5) (xy 21 24.5)
        (xy 79 24.5) (xy 79 49.5) (xy 21 49.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 32.5) (xy 19 32.5) (xy 19 30.5) (xy 21 30.5) (xy 21 24.5)
        (xy 79 24.5) (xy 79 49.5) (xy 21 49.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 35.5) (xy 19 35.5) (xy 19 33.5) (xy 21 33.5) (xy 21 24.5)
        (xy 79 24.5) (xy 79 49.5) (xy 21 49.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 36.5) (xy 21 36.5) (xy 21 24.5) (xy 79 24.5) (xy 79 42.5)
        (xy 70 42.5) (xy 70 33.75) (xy 67.75 31.5) (xy 59.75 31.5) (xy 59.75 30.75)
        (xy 56.75 27.75) (xy 43.5 27.75) (xy 40.25 30.75) (xy 40.25 31.5) (xy 33.25 31.5)
        (xy 33 31.5) (xy 32.5 31.5) (xy 30 33.75) (xy 30 42.5) (xy 21 42.5)
        (xy 21 38.5) (xy 19 38.5)
      )
    )
  )
  (zone (net 39) (net_name /CH_GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 38.65) (xy 21 38.65) (xy 21 24.5) (xy 78.75 24.5) (xy 78.75 42.5)
        (xy 70 42.5) (xy 70 33.75) (xy 67.75 31.5) (xy 59.75 31.5) (xy 59.75 30.75)
        (xy 56.75 27.75) (xy 43.5 27.75) (xy 40.25 30.75) (xy 40.25 31.5) (xy 32.5 31.5)
        (xy 30 33.75) (xy 30 42.5) (xy 21 42.5) (xy 21 39.35) (xy 19 39.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.35)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 51.95 36.9) (xy 51.3 36.9) (xy 51.3 36.55) (xy 51.3 36.25) (xy 50.5 36.25)
        (xy 50.5 35.45) (xy 51.95 35.5)
      )
    )
  )
  (zone (net 39) (net_name /CH_GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 39.5) (xy 21 39.5) (xy 21 24.5) (xy 78.75 24.5) (xy 78.75 42.5)
        (xy 70 42.5) (xy 70 33.75) (xy 67.75 31.5) (xy 59.75 31.5) (xy 59.75 30.75)
        (xy 56.75 27.75) (xy 43.5 27.75) (xy 40.25 30.75) (xy 40.25 31.5) (xy 32.5 31.5)
        (xy 30 33.75) (xy 30 42.5) (xy 21 42.5) (xy 21 41.5) (xy 19 41.5)
      )
    )
  )
  (zone (net 39) (net_name /CH_GND) (layer In1.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 42) (xy 21 42) (xy 21 24.5) (xy 78.75 24.5) (xy 78.75 42.5)
        (xy 70 42.5) (xy 70 33.75) (xy 67.75 31.5) (xy 59.75 31.5) (xy 59.75 30.75)
        (xy 56.75 27.75) (xy 43.5 27.75) (xy 40.25 30.75) (xy 40.25 31.5) (xy 32.5 31.5)
        (xy 30 33.75) (xy 30 42.5) (xy 21 42.5) (xy 21 43.5) (xy 19 43.5)
      )
    )
  )
  (zone (net 39) (net_name /CH_GND) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 44) (xy 20.85 44) (xy 21 24.5) (xy 78.75 24.5) (xy 78.75 42.5)
        (xy 70 42.5) (xy 70 33.75) (xy 67.75 31.5) (xy 59.75 31.5) (xy 59.75 30.75)
        (xy 56.75 27.75) (xy 43.5 27.75) (xy 40.25 30.75) (xy 40.25 31.5) (xy 32.5 31.5)
        (xy 30 33.75) (xy 30 42.5) (xy 25.45 42.45) (xy 21 42.5) (xy 21 44.5)
        (xy 21 45.5) (xy 19 45.5)
      )
    )
  )
)
