(kicad_pcb (version 3) (host pcbnew "(2013-07-07 BZR 4022)-stable")
  (general
    (links 21)
    (no_connects 0)
    (area 71.762258 69.659499 115.764733 124.269501)
    (thickness 1.6002)
    (drawings 81)
    (tracks 111)
    (zones 0)
    (modules 15)
    (nets 9)
  )
  (page A4)
  (layers
    (15 Front signal)
    (0 Back signal)
    (16 B.Adhes user)
    (17 F.Adhes user)
    (18 B.Paste user)
    (19 F.Paste user)
    (20 B.SilkS user)
    (21 F.SilkS user)
    (22 B.Mask user)
    (23 F.Mask user)
    (24 Dwgs.User user)
    (25 Cmts.User user)
    (26 Eco1.User user)
    (27 Eco2.User user)
    (28 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.381)
    (edge_width 0.381)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 16.15948 16.15948)
    (pad_drill 0)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFBF)
    (pcbplotparams
      (layerselection 284196865)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotothertext true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory badgeMirrored/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 N-000003)
  (net 3 N-000004)
  (net 4 N-000005)
  (net 5 N-000006)
  (net 6 N-000007)
  (net 7 N-000008)
  (net 8 N-000009)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.762)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "")
    (add_net GND)
    (add_net N-000003)
    (add_net N-000004)
    (add_net N-000005)
    (add_net N-000006)
    (add_net N-000007)
    (add_net N-000008)
    (add_net N-000009)
  )
  (module Batt_conn_20mm_largepad (layer Front) (tedit 4FBFB435)
    (at 92.71 107.823)
    (fp_text reference BT1 (at 0.254 -11.938) (layer F.SilkS) hide)
    (fp_text value BATTERY (at 0 -8.636) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -10.16 0) (size 2.54 5.08) (drill oval 1.00076 2.99974)
      (layers *.Cu *.Mask)
      (net 6 N-000007)
    )
    (pad 1 thru_hole oval (at 10.16 0) (size 2.54 5.08) (drill oval 1.00076 2.99974)
      (layers *.Cu *.Mask)
      (net 6 N-000007)
    )
    (pad 2 thru_hole circle (at 0 0) (size 16.15948 16.15948)
      (layers Back B.Mask)
      (net 1 GND)
      (clearance 0.254)
    )
  )
  (module robot (layer Front) (tedit 4FBF7B18)
    (at 89.535 83.1088)
    (fp_text reference RB1 (at 20.955 -3.81) (layer F.SilkS) hide)
    (fp_text value ROBOT (at 21.59 -6.985) (layer F.SilkS) hide)
  )
  (module LED-5MM_larg_pad (layer Front) (tedit 4FBF77FC)
    (at 92.71 92.71)
    (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 5mm 5MM 100mil 2,54mm")
    (attr virtual)
    (fp_text reference D1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value LED_TH (at 0 3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.27 0) (size 2.032 2.032) (drill 0.8128)
      (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 N-000007)
    )
    (pad 2 thru_hole circle (at 1.27 0) (size 2.032 2.032) (drill 0.8128)
      (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 GND)
    )
    (model discret/leds/led5_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT323 (layer Front) (tedit 4FBA27E5)
    (at 83.566 97.409 270)
    (tags "SMD SOT")
    (attr smd)
    (fp_text reference Q1 (at 0.127 -2.032 270) (layer F.SilkS))
    (fp_text value NPN_S0323 (at 0 0 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.65024 -0.94996 270) (size 0.59944 1.00076)
      (layers Front F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 1 smd rect (at 0.65024 -0.94996 270) (size 0.59944 1.00076)
      (layers Front F.Paste F.Mask)
      (net 3 N-000004)
    )
    (pad 3 smd rect (at 0 0.94996 270) (size 0.59944 1.00076)
      (layers Front F.Paste F.Mask)
      (net 2 N-000003)
    )
    (model smd/SOT323.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT323 (layer Front) (tedit 450AC34A)
    (at 101.092 97.409)
    (tags "SMD SOT")
    (attr smd)
    (fp_text reference Q2 (at 0.127 -2.032) (layer F.SilkS))
    (fp_text value NPN_S0323 (at 0 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.65024 -0.94996) (size 0.59944 1.00076)
      (layers Front F.Paste F.Mask)
      (net 1 GND)
    )
    (pad 1 smd rect (at 0.65024 -0.94996) (size 0.59944 1.00076)
      (layers Front F.Paste F.Mask)
      (net 8 N-000009)
    )
    (pad 3 smd rect (at 0 0.94996) (size 0.59944 1.00076)
      (layers Front F.Paste F.Mask)
      (net 4 N-000005)
    )
    (model smd/SOT323.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer Front) (tedit 42806E24)
    (at 84.455 93.345)
    (attr smd)
    (fp_text reference C1 (at 0 0) (layer F.SilkS))
    (fp_text value 47u (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 2 N-000003)
    )
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 8 N-000009)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer Front) (tedit 42806E24)
    (at 100.965 93.345 180)
    (attr smd)
    (fp_text reference C2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 47u (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 4 N-000005)
    )
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 3 N-000004)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer Front) (tedit 42806E24)
    (at 82.55 88.9 270)
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 470 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 5 N-000006)
    )
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 2 N-000003)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer Front) (tedit 42806E24)
    (at 88.265 88.9 270)
    (attr smd)
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 6 N-000007)
    )
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 3 N-000004)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer Front) (tedit 42806E24)
    (at 97.79 88.9 270)
    (attr smd)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 6 N-000007)
    )
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 8 N-000009)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SM1206 (layer Front) (tedit 42806E24)
    (at 102.87 88.9 270)
    (attr smd)
    (fp_text reference R4 (at 0 0 270) (layer F.SilkS))
    (fp_text value 470 (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 7 N-000008)
    )
    (pad 2 smd rect (at 1.651 0 270) (size 1.524 2.032)
      (layers Front F.Paste F.Mask)
      (net 4 N-000005)
    )
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED-1206 (layer Front) (tedit 4FBA50FE)
    (at 92.8116 96.9772)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at 0.254 -1.524) (layer F.SilkS) hide)
    (fp_text value LED_SMD (at 0 1.524) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086)
      (layers Front F.Paste F.Mask)
      (net 6 N-000007)
    )
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086)
      (layers Front F.Paste F.Mask)
      (net 1 GND)
    )
  )
  (module 1pin_badge_no_edge (layer Front) (tedit 4DD2929B)
    (at 92.71 80.01)
    (fp_text reference P1 (at -0.254 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at -0.254 3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 1.50114)
      (layers *.Cu *.Mask)
      (clearance 0.508)
    )
  )
  (module LED-1206 (layer Front) (tedit 49BFA1FF)
    (at 88.265 76.2 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D3 (at 0.254 -1.524 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086)
      (layers Front F.Paste F.Mask)
      (net 6 N-000007)
    )
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086)
      (layers Front F.Paste F.Mask)
      (net 5 N-000006)
    )
  )
  (module LED-1206 (layer Front) (tedit 49BFA1FF)
    (at 97.155 76.2)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at 0.254 -1.524) (layer F.SilkS))
    (fp_text value LED (at 0 1.524) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086)
      (layers Front F.Paste F.Mask)
      (net 6 N-000007)
    )
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086)
      (layers Front F.Paste F.Mask)
      (net 7 N-000008)
    )
  )
  (gr_text "PCBs\nmanufactured by:\nwww.pcb-pool.com" (at 93.091 83.439) (layer B.SilkS))
  (gr_text + (at 94.615 74.93) (layer F.SilkS))
  (gr_text + (at 90.805 74.93) (layer F.SilkS))
  (gr_text "badge design:\nre-innovation.co.uk" (at 92.456 118.11) (layer B.SilkS))
  (gr_text www.nottinghack.org.uk (at 92.71 96.52) (layer B.SilkS))
  (gr_arc (start 93.726 73.533) (end 93.345 69.85) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 92.329 74.295) (end 87.884 73.279) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 80.264 90.297) (end 76.454 90.297) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 80.264 85.217) (end 80.264 86.487) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 84.709 85.217) (end 80.264 85.217) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 84.709 81.534) (end 84.709 85.217) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 75.565 90.297) (end 76.581 90.297) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 75.565 109.601) (end 75.565 90.297) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 76.962 110.998) (end 75.565 109.601) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 80.137 110.998) (end 76.962 110.998) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 80.137 111.506) (end 80.137 110.998) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 81.153 111.506) (end 80.137 111.506) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 81.153 117.983) (end 81.153 111.506) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 80.137 117.983) (end 81.153 117.983) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 80.137 124.079) (end 80.137 117.983) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 104.648 124.079) (end 80.137 124.079) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 104.648 117.983) (end 104.648 124.079) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 103.759 117.983) (end 104.648 117.983) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 103.759 111.633) (end 103.759 117.983) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 105.283 111.633) (end 103.759 111.633) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 105.283 111.125) (end 105.283 111.633) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 108.458 111.125) (end 105.283 111.125) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 109.728 109.855) (end 108.458 111.125) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 109.728 90.297) (end 109.728 109.855) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 108.966 90.297) (end 109.728 90.297) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 105.283 85.344) (end 105.283 86.487) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 100.711 85.344) (end 105.283 85.344) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 100.711 81.661) (end 100.711 85.344) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 103.378 81.661) (end 100.711 81.661) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 103.378 75.692) (end 103.378 81.661) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 100.711 75.692) (end 103.378 75.692) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 100.711 73.152) (end 100.711 75.692) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 97.409 73.152) (end 100.711 73.152) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 84.963 73.152) (end 88.011 73.152) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 105.156 90.424) (end 105.283 86.36) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_text Hackspace (at 106.934 98.298 90) (layer F.SilkS))
  (gr_text Nottingham (at 78.4098 98.298 90) (layer F.SilkS))
  (gr_line (start 84.8868 75.7174) (end 84.8868 73.2536) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 82.1436 75.7174) (end 84.8868 75.7174) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 82.1436 81.534) (end 82.1436 75.7174) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 84.709 81.534) (end 82.1436 81.534) (angle 90) (layer Edge.Cuts) (width 0.381))
)
