(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 0)
    (no_connects 21)
    (area 132.016499 88.836499 165.163501 121.983501)
    (thickness 1.6002)
    (drawings 21)
    (tracks 158)
    (zones 0)
    (modules 8)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad4)")
  (net 7 "Net-(J1-Pad5)")
  (net 8 "Net-(J1-Pad6)")
  (net 9 "Net-(J1-Pad7)")
  (net 10 "Net-(J1-Pad8)")
  (net 11 "Net-(J1-Pad9)")
  (net 12 "Net-(J1-Pad10)")
  (net 13 "Net-(J1-Pad11)")
  (net 14 "Net-(J1-Pad12)")
  (net 15 "Net-(J2-Pad1)")
  (net 16 "Net-(J3-Pad3)")
  (net 17 "Net-(J3-Pad4)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A07CB46)
    (at 148.209 107.696)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X12_NO_SILK (layer F.Cu) (tedit 5A07CB13)
    (at 162.56 119.38 180)
    (descr "PLATED THROUGH HOLE -12 PIN NO SILK")
    (tags "PLATED THROUGH HOLE -12 PIN NO SILK")
    (attr virtual)
    (fp_text reference J1 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value nixie (at 13.843 -1.651 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 15.24 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at 20.32 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at 22.86 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at 25.4 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at 27.94 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(J1-Pad12)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X02_NO_SILK (layer F.Cu) (tedit 5A07D131)
    (at 137.033 109.22 270)
    (descr "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J2 (at 0.254 -1.7018 270) (layer F.SilkS) hide)
    (fp_text value jumper (at 1.27 -1.397 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 14 "Net-(J1-Pad12)"))
  )
  (module SparkFun-Connectors:SparkFun-Connectors-1X04_NO_SILK (layer F.Cu) (tedit 5A07D547)
    (at 152.4 91.44 180)
    (descr "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J3 (at 0.254 -1.7018 180) (layer F.SilkS) hide)
    (fp_text value led (at 3.81 -1.905 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 16 "Net-(J3-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(J3-Pad4)"))
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5A07CA53)
    (at 148.5011 105.0036)
    (attr smd)
    (fp_text reference LED1 (at 3.175 -0.254 90) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J3-Pad4)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3-DI smd rect (at -1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad3)"))
    (pad 4-VD smd rect (at -1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module nixies-us:nixies-us-IN-2-DSUB (layer F.Cu) (tedit 200000)
    (at 148.59 105.41)
    (attr virtual)
    (fp_text reference N1 (at -10.795 0 270) (layer F.SilkS))
    (fp_text value IN-2 (at 10.795 0 90) (layer F.SilkS))
    (fp_text user Top (at 0 -7.62) (layer F.SilkS))
    (pad 0 thru_hole circle (at -4.7498 0) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 13 "Net-(J1-Pad11)"))
    (pad 1 thru_hole circle (at 0 4.7498) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 2 thru_hole circle (at 2.3749 4.11226) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 3 thru_hole circle (at 4.11226 2.3749) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(J1-Pad4)"))
    (pad 4 thru_hole circle (at 4.7498 0) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(J1-Pad5)"))
    (pad 5 thru_hole circle (at 4.11226 -2.3749) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at 2.3749 -4.11226) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(J1-Pad7)"))
    (pad 7 thru_hole circle (at 0 -4.7498) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(J1-Pad8)"))
    (pad 8 thru_hole circle (at -2.3749 -4.11226) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 9 thru_hole circle (at -4.11226 -2.3749) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(J1-Pad10)"))
    (pad A thru_hole circle (at -4.11226 2.3749) (size 2.18186 2.18186) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(J2-Pad1)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 5A07D137)
    (at 134.62 110.49 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R1 (at -0.889 -0.889 270) (layer F.SilkS) hide)
    (fp_text value R (at -0.39878 4.20116 270) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad1)"))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad12)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad1)"))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad12)"))
  )
  (module logos:mermaid_l (layer F.Cu) (tedit 0)
    (at 135.382 93.726)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text Gnd (at 152.4 89.535) (layer F.SilkS))
  (gr_text Vcc (at 149.86 89.535) (layer F.SilkS))
  (gr_text Din (at 147.32 89.535) (layer F.SilkS))
  (gr_text Dout (at 144.78 89.535) (layer F.SilkS))
  (gr_text NC (at 162.56 117.475) (layer F.SilkS))
  (gr_text 1 (at 160.02 117.475) (layer F.SilkS))
  (gr_text 2 (at 157.48 117.475) (layer F.SilkS))
  (gr_text 3 (at 154.94 117.475) (layer F.SilkS))
  (gr_text 4 (at 152.4 117.475) (layer F.SilkS))
  (gr_text 5 (at 149.86 117.475) (layer F.SilkS))
  (gr_text 6 (at 147.32 117.475) (layer F.SilkS))
  (gr_text 7 (at 144.78 117.475) (layer F.SilkS))
  (gr_text 8 (at 142.24 117.475) (layer F.SilkS))
  (gr_text 9 (at 139.7 117.475) (layer F.SilkS))
  (gr_text 0 (at 137.16 117.475) (layer F.SilkS))
  (gr_text A (at 134.62 117.475) (layer F.SilkS))
  (gr_text nixies.us (at 138.176 93.726 90) (layer F.Mask))
  (gr_line (start 132.08 88.9) (end 132.08 121.92) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 88.9) (end 132.08 88.9) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 121.92) (end 165.1 88.9) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 132.08 121.92) (end 165.1 121.92) (layer Edge.Cuts) (width 0.127))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.715 98.425) (xy 132.715 89.535) (xy 139.065 89.535) (xy 139.065 98.425)
      )
    )
  )
)
