(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 34)
    (no_connects 6)
    (area 144.924999 88.924999 155.075001 111.075001)
    (thickness 1.6)
    (drawings 20)
    (tracks 126)
    (zones 0)
    (modules 16)
    (nets 15)
  )
  (page A4)
  (title_block
    (title "IR Beacon Board")
    (date 2017-04-28)
    (rev 2.0)
    (company "ECE 445")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 10)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory images))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(Q1-Pad1)")
  (net 5 /~RST)
  (net 6 "Net-(U2-Pad4)")
  (net 7 VCC)
  (net 8 /RAIL_L)
  (net 9 /RAIL_R)
  (net 10 +1V8)
  (net 11 /PB2)
  (net 12 /PB0)
  (net 13 /PB1)
  (net 14 "Net-(JP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /~RST)
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(U2-Pad4)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net /RAIL_L)
    (add_net /RAIL_R)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net VCC)
  )
  (net_class Tight ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5902B607)
    (at 147 103 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 +1V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5902B600)
    (at 146.8 106)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 47 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5902B60E)
    (at 150 104.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58CB11E2)
    (at 150 106 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value IR (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-143 (layer F.Cu) (tedit 5902B620)
    (at 146.8 95.2 270)
    (descr SOT-143)
    (tags SOT-143)
    (attr smd)
    (fp_text reference D2 (at 0.25 0 360) (layer F.SilkS) hide)
    (fp_text value BAS4002A (at -0.28 2.48 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.77 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0.95 180) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /RAIL_L))
    (pad 3 smd rect (at 1.1 0.95 180) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /RAIL_R))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-143.wrl
      (at (xyz 0 -0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5902B639)
    (at 153.2 105 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 0 360) (layer F.SilkS) hide)
    (fp_text value BSS138 (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5902B636)
    (at 146.8 100.6 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 0 360) (layer F.SilkS) hide)
    (fp_text value MIC5225-1.8YM5 (at 0 2.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 +1V8))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5902B618)
    (at 147 98.2 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5902B61D)
    (at 153 96 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 +1V8))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /~RST))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5902B615)
    (at 153.2 101.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /PB0))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5902B612)
    (at 153.2 102.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 5902B631)
    (at 153.2 98.6 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value ATTINY10-TS (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 /PB0))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 /PB1))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 /PB2))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /~RST))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 +1V8))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm_SMD (layer B.Cu) (tedit 5902B409)
    (at 150 100 90)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J3 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value TPI (at 0 -4.87 90) (layer B.Fab))
    (fp_text user %R (at 0 4.87 90) (layer B.Fab))
    (pad 1 smd rect (at -2.77 2.54 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 12 /PB0))
    (pad 2 smd rect (at 2.77 2.54 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 10 +1V8))
    (pad 3 smd rect (at -2.77 0 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 13 /PB1))
    (pad 4 smd rect (at 2.77 0 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 11 /PB2))
    (pad 5 smd rect (at -2.77 -2.54 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 5 /~RST))
    (pad 6 smd rect (at 2.77 -2.54 90) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bcan:Pad_Length10mm_Width3.5mm (layer F.Cu) (tedit 5902B5E5)
    (at 150 109.25 90)
    (fp_text reference J2 (at 0 -5.75 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 5.75 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.5 10) (layers F.Cu F.Mask)
      (net 9 /RAIL_R))
  )
  (module bcan:Pad_Length10mm_Width3.5mm (layer F.Cu) (tedit 5902B5E3)
    (at 150 90.75 90)
    (fp_text reference J1 (at 0 -5.75 90) (layer F.SilkS) hide)
    (fp_text value L (at 0 5.75 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.5 10) (layers F.Cu F.Mask)
      (net 8 /RAIL_L))
  )
  (module bcan:Solder_Jumper_NC_Small (layer F.Cu) (tedit 5908EB48)
    (at 146.8 104.45)
    (fp_text reference JP1 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value +1V8 (at 0 1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 1) (layers F.Cu F.Paste)
      (net 14 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 1) (layers F.Cu F.Paste)
      (net 10 +1V8))
    (pad "" smd rect (at 0 0) (size 2 1) (layers F.Paste F.Mask))
    (pad 1 smd trapezoid (at -0.45 -0.25) (size 0.6 0.5) (rect_delta 0 0.5 ) (layers F.Cu F.Paste)
      (net 14 "Net-(JP1-Pad1)"))
    (pad 2 smd trapezoid (at 0.45 0.25) (size 0.6 0.5) (rect_delta 0 0.5 ) (layers F.Cu F.Paste)
      (net 10 +1V8))
    (pad 1 smd trapezoid (at -0.45 0.25 180) (size 0.6 0.5) (rect_delta 0 0.5 ) (layers F.Cu F.Paste)
      (net 14 "Net-(JP1-Pad1)"))
    (pad 2 smd trapezoid (at 0.45 -0.25 180) (size 0.6 0.5) (rect_delta 0 0.5 ) (layers F.Cu F.Paste)
      (net 10 +1V8))
  )
  (gr_text v2.0 (at 145.8 94 270) (layer B.Mask))
  (gr_arc (start 146 90) (end 145 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146 110) (end 146 111) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154 110) (end 155 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154 90) (end 154 89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text bcan.io (at 150 100) (layer B.SilkS))
  (gr_text TPI (at 154.4 100 270) (layer B.SilkS))
  (gr_text ~RST (at 147.4 106 270) (layer B.SilkS))
  (gr_text 1V8 (at 152.54 94 270) (layer B.SilkS))
  (gr_text GND (at 147.46 94 270) (layer B.SilkS))
  (gr_text PB2 (at 150 94 270) (layer B.SilkS))
  (gr_text PB1 (at 150 106 270) (layer B.SilkS))
  (gr_text PB0 (at 152.54 106 270) (layer B.SilkS))
  (gr_text LEFT (at 150 91.2) (layer B.Mask))
  (gr_text RIGHT (at 150 109) (layer B.Mask))
  (gr_line (start 154 111) (end 146 111) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146 89) (end 154 89) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 110) (end 145 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155 90) (end 155 110) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 155 93.8) (xy 153.2 95) (xy 153.2 94.2) (xy 151.8 94.2) (xy 151.8 93.4)
        (xy 153.2 93.4) (xy 153.2 92.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 145 89) (xy 155 89) (xy 155 111) (xy 145 111)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 145 89) (xy 155 89) (xy 155 111) (xy 145 111)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 153.6 103.6) (xy 154.6 103) (xy 154.6 104.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 148.5 92.7) (xy 151.5 92.7) (xy 151.5 103.75) (xy 148.5 103.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 107.5) (xy 155 107.5) (xy 155 110.35) (xy 145 110.35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 89.65) (xy 155 89.65) (xy 155 92.5) (xy 145 92.5)
      )
    )
  )
)
