(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.57)
    (drawings 263)
    (tracks 940)
    (zones 0)
    (modules 32)
    (nets 109)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.7)
    (zone_45_only no)
    (trace_min 0.2032)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4064)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2032)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.699999 5.699999)
    (pad_drill 3.200001)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 PIN1_17)
  (net 2 PIN1_16)
  (net 3 PIN1_41)
  (net 4 GND)
  (net 5 PIN1_12)
  (net 6 PIN1_11)
  (net 7 PIN1_10)
  (net 8 PIN1_9)
  (net 9 PIN1_7)
  (net 10 PIN1_6)
  (net 11 PIN1_5)
  (net 12 PIN1_4)
  (net 13 PIN1_2)
  (net 14 PIN1_1)
  (net 15 PIN1_20)
  (net 16 PIN1_19)
  (net 17 PIN1_21)
  (net 18 PIN1_30)
  (net 19 PIN1_31)
  (net 20 PIN1_32)
  (net 21 PIN1_33)
  (net 22 PIN1_34)
  (net 23 PIN1_35)
  (net 24 3V3_EN_1)
  (net 25 PIN1_39)
  (net 26 PIN1_40)
  (net 27 PIN1_15)
  (net 28 PIN1_14)
  (net 29 PIN1_43)
  (net 30 FRAM_HOLD_1)
  (net 31 FRAM_WP_1)
  (net 32 FRAM_CS_1)
  (net 33 FRAM_MOSI_1)
  (net 34 FRAM_MISO_1)
  (net 35 FRAM_SCK_1)
  (net 36 FRAM_3V3_1)
  (net 37 PIN2_17)
  (net 38 PIN2_16)
  (net 39 PIN2_41)
  (net 40 PIN2_12)
  (net 41 PIN2_11)
  (net 42 PIN2_10)
  (net 43 PIN2_9)
  (net 44 PIN2_7)
  (net 45 PIN2_6)
  (net 46 PIN2_5)
  (net 47 PIN2_4)
  (net 48 PIN2_2)
  (net 49 PIN2_1)
  (net 50 PIN2_20)
  (net 51 PIN2_19)
  (net 52 PIN2_21)
  (net 53 PIN2_30)
  (net 54 PIN2_31)
  (net 55 PIN2_32)
  (net 56 PIN2_33)
  (net 57 PIN2_34)
  (net 58 PIN2_35)
  (net 59 3V3_EN_2)
  (net 60 PIN2_40)
  (net 61 PIN2_15)
  (net 62 PIN2_14)
  (net 63 PIN2_43)
  (net 64 FRAM_HOLD_2)
  (net 65 FRAM_WP_2)
  (net 66 FRAM_CS_2)
  (net 67 FRAM_MOSI_2)
  (net 68 FRAM_MISO_2)
  (net 69 FRAM_SCK_2)
  (net 70 FRAM_3V3_2)
  (net 71 PIN3_17)
  (net 72 PIN3_16)
  (net 73 PIN3_41)
  (net 74 PIN3_12)
  (net 75 PIN3_11)
  (net 76 PIN3_10)
  (net 77 PIN3_9)
  (net 78 PIN3_7)
  (net 79 PIN3_6)
  (net 80 PIN3_5)
  (net 81 PIN3_4)
  (net 82 PIN3_2)
  (net 83 PIN3_1)
  (net 84 PIN3_20)
  (net 85 PIN3_19)
  (net 86 PIN3_21)
  (net 87 PIN3_30)
  (net 88 PIN3_31)
  (net 89 PIN3_32)
  (net 90 PIN3_33)
  (net 91 PIN3_34)
  (net 92 PIN3_35)
  (net 93 3V3_EN_3)
  (net 94 PIN3_40)
  (net 95 PIN3_15)
  (net 96 PIN3_14)
  (net 97 PIN3_43)
  (net 98 FRAM_HOLD_3)
  (net 99 FRAM_WP_3)
  (net 100 FRAM_CS_3)
  (net 101 FRAM_MOSI_3)
  (net 102 FRAM_MISO_3)
  (net 103 FRAM_SCK_3)
  (net 104 FRAM_3V3_3)
  (net 105 +5V)
  (net 106 KEY)
  (net 107 PIN2_39)
  (net 108 PIN3_39)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.25)
    (add_net +5V)
    (add_net 3V3_EN_1)
    (add_net 3V3_EN_2)
    (add_net 3V3_EN_3)
    (add_net FRAM_3V3_1)
    (add_net FRAM_3V3_2)
    (add_net FRAM_3V3_3)
    (add_net FRAM_CS_1)
    (add_net FRAM_CS_2)
    (add_net FRAM_CS_3)
    (add_net FRAM_HOLD_1)
    (add_net FRAM_HOLD_2)
    (add_net FRAM_HOLD_3)
    (add_net FRAM_MISO_1)
    (add_net FRAM_MISO_2)
    (add_net FRAM_MISO_3)
    (add_net FRAM_MOSI_1)
    (add_net FRAM_MOSI_2)
    (add_net FRAM_MOSI_3)
    (add_net FRAM_SCK_1)
    (add_net FRAM_SCK_2)
    (add_net FRAM_SCK_3)
    (add_net FRAM_WP_1)
    (add_net FRAM_WP_2)
    (add_net FRAM_WP_3)
    (add_net GND)
    (add_net KEY)
    (add_net PIN1_1)
    (add_net PIN1_10)
    (add_net PIN1_11)
    (add_net PIN1_12)
    (add_net PIN1_14)
    (add_net PIN1_15)
    (add_net PIN1_16)
    (add_net PIN1_17)
    (add_net PIN1_19)
    (add_net PIN1_2)
    (add_net PIN1_20)
    (add_net PIN1_21)
    (add_net PIN1_30)
    (add_net PIN1_31)
    (add_net PIN1_32)
    (add_net PIN1_33)
    (add_net PIN1_34)
    (add_net PIN1_35)
    (add_net PIN1_39)
    (add_net PIN1_4)
    (add_net PIN1_40)
    (add_net PIN1_41)
    (add_net PIN1_43)
    (add_net PIN1_5)
    (add_net PIN1_6)
    (add_net PIN1_7)
    (add_net PIN1_9)
    (add_net PIN2_1)
    (add_net PIN2_10)
    (add_net PIN2_11)
    (add_net PIN2_12)
    (add_net PIN2_14)
    (add_net PIN2_15)
    (add_net PIN2_16)
    (add_net PIN2_17)
    (add_net PIN2_19)
    (add_net PIN2_2)
    (add_net PIN2_20)
    (add_net PIN2_21)
    (add_net PIN2_30)
    (add_net PIN2_31)
    (add_net PIN2_32)
    (add_net PIN2_33)
    (add_net PIN2_34)
    (add_net PIN2_35)
    (add_net PIN2_39)
    (add_net PIN2_4)
    (add_net PIN2_40)
    (add_net PIN2_41)
    (add_net PIN2_43)
    (add_net PIN2_5)
    (add_net PIN2_6)
    (add_net PIN2_7)
    (add_net PIN2_9)
    (add_net PIN3_1)
    (add_net PIN3_10)
    (add_net PIN3_11)
    (add_net PIN3_12)
    (add_net PIN3_14)
    (add_net PIN3_15)
    (add_net PIN3_16)
    (add_net PIN3_17)
    (add_net PIN3_19)
    (add_net PIN3_2)
    (add_net PIN3_20)
    (add_net PIN3_21)
    (add_net PIN3_30)
    (add_net PIN3_31)
    (add_net PIN3_32)
    (add_net PIN3_33)
    (add_net PIN3_34)
    (add_net PIN3_35)
    (add_net PIN3_39)
    (add_net PIN3_4)
    (add_net PIN3_40)
    (add_net PIN3_41)
    (add_net PIN3_43)
    (add_net PIN3_5)
    (add_net PIN3_6)
    (add_net PIN3_7)
    (add_net PIN3_9)
  )
  (module MountingHole:MountingHole_6.4mm_M6 (layer F.Cu) (tedit 56D1B4CB)
    (at 70.358 113.043)
    (descr "Mounting Hole 6.4mm, no annular, M6")
    (tags "mounting hole 6.4mm no annular m6")
    (attr virtual)
    (fp_text reference h15 (at 0 -7.4) (layer F.SilkS) hide)
    (fp_text value MountingHole_6.4mm_M6 (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6.4 6.4) (drill 6.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_6.4mm_M6 (layer F.Cu) (tedit 56D1B4CB)
    (at 155.438 116.835)
    (descr "Mounting Hole 6.4mm, no annular, M6")
    (tags "mounting hole 6.4mm no annular m6")
    (attr virtual)
    (fp_text reference h16 (at 0 -7.4) (layer F.SilkS) hide)
    (fp_text value MountingHole_6.4mm_M6 (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6.4 6.4) (drill 6.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_6.4mm_M6 (layer F.Cu) (tedit 56D1B4CB)
    (at 155.451 36.8427)
    (descr "Mounting Hole 6.4mm, no annular, M6")
    (tags "mounting hole 6.4mm no annular m6")
    (attr virtual)
    (fp_text reference h14 (at 0 -7.4) (layer F.SilkS) hide)
    (fp_text value MountingHole_6.4mm_M6 (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6.4 6.4) (drill 6.4) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_6.4mm_M6 (layer F.Cu) (tedit 56D1B4CB)
    (at 70.8685 39.3649)
    (descr "Mounting Hole 6.4mm, no annular, M6")
    (tags "mounting hole 6.4mm no annular m6")
    (attr virtual)
    (fp_text reference h13 (at 0 -7.4) (layer F.SilkS) hide)
    (fp_text value MountingHole_6.4mm_M6 (at 0 7.4) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 6.4 6.4) (drill 6.4) (layers *.Cu *.Mask))
  )
  (module MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH (layer F.Cu) (tedit 6088CFB1)
    (at 105.869 61.5493)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference Pico2 (at 0 0) (layer F.SilkS))
    (fp_text value Pico (at 0 2.159) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 PIN2_1))
    (pad 2 thru_hole oval (at -8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 48 PIN2_2))
    (pad 3 thru_hole rect (at -8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole oval (at -8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 47 PIN2_4))
    (pad 5 thru_hole oval (at -8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 46 PIN2_5))
    (pad 6 thru_hole oval (at -8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 PIN2_6))
    (pad 7 thru_hole oval (at -8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 PIN2_7))
    (pad 8 thru_hole rect (at -8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 9 thru_hole oval (at -8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 43 PIN2_9))
    (pad 10 thru_hole oval (at -8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 42 PIN2_10))
    (pad 11 thru_hole oval (at -8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 41 PIN2_11))
    (pad 12 thru_hole oval (at -8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 PIN2_12))
    (pad 13 thru_hole rect (at -8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole oval (at -8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 62 PIN2_14))
    (pad 15 thru_hole oval (at -8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 61 PIN2_15))
    (pad 16 thru_hole oval (at -8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 PIN2_16))
    (pad 17 thru_hole oval (at -8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 PIN2_17))
    (pad 18 thru_hole rect (at -8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 19 thru_hole oval (at -8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 51 PIN2_19))
    (pad 20 thru_hole oval (at -8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 50 PIN2_20))
    (pad 21 thru_hole oval (at 8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 52 PIN2_21))
    (pad 22 thru_hole oval (at 8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 69 FRAM_SCK_2))
    (pad 23 thru_hole rect (at 8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 24 thru_hole oval (at 8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 64 FRAM_HOLD_2))
    (pad 25 thru_hole oval (at 8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 65 FRAM_WP_2))
    (pad 26 thru_hole oval (at 8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 66 FRAM_CS_2))
    (pad 27 thru_hole oval (at 8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 67 FRAM_MOSI_2))
    (pad 28 thru_hole rect (at 8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 29 thru_hole oval (at 8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 68 FRAM_MISO_2))
    (pad 30 thru_hole oval (at 8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 53 PIN2_30))
    (pad 31 thru_hole oval (at 8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 54 PIN2_31))
    (pad 32 thru_hole oval (at 8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 55 PIN2_32))
    (pad 33 thru_hole rect (at 8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 56 PIN2_33))
    (pad 34 thru_hole oval (at 8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 57 PIN2_34))
    (pad 35 thru_hole oval (at 8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 58 PIN2_35))
    (pad 36 thru_hole oval (at 8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 70 FRAM_3V3_2))
    (pad 37 thru_hole oval (at 8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 59 3V3_EN_2))
    (pad 38 thru_hole rect (at 8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 39 thru_hole oval (at 8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 107 PIN2_39))
    (pad 40 thru_hole oval (at 8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 60 PIN2_40))
    (pad 1 smd rect (at -8.89 -24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 49 PIN2_1))
    (pad 2 smd rect (at -8.89 -21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 48 PIN2_2))
    (pad 3 smd rect (at -8.89 -19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -8.89 -16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 47 PIN2_4))
    (pad 5 smd rect (at -8.89 -13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 46 PIN2_5))
    (pad 6 smd rect (at -8.89 -11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 45 PIN2_6))
    (pad 7 smd rect (at -8.89 -8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 44 PIN2_7))
    (pad 8 smd rect (at -8.89 -6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 9 smd rect (at -8.89 -3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 43 PIN2_9))
    (pad 10 smd rect (at -8.89 -1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 42 PIN2_10))
    (pad 11 smd rect (at -8.89 1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 41 PIN2_11))
    (pad 12 smd rect (at -8.89 3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 40 PIN2_12))
    (pad 13 smd rect (at -8.89 6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 14 smd rect (at -8.89 8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 62 PIN2_14))
    (pad 15 smd rect (at -8.89 11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 61 PIN2_15))
    (pad 16 smd rect (at -8.89 13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 38 PIN2_16))
    (pad 17 smd rect (at -8.89 16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 37 PIN2_17))
    (pad 18 smd rect (at -8.89 19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 19 smd rect (at -8.89 21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 51 PIN2_19))
    (pad 20 smd rect (at -8.89 24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 50 PIN2_20))
    (pad 40 smd rect (at 8.89 -24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 60 PIN2_40))
    (pad 39 smd rect (at 8.89 -21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 107 PIN2_39))
    (pad 38 smd rect (at 8.89 -19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 37 smd rect (at 8.89 -16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 59 3V3_EN_2))
    (pad 36 smd rect (at 8.89 -13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 70 FRAM_3V3_2))
    (pad 35 smd rect (at 8.89 -11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 58 PIN2_35))
    (pad 34 smd rect (at 8.89 -8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 57 PIN2_34))
    (pad 33 smd rect (at 8.89 -6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 56 PIN2_33))
    (pad 32 smd rect (at 8.89 -3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 55 PIN2_32))
    (pad 31 smd rect (at 8.89 -1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 54 PIN2_31))
    (pad 30 smd rect (at 8.89 1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 53 PIN2_30))
    (pad 29 smd rect (at 8.89 3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 68 FRAM_MISO_2))
    (pad 28 smd rect (at 8.89 6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 27 smd rect (at 8.89 8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 67 FRAM_MOSI_2))
    (pad 26 smd rect (at 8.89 11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 66 FRAM_CS_2))
    (pad 25 smd rect (at 8.89 13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 65 FRAM_WP_2))
    (pad 24 smd rect (at 8.89 16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 64 FRAM_HOLD_2))
    (pad 23 smd rect (at 8.89 19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 22 smd rect (at 8.89 21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 69 FRAM_SCK_2))
    (pad 21 smd rect (at 8.89 24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 52 PIN2_21))
    (pad "" np_thru_hole oval (at -2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad 41 smd rect (at -2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 39 PIN2_41))
    (pad 41 thru_hole oval (at -2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 PIN2_41))
    (pad 42 smd rect (at 0 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 42 thru_hole rect (at 0 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 43 smd rect (at 2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 63 PIN2_43))
    (pad 43 thru_hole oval (at 2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 63 PIN2_43))
    (model "C:/Users/bsztu/College/y4.2/msd/KiCad-RP-Pico-main/RP-Pico Libraries/Pico.wrl"
      (offset (xyz -10.5 -25 0))
      (scale (xyz 10 10 10))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 111.569 38.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h6 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 100.169 85.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h7 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 126.569 38.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h9 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 126.569 85.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h11 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 137.969 38.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h10 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 137.969 85.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h12 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 111.569 85.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h8 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 100.169 38.0493)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h5 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 85.169 45.6693)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h2 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 73.769 92.6693)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h3 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 73.769 45.6693)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h1 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.1mm (layer F.Cu) (tedit 5B924765)
    (at 85.169 92.6693)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference h4 (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.1mm (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
  )
  (module MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH (layer F.Cu) (tedit 6088CFB1)
    (at 132.269 61.5493)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference Pico3 (at 0 0) (layer F.SilkS))
    (fp_text value Pico (at 0 2.159) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 83 PIN3_1))
    (pad 2 thru_hole oval (at -8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 82 PIN3_2))
    (pad 3 thru_hole rect (at -8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole oval (at -8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 81 PIN3_4))
    (pad 5 thru_hole oval (at -8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 80 PIN3_5))
    (pad 6 thru_hole oval (at -8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 79 PIN3_6))
    (pad 7 thru_hole oval (at -8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 78 PIN3_7))
    (pad 8 thru_hole rect (at -8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 9 thru_hole oval (at -8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 77 PIN3_9))
    (pad 10 thru_hole oval (at -8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 76 PIN3_10))
    (pad 11 thru_hole oval (at -8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 75 PIN3_11))
    (pad 12 thru_hole oval (at -8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 74 PIN3_12))
    (pad 13 thru_hole rect (at -8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole oval (at -8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 96 PIN3_14))
    (pad 15 thru_hole oval (at -8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 95 PIN3_15))
    (pad 16 thru_hole oval (at -8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 72 PIN3_16))
    (pad 17 thru_hole oval (at -8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 71 PIN3_17))
    (pad 18 thru_hole rect (at -8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 19 thru_hole oval (at -8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 85 PIN3_19))
    (pad 20 thru_hole oval (at -8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 84 PIN3_20))
    (pad 21 thru_hole oval (at 8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 86 PIN3_21))
    (pad 22 thru_hole oval (at 8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 103 FRAM_SCK_3))
    (pad 23 thru_hole rect (at 8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 24 thru_hole oval (at 8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 98 FRAM_HOLD_3))
    (pad 25 thru_hole oval (at 8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 99 FRAM_WP_3))
    (pad 26 thru_hole oval (at 8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 100 FRAM_CS_3))
    (pad 27 thru_hole oval (at 8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 101 FRAM_MOSI_3))
    (pad 28 thru_hole rect (at 8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 29 thru_hole oval (at 8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 102 FRAM_MISO_3))
    (pad 30 thru_hole oval (at 8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 87 PIN3_30))
    (pad 31 thru_hole oval (at 8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 88 PIN3_31))
    (pad 32 thru_hole oval (at 8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 89 PIN3_32))
    (pad 33 thru_hole rect (at 8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 90 PIN3_33))
    (pad 34 thru_hole oval (at 8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 91 PIN3_34))
    (pad 35 thru_hole oval (at 8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 92 PIN3_35))
    (pad 36 thru_hole oval (at 8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 104 FRAM_3V3_3))
    (pad 37 thru_hole oval (at 8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 93 3V3_EN_3))
    (pad 38 thru_hole rect (at 8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 39 thru_hole oval (at 8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 108 PIN3_39))
    (pad 40 thru_hole oval (at 8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 94 PIN3_40))
    (pad 1 smd rect (at -8.89 -24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 83 PIN3_1))
    (pad 2 smd rect (at -8.89 -21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 82 PIN3_2))
    (pad 3 smd rect (at -8.89 -19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -8.89 -16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 81 PIN3_4))
    (pad 5 smd rect (at -8.89 -13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 80 PIN3_5))
    (pad 6 smd rect (at -8.89 -11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 79 PIN3_6))
    (pad 7 smd rect (at -8.89 -8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 78 PIN3_7))
    (pad 8 smd rect (at -8.89 -6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 9 smd rect (at -8.89 -3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 77 PIN3_9))
    (pad 10 smd rect (at -8.89 -1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 76 PIN3_10))
    (pad 11 smd rect (at -8.89 1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 75 PIN3_11))
    (pad 12 smd rect (at -8.89 3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 74 PIN3_12))
    (pad 13 smd rect (at -8.89 6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 14 smd rect (at -8.89 8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 96 PIN3_14))
    (pad 15 smd rect (at -8.89 11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 95 PIN3_15))
    (pad 16 smd rect (at -8.89 13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 72 PIN3_16))
    (pad 17 smd rect (at -8.89 16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 71 PIN3_17))
    (pad 18 smd rect (at -8.89 19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 19 smd rect (at -8.89 21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 85 PIN3_19))
    (pad 20 smd rect (at -8.89 24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 84 PIN3_20))
    (pad 40 smd rect (at 8.89 -24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 94 PIN3_40))
    (pad 39 smd rect (at 8.89 -21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 108 PIN3_39))
    (pad 38 smd rect (at 8.89 -19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 37 smd rect (at 8.89 -16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 93 3V3_EN_3))
    (pad 36 smd rect (at 8.89 -13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 104 FRAM_3V3_3))
    (pad 35 smd rect (at 8.89 -11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 92 PIN3_35))
    (pad 34 smd rect (at 8.89 -8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 91 PIN3_34))
    (pad 33 smd rect (at 8.89 -6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 90 PIN3_33))
    (pad 32 smd rect (at 8.89 -3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 89 PIN3_32))
    (pad 31 smd rect (at 8.89 -1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 88 PIN3_31))
    (pad 30 smd rect (at 8.89 1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 87 PIN3_30))
    (pad 29 smd rect (at 8.89 3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 102 FRAM_MISO_3))
    (pad 28 smd rect (at 8.89 6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 27 smd rect (at 8.89 8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 101 FRAM_MOSI_3))
    (pad 26 smd rect (at 8.89 11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 100 FRAM_CS_3))
    (pad 25 smd rect (at 8.89 13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 99 FRAM_WP_3))
    (pad 24 smd rect (at 8.89 16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 98 FRAM_HOLD_3))
    (pad 23 smd rect (at 8.89 19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 22 smd rect (at 8.89 21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 103 FRAM_SCK_3))
    (pad 21 smd rect (at 8.89 24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 86 PIN3_21))
    (pad "" np_thru_hole oval (at -2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad 41 smd rect (at -2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 73 PIN3_41))
    (pad 41 thru_hole oval (at -2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 73 PIN3_41))
    (pad 42 smd rect (at 0 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 42 thru_hole rect (at 0 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 43 smd rect (at 2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 97 PIN3_43))
    (pad 43 thru_hole oval (at 2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 97 PIN3_43))
    (model "C:/Users/bsztu/College/y4.2/msd/KiCad-RP-Pico-main/RP-Pico Libraries/Pico.wrl"
      (offset (xyz -10.5 -25 0))
      (scale (xyz 10 10 10))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:1375795-2 (layer F.Cu) (tedit 0)
    (at 151.638 45.212 90)
    (descr 1375795-2)
    (tags Connector)
    (fp_text reference PC104 (at -31.474 0.031 90) (layer F.SilkS))
    (fp_text value 1375795-2 (at -31.474 0.031 90) (layer F.SilkS) hide)
    (fp_text user %R (at -31.474 0.031 90) (layer F.Fab))
    (pad 104 thru_hole circle (at -1.79 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 103 thru_hole circle (at -4.33 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 102 thru_hole circle (at -6.87 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 101 thru_hole circle (at -9.41 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 105 +5V))
    (pad 100 thru_hole circle (at -11.95 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 99 thru_hole circle (at -14.49 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 98 thru_hole circle (at -17.03 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 97 thru_hole circle (at -19.57 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 96 thru_hole circle (at -22.11 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 95 thru_hole circle (at -24.65 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 94 thru_hole circle (at -27.19 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 93 thru_hole circle (at -29.73 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 92 thru_hole circle (at -32.27 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 91 thru_hole circle (at -34.81 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 90 thru_hole circle (at -37.35 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 89 thru_hole circle (at -39.89 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 88 thru_hole circle (at -42.43 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 87 thru_hole circle (at -44.97 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 86 thru_hole circle (at -47.51 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 85 thru_hole circle (at -50.05 3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 84 thru_hole circle (at -1.79 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 106 KEY))
    (pad 83 thru_hole circle (at -4.33 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 82 thru_hole circle (at -6.87 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 81 thru_hole circle (at -9.41 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 80 thru_hole circle (at -11.95 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 79 thru_hole circle (at -14.49 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 78 thru_hole circle (at -17.03 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 77 thru_hole circle (at -19.57 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 76 thru_hole circle (at -22.11 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 75 thru_hole circle (at -24.65 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 74 thru_hole circle (at -27.19 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 73 thru_hole circle (at -29.73 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 72 thru_hole circle (at -32.27 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 71 thru_hole circle (at -34.81 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 70 thru_hole circle (at -37.35 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 69 thru_hole circle (at -39.89 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 68 thru_hole circle (at -42.43 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 67 thru_hole circle (at -44.97 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 66 thru_hole circle (at -47.51 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 65 thru_hole circle (at -50.05 1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 64 thru_hole circle (at 8.37 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 63 thru_hole circle (at 8.37 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 62 thru_hole circle (at 5.83 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 61 thru_hole circle (at 5.83 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 60 thru_hole circle (at 3.29 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 59 thru_hole circle (at 3.29 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 58 thru_hole circle (at 0.75 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 57 thru_hole circle (at 0.75 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 105 +5V))
    (pad 56 thru_hole circle (at -1.79 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 55 thru_hole circle (at -1.79 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 54 thru_hole circle (at -4.33 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 53 thru_hole circle (at -4.33 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 52 thru_hole circle (at -6.87 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 51 thru_hole circle (at -6.87 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 50 thru_hole circle (at -9.41 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 49 thru_hole circle (at -9.41 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 48 thru_hole circle (at -11.95 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 47 thru_hole circle (at -11.95 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 46 thru_hole circle (at -14.49 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 45 thru_hole circle (at -14.49 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 44 thru_hole circle (at -17.03 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 43 thru_hole circle (at -17.03 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 42 thru_hole circle (at -19.57 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 41 thru_hole circle (at -19.57 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 40 thru_hole circle (at -22.11 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 39 thru_hole circle (at -22.11 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at -24.65 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 37 thru_hole circle (at -24.65 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 36 thru_hole circle (at -27.19 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at -27.19 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at -29.73 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 33 thru_hole circle (at -29.73 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 32 thru_hole circle (at -32.27 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 31 thru_hole circle (at -32.27 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 30 thru_hole circle (at -34.81 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 29 thru_hole circle (at -34.81 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 28 thru_hole circle (at -37.35 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 27 thru_hole circle (at -37.35 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 26 thru_hole circle (at -39.89 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 25 thru_hole circle (at -39.89 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 24 thru_hole circle (at -42.43 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 23 thru_hole circle (at -42.43 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 22 thru_hole circle (at -44.97 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 21 thru_hole circle (at -44.97 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at -47.51 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at -47.51 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 106 KEY))
    (pad 18 thru_hole circle (at -50.05 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at -50.05 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -52.59 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at -52.59 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 14 thru_hole circle (at -55.13 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 13 thru_hole circle (at -55.13 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -57.67 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at -57.67 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at -60.21 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -60.21 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -62.75 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at -62.75 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -65.29 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -65.29 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 105 +5V))
    (pad 4 thru_hole circle (at -67.83 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -67.83 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -70.37 -1.27 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -70.37 -3.81 90) (size 1.85 1.85) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 GND))
    (model C:\Users\bsztu\Desktop\LibraryLoader\SamacSys_Parts.3dshapes\1375795-2.stp
      (offset (xyz -30.99999953442717 -0.2099999902896051 10.97000010227586))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomPin:CustomBigBoi (layer F.Cu) (tedit 613A8F9E)
    (at 136.398 116.332)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference P3 (at 0 -1.56) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 108 PIN3_39))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (offset (xyz 0 0 -4))
      (scale (xyz 1 1 2))
      (rotate (xyz 0 180 0))
    )
  )
  (module CustomPin:CustomBigBoi (layer F.Cu) (tedit 613A8F9E)
    (at 133.858 116.332)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference P2 (at 0 -1.56) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 107 PIN2_39))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (offset (xyz 0 0 -4))
      (scale (xyz 1 1 2))
      (rotate (xyz 0 180 0))
    )
  )
  (module CustomPin:CustomBigBoi (layer F.Cu) (tedit 613A8F9E)
    (at 131.318 116.332)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (fp_text reference P1 (at 0 -1.56) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 1.56) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 25 PIN1_39))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl
      (offset (xyz 0 0 -4))
      (scale (xyz 1 1 2))
      (rotate (xyz 0 180 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x16_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 101.039 107.805 270)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference 1A1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 0 32.06 90) (layer F.Fab))
    (fp_text user %R (at 0 15) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 PIN1_1))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 PIN1_2))
    (pad 3 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 PIN1_4))
    (pad 5 thru_hole oval (at 0 8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 PIN1_5))
    (pad 6 thru_hole oval (at 0 10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 PIN1_6))
    (pad 7 thru_hole oval (at 0 12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 PIN1_7))
    (pad 8 thru_hole oval (at 0 14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 9 thru_hole oval (at 0 16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 PIN1_9))
    (pad 10 thru_hole oval (at 0 18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 PIN1_10))
    (pad 11 thru_hole oval (at 0 20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 PIN1_11))
    (pad 12 thru_hole oval (at 0 22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 PIN1_12))
    (pad 13 thru_hole oval (at 0 24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole oval (at 0 26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 PIN1_41))
    (pad 15 thru_hole oval (at 0 28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 PIN1_16))
    (pad 16 thru_hole oval (at 0 30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 PIN1_17))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x16_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MCU_RaspberryPi_and_Boards:RPi_Pico_SMD_TH (layer F.Cu) (tedit 6088CFB1)
    (at 79.469 69.1693)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference Pico1 (at 0 0) (layer F.SilkS))
    (fp_text value Pico (at 0 2.159) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole oval (at -8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 PIN1_1))
    (pad 2 thru_hole oval (at -8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 13 PIN1_2))
    (pad 3 thru_hole rect (at -8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole oval (at -8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 PIN1_4))
    (pad 5 thru_hole oval (at -8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 PIN1_5))
    (pad 6 thru_hole oval (at -8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 PIN1_6))
    (pad 7 thru_hole oval (at -8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 PIN1_7))
    (pad 8 thru_hole rect (at -8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 9 thru_hole oval (at -8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 PIN1_9))
    (pad 10 thru_hole oval (at -8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 PIN1_10))
    (pad 11 thru_hole oval (at -8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 PIN1_11))
    (pad 12 thru_hole oval (at -8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 PIN1_12))
    (pad 13 thru_hole rect (at -8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole oval (at -8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 PIN1_14))
    (pad 15 thru_hole oval (at -8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 PIN1_15))
    (pad 16 thru_hole oval (at -8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 PIN1_16))
    (pad 17 thru_hole oval (at -8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 PIN1_17))
    (pad 18 thru_hole rect (at -8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 19 thru_hole oval (at -8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 PIN1_19))
    (pad 20 thru_hole oval (at -8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 PIN1_20))
    (pad 21 thru_hole oval (at 8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 PIN1_21))
    (pad 22 thru_hole oval (at 8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 FRAM_SCK_1))
    (pad 23 thru_hole rect (at 8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 24 thru_hole oval (at 8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 FRAM_HOLD_1))
    (pad 25 thru_hole oval (at 8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 FRAM_WP_1))
    (pad 26 thru_hole oval (at 8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 FRAM_CS_1))
    (pad 27 thru_hole oval (at 8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 FRAM_MOSI_1))
    (pad 28 thru_hole rect (at 8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 29 thru_hole oval (at 8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 FRAM_MISO_1))
    (pad 30 thru_hole oval (at 8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 PIN1_30))
    (pad 31 thru_hole oval (at 8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 PIN1_31))
    (pad 32 thru_hole oval (at 8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 PIN1_32))
    (pad 33 thru_hole rect (at 8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 PIN1_33))
    (pad 34 thru_hole oval (at 8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 PIN1_34))
    (pad 35 thru_hole oval (at 8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 PIN1_35))
    (pad 36 thru_hole oval (at 8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 FRAM_3V3_1))
    (pad 37 thru_hole oval (at 8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 24 3V3_EN_1))
    (pad 38 thru_hole rect (at 8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 39 thru_hole oval (at 8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 25 PIN1_39))
    (pad 40 thru_hole oval (at 8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 PIN1_40))
    (pad 1 smd rect (at -8.89 -24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 14 PIN1_1))
    (pad 2 smd rect (at -8.89 -21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 13 PIN1_2))
    (pad 3 smd rect (at -8.89 -19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -8.89 -16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 12 PIN1_4))
    (pad 5 smd rect (at -8.89 -13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 11 PIN1_5))
    (pad 6 smd rect (at -8.89 -11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 10 PIN1_6))
    (pad 7 smd rect (at -8.89 -8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 9 PIN1_7))
    (pad 8 smd rect (at -8.89 -6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 9 smd rect (at -8.89 -3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 8 PIN1_9))
    (pad 10 smd rect (at -8.89 -1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 7 PIN1_10))
    (pad 11 smd rect (at -8.89 1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 6 PIN1_11))
    (pad 12 smd rect (at -8.89 3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 5 PIN1_12))
    (pad 13 smd rect (at -8.89 6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 14 smd rect (at -8.89 8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 28 PIN1_14))
    (pad 15 smd rect (at -8.89 11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 27 PIN1_15))
    (pad 16 smd rect (at -8.89 13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 2 PIN1_16))
    (pad 17 smd rect (at -8.89 16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 1 PIN1_17))
    (pad 18 smd rect (at -8.89 19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 19 smd rect (at -8.89 21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 16 PIN1_19))
    (pad 20 smd rect (at -8.89 24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 15 PIN1_20))
    (pad 40 smd rect (at 8.89 -24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 26 PIN1_40))
    (pad 39 smd rect (at 8.89 -21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 25 PIN1_39))
    (pad 38 smd rect (at 8.89 -19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 37 smd rect (at 8.89 -16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 24 3V3_EN_1))
    (pad 36 smd rect (at 8.89 -13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 36 FRAM_3V3_1))
    (pad 35 smd rect (at 8.89 -11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 23 PIN1_35))
    (pad 34 smd rect (at 8.89 -8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 22 PIN1_34))
    (pad 33 smd rect (at 8.89 -6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 21 PIN1_33))
    (pad 32 smd rect (at 8.89 -3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 20 PIN1_32))
    (pad 31 smd rect (at 8.89 -1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 19 PIN1_31))
    (pad 30 smd rect (at 8.89 1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 18 PIN1_30))
    (pad 29 smd rect (at 8.89 3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 34 FRAM_MISO_1))
    (pad 28 smd rect (at 8.89 6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 27 smd rect (at 8.89 8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 33 FRAM_MOSI_1))
    (pad 26 smd rect (at 8.89 11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 32 FRAM_CS_1))
    (pad 25 smd rect (at 8.89 13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 31 FRAM_WP_1))
    (pad 24 smd rect (at 8.89 16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 30 FRAM_HOLD_1))
    (pad 23 smd rect (at 8.89 19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 22 smd rect (at 8.89 21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 35 FRAM_SCK_1))
    (pad 21 smd rect (at 8.89 24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers F.Cu F.Mask)
      (net 17 PIN1_21))
    (pad "" np_thru_hole oval (at -2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.725 -24) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad 41 smd rect (at -2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 3 PIN1_41))
    (pad 41 thru_hole oval (at -2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 PIN1_41))
    (pad 42 smd rect (at 0 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 4 GND))
    (pad 42 thru_hole rect (at 0 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 43 smd rect (at 2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers F.Cu F.Mask)
      (net 29 PIN1_43))
    (pad 43 thru_hole oval (at 2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 PIN1_43))
    (model "C:/Users/bsztu/College/y4.2/msd/KiCad-RP-Pico-main/RP-Pico Libraries/Pico.wrl"
      (offset (xyz -10.5 -25 0))
      (scale (xyz 10 10 10))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x09_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 122.989 92.0877 90)
    (descr "Through hole straight pin header, 1x09, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.00mm single row")
    (fp_text reference 3C1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Male (at 0 18.06 90) (layer F.Fab))
    (fp_text user %R (at 0 8) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 98 FRAM_HOLD_3))
    (pad 8 thru_hole oval (at 0 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 99 FRAM_WP_3))
    (pad 7 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 100 FRAM_CS_3))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 FRAM_MOSI_3))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 FRAM_MISO_3))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 FRAM_SCK_3))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 FRAM_3V3_3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 FRAM_3V3_3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x09_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x16_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 140.567 102.396 270)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference 3B1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 0 32.06 90) (layer F.Fab))
    (fp_text user %R (at 0 15) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 PIN3_20))
    (pad 15 thru_hole oval (at 0 28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 PIN3_19))
    (pad 14 thru_hole oval (at 0 26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 PIN3_21))
    (pad 13 thru_hole oval (at 0 24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 12 thru_hole oval (at 0 22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 PIN3_30))
    (pad 11 thru_hole oval (at 0 20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 PIN3_31))
    (pad 10 thru_hole oval (at 0 18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 89 PIN3_32))
    (pad 9 thru_hole oval (at 0 16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 90 PIN3_33))
    (pad 8 thru_hole oval (at 0 14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 91 PIN3_34))
    (pad 7 thru_hole oval (at 0 12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 92 PIN3_35))
    (pad 6 thru_hole oval (at 0 10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 93 3V3_EN_3))
    (pad 5 thru_hole oval (at 0 8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 PIN3_39))
    (pad 4 thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 94 PIN3_40))
    (pad 3 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 95 PIN3_15))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 PIN3_14))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 PIN3_43))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x16_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x16_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 138.242 107.749 270)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference 3A1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 0 32.06 90) (layer F.Fab))
    (fp_text user %R (at 0 15) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 PIN3_17))
    (pad 15 thru_hole oval (at 0 28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 PIN3_16))
    (pad 14 thru_hole oval (at 0 26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 PIN3_41))
    (pad 13 thru_hole oval (at 0 24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 12 thru_hole oval (at 0 22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 PIN3_12))
    (pad 11 thru_hole oval (at 0 20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 PIN3_11))
    (pad 10 thru_hole oval (at 0 18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 PIN3_10))
    (pad 9 thru_hole oval (at 0 16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 PIN3_9))
    (pad 8 thru_hole oval (at 0 14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 7 thru_hole oval (at 0 12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 PIN3_7))
    (pad 6 thru_hole oval (at 0 10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 PIN3_6))
    (pad 5 thru_hole oval (at 0 8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 PIN3_5))
    (pad 4 thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 PIN3_4))
    (pad 3 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 PIN3_2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 PIN3_1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x16_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x09_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 96.4784 92.108 90)
    (descr "Through hole straight pin header, 1x09, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.00mm single row")
    (fp_text reference 2C1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Male (at 0 18.06 90) (layer F.Fab))
    (fp_text user %R (at 7.62 25.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 FRAM_3V3_2))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 FRAM_3V3_2))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 FRAM_SCK_2))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 FRAM_MISO_2))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 FRAM_MOSI_2))
    (pad 7 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 FRAM_CS_2))
    (pad 8 thru_hole oval (at 0 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 FRAM_WP_2))
    (pad 9 thru_hole oval (at 0 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 FRAM_HOLD_2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x09_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x16_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 126.477 97.1423 270)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference 2B1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at -10.922 49.276 90) (layer F.Fab))
    (fp_text user %R (at 0 15) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 PIN2_43))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 PIN2_14))
    (pad 3 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 PIN2_15))
    (pad 4 thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 PIN2_40))
    (pad 5 thru_hole oval (at 0 8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 PIN2_39))
    (pad 6 thru_hole oval (at 0 10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 3V3_EN_2))
    (pad 7 thru_hole oval (at 0 12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 PIN2_35))
    (pad 8 thru_hole oval (at 0 14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 PIN2_34))
    (pad 9 thru_hole oval (at 0 16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 PIN2_33))
    (pad 10 thru_hole oval (at 0 18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 PIN2_32))
    (pad 11 thru_hole oval (at 0 20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 PIN2_31))
    (pad 12 thru_hole oval (at 0 22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 PIN2_30))
    (pad 13 thru_hole oval (at 0 24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole oval (at 0 26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 PIN2_21))
    (pad 15 thru_hole oval (at 0 28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 PIN2_19))
    (pad 16 thru_hole oval (at 0 30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 PIN2_20))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x16_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x16_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 126.502 114.651 270)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference 2A1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 0 32.06 90) (layer F.Fab))
    (fp_text user %R (at 0 15) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 PIN2_17))
    (pad 15 thru_hole oval (at 0 28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 PIN2_16))
    (pad 14 thru_hole oval (at 0 26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 PIN2_41))
    (pad 13 thru_hole oval (at 0 24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 12 thru_hole oval (at 0 22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 PIN2_12))
    (pad 11 thru_hole oval (at 0 20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 PIN2_11))
    (pad 10 thru_hole oval (at 0 18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 PIN2_10))
    (pad 9 thru_hole oval (at 0 16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 PIN2_9))
    (pad 8 thru_hole oval (at 0 14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 7 thru_hole oval (at 0 12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 PIN2_7))
    (pad 6 thru_hole oval (at 0 10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 PIN2_6))
    (pad 5 thru_hole oval (at 0 8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 PIN2_5))
    (pad 4 thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 PIN2_4))
    (pad 3 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 PIN2_2))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 PIN2_1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x16_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x09_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 71.087 99.6493 90)
    (descr "Through hole straight pin header, 1x09, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.00mm single row")
    (fp_text reference 1C1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x09_Male (at 0 18.06 90) (layer F.Fab))
    (fp_text user %R (at 0 8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 FRAM_3V3_1))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 FRAM_3V3_1))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 FRAM_SCK_1))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 FRAM_MISO_1))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 FRAM_MOSI_1))
    (pad 7 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 FRAM_CS_1))
    (pad 8 thru_hole oval (at 0 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 FRAM_WP_1))
    (pad 9 thru_hole oval (at 0 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 FRAM_HOLD_1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x09_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_1x16_P2.00mm_Vertical (layer F.Cu) (tedit 59FED667)
    (at 101.059 103.713 270)
    (descr "Through hole straight pin header, 1x16, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.00mm single row")
    (fp_text reference 1B1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value Conn_01x16_Male (at 0 32.06 90) (layer F.Fab))
    (fp_text user %R (at 0 15) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 PIN1_20))
    (pad 15 thru_hole oval (at 0 28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 PIN1_19))
    (pad 14 thru_hole oval (at 0 26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 PIN1_21))
    (pad 13 thru_hole oval (at 0 24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 12 thru_hole oval (at 0 22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 PIN1_30))
    (pad 11 thru_hole oval (at 0 20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 PIN1_31))
    (pad 10 thru_hole oval (at 0 18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 PIN1_32))
    (pad 9 thru_hole oval (at 0 16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 PIN1_33))
    (pad 8 thru_hole oval (at 0 14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 PIN1_34))
    (pad 7 thru_hole oval (at 0 12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 PIN1_35))
    (pad 6 thru_hole oval (at 0 10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 3V3_EN_1))
    (pad 5 thru_hole oval (at 0 8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 PIN1_39))
    (pad 4 thru_hole oval (at 0 6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 PIN1_40))
    (pad 3 thru_hole oval (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 PIN1_15))
    (pad 2 thru_hole oval (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 PIN1_14))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 PIN1_43))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x16_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 3.10 (at 120.16994 109.64926) (layer F.SilkS))
  (gr_text 3.06 (at 128.1049 109.69752) (layer F.SilkS))
  (gr_text 3.41 (at 112.0902 109.64926) (layer F.SilkS))
  (gr_text 3.01 (at 138.20648 109.67974) (layer F.SilkS))
  (gr_text GND (at 114.12728 109.64926) (layer F.SilkS))
  (gr_text 3.04 (at 132.12064 109.67974) (layer F.SilkS))
  (gr_text 3.17 (at 108.1786 109.63148) (layer F.SilkS))
  (gr_text GND (at 134.1374 109.69752) (layer F.SilkS))
  (gr_text 3.16 (at 110.18012 109.6772) (layer F.SilkS))
  (gr_text 3.05 (at 130.16738 109.71276) (layer F.SilkS))
  (gr_text 3.09 (at 122.17146 109.66704) (layer F.SilkS))
  (gr_text 3.07 (at 126.12878 109.65942) (layer F.SilkS))
  (gr_text 3.02 (at 136.15416 109.69752) (layer F.SilkS))
  (gr_text 3.11 (at 118.15064 109.66704) (layer F.SilkS))
  (gr_text GND (at 124.09932 109.66704) (layer F.SilkS))
  (gr_text 3.12 (at 116.13896 109.65942) (layer F.SilkS))
  (gr_text 3.37 (at 130.30302 104.57764) (layer F.SilkS))
  (gr_text 3.21 (at 114.28832 104.52938) (layer F.SilkS))
  (gr_text 3.33 (at 124.36958 104.54716) (layer F.SilkS))
  (gr_text 3.31 (at 120.34876 104.54716) (layer F.SilkS))
  (gr_text GND (at 116.3254 104.52938) (layer F.SilkS))
  (gr_text 3.32 (at 122.36806 104.52938) (layer F.SilkS))
  (gr_text 3.40 (at 134.31876 104.55986) (layer F.SilkS))
  (gr_text 3.39 (at 132.3655 104.59288) (layer F.SilkS))
  (gr_text 3.30 (at 118.33708 104.53954) (layer F.SilkS))
  (gr_text 3.43 (at 140.4046 104.55986) (layer F.SilkS))
  (gr_text 3.20 (at 110.37672 104.5116) (layer F.SilkS))
  (gr_text 3.14 (at 138.35228 104.57764) (layer F.SilkS))
  (gr_text 3.35 (at 128.3269 104.53954) (layer F.SilkS))
  (gr_text 3.15 (at 136.33552 104.57764) (layer F.SilkS))
  (gr_text 3.34 (at 126.29744 104.54716) (layer F.SilkS))
  (gr_text 3.19 (at 112.37824 104.55732) (layer F.SilkS))
  (gr_text 3.27 (at 132.4102 94.08414) (layer F.SilkS))
  (gr_text 3.29 (at 130.45186 94.04096) (layer F.SilkS))
  (gr_text 3.36 (at 124.36856 94.07906) (layer F.SilkS))
  (gr_text "3.22\n" (at 128.34874 94.02572) (layer F.SilkS))
  (gr_text 3.24 (at 138.38174 94.08414) (layer F.SilkS))
  (gr_text 3.25 (at 136.30148 94.12986) (layer F.SilkS))
  (gr_text 3.26 (at 134.37616 94.08414) (layer F.SilkS))
  (gr_text 3.36 (at 122.41022 94.0562) (layer F.SilkS))
  (gr_text GND (at 126.39802 94.0689) (layer F.SilkS))
  (gr_text 3.42 (at 132.22834 88.74506) (layer F.SilkS))
  (gr_text 3.41 (at 129.72136 88.67902) (layer F.SilkS))
  (gr_text 3.43 (at 134.93344 88.773) (layer F.SilkS))
  (gr_text "3.24\n" (at 144.49146 77.99578) (layer F.SilkS))
  (gr_text 3.30 (at 144.52194 62.93866) (layer F.SilkS))
  (gr_text 3.22 (at 144.45336 83.01482) (layer F.SilkS))
  (gr_text 3.23 (at 144.43304 80.5561) (layer F.SilkS))
  (gr_text 3.28 (at 144.4813 67.9958) (layer F.SilkS))
  (gr_text 3.35 (at 144.47368 50.19548) (layer F.SilkS))
  (gr_text "3.29\n" (at 144.53972 65.43548) (layer F.SilkS))
  (gr_text 3.36 (at 144.4813 47.7393) (layer F.SilkS))
  (gr_text 3.32 (at 144.45336 57.71134) (layer F.SilkS))
  (gr_text 3.31 (at 144.43304 60.2996) (layer F.SilkS))
  (gr_text 3.26 (at 144.4813 73.04278) (layer F.SilkS))
  (gr_text 3.38 (at 144.4813 42.69232) (layer F.SilkS))
  (gr_text 3.25 (at 144.47368 75.49896) (layer F.SilkS))
  (gr_text "3.39\n" (at 144.53972 40.132) (layer F.SilkS))
  (gr_text 3.21 (at 144.43304 85.60308) (layer F.SilkS))
  (gr_text 3.27 (at 144.50162 70.45452) (layer F.SilkS))
  (gr_text "3.34\n" (at 144.49146 52.6923) (layer F.SilkS))
  (gr_text 3.33 (at 144.43304 55.25262) (layer F.SilkS))
  (gr_text 3.37 (at 144.50162 45.15104) (layer F.SilkS))
  (gr_text 3.40 (at 144.52194 37.63518) (layer F.SilkS))
  (gr_text 3.09 (at 120.16588 57.62752) (layer F.SilkS))
  (gr_text "3.04\n" (at 120.21414 45.06722) (layer F.SilkS))
  (gr_text 3.12 (at 120.25224 65.35166) (layer F.SilkS))
  (gr_text 3.17 (at 120.20398 77.91196) (layer F.SilkS))
  (gr_text 3.13 (at 120.19382 67.91198) (layer F.SilkS))
  (gr_text 3.06 (at 120.1862 50.11166) (layer F.SilkS))
  (gr_text 3.19 (at 120.16588 82.931) (layer F.SilkS))
  (gr_text 3.08 (at 120.14556 55.1688) (layer F.SilkS))
  (gr_text "3.05\n" (at 120.19382 47.65548) (layer F.SilkS))
  (gr_text 3.16 (at 120.1862 75.41514) (layer F.SilkS))
  (gr_text 3.20 (at 120.14556 85.51926) (layer F.SilkS))
  (gr_text 3.01 (at 120.23446 37.55136) (layer F.SilkS))
  (gr_text 3.11 (at 120.23446 62.85484) (layer F.SilkS))
  (gr_text 3.18 (at 120.14556 80.47228) (layer F.SilkS))
  (gr_text 3.10 (at 120.14556 60.21578) (layer F.SilkS))
  (gr_text "3.02\n" (at 120.25224 40.04818) (layer F.SilkS))
  (gr_text 3.15 (at 120.19382 72.95896) (layer F.SilkS))
  (gr_text 3.14 (at 120.21414 70.3707) (layer F.SilkS))
  (gr_text 3.03 (at 120.19382 42.6085) (layer F.SilkS))
  (gr_text 3.07 (at 120.20398 52.60848) (layer F.SilkS))
  (gr_text 2.10 (at 108.55198 116.51742) (layer F.SilkS))
  (gr_text 2.06 (at 116.48694 116.56568) (layer F.SilkS))
  (gr_text 2.41 (at 100.47224 116.51742) (layer F.SilkS))
  (gr_text 2.01 (at 126.58852 116.5479) (layer F.SilkS))
  (gr_text GND (at 102.50932 116.51742) (layer F.SilkS))
  (gr_text 2.04 (at 120.50268 116.5479) (layer F.SilkS))
  (gr_text 2.17 (at 96.56064 116.49964) (layer F.SilkS))
  (gr_text GND (at 122.51944 116.56568) (layer F.SilkS))
  (gr_text 2.16 (at 98.56216 116.54536) (layer F.SilkS))
  (gr_text 2.05 (at 118.54942 116.58092) (layer F.SilkS))
  (gr_text 2.09 (at 110.5535 116.5352) (layer F.SilkS))
  (gr_text 2.07 (at 114.51082 116.52758) (layer F.SilkS))
  (gr_text 2.02 (at 124.5362 116.56568) (layer F.SilkS))
  (gr_text 2.11 (at 106.53268 116.5352) (layer F.SilkS))
  (gr_text GND (at 112.48136 116.5352) (layer F.SilkS))
  (gr_text 2.12 (at 104.521 116.52758) (layer F.SilkS))
  (gr_text 2.37 (at 116.41836 99.09048) (layer F.SilkS))
  (gr_text 2.21 (at 100.40366 99.04222) (layer F.SilkS))
  (gr_text 2.33 (at 110.48492 99.06) (layer F.SilkS))
  (gr_text 2.31 (at 106.4641 99.06) (layer F.SilkS))
  (gr_text GND (at 102.44074 99.04222) (layer F.SilkS))
  (gr_text 2.32 (at 108.4834 99.04222) (layer F.SilkS))
  (gr_text 2.40 (at 120.4341 99.0727) (layer F.SilkS))
  (gr_text 2.39 (at 118.48084 99.10572) (layer F.SilkS))
  (gr_text 2.30 (at 104.45242 99.05238) (layer F.SilkS))
  (gr_text 2.43 (at 126.51994 99.0727) (layer F.SilkS))
  (gr_text 2.20 (at 96.49206 99.02444) (layer F.SilkS))
  (gr_text 2.14 (at 124.46762 99.09048) (layer F.SilkS))
  (gr_text 2.35 (at 114.44224 99.05238) (layer F.SilkS))
  (gr_text 2.15 (at 122.45086 99.09048) (layer F.SilkS))
  (gr_text 2.34 (at 112.41278 99.06) (layer F.SilkS))
  (gr_text 2.19 (at 98.49358 99.07016) (layer F.SilkS))
  (gr_text 2.25 (at 110.32998 94.18828) (layer F.SilkS))
  (gr_text 2.26 (at 108.40466 94.14256) (layer F.SilkS))
  (gr_text 2.24 (at 112.41024 94.14256) (layer F.SilkS))
  (gr_text 2.27 (at 106.4387 94.14256) (layer F.SilkS))
  (gr_text GND (at 100.41128 94.16796) (layer F.SilkS))
  (gr_text 2.36 (at 98.38182 94.17812) (layer F.SilkS))
  (gr_text 2.29 (at 104.48036 94.09938) (layer F.SilkS))
  (gr_text "2.22\n" (at 102.40264 94.12478) (layer F.SilkS))
  (gr_text 2.36 (at 96.42348 94.15526) (layer F.SilkS))
  (gr_text "2.24\n" (at 117.89842 77.91704) (layer F.SilkS))
  (gr_text "2.29\n" (at 117.94668 65.35674) (layer F.SilkS))
  (gr_text 2.28 (at 117.88826 67.91706) (layer F.SilkS))
  (gr_text 2.30 (at 117.9289 62.85992) (layer F.SilkS))
  (gr_text 2.35 (at 117.88064 50.11674) (layer F.SilkS))
  (gr_text 2.22 (at 117.86032 82.93608) (layer F.SilkS))
  (gr_text 2.23 (at 117.84 80.47736) (layer F.SilkS))
  (gr_text 2.31 (at 117.84 60.22086) (layer F.SilkS))
  (gr_text 2.25 (at 117.88064 75.42022) (layer F.SilkS))
  (gr_text 2.21 (at 117.84 85.52434) (layer F.SilkS))
  (gr_text 2.27 (at 117.90858 70.37578) (layer F.SilkS))
  (gr_text 2.26 (at 117.88826 72.96404) (layer F.SilkS))
  (gr_text 2.33 (at 117.84 55.17388) (layer F.SilkS))
  (gr_text "2.34\n" (at 117.89842 52.61356) (layer F.SilkS))
  (gr_text 2.32 (at 117.86032 57.6326) (layer F.SilkS))
  (gr_text "2.39\n" (at 117.94668 40.05326) (layer F.SilkS))
  (gr_text 2.38 (at 117.88826 42.61358) (layer F.SilkS))
  (gr_text 2.37 (at 117.90858 45.0723) (layer F.SilkS))
  (gr_text 2.40 (at 117.9289 37.55644) (layer F.SilkS))
  (gr_text 2.36 (at 117.88826 47.66056) (layer F.SilkS))
  (gr_text 2.41 (at 103.2731 88.66124) (layer F.SilkS))
  (gr_text 2.43 (at 108.48518 88.75522) (layer F.SilkS))
  (gr_text 2.42 (at 105.78008 88.72728) (layer F.SilkS))
  (gr_text 2.15 (at 93.74302 73.1266) (layer F.SilkS))
  (gr_text 2.07 (at 93.75318 52.77612) (layer F.SilkS))
  (gr_text 2.03 (at 93.74302 42.77614) (layer F.SilkS))
  (gr_text 2.14 (at 93.76334 70.53834) (layer F.SilkS))
  (gr_text 2.09 (at 93.71508 57.79516) (layer F.SilkS))
  (gr_text "2.04\n" (at 93.76334 45.23486) (layer F.SilkS))
  (gr_text 2.12 (at 93.80144 65.5193) (layer F.SilkS))
  (gr_text 2.17 (at 93.75318 78.0796) (layer F.SilkS))
  (gr_text 2.13 (at 93.74302 68.07962) (layer F.SilkS))
  (gr_text 2.06 (at 93.7354 50.2793) (layer F.SilkS))
  (gr_text 2.19 (at 93.71508 83.09864) (layer F.SilkS))
  (gr_text 2.08 (at 93.69476 55.33644) (layer F.SilkS))
  (gr_text "2.05\n" (at 93.74302 47.82312) (layer F.SilkS))
  (gr_text 2.16 (at 93.7354 75.58278) (layer F.SilkS))
  (gr_text 2.20 (at 93.69476 85.6869) (layer F.SilkS))
  (gr_text 2.01 (at 93.78366 37.719) (layer F.SilkS))
  (gr_text 2.11 (at 93.78366 63.02248) (layer F.SilkS))
  (gr_text 2.18 (at 93.69476 80.63992) (layer F.SilkS))
  (gr_text 2.10 (at 93.69476 60.38342) (layer F.SilkS))
  (gr_text "2.02\n" (at 93.80144 40.21582) (layer F.SilkS))
  (gr_text 1.17 (at 66.73342 85.51418) (layer F.SilkS))
  (gr_text 1.12 (at 66.78168 72.95388) (layer F.SilkS))
  (gr_text 1.13 (at 66.72326 75.5142) (layer F.SilkS))
  (gr_text 1.11 (at 66.7639 70.45706) (layer F.SilkS))
  (gr_text 1.06 (at 66.71564 57.71388) (layer F.SilkS))
  (gr_text 1.19 (at 66.69532 90.53322) (layer F.SilkS))
  (gr_text 1.18 (at 66.675 88.0745) (layer F.SilkS))
  (gr_text 1.10 (at 66.675 67.818) (layer F.SilkS))
  (gr_text 1.16 (at 66.71564 83.01736) (layer F.SilkS))
  (gr_text 1.20 (at 66.675 93.12148) (layer F.SilkS))
  (gr_text 1.14 (at 66.74358 77.97292) (layer F.SilkS))
  (gr_text 1.15 (at 66.72326 80.56118) (layer F.SilkS))
  (gr_text 1.08 (at 66.675 62.77102) (layer F.SilkS))
  (gr_text 1.07 (at 66.73342 60.2107) (layer F.SilkS))
  (gr_text 1.09 (at 66.69532 65.22974) (layer F.SilkS))
  (gr_text "1.02\n" (at 66.78168 47.6504) (layer F.SilkS))
  (gr_text 1.03 (at 66.72326 50.21072) (layer F.SilkS))
  (gr_text "1.04\n" (at 66.74358 52.66944) (layer F.SilkS))
  (gr_text 1.01 (at 66.7639 45.15358) (layer F.SilkS))
  (gr_text "1.05\n" (at 66.72326 55.2577) (layer F.SilkS))
  (gr_text 1.25 (at 91.55684 83.0834) (layer F.SilkS))
  (gr_text 1.21 (at 91.5162 93.18752) (layer F.SilkS))
  (gr_text 1.23 (at 91.5162 88.14054) (layer F.SilkS))
  (gr_text "1.24\n" (at 91.57462 85.58022) (layer F.SilkS))
  (gr_text 1.22 (at 91.53652 90.59926) (layer F.SilkS))
  (gr_text "1.29\n" (at 91.62288 73.01992) (layer F.SilkS))
  (gr_text 1.28 (at 91.56446 75.58024) (layer F.SilkS))
  (gr_text 1.27 (at 91.58478 78.03896) (layer F.SilkS))
  (gr_text 1.30 (at 91.6051 70.5231) (layer F.SilkS))
  (gr_text 1.26 (at 91.56446 80.62722) (layer F.SilkS))
  (gr_text "1.34\n" (at 91.57462 60.27674) (layer F.SilkS))
  (gr_text 1.33 (at 91.5162 62.83706) (layer F.SilkS))
  (gr_text 1.32 (at 91.53652 65.29578) (layer F.SilkS))
  (gr_text 1.35 (at 91.55684 57.77992) (layer F.SilkS))
  (gr_text 1.31 (at 91.5162 67.88404) (layer F.SilkS))
  (gr_text 1.06 (at 91.11234 109.55782) (layer F.SilkS))
  (gr_text 1.41 (at 75.09764 109.50956) (layer F.SilkS))
  (gr_text 1.09 (at 85.1789 109.52734) (layer F.SilkS))
  (gr_text 1.11 (at 81.15808 109.52734) (layer F.SilkS))
  (gr_text GND (at 77.13472 109.50956) (layer F.SilkS))
  (gr_text 1.10 (at 83.17738 109.50956) (layer F.SilkS))
  (gr_text 1.04 (at 95.12808 109.54004) (layer F.SilkS))
  (gr_text 1.05 (at 93.17482 109.57306) (layer F.SilkS))
  (gr_text 1.12 (at 79.1464 109.51972) (layer F.SilkS))
  (gr_text 1.01 (at 101.21392 109.54004) (layer F.SilkS))
  (gr_text 1.17 (at 71.18604 109.49178) (layer F.SilkS))
  (gr_text 1.02 (at 99.1616 109.55782) (layer F.SilkS))
  (gr_text 1.07 (at 89.13622 109.51972) (layer F.SilkS))
  (gr_text GND (at 97.14484 109.55782) (layer F.SilkS))
  (gr_text GND (at 87.10676 109.52734) (layer F.SilkS))
  (gr_text 1.16 (at 73.18756 109.5375) (layer F.SilkS))
  (gr_text 1.43 (at 101.06406 105.5878) (layer F.SilkS))
  (gr_text 1.14 (at 99.01174 105.60558) (layer F.SilkS))
  (gr_text 1.15 (at 96.99498 105.60558) (layer F.SilkS))
  (gr_text 1.40 (at 94.97822 105.5878) (layer F.SilkS))
  (gr_text 1.39 (at 93.02496 105.62082) (layer F.SilkS))
  (gr_text 1.37 (at 90.96248 105.60558) (layer F.SilkS))
  (gr_text 1.35 (at 88.98636 105.56748) (layer F.SilkS))
  (gr_text 1.34 (at 86.9569 105.5751) (layer F.SilkS))
  (gr_text 1.33 (at 85.02904 105.5751) (layer F.SilkS))
  (gr_text 1.32 (at 83.02752 105.55732) (layer F.SilkS))
  (gr_text 1.31 (at 81.00822 105.5751) (layer F.SilkS))
  (gr_text 1.30 (at 78.99654 105.56748) (layer F.SilkS))
  (gr_text GND (at 76.98486 105.55732) (layer F.SilkS))
  (gr_text 1.21 (at 74.94778 105.55732) (layer F.SilkS))
  (gr_text 1.19 (at 73.0377 105.58526) (layer F.SilkS))
  (gr_text 1.20 (at 71.03618 105.53954) (layer F.SilkS))
  (gr_text 1.24 (at 86.9315 101.60254) (layer F.SilkS))
  (gr_text 1.25 (at 84.85124 101.64826) (layer F.SilkS))
  (gr_text 1.26 (at 82.92592 101.60254) (layer F.SilkS))
  (gr_text 1.27 (at 80.95996 101.60254) (layer F.SilkS))
  (gr_text 1.29 (at 79.00162 101.55936) (layer F.SilkS))
  (gr_text "1.22\n" (at 76.90104 101.5238) (layer F.SilkS))
  (gr_text GND (at 75.00112 101.55174) (layer F.SilkS))
  (gr_text 1.36 (at 72.97166 101.5619) (layer F.SilkS))
  (gr_text 1.36 (at 71.01332 101.53904) (layer F.SilkS))
  (gr_text 1.43 (at 82.09026 96.72066) (layer F.SilkS))
  (gr_text 1.42 (at 79.4258 96.7105) (layer F.SilkS))
  (gr_text 1.41 (at 76.91882 96.64446) (layer F.SilkS))
  (gr_text "1.39\n" (at 91.62288 47.71644) (layer F.SilkS))
  (gr_text 1.37 (at 91.58478 52.73548) (layer F.SilkS))
  (gr_text 1.38 (at 91.56446 50.27676) (layer F.SilkS))
  (gr_text 1.36 (at 91.56446 55.32374) (layer F.SilkS))
  (gr_text 1.40 (at 91.6051 45.21962) (layer F.SilkS))
  (gr_text "RIT SPEX Team Avionics Board - MSD P21103 Rev C" (at 112.57026 119.1387) (layer F.SilkS))
  (gr_circle (center 70.866 39.37) (end 74.168 39.37) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.528 121.92) (end 65.278 121.92) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 160.528 31.75) (end 160.528 121.92) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 65.278 31.75) (end 160.528 31.75) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 65.278 121.92) (end 65.278 31.75) (layer Edge.Cuts) (width 0.2032))
  (zone (net 4) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.094945 31.75) (xy 160.528 31.75) (xy 160.528 57.516123) (xy 160.5407 121.91238) (xy 160.528 121.912368)
        (xy 160.528 121.92) (xy 65.278 121.92) (xy 65.278 54.29123) (xy 65.27292 31.75508) (xy 65.278 31.75508)
        (xy 65.278 31.75) (xy 65.285621 31.75) (xy 65.28562 31.74746)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71.55942 36.12388) (xy 72.51446 36.50996) (xy 73.27646 37.11956) (xy 73.8124 37.846) (xy 74.15022 38.94582)
        (xy 74.09942 40.14724) (xy 73.53046 41.37406) (xy 72.83958 42.0243) (xy 71.54926 42.64406) (xy 70.2183 42.65422)
        (xy 69.12356 42.19702) (xy 68.36156 41.57726) (xy 67.7418 40.53078) (xy 67.56908 39.31412) (xy 67.7926 38.08476)
        (xy 68.48348 37.1094) (xy 69.215 36.4998) (xy 70.38086 36.08324)
      )
    )
  )
)
