(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.00508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "+48V")
  (net 4 "Net-(R2-Pad1)")
  (net 5 "Net-(R5-Pad1)")
  (net 6 "GND3")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(Q1-Pad1)")
  (net 9 "Net-(Q1-Pad3)")
  (net 10 "Net-(Q4-Pad3)")
  (net 11 "Net-(Q2-Pad3)")
  (net 12 "Net-(Q3-Pad1)")
  (net 13 "Net-(Q3-Pad3)")
  (net 14 "Net-(Q4-Pad1)")
  (net 15 "unconnected-(D3-Pad2)")
  (net 16 "unconnected-(U3-Pad3)")
  (net 17 "unconnected-(U4-Pad3)")
  (net 18 "unconnected-(D4-Pad2)")
  (net 19 "Net-(J3-Pad4)")
  (net 20 "Net-(J3-Pad5)")
  (net 21 "Net-(J1-Pad2)")
  (net 22 "Net-(D1-Pad1)")
  (net 23 "Net-(D1-Pad2)")
  (net 24 "Net-(D2-Pad1)")
  (net 25 "Net-(J2-Pad2)")
  (net 26 "Net-(U1-Pad4)")
  (net 27 "Net-(U1-Pad6)")
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 86.868 45.425)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q3" (at -3.788 0.505) (layer "F.SilkS"))
    (fp_text value "2N7002" (at 2.532 11.165 -180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 -0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(Q3-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 1.5 0) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(Q3-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HP-Chopper-Photocell-Driver:PinHeader_1x03_Corner_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 0)
    (at 74.735 41.955)
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.565 -0.585 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.15 -0.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+48V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -1.15 1.95) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 1.39 1.95) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0)
      (chamfer_ratio 0.2) (chamfer top_left top_right bottom_left bottom_right)
      (net 6 "GND3") (pinfunction "Pin_3") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.172 40.64 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at -0.428 2.18) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at -0.1 0.1) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 11 "Net-(Q2-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 25 "Net-(J2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.64 41.9 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -3.14 0.42) (layer "F.SilkS"))
    (fp_text value "R" (at 0.2 -2.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 4 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 10 "Net-(Q4-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.89 46.95)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at -0.56 -1.74 unlocked) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 21 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 9 "Net-(Q1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 78.83 52.19 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -2.81 -0.06) (layer "F.SilkS"))
    (fp_text value "47K" (at -5.81 -0.09) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 26 "Net-(U1-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 102.01 50.24 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 1.61 1.77) (layer "F.SilkS"))
    (fp_text value "BZX84-A5V1" (at -7.3 2.62) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -1.5 0.95 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(D3-Pad2)") (pintype "no_connect"))
    (pad "3" smd roundrect (at 1.5 0 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "K") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "H11F1:DIP762W46P254L889H508Q6" (layer "F.Cu")
    (tedit 62CCA2CD)
    (at 74.98 34.52 90)
    (property "MANUFACTURER" "ON Semiconductor")
    (property "PARTREV" "LTR")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 2.97 6.07) (layer "F.SilkS"))
    (fp_text value "H11F1" (at -0.5 -0.17) (layer "F.Fab"))
    (pad "" smd circle (at 3.81 0 90) (size 1.248 1.248) (layers "F.SilkS"))
    (pad "" smd circle (at 3.81 -2.54 90) (size 1.248 1.248) (layers "F.SilkS"))
    (pad "" smd circle (at 3.81 2.54 90) (size 1.248 1.248) (layers "F.SilkS"))
    (pad "1" thru_hole rect (at -3.81 -2.54 90) (size 1.248 1.248) (drill 0.74) (layers *.Cu *.Mask)
      (net 3 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.81 0 90) (size 1.248 1.248) (drill 0.74) (layers *.Cu *.Mask)
      (net 4 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "3" thru_hole circle (at -3.81 2.54 90) (size 1.248 1.248) (drill 0.74) (layers *.Cu *.Mask)
      (net 17 "unconnected-(U4-Pad3)") (pintype "no_connect"))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 72.42 54.52 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 3.34 0.05) (layer "F.SilkS"))
    (fp_text value "1/25" (at 4.56 -1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 270) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 66.13 47.08 -90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q4" (at 1.81 1.99 unlocked) (layer "F.SilkS"))
    (fp_text value "2N7002" (at 0 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 -0.95 270) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(Q4-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -1.5 0.95 270) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 1.5 0 270) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(Q4-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 52.6 48.88)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J21" (at -3.16 -0.01 -180) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 75.79 54.11 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0.11 -1.65) (layer "F.SilkS"))
    (fp_text value "100R" (at 0.27 -3.07) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 20 "Net-(J3-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 27 "Net-(U1-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Left" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 87.555 38.995 90)
    (descr "surface-mounted straight pin header, 1x05, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x05 2.54mm single row style1 pin1 left")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at -9.42 -4.12) (layer "F.SilkS"))
    (fp_text value "ICSP/CAL" (at -9.47 2.01) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.655 -5.08 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1-Pad4)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.655 -2.54 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -1.655 0 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.655 2.54 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at -1.655 5.08 90) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(J3-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical_SMD_Pin1Left.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 75.692 48.514 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0.324 2.872) (layer "F.SilkS"))
    (fp_text value "2N7002" (at 0 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(Q1-Pad1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 1.5 0 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(Q1-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_PLCC_2835_Handsoldering" (layer "F.Cu")
    (tedit 5C65228D)
    (at 52.41 52.01 180)
    (descr "https://www.luckylight.cn/media/component/data-sheet/R2835BC-B2M-M10.pdf")
    (tags "LED")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 3.914637 1.075363) (layer "F.SilkS"))
    (fp_text value "LED" (at -3.994637 0.844637) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.05 0 180) (size 2.5 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.525 0 180) (size 1.55 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_PLCC_2835.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 53.2 39.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J12" (at 3.24 -0.87 -180) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 82.67 55.36 180)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "BZX84-B12V" (at -5.8 -3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(D4-Pad2)") (pintype "no_connect"))
    (pad "3" smd rect (at 1.5 0 180) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(U1-Pad4)") (pinfunction "K") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 68.335 53.683721 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 2.845 4.56) (layer "F.SilkS"))
    (fp_text value "PIC12F752-ISN" (at 5.076279 2.915) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(Q3-Pad1)") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(Q4-Pad1)") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(U1-Pad4)") (pinfunction "GP3") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(Q1-Pad1)") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1-Pad6)") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J3-Pad4)") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 53.08 55.12)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J22" (at 3.24 -0.87 -180) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "H11F1:DIP762W46P254L889H508Q6" (layer "F.Cu")
    (tedit 62CCA2CD)
    (at 99.6 34.46 90)
    (property "MANUFACTURER" "ON Semiconductor")
    (property "PARTREV" "LTR")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 2.91 -6.12) (layer "F.SilkS"))
    (fp_text value "H11F1" (at -0.48 0.17) (layer "F.Fab"))
    (pad "" smd circle (at 3.81 0 90) (size 1.248 1.248) (layers "F.SilkS"))
    (pad "" smd circle (at 3.81 -2.54 90) (size 1.248 1.248) (layers "F.SilkS"))
    (pad "" smd circle (at 3.81 2.54 90) (size 1.248 1.248) (layers "F.SilkS"))
    (pad "1" thru_hole rect (at -3.81 -2.54 90) (size 1.248 1.248) (drill 0.74) (layers *.Cu *.Mask)
      (net 3 "+48V") (pintype "passive"))
    (pad "2" thru_hole circle (at -3.81 0 90) (size 1.248 1.248) (drill 0.74) (layers *.Cu *.Mask)
      (net 5 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "3" thru_hole circle (at -3.81 2.54 90) (size 1.248 1.248) (drill 0.74) (layers *.Cu *.Mask)
      (net 16 "unconnected-(U3-Pad3)") (pintype "no_connect"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 50.44 39.31)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J13" (at -2.17 -2.06) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2) (chamfer top_left top_right bottom_right)
      (net 6 "GND3") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 50.32 55.12)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J23" (at -2.17 -2.06) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2) (chamfer top_left top_right bottom_right)
      (net 6 "GND3") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_PLCC_2835_Handsoldering" (layer "F.Cu")
    (tedit 5C65228D)
    (at 52.53 36.2 180)
    (descr "https://www.luckylight.cn/media/component/data-sheet/R2835BC-B2M-M10.pdf")
    (tags "LED")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 3.914637 1.075363) (layer "F.SilkS"))
    (fp_text value "LED" (at -3.994637 0.844637) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.05 0 180) (size 2.5 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.525 0 180) (size 1.55 2.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_PLCC_2835.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 105.918 44.958 90)
    (descr "SOT-23, Handsoldering")
    (tags "SOT-23")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 1.668 2.022) (layer "F.SilkS"))
    (fp_text value "2N7002" (at 0 2.5 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 -0.95 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(J3-Pad4)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -1.5 0.95 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 1.5 0 90) (size 1.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(Q2-Pad3)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 78.82 55.35 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 2.53 0.06) (layer "F.SilkS"))
    (fp_text value "10n" (at 3.73 0.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 20 "Net-(J3-Pad5)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.552 50.546 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.136 2.062) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.82 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 3 "+48V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 1 "+5V") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HP-Chopper-Photocell-Driver:PinHeader_1x03_Corner_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 0)
    (at 100.065 41.955)
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.255 -0.695 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x03" (at 0 1 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.15 -0.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+48V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -1.15 1.95) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole roundrect (at 1.39 1.95) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.2) (chamfer top_left top_right bottom_right)
      (net 6 "GND3") (pinfunction "Pin_3") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 94.488 45.37 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.458 1.95) (layer "F.SilkS"))
    (fp_text value "R" (at 1.16 -3 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 5 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 13 "Net-(Q3-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Left" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 66.04 40.03)
    (descr "surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x03 2.54mm single row style1 pin1 left")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J4" (at 2.286 -3.2 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "+" (at 2.15 1.5 -90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.655 -2.54) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "GND3") (pinfunction "Pin_1") (pintype "power_out"))
    (pad "2" smd rect (at 1.655 0) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+48V") (pinfunction "Pin_2") (pintype "power_out"))
    (pad "3" smd roundrect (at -1.655 2.54) (size 2.51 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical_SMD_Pin1Left.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 52.72 33.07)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "HP-Chopper-Photocell-Driver.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at -3.16 -0.01 -180) (layer "F.SilkS"))
    (fp_text value "Conn_01x01" (at 0 2.33) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(D1-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 107.16 32.78) (end 107.16 29.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 90.54 29.8) (end 107.16 29.8) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 52.694637 36.195363) (end 58.794637 36.195363) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_arc (start 110.25 55.59) (mid 107.25 52.59) (end 110.25 49.59) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 90.54 32.58) (mid 87.54 35.58) (end 84.54 32.58) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 67.83 32.71) (mid 66.95132 34.83132) (end 64.83 35.71) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 84.54 32.58) (end 84.54 29.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.16 35.78) (end 113 35.78) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 90.54 32.58) (end 90.54 29.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113 59.8) (end 62 59.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 64.83 35.71) (end 62 35.71) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 110.16 35.78) (mid 108.03868 34.90132) (end 107.16 32.78) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 67.83 29.8) (end 84.54 29.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.25 49.59) (end 113 49.59) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 62 59.8) (end 62 35.71) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113 35.78) (end 113 49.59) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 67.83 32.71) (end 67.83 29.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113 55.59) (end 113 59.8) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 52.574637 52.005363) (end 58.674637 52.005363) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_line (start 110.25 55.59) (end 113 55.59) (layer "Edge.Cuts") (width 0.1))
  (gr_text "HP Photocell Chopper Driver V1.2\nDavid Wise, 2022\nCC-BY-SA" (at 83.73 53.34) (layer "B.SilkS"))
  (gr_text "POT" (at 92.73 50.55 -90) (layer "F.SilkS"))
  (gr_text "PGD" (at 91.61 35.13 -90) (layer "F.SilkS"))
  (gr_text "GND" (at 87.51 42.76) (layer "F.SilkS"))
  (gr_text "BT" (at 82.3 50.01 -90) (layer "F.SilkS"))
  (gr_text "VCC" (at 83.18 35.08 -90) (layer "F.SilkS"))
  (gr_text "-" (at 63.39 44.52 -90) (layer "F.SilkS"))
  (gr_text "G" (at 63.23 39.29 -90) (layer "F.SilkS"))
  (gr_text "MCLR" (at 81.16 35.08 -90) (layer "F.SilkS"))
  (gr_text "PGC" (at 93.37 35.13 -90) (layer "F.SilkS"))
  (gr_text "U3&U4 pins 4-6\nair-wired off board" (at 87.13 27.92) (layer "Cmts.User"))
  (zone (net 6) (net_name "GND3") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 55.21 47.85)
        (xy 56.5 49.25)
        (xy 57.28 51.05)
        (xy 57.35 52.54)
        (xy 56.7 54.37)
        (xy 55.71 55.58)
        (xy 54.08 56.46)
        (xy 52 56.42)
        (xy 49.82 56.06)
        (xy 48.55 54.82)
        (xy 47.93 53.19)
        (xy 47.86 51.11)
        (xy 48.97 48.78)
        (xy 50.44 47.59)
        (xy 51.9 47.19)
        (xy 53.47 47.18)
      )
    )
  )
  (zone (net 6) (net_name "GND3") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.29 26.14)
        (xy 113.91 63.01)
        (xy 60.94 61.03)
        (xy 59.97 25.28)
      )
    )
  )
  (zone (net 6) (net_name "GND3") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3) (island_removal_mode 2) (island_area_min 10))
    (polygon
      (pts
        (xy 55.33 32.04)
        (xy 56.62 33.44)
        (xy 57.4 35.24)
        (xy 57.47 36.73)
        (xy 56.82 38.56)
        (xy 55.83 39.77)
        (xy 54.2 40.65)
        (xy 52.12 40.61)
        (xy 49.94 40.25)
        (xy 48.67 39.01)
        (xy 48.05 37.38)
        (xy 47.98 35.3)
        (xy 49.09 32.97)
        (xy 50.56 31.78)
        (xy 52.02 31.38)
        (xy 53.59 31.37)
      )
    )
  )
  (zone (net 6) (net_name "GND3") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.26 60.94)
        (xy 61.13 60.59)
        (xy 60.91 28.69)
        (xy 113.83 28.39)
      )
    )
  )
)
