(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Spectrum Analyzer: IF and Log Amp")
    (date "2022-06-17")
    (rev "0.0")
    (company "Andy McCann KA3KAF and Doug McCann KA3KAG")
    (comment 2 "Wes Hayward W7ZOI")
    (comment 3 "Original Design By:")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 95.3516 129.1844)
    (pcbplotparams
      (layerselection 0x0000020_7ffffffe)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits false)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 3)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C304-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C305-Pad1)")
  (net 4 "Net-(C305-Pad2)")
  (net 5 "Net-(C306-Pad1)")
  (net 6 "Net-(C307-Pad1)")
  (net 7 "Net-(C308-Pad1)")
  (net 8 "+5")
  (net 9 "Net-(C310-Pad1)")
  (net 10 "Net-(C311-Pad1)")
  (net 11 "Net-(C312-Pad2)")
  (net 12 "+10")
  (net 13 "Net-(C314-Pad1)")
  (net 14 "Net-(C314-Pad2)")
  (net 15 "Net-(C317-Pad2)")
  (net 16 "Net-(C318-Pad1)")
  (net 17 "Net-(C319-Pad1)")
  (net 18 "Net-(C320-Pad2)")
  (net 19 "Net-(C321-Pad1)")
  (net 20 "Net-(C322-Pad2)")
  (net 21 "Net-(C301-Pad3)")
  (net 22 "Net-(C303-Pad3)")
  (net 23 "+15")
  (net 24 "Net-(R313-Pad1)")
  (net 25 "Net-(R314-Pad2)")
  (net 26 "Net-(R315-Pad2)")
  (net 27 "Net-(R318-Pad1)")
  (net 28 "Net-(C324-Pad1)")
  (net 29 "Net-(R320-Pad1)")
  (net 30 "unconnected-(U304-Pad3)")
  (net 31 "unconnected-(U304-Pad5)")
  (net 32 "unconnected-(U305-Pad4)")
  (net 33 "unconnected-(U305-Pad5)")
  (net 34 "unconnected-(U305-Pad8)")
  (net 35 "Net-(C302-Pad3)")
  (net 36 "Net-(C323-Pad1)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 141.8336 96.6724 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R312" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "10" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "+10") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C312-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 156.3116 102.0064)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R317" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "+5") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C318-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 136.4996 119.5264)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L301" (at 0 -2.55) (layer "F.SilkS"))
    (fp_text value "1.05u" (at 0 8.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(C314-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.5676 101.7524 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R311" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "10" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "+15") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C310-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 121.5136 119.2784)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C305" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".01u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "Net-(C305-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(C305-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "if-log-amp:MOLEX_73391-0060" (layer "F.Cu")
    (tedit 62B0E504)
    (at 163.9316 123.0884)
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J306" (at -0.825265 -4.836565) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 6.06363 4.86791) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 36 "Net-(C323-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 -2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 -2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "4" thru_hole circle locked (at -2.54 2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle locked (at 2.54 2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/73391-0065.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/73391-0065.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "if-log-amp:AD603AQ" (layer "F.Cu")
    (tedit 0)
    (at 130.4036 105.5624)
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "if-log-amp-spice\\ad603a.cir")
    (property "Spice_Model" "AD603A")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U301" (at 4.0132 0.4572) (layer "F.SilkS"))
    (fp_text value "AD603AQ" (at 4.0132 5.0292 90) (layer "F.SilkS"))
    (fp_text user "*" (at 2.4892 -0.5588) (layer "F.SilkS"))
    (fp_text user "*" (at 1.7272 -0.5588) (layer "F.SilkS"))
    (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer "Cmts.User"))
    (fp_text user "0.3in/7.62mm" (at 3.81 -3.7465) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.06in/1.524mm" (at 10.668 0) (layer "Cmts.User"))
    (fp_text user "0.06in/1.524mm" (at 0 11.3665) (layer "Cmts.User"))
    (fp_text user "*" (at 0.127 0) (layer "F.Fab"))
    (fp_text user "*" (at 0.127 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(C307-Pad1)") (pinfunction "GPOS") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(C308-Pad1)") (pinfunction "GNEG") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 "Net-(C305-Pad2)") (pinfunction "VINP") (pintype "passive"))
    (pad "4" thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(C306-Pad1)") (pinfunction "COMM") (pintype "passive"))
    (pad "5" thru_hole circle (at 7.62 7.62) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(C311-Pad1)") (pinfunction "FDBK") (pintype "passive"))
    (pad "6" thru_hole circle (at 7.62 5.08) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "VNEG") (pintype "power_in"))
    (pad "7" thru_hole circle (at 7.62 2.54) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 24 "Net-(R313-Pad1)") (pinfunction "VOUT") (pintype "passive"))
    (pad "8" thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(C312-Pad2)") (pinfunction "VPOS") (pintype "power_in"))
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/AD603AQ.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 147.6876 114.4524)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C314" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value "5.6p" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 "Net-(C314-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 "Net-(C314-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "if-log-amp:MOLEX_73391-0060" (layer "F.Cu")
    (tedit 62B0E504)
    (at 107.7976 109.6264)
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_Coaxial")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J301" (at -0.825265 -4.836565) (layer "F.SilkS"))
    (fp_text value "Conn_Coaxial" (at 6.06363 4.86791) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(C305-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 -2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 -2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "4" thru_hole circle locked (at -2.54 2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (pad "5" thru_hole circle locked (at 2.54 2.54) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/73391-0065.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/73391-0065.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 121.7422 113.8174 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R309" (at 3.937 0.0134 90) (layer "F.SilkS"))
    (fp_text value "4.3k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C308-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "+10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 117.7036 116.9924 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R303" (at 3.4798 -0.0642 90) (layer "F.SilkS"))
    (fp_text value "100" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C305-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 117.1956 100.9904 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R308" (at 3.8608 -0.127) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C307-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C302-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 99.4156 125.3744)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H301" (at 0 -2.794) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 121.7676 102.0064)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C307" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(C307-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 175.6156 120.8024)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C322" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 20 "Net-(C322-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 153.0096 107.5944)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C318" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 "Net-(C318-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 141.3256 108.1024)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R313" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R313-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C314-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 156.0576 91.0844 180)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "if-log-amp-spice\\fairch.lib")
    (property "Spice_Model" "1N4152")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "D")
    (attr through_hole)
    (fp_text reference "D301" (at 3.81 -2.12) (layer "F.SilkS"))
    (fp_text value "1N4152" (at 3.81 2.12) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C319-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "+10") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "if-log-amp:GKG60015" (layer "F.Cu")
    (tedit 0)
    (at 150.8191 120.8024)
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C315" (at 2.54 -2.032) (layer "F.SilkS"))
    (fp_text value "12-60p" (at 2.6985 2.286) (layer "F.SilkS"))
    (fp_text user "*" (at 1.9365 0.508) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 14 "Net-(C314-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.08 0) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWire-0.15sqmm_1x02_P4mm_D0.5mm_OD1.5mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 97.1296 112.6744)
    (descr "Soldered wire connection, for 2 times 0.15 mm² wires, basic insulation, conductor diameter 0.5mm, outer diameter 1.5mm, size source Multi-Contact FLEXI-E 0.15 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.15sqmm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J303" (at 2 -2.05) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(C302-Pad3)") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWire-0.15sqmm_1x02_P4mm_D0.5mm_OD1.5mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 97.1296 103.5304)
    (descr "Soldered wire connection, for 2 times 0.15 mm² wires, basic insulation, conductor diameter 0.5mm, outer diameter 1.5mm, size source Multi-Contact FLEXI-E 0.15 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.15sqmm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J302" (at 2 -2.05) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(C301-Pad3)") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 145.8976 121.0564)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C316" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value "180p" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 "Net-(C314-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 100.4316 118.9595 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C304" (at 1.25 -3.75 90) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.25 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C304-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "if-log-amp:CA3140EZ" (layer "F.Cu")
    (tedit 0)
    (at 173.2661 107.0864)
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "if-log-amp-spice\\ca3140.sub")
    (property "Spice_Model" "ca3140")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U305" (at 4.1275 3.81) (layer "F.SilkS"))
    (fp_text value "CA3140" (at 4.1275 7) (layer "F.SilkS"))
    (fp_text user "*" (at 2.2987 -0.3048) (layer "F.SilkS"))
    (fp_text user "*" (at 1.5367 -0.3048) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.06in/1.524mm" (at 0 11.303) (layer "Cmts.User"))
    (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer "Cmts.User"))
    (fp_text user "0.025in/0.635mm" (at 11.303 0) (layer "Cmts.User"))
    (fp_text user "0.325in/8.255mm" (at 4.1275 -3.683) (layer "Cmts.User"))
    (fp_text user "*" (at 0.8255 0) (layer "F.Fab"))
    (fp_text user "*" (at 0.8255 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "NULL") (pintype "passive"))
    (pad "2" thru_hole rect (at 0 2.54) (size 1.524 0.635) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "Net-(R318-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole rect (at 0 5.08) (size 1.524 0.635) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "Net-(C321-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole rect (at 0 7.62) (size 1.524 0.635) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "unconnected-(U305-Pad4)") (pinfunction "V-") (pintype "power_in+no_connect"))
    (pad "5" thru_hole rect (at 8.255 7.62) (size 1.524 0.635) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "unconnected-(U305-Pad5)") (pinfunction "NULL") (pintype "passive+no_connect"))
    (pad "6" thru_hole rect (at 8.255 5.08) (size 1.524 0.635) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "Net-(R320-Pad1)") (pintype "output"))
    (pad "7" thru_hole rect (at 8.255 2.54) (size 1.524 0.635) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "Net-(C322-Pad2)") (pinfunction "V+") (pintype "power_in"))
    (pad "8" thru_hole rect (at 8.255 0) (size 1.524 0.635) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "unconnected-(U305-Pad8)") (pinfunction "STRB") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/CA3104.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 99.4156 84.4804)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H302" (at 0 3.302) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 183.4896 98.1964 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R320" (at 3.8862 -0.1524) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R320-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R318-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 105.2576 123.8504)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R307" (at 3.6322 -0.0762) (layer "F.SilkS"))
    (fp_text value "51" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C304-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C306-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "if-log-amp:AD8307AN" (layer "F.Cu")
    (tedit 0)
    (at 165.4556 113.9444 180)
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "R")
    (attr through_hole)
    (fp_text reference "U304" (at 3.8608 7.6708) (layer "F.SilkS"))
    (fp_text value "AD8307AN" (at 3.81 2.5908 90) (layer "F.SilkS"))
    (fp_text user "*" (at 1.3208 -0.9652) (layer "F.SilkS"))
    (fp_text user "*" (at 1.3208 -0.2032) (layer "F.SilkS"))
    (fp_text user "0.06in/1.524mm" (at 0 11.303) (layer "Cmts.User"))
    (fp_text user "0.06in/1.524mm" (at 10.668 0) (layer "Cmts.User"))
    (fp_text user "0.3in/7.62mm" (at 3.81 -3.683) (layer "Cmts.User"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer "Cmts.User"))
    (fp_text user "*" (at 0.508 0) (layer "F.Fab"))
    (fp_text user "*" (at 0.508 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 "Net-(C320-Pad2)") (pinfunction "INM") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 2.54 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "COM") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 5.08 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "unconnected-(U304-Pad3)") (pinfunction "OFS") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at 0 7.62 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "Net-(C321-Pad1)") (pinfunction "OUT") (pintype "passive"))
    (pad "5" thru_hole circle (at 7.62 7.62 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "unconnected-(U304-Pad5)") (pinfunction "INT") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 7.62 5.08 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "Net-(C318-Pad1)") (pinfunction "ENB") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.62 2.54 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "Net-(C318-Pad1)") (pinfunction "VPS") (pintype "power_in"))
    (pad "8" thru_hole circle (at 7.62 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "Net-(C317-Pad2)") (pinfunction "INP") (pintype "passive"))
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/AD8307AN.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 168.5036 107.0864)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C321" (at 0.762 3.302) (layer "F.SilkS"))
    (fp_text value ".001u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 "Net-(C321-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 97.1296 97.4344)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R305" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "510" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C301-Pad3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C303-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 167.7536 102.2604)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C309" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 "+5") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.15sqmm_1x02_P4mm_D0.5mm_OD1.5mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 180.9496 119.5324)
    (descr "Soldered wire connection, for 2 times 0.15 mm² wires, basic insulation, conductor diameter 0.5mm, outer diameter 1.5mm, size source Multi-Contact FLEXI-E 0.15 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.15sqmm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J305" (at 2 -2.05) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(C324-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "if-log-amp:Potentiometer_Bourns_3386G_Vertical" (layer "F.Cu")
    (tedit 0)
    (at 165.4556 92.3544 90)
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "if-log-amp-spice\\Pot2.lib")
    (property "Spice_Model" "pot_lin2")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "RV302" (at 5.31 -5.7 90 unlocked) (layer "F.SilkS"))
    (fp_text value "100" (at 5.8 4.03 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.455 -2.765 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -0.315 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R315-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 9.845 -2.54 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -0.315 -5.08 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/30338-71600_ASM.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/if-log-amp-models/if-log-amp-3D/30338-71600_ASM.wrl"
      (offset (xyz 5.65 2.5 2.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 -90))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 168.2616 113.9444)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C320" (at 0.75 3.556) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 "Net-(C320-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 175.8696 94.3864)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R321" (at 3.81 -0.0508) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R320-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(C323-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 146.6596 85.2424)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R315" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1.5k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R314-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R315-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 142.8616 114.4524)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C311" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value "18u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(C311-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 105.2576 120.2944)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R302" (at 3.7338 0.254) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C304-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 121.3245 94.1324)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C313" (at 5.777112 -1.27) (layer "F.SilkS"))
    (fp_text value "22u" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "+10") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 125.6912 109.2962)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C308" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 "Net-(C308-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 173.8496 90.3224)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C310" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".22u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 "Net-(C310-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 184.7596 114.9604 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R319" (at 3.5052 -0.0508 90) (layer "F.SilkS"))
    (fp_text value "51" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(C322-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C324-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 105.5116 116.4844)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R301" (at 3.81 0.0762) (layer "F.SilkS"))
    (fp_text value "2.2k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "+10") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C304-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 183.2356 125.3744)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H304" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 137.0196 101.4984)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C312" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 "Net-(C312-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 158.8516 98.0484)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "if-log-amp-spice\\78L05_TEST.sub")
    (property "Spice_Model" "X78L05")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "3 2 1")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U302" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "L78L05_TO92" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "+5") (pinfunction "VO") (pintype "power_out"))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 "Net-(C310-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 117.7036 106.3244 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R310" (at 3.81 -0.0134 90) (layer "F.SilkS"))
    (fp_text value "5.6k" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C308-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 121.5256 125.8824)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C306" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 "Net-(C306-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 170.2816 91.3384 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R316" (at 3.7846 -0.0762 90) (layer "F.SilkS"))
    (fp_text value "10" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.506 -0.022 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "+15") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C319-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 96.8756 93.3704)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R304" (at 4.064 0) (layer "F.SilkS"))
    (fp_text value "680" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "+10") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(C301-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 183.2356 84.4804)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H303" (at 0 4.826) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 145.6556 99.4664)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C319" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value ".1u" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 "Net-(C319-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.15sqmm_1x02_P4mm_D0.5mm_OD1.5mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 97.1296 108.1024)
    (descr "Soldered wire connection, for 2 times 0.15 mm² wires, basic insulation, conductor diameter 0.5mm, outer diameter 1.5mm, size source Multi-Contact FLEXI-E 0.15 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.15sqmm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J304" (at 2 -2.05) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 2 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(C303-Pad3)") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWire-0.15sqmm_1x01_D0.5mm_OD1.5mm" (layer "F.Cu")
    (tedit 5EB70B42)
    (at 177.6476 84.7344)
    (descr "Soldered wire connection, for a single 0.15 mm² wire, basic insulation, conductor diameter 0.5mm, outer diameter 1.5mm, size source Multi-Contact FLEXI-E 0.15 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.15sqmm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J307" (at 0 -2.05) (layer "F.SilkS"))
    (fp_text value "Board to Box Ground" (at 0 2.05) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (tedit 5A1DD157)
    (at 142.5956 92.3544)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Lib_File" "if-log-amp-spice\\lm317.lib")
    (property "Spice_Model" "LM317TI")
    (property "Spice_Netlist_Enabled" "Y")
    (property "Spice_Node_Sequence" "3 1 2")
    (property "Spice_Primitive" "X")
    (attr through_hole)
    (fp_text reference "U303" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "LM317L_TO92" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 "Net-(R314-Pad2)") (pinfunction "ADJ") (pintype "input"))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 "+10") (pinfunction "VO") (pintype "power_out"))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 "Net-(C319-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Radial_D4.0mm_H5.0mm_P1.50mm" (layer "F.Cu")
    (tedit 5BC5C9B9)
    (at 153.0216 114.4524)
    (descr "C, Radial series, Radial, pin pitch=1.50mm, diameter=4mm, height=5mm, Non-Polar Electrolytic Capacitor")
    (tags "C Radial series Radial pin pitch 1.50mm diameter 4mm height 5mm Non-Polar Electrolytic Capacitor")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C317" (at 0.75 -3.25) (layer "F.SilkS"))
    (fp_text value "5.6p" (at 0.75 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 14 "Net-(C314-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 15 "Net-(C317-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Radial_D4.0mm_H5.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 142.8496 85.2424 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R314" (at 4.064 0) (layer "F.SilkS"))
    (fp_text value "220" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "+10") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R314-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 109.8296 94.8944)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R306" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(C303-Pad3)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 175.8696 101.9048)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "if-and-log-amp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R318" (at 3.8608 0) (layer "F.SilkS"))
    (fp_text value "680" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R318-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 95.3516 84.622991) (mid 96.583682 81.648482) (end 99.558191 80.4164) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 187.0456 125.195725) (mid 185.877344 128.016144) (end 183.056925 129.1844) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 99.903961 129.1844) (mid 96.684956 127.851044) (end 95.3516 124.632039) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 187.0456 125.195725) (end 187.0456 84.926181) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 99.903961 129.1844) (end 183.056925 129.1844) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 95.3516 84.622991) (end 95.3516 124.632039) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 182.535819 80.4164) (mid 185.724716 81.737284) (end 187.0456 84.926181) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 182.535819 80.4164) (end 99.558191 80.4164) (layer "Edge.Cuts") (width 0.16))
  (gr_text "Spectrum Analyzer\nIF and Log Amp Board Rev 0.0\n\nAndy McCann KA3KAF\nDoug McCann KA3KAG" (at 116.1796 85.7504) (layer "F.SilkS"))
  (gr_text "Box to \nBrd GND" (at 174.3456 84.4804) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.0296 81.9404)
        (xy 187.0456 84.2264)
        (xy 187.0456 125.3744)
        (xy 183.9976 129.1844)
        (xy 99.6696 129.1844)
        (xy 96.8756 127.9144)
        (xy 95.3516 125.6284)
        (xy 95.3516 84.2264)
        (xy 96.8756 81.4324)
        (xy 99.9236 80.4164)
        (xy 182.4736 80.4164)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.5216 81.6864)
        (xy 187.0456 84.2264)
        (xy 187.0456 125.6284)
        (xy 186.0296 127.6604)
        (xy 183.9976 129.1844)
        (xy 99.9236 129.1844)
        (xy 96.3676 127.6604)
        (xy 95.3516 124.8664)
        (xy 96.3676 81.9404)
        (xy 99.4156 80.4164)
        (xy 183.2356 80.4164)
      )
    )
  )
)
