(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Beetje 32U4 Blok")
    (date "2018-08-10")
    (rev "0.0")
    (company "www.MakersBox.us")
    (comment 1 "648.ken@gmail.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "/10")
  (net 2 "/04")
  (net 3 "/05")
  (net 4 "/06")
  (net 5 "/07")
  (net 6 "/08")
  (net 7 "/09")
  (net 8 "/11")
  (net 9 "/12")
  (net 10 "/18")
  (net 11 "/19")
  (net 12 "/20")
  (net 13 "/03")
  (net 14 "GND")
  (net 15 "+5V")
  (net 16 "/LED1")
  (net 17 "Net-(D1-Pad1)")
  (net 18 "Net-(D2-Pad1)")
  (net 19 "Net-(D5-Pad1)")
  (net 20 "unconnected-(U1-Pad7)")
  (net 21 "unconnected-(X2-Pad6)")
  (net 22 "Net-(D3-Pad1)")
  (net 23 "/VSS")
  (net 24 "/02")
  (net 25 "/13")
  (net 26 "/14")
  (net 27 "/15")
  (net 28 "/16")
  (net 29 "/17")
  (net 30 "/SCL")
  (net 31 "/SDA")
  (net 32 "+12V")
  (net 33 "/PWM")
  (net 34 "/TACH")
  (net 35 "/DETECT")
  (net 36 "Net-(D4-Pad1)")
  (net 37 "Net-(A0-Pad1)")
  (net 38 "Net-(JUMP1-Pad2)")
  (net 39 "Net-(JUMP2-Pad2)")
  (footprint "footprints:MEC8-113-CARD_2" locked (layer "F.Cu")
    (tedit 637EA67F)
    (at 0 -0.1 90)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X0" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer "F.Fab"))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 50.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start -1 47.5) (end -1 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 9.4 6.5) (mid 8.692893 6.207107) (end 8.4 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 17 0) (mid 17.353553 0.146447) (end 17.5 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 8.5 51.5) (mid 10 50) (end 11.5 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 5.5) (mid 10.507107 6.207107) (end 9.8 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start -1 7.5) (mid -0.707107 6.792893) (end 0 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 7.9 0) (mid 8.253553 0.146447) (end 8.4 0.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 20 6.5) (mid 20.707107 6.792893) (end 21 7.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 21 50.5) (mid 20.707107 51.207107) (end 20 51.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 5.5) (mid 2.207107 6.207107) (end 1.5 6.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 18.5 6.5) (mid 17.792893 6.207107) (end 17.5 5.5) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 10.8 0.5) (mid 10.946447 0.146447) (end 11.3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 2.5 0.5) (mid 2.646447 0.146447) (end 3 0) (layer "Edge.Cuts") (width 0.12))
    (fp_arc (start 0 51.5) (mid -0.707107 51.207107) (end -1 50.5) (layer "Edge.Cuts") (width 0.12))
    (pad "1" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/LED1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "/10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "/PWM") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/TACH") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "+5V") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at 3.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/11") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at 4.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/12") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at 5.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "/13") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at 6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/14") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at 6.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "/15") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at 7.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/16") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect locked (at 11.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/17") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at 12.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/18") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at 13.2 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/19") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at 14 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/20") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at 14.8 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SCL") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect locked (at 15.6 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/SDA") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect locked (at 16.4 2.25 90) (size 0.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "Pin_26") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 18.669 -4.445 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -2.225 0) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 0.011 1.484 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 12.5 -2.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "0" (at -1.47 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "/VSS") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D5-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 46.322 -17.526)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at -1.905 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(D2-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Ultrafit2P" (layer "F.Cu")
    (tedit 6464F1C5)
    (at 13.75 -9.5 180)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 4.5 -1.75 180) (layer "F.SilkS") hide)
    (fp_text value "12V!" (at 1.304 4.978 180) (layer "F.SilkS"))
    (fp_text user "1723101102" (at 1.749984 -15.36 180) (layer "F.SilkS") hide)
    (fp_text user "ULTRAFIT_RA_HEADER,_SINGLE_ROW_-2_CKT" (at 1.749984 -12.82 180) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer "Cmts.User"))
    (fp_text user "ULTRAFIT_RA_HEADER,_SINGLE_ROW_-2_CKT" (at 1.749984 -12.82 180) (layer "F.Fab"))
    (fp_text user "1723101102" (at 1.749984 -15.36 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 1.75 7.91 180) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.52 1.52) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 3.500001 0 180) (size 1.52 1.52) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "GND") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 12.2 -2.5 180)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -2.62) (layer "F.SilkS") hide)
    (fp_text value "0.1" (at -0.2625 -2.45) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -3.05 0 180) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 23 "/VSS") (pintype "passive"))
    (pad "2" smd roundrect locked (at 3.05 0 180) (size 1.4 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.178571)
      (net 19 "Net-(D5-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 23.25 -3.25 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 1.25 3.25) (layer "F.SilkS") hide)
    (fp_text value "INA219AxD" (at -0.25 -3.25) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pinfunction "A1") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(A0-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "5" smd roundrect locked (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "+5V") (pinfunction "VS") (pintype "power_in"))
    (pad "6" smd roundrect locked (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/VSS") (pinfunction "IN-") (pintype "input"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(D5-Pad1)") (pinfunction "IN+") (pintype "input"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:DFN-8-1EP_3x2mm" (layer "F.Cu")
    (tedit 638826C0)
    (at 40.5 -2)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -2.55 180) (layer "F.SilkS") hide)
    (fp_text value "24LC32" (at 0 2 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at -1.5 0 270) (layer "F.Fab"))
    (pad "" smd rect locked (at 0.325 0.375) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.325 -0.375) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at 0.325 -0.375) (size 0.5 0.6) (layers "F.Paste"))
    (pad "" smd rect locked (at -0.325 0.375) (size 0.5 0.6) (layers "F.Paste"))
    (pad "1" smd rect locked (at -1.45 -0.75) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(JUMP1-Pad2)") (pinfunction "A0") (pintype "input"))
    (pad "2" smd rect locked (at -1.45 -0.25) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(JUMP2-Pad2)") (pinfunction "A1") (pintype "input"))
    (pad "3" smd rect locked (at -1.45 0.25) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "A2") (pintype "input"))
    (pad "4" smd rect locked (at -1.45 0.75) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect locked (at 1.45 0.75) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "6" smd rect locked (at 1.45 0.25) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "7" smd rect locked (at 1.45 -0.25) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(U1-Pad7)") (pinfunction "WP") (pintype "input+no_connect"))
    (pad "8" smd rect locked (at 1.45 -0.75) (size 0.75 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "9" smd rect locked (at 0 0) (size 1.3 1.5) (layers "F.Cu" "F.Mask"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636E7B24)
    (at 23.2 -19.5 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "12V" (at 2.626 0 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "+12V") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 23.25 -17.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at -1.905 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(D4-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636E7B24)
    (at 46.322 -19.558 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "DET" (at -2.95 0 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/DETECT") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636E7B24)
    (at 37.884 -19.558 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "PWM" (at -3 0 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/LED1") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:Harwin_Gecko-G125-MVX0605L0X_2x03_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 647A57D0)
    (at 25.5 -11.5)
    (descr "Harwin Gecko Connector, 6 pins, dual row male, vertical entry, no latches, PN:G125-MVX0605L0X")
    (tags "connector harwin gecko")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X1" (at 1.5 -3) (layer "F.SilkS") hide)
    (fp_text value "Gecko 6P" (at 1 3) (layer "F.SilkS") hide)
    (fp_text user "G125-MV10605L0P" (at 1.75 -2.75 unlocked) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.25 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 23 "/VSS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.5 0) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/TACH") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 33 "/PWM") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 1.25 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 15 "+5V") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.5 -1.25) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 35 "/DETECT") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KIPRJMOD}/3D/G125-MV10605L0P.stp"
      (offset (xyz 1.25 0.6 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 37.858 -17.526)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at -1.905 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Harwin_Gecko-G125-FVX0605L0X_2x03_P1.25mm_Vertical" (layer "F.Cu")
    (tedit 6378182F)
    (at 40 -11.5 180)
    (descr "Harwin Gecko Connector, 6 pins, dual row female, vertical entry, PN:G125-FVX0605L0X")
    (tags "connector harwin gecko")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X2" (at 1 -2) (layer "F.SilkS") hide)
    (fp_text value "Gecko 6P" (at 5.072 -3.4) (layer "F.SilkS") hide)
    (fp_text user "G125-FV10605L0P" (at 1 -2.102) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 23 "/VSS") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.25 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 33 "/PWM") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.5 0 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 34 "/TACH") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 0 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 1.25 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 14 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.5 1.25 180) (size 0.95 0.95) (drill 0.55) (layers *.Cu *.Mask)
      (net 21 "unconnected-(X2-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3D/G125-FV10605L0P.stp"
      (offset (xyz 1 -0.5 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-128" (layer "F.Cu")
    (tedit 5D3216F4)
    (at 21.336 -7.874)
    (descr "D_SOD-128 (CFP5 SlimSMAW), https://assets.nexperia.com/documents/outline-drawing/SOD128.pdf")
    (tags "D_SOD-128")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 0) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2 0) (size 1.4 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2.2 0) (size 1.4 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-128.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-128" (layer "F.Cu")
    (tedit 5D3216F4)
    (at 19.558 -13.462 90)
    (descr "D_SOD-128 (CFP5 SlimSMAW), https://assets.nexperia.com/documents/outline-drawing/SOD128.pdf")
    (tags "D_SOD-128")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "D" (at 0 2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.2 0 90) (size 1.4 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 2.2 0 90) (size 1.4 2.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "+12V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-128.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 29.214 -5.08)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "A0" (at 1.774 0) (layer "F.SilkS"))
    (fp_text value "Jumper" (at 0 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(A0-Pad1)") (pinfunction "A") (pintype "passive") (clearance 0.1))
    (pad "2" smd rect (at 0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "B") (pintype "passive") (clearance 0.1))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 35.937 -5.08)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "JUMP1" (at 0 -1.25) (layer "F.SilkS") hide)
    (fp_text value "A1" (at -1.838 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "A") (pintype "passive") (clearance 0.1))
    (pad "2" smd rect (at 0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(JUMP1-Pad2)") (pinfunction "B") (pintype "passive") (clearance 0.1))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 29.222 -2.667)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at 2.147 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(A0-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 35.941 -1.016)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.159 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(JUMP2-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 35.941 -3.937)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "JUMP2" (at 0 -1.25) (layer "F.SilkS") hide)
    (fp_text value "A0" (at -1.778 0.127) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "A") (pintype "passive") (clearance 0.1))
    (pad "2" smd rect (at 0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(JUMP2-Pad2)") (pinfunction "B") (pintype "passive") (clearance 0.1))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 30.226 -17.526)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at -1.905 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D3-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 29.21 -1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.159 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 29.206 -3.937)
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "A1" (at 1.782 0) (layer "F.SilkS"))
    (fp_text value "Jumper" (at 0 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect (at -0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "A") (pintype "passive") (clearance 0.1))
    (pad "2" smd rect (at 0.25 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "B") (pintype "passive") (clearance 0.1))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636E7A48)
    (at 35.929 -2.667)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.147 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(JUMP1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636E7B24)
    (at 30.188 -19.558 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "project.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "5V" (at 2.07 0 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "ken.olsen@agilityrobotics.com" (at 27 -1.5) (layer "B.SilkS"))
  (gr_text "Rev 0.2\nOct 2023" (at 13.5 -1.25) (layer "B.SilkS"))
  (gr_text "Rapid Prototyping Card" (at 27 -3) (layer "B.SilkS"))
  (gr_text "Molex UltraFit\n1723101102" (at 12.3 -12.5) (layer "B.SilkS"))
  (gr_text "FAN TESTER" (at 32 -7.75) (layer "F.SilkS"))
)
