<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0.635" y1="-0.635" x2="28.575" y2="-0.635" width="0.4064" layer="20"/>
<wire x1="28.575" y1="-0.635" x2="28.575" y2="34.925" width="0.4064" layer="20"/>
<wire x1="28.575" y1="34.925" x2="0.635" y2="34.925" width="0.4064" layer="20"/>
<wire x1="0.635" y1="34.925" x2="0.635" y2="-0.635" width="0.4064" layer="20"/>
<text>-</text>
<text>+</text>
<text>-</text>
<text>104</text>
<text>104</text>
<text>10k</text>
<text>D:/Cool Pictures/Stencils/aviators.bmp</text>
<text>A0</text>
<text>A5</text>
<text>D9</text>
<text>D13</text>
<text>CDLA Custom Micro. Get REKD</text>
</plain>
<libraries>
<library name="fairchild-semic">
<packages>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt; 28-Pin Narrow PDIP</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="UM-5S">
<description>&lt;b&gt;Monolithic Crystal Filters&lt;/b&gt;&lt;p&gt;
Source: ECM Electronics Limited</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X03_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X04">
</package>
<package name="1X06">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="con-amp">
<packages>
<package name="1X2MTA">
<description>&lt;b&gt;AMP MTA connector&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$2" library="fairchild-semic" package="DIL28-3" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="crystal" package="UM-5S" value="">
<attribute name="VALUE"/>
</element>
<element name="E$4" library="rcl" package="C050-030X075" value="">
<attribute name="VALUE"/>
</element>
<element name="E$5" library="rcl" package="C050-030X075" value="">
<attribute name="VALUE"/>
</element>
<element name="E$6" library="SparkFun" package="1X03_LOCK_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="E$7" library="con-amp" package="1X2MTA" value="">
<attribute name="VALUE"/>
</element>
<element name="E$11" library="rcl" package="0207/5V" value="">
<attribute name="VALUE"/>
</element>
<element name="E$13" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="E$14" library="SparkFun" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="E$15" library="SparkFun" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="E$8" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="E$17" library="pinhead" package="2X02" value="">
<attribute name="VALUE"/>
</element>
<element name="E$1" library="SparkFun" package="1X05" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="E$6" pad="2"/>
<contactref element="E$7" pad="1"/>
<contactref element="E$3" pad="2"/>
<contactref element="E$4" pad="1"/>
<contactref element="E$2" pad="8"/>
<contactref element="E$2" pad="22"/>
<contactref element="E$17" pad="4"/>
<contactref element="E$17" pad="3"/>
<contactref element="E$13" pad="2"/>
<contactref element="E$13" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="E$5" pad="2"/>
<contactref element="E$13" pad="6"/>
</signal>
<signal name="S$4">
<contactref element="E$2" pad="2"/>
<contactref element="E$14" pad="5"/>
<contactref element="E$13" pad="4"/>
</signal>
<signal name="S$5">
<contactref element="E$14" pad="4"/>
<contactref element="E$2" pad="3"/>
<contactref element="E$13" pad="5"/>
</signal>
<signal name="S$6">
<contactref element="E$2" pad="4"/>
<contactref element="E$14" pad="3"/>
</signal>
<signal name="S$7">
<contactref element="E$14" pad="2"/>
<contactref element="E$2" pad="5"/>
</signal>
<signal name="S$8">
<contactref element="E$2" pad="6"/>
<contactref element="E$14" pad="1"/>
</signal>
<signal name="S$12">
<contactref element="E$2" pad="11"/>
<contactref element="E$15" pad="4"/>
</signal>
<signal name="S$13">
<contactref element="E$15" pad="3"/>
<contactref element="E$2" pad="12"/>
</signal>
<signal name="S$14">
<contactref element="E$2" pad="13"/>
<contactref element="E$15" pad="2"/>
</signal>
<signal name="S$15">
<contactref element="E$15" pad="1"/>
<contactref element="E$2" pad="14"/>
</signal>
<signal name="S$16">
<contactref element="E$2" pad="9"/>
<contactref element="E$3" pad="1"/>
</signal>
<signal name="S$17">
<contactref element="E$2" pad="10"/>
<contactref element="E$3" pad="3"/>
</signal>
<signal name="S$18">
<contactref element="E$8" pad="6"/>
<contactref element="E$2" pad="28"/>
</signal>
<signal name="S$19">
<contactref element="E$2" pad="27"/>
<contactref element="E$8" pad="5"/>
</signal>
<signal name="S$20">
<contactref element="E$8" pad="4"/>
<contactref element="E$2" pad="26"/>
</signal>
<signal name="S$21">
<contactref element="E$2" pad="25"/>
<contactref element="E$8" pad="3"/>
</signal>
<signal name="S$22">
<contactref element="E$8" pad="2"/>
<contactref element="E$2" pad="24"/>
</signal>
<signal name="S$23">
<contactref element="E$2" pad="23"/>
<contactref element="E$8" pad="1"/>
</signal>
<signal name="S$24">
<contactref element="E$13" pad="3"/>
<contactref element="E$6" pad="1"/>
<contactref element="E$4" pad="2"/>
<contactref element="E$2" pad="7"/>
<contactref element="E$2" pad="21"/>
<contactref element="E$2" pad="20"/>
<contactref element="E$17" pad="2"/>
<contactref element="E$17" pad="1"/>
<contactref element="E$11" pad="1"/>
</signal>
<signal name="S$11">
</signal>
<signal name="S$3">
<contactref element="E$2" pad="1"/>
<contactref element="E$11" pad="2"/>
<contactref element="E$5" pad="1"/>
</signal>
<signal name="S$28">
</signal>
<signal name="S$29">
</signal>
<signal name="S$9">
<contactref element="E$6" pad="3"/>
<contactref element="E$7" pad="2"/>
</signal>
<signal name="S$1">
<contactref element="E$1" pad="5"/>
<contactref element="E$2" pad="19"/>
</signal>
<signal name="S$10">
<contactref element="E$2" pad="18"/>
<contactref element="E$1" pad="4"/>
</signal>
<signal name="S$25">
<contactref element="E$1" pad="3"/>
<contactref element="E$2" pad="17"/>
</signal>
<signal name="S$26">
<contactref element="E$2" pad="16"/>
<contactref element="E$1" pad="2"/>
</signal>
<signal name="S$27">
<contactref element="E$1" pad="1"/>
<contactref element="E$2" pad="15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
