<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="-0.254" y1="0" x2="-0.254" y2="28.194" width="0.1524" layer="20"/>
<wire x1="-0.254" y1="28.194" x2="0" y2="28.448" width="0.1524" layer="20" curve="-90"/>
<wire x1="0" y1="28.448" x2="10.16" y2="28.448" width="0.1524" layer="20"/>
<wire x1="10.16" y1="28.448" x2="10.414" y2="28.194" width="0.1524" layer="20" curve="-90"/>
<wire x1="10.414" y1="28.194" x2="10.414" y2="23.114" width="0.1524" layer="20"/>
<wire x1="10.414" y1="23.114" x2="10.668" y2="22.86" width="0.1524" layer="20" curve="90"/>
<wire x1="10.668" y1="22.86" x2="22.606" y2="22.86" width="0.1524" layer="20"/>
<wire x1="22.606" y1="22.86" x2="22.86" y2="22.606" width="0.1524" layer="20" curve="-90"/>
<wire x1="22.86" y1="22.606" x2="22.86" y2="0" width="0.1524" layer="20"/>
<wire x1="22.86" y1="0" x2="22.606" y2="-0.254" width="0.1524" layer="20" curve="-90"/>
<wire x1="22.606" y1="-0.254" x2="0" y2="-0.254" width="0.1524" layer="20"/>
<wire x1="0" y1="-0.254" x2="-0.254" y2="0" width="0.1524" layer="20" curve="-90"/>
<text>TAG</text>
<text>UPS</text>
<text>3V3</text>
<text>GND</text>
<text>VCC</text>
<text>SW1</text>
<text>GEEKWORM
MONITOR 0.1</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
</packages>
</library>
<library name="xose">
<packages>
<package name="0805">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="2X4">
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="2X3EDGE">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="geekworm-monitor">
<description>Generated from &lt;b&gt;geekworm-monitor.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MICROBUILDER_CR1220-2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B2" library="geekworm-monitor" package="MICROBUILDER_CR1220-2" value="cr1220"/>
<element name="IC2" library="adafruit" package="SO16W" value="DS3231/SO"/>
<element name="Q2" library="xose" package="SOT23" value=""/>
<element name="R1" library="xose" package="0805" value="200"/>
<element name="IC1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
</element>
<element name="R4" library="xose" package="0805" value="10K"/>
<element name="R3" library="xose" package="0805" value="10K"/>
<element name="C1" library="xose" package="0805" value="100nF"/>
<element name="Q1" library="xose" package="SOT23" value=""/>
<element name="R2" library="xose" package="0805" value="200"/>
<element name="JP2" library="xose" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-11443"/>
</element>
<element name="JP1" library="xose" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-11443"/>
</element>
<element name="JP3" library="xose" package="2X4" value=""/>
<element name="J1" library="xose" package="2X3EDGE" value="ISP"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="Q2" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC2" pad="13"/>
<contactref element="B2" pad="-"/>
<contactref element="JP3" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="SW1">
<contactref element="Q2" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="MODE">
<contactref element="IC1" pad="5"/>
<contactref element="J1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="~IDLE">
<contactref element="IC1" pad="7"/>
<contactref element="JP3" pad="8"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="IC2" pad="15"/>
<contactref element="R4" pad="1"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="IC2" pad="16"/>
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VBAT">
<contactref element="IC2" pad="14"/>
<contactref element="B2" pad="+"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="J1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="IC1" pad="6"/>
<contactref element="IC2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="TAG">
<contactref element="R2" pad="1"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="5V">
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="JP2" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
