<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="26.6725" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="78.73" y2="0" width="0" layer="20"/>
<wire x1="78.73" y1="0" x2="80" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="80" y1="1.27" x2="80" y2="26.672409375" width="0" layer="20"/>
<wire x1="80" y1="26.672409375" x2="78.729909375" y2="27.942409375" width="0" layer="20" curve="90.004089"/>
<wire x1="78.729909375" y1="27.942409375" x2="44.45" y2="27.94" width="0" layer="20"/>
<wire x1="35.5625" y1="27.9425" x2="1.27" y2="27.9425" width="0" layer="20"/>
<wire x1="1.27" y1="27.9425" x2="0" y2="26.6725" width="0" layer="20" curve="90"/>
<text>VCO II</text>
<wire x1="35.56" y1="27.94" x2="44.45" y2="27.94" width="0" layer="20" curve="-120.510237"/>
<text>v1.0</text>
<text>Advanced Electronic Musical Instrument Technology - since 1981 - Belgium</text>
</plain>
<libraries>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="416_Expander">
<description>Generated from &lt;b&gt;416_Expander.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="DIODE">
<description>1N4148</description>
</package>
<package name="TRIMMER-BOURNS-3296W-10T">
<description>Bourns 3296W series ~ top-adj, 10-t ~ straight pins</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline Package 16&lt;/b&gt;</description>
</package>
<package name="BEAD_0805">
<description>BEAD 0805</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR 0805&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="LOGO-AEMIT">
<description>Logo AEMIT</description>
</package>
<package name="POWER_10">
<description>10-p Eurorack supply connector</description>
</package>
<package name="CAP_ELCO_SMD_1UF">
<description>Elco Panasonic 1u, 10u</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR 0805&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="MH_3MM_SM">
<description>3mm mounting hole with small keepout perimeter</description>
</package>
<package name="PINHEAD_8P_MALE">
<description>Header 8-pins MALE (Preci-DIp)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="79L05" library="linear" package="TO92" value="79L05">
<attribute name="VALUE"/>
</element>
<element name="D2" library="416_Expander" package="DIODE" value="DIODE_TH"/>
<element name="C7" library="416_Expander" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="416_Expander" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="416_Expander" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="416_Expander" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="416_Expander" package="SO16" value="3340">
<attribute name="VALUE"/>
</element>
<element name="L1" library="416_Expander" package="BEAD_0805" value="BEADSMD"/>
<element name="L2" library="416_Expander" package="BEAD_0805" value="BEADSMD"/>
<element name="R1" library="416_Expander" package="R0805" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="416_Expander" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="416_Expander" package="R0805" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="416_Expander" package="R0805" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="416_Expander" package="R0805" value="1k8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="416_Expander" package="R0805" value="68k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="416_Expander" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="416_Expander" package="R0805" value="7k5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="416_Expander" package="R0805" value="120k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="416_Expander" package="R0805" value="36k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="416_Expander" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="416_Expander" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="416_Expander" package="R0805" value="1M2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="416_Expander" package="R0805" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="416_Expander" package="R0805" value="3k9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="416_Expander" package="R0805" value="220k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="416_Expander" package="R0805" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="416_Expander" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="416_Expander" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="416_Expander" package="R0805" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SCALE" library="416_Expander" package="TRIMMER-BOURNS-3296W-10T" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SUPPLY-IN" library="416_Expander" package="POWER_10" value="POWER_SIMPLE10"/>
<element name="U$1" library="416_Expander" package="LOGO-AEMIT" value="LOGO-AEMIT10MM"/>
<element name="HFT" library="416_Expander" package="TRIMMER-BOURNS-3296W-10T" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="416_Expander" package="R0805" value="1M2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="416_Expander" package="CAP_ELCO_SMD_1UF" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="416_Expander" package="CAP_ELCO_SMD_1UF" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="416_Expander" package="CAP_ELCO_SMD_1UF" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="416_Expander" package="CAP_ELCO_SMD_1UF" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="416_Expander" package="CAP_ELCO_SMD_1UF" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="416_Expander" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="416_Expander" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="416_Expander" package="SO08" value="TL072">
<attribute name="VALUE"/>
</element>
<element name="C12" library="416_Expander" package="C0805" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="416_Expander" package="C0805" value="1n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="416_Expander" package="MH_3MM_SM" value="MH-3MM_SM"/>
<element name="IC3" library="416_Expander" package="SO08" value="TL072">
<attribute name="VALUE"/>
</element>
<element name="C13" library="416_Expander" package="C0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="416_Expander" package="C0805" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="416_Expander" package="C0805" value="1n2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="416_Expander" package="C0805" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="416_Expander" package="C0805" value="10n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="416_Expander" package="PINHEAD_8P_MALE" value="PINHEAD_8_PRECIDIP_M"/>
<element name="H2" library="416_Expander" package="PINHEAD_8P_MALE" value="PINHEAD_8_PRECIDIP_M"/>
</elements>
<signals>
<signal name="AGND">
<contactref element="79L05" pad="1"/>
<contactref element="SUPPLY-IN" pad="3"/>
<contactref element="SUPPLY-IN" pad="4"/>
<contactref element="SUPPLY-IN" pad="5"/>
<contactref element="SUPPLY-IN" pad="6"/>
<contactref element="SUPPLY-IN" pad="7"/>
<contactref element="SUPPLY-IN" pad="8"/>
<contactref element="R8" pad="1"/>
<contactref element="IC1" pad="12"/>
<contactref element="R18" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="HFT" pad="3"/>
<contactref element="C16" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="5"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="H1" pad="2"/>
</signal>
<signal name="-12V">
<contactref element="L2" pad="P$2"/>
<contactref element="79L05" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="R20" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC3" pad="4"/>
<contactref element="H1" pad="1"/>
</signal>
<signal name="-5V">
<contactref element="79L05" pad="3"/>
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="SCALE" pad="3"/>
<contactref element="SCALE" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="H2" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="L1" pad="P$2"/>
<contactref element="IC1" pad="16"/>
<contactref element="R3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC3" pad="8"/>
<contactref element="H1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="SUPPLY-IN" pad="9"/>
<contactref element="SUPPLY-IN" pad="10"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="SUPPLY-IN" pad="1"/>
<contactref element="SUPPLY-IN" pad="2"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="N$36">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$48">
<contactref element="R6" pad="1"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="R15" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="PLS">
<contactref element="IC1" pad="4"/>
<contactref element="R13" pad="2"/>
<contactref element="H2" pad="8"/>
</signal>
<signal name="STIJG">
<contactref element="R10" pad="1"/>
<contactref element="H2" pad="6"/>
</signal>
<signal name="TRI">
<contactref element="R12" pad="2"/>
<contactref element="H2" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="6"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="HS">
<contactref element="R14" pad="2"/>
<contactref element="H1" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$19">
<contactref element="R17" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="SS">
<contactref element="R16" pad="2"/>
<contactref element="H1" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="D2" pad="C"/>
<contactref element="R18" pad="2"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="D2" pad="A"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="PWM">
<contactref element="R19" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="H1" pad="7"/>
</signal>
<signal name="N$24">
<contactref element="R21" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="C13" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R21" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="CV-SUM">
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="15"/>
<contactref element="R7" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="H1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="10"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R9" pad="2"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$11">
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="RANGE">
<contactref element="IC1" pad="11"/>
<contactref element="C18" pad="2"/>
<contactref element="H1" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="1"/>
<contactref element="HFT" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="7"/>
<contactref element="HFT" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="SCALE" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="C17" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
