(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 52)
    (no_connects 0)
    (area 80.660457 60.9126 153.019543 144.9274)
    (thickness 1.6)
    (drawings 6)
    (tracks 135)
    (zones 0)
    (modules 34)
    (nets 78)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +12V)
  (net 4 -12V)
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D4-Pad1)")
  (net 9 "Net-(D5-Pad2)")
  (net 10 "Net-(D6-Pad1)")
  (net 11 "Net-(J1-Pad9)")
  (net 12 "Net-(J1-Pad7)")
  (net 13 "Net-(J1-Pad5)")
  (net 14 "Net-(J1-Pad3)")
  (net 15 "Net-(J1-Pad1)")
  (net 16 "Net-(J2-Pad1)")
  (net 17 "Net-(Q1-Pad3)")
  (net 18 "Net-(Q2-Pad3)")
  (net 19 "Net-(R1-Pad1)")
  (net 20 +3V3)
  (net 21 "Net-(R2-Pad1)")
  (net 22 "Net-(R2-Pad2)")
  (net 23 "Net-(R3-Pad1)")
  (net 24 "Net-(R4-Pad1)")
  (net 25 "Net-(R6-Pad2)")
  (net 26 "Net-(R12-Pad2)")
  (net 27 "Net-(R11-Pad2)")
  (net 28 "Net-(RV1-Pad2)")
  (net 29 "Net-(U1-Pad17)")
  (net 30 "Net-(U1-Pad18)")
  (net 31 "Net-(U1-Pad19)")
  (net 32 "Net-(U1-Pad20)")
  (net 33 "Net-(U1-Pad16)")
  (net 34 "Net-(U1-Pad15)")
  (net 35 "Net-(U1-Pad14)")
  (net 36 "Net-(U1-Pad21)")
  (net 37 "Net-(U1-Pad22)")
  (net 38 "Net-(U1-Pad23)")
  (net 39 "Net-(U1-Pad24)")
  (net 40 "Net-(U1-Pad25)")
  (net 41 "Net-(U1-Pad26)")
  (net 42 "Net-(U1-Pad28)")
  (net 43 "Net-(U1-Pad29)")
  (net 44 "Net-(U1-Pad31)")
  (net 45 "Net-(U1-Pad32)")
  (net 46 "Net-(U1-Pad34)")
  (net 47 "Net-(U1-Pad35)")
  (net 48 "Net-(U1-Pad36)")
  (net 49 "Net-(U1-Pad37)")
  (net 50 "Net-(U1-Pad13)")
  (net 51 "Net-(U1-Pad12)")
  (net 52 "Net-(U1-Pad11)")
  (net 53 "Net-(U1-Pad10)")
  (net 54 "Net-(U1-Pad9)")
  (net 55 "Net-(U1-Pad8)")
  (net 56 "Net-(U1-Pad7)")
  (net 57 "Net-(U1-Pad6)")
  (net 58 "Net-(U1-Pad5)")
  (net 59 "Net-(U1-Pad4)")
  (net 60 "Net-(U1-Pad3)")
  (net 61 "Net-(U1-Pad2)")
  (net 62 "Net-(U1-Pad38)")
  (net 63 "Net-(U1-Pad39)")
  (net 64 "Net-(U1-Pad40)")
  (net 65 "Net-(U1-Pad41)")
  (net 66 "Net-(U1-Pad42)")
  (net 67 "Net-(U1-Pad43)")
  (net 68 "Net-(U1-Pad44)")
  (net 69 "Net-(U1-Pad45)")
  (net 70 "Net-(U1-Pad46)")
  (net 71 "Net-(U1-Pad47)")
  (net 72 "Net-(U1-Pad48)")
  (net 73 "Net-(U1-Pad49)")
  (net 74 "Net-(U1-Pad50)")
  (net 75 "Net-(U1-Pad51)")
  (net 76 "Net-(U1-Pad52)")
  (net 77 -12VA)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net +3V3)
    (add_net -12V)
    (add_net -12VA)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad44)")
    (add_net "Net-(U1-Pad45)")
    (add_net "Net-(U1-Pad46)")
    (add_net "Net-(U1-Pad47)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5A7CBB37)
    (at 95.25 107.95 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.46 90) (layer F.SilkS))
    (fp_text value 47uF (at 1.25 4.46 90) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A7CBA56)
    (at 121.92 86.36)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D4.7mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5A7CBA50)
    (at 114.3 86.36)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.56) (layer F.SilkS))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -12V))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBAC3)
    (at 138.43 77.47 270)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 3.81 -2.41 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBABF)
    (at 146.05 85.09 90)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 3.81 -2.41 90) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CB9B0)
    (at 124.46 82.55 90)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at 3.81 -2.41 90) (layer F.SilkS))
    (fp_text value D_Zener (at 3.81 2.41 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 114.3 74.93 270)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D4 (at 3.81 -2.41 270) (layer F.SilkS))
    (fp_text value D_Zener (at 3.81 2.41 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 -12V))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CB982)
    (at 99.06 85.09 90)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D5 (at 3.81 -2.41 90) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CB985)
    (at 106.68 77.47 270)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D6 (at 3.81 -2.41 270) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41 270) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module euro_parts:Euro_Header_10-pin_TH (layer F.Cu) (tedit 5A7CB9D8)
    (at 119.38 68.58 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at -3.56 -3.19 540) (layer F.SilkS) hide)
    (fp_text value Conn_02x05_Odd_Even (at -3.937 1.397 360) (layer F.SilkS) hide)
    (fp_text user -12V (at -4.648 5.67 270) (layer F.SilkS))
    (pad 10 thru_hole oval (at 1.27 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 9 thru_hole oval (at -1.27 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 1.27 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at -1.27 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 1.27 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at -1.27 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 1.27 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at -1.27 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 1.27 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at -1.27 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 1.269999980926514 -5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A7CBADB)
    (at 146.05 72.39 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value 2N3904 (at 1.27 2.79 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 17 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A7CBA2B)
    (at 106.68 72.39 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value 2N3906 (at 1.27 2.79 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 9 "Net-(D5-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 18 "Net-(Q2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBB7F)
    (at 91.44 134.62)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.31) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBB5C)
    (at 91.44 115.57)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBB6F)
    (at 91.44 128.27)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.31) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBB65)
    (at 91.44 121.92)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 2K (at 3.81 2.31) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R4-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBAD5)
    (at 132.08 71.12)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBB07)
    (at 132.08 77.47 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 75K (at 3.81 2.31 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBA9E)
    (at 132.08 90.17 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 100K (at 3.81 2.31 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBAAA)
    (at 138.43 90.17)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 20K (at 3.81 2.31) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBAB6)
    (at 146.05 97.79 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 3.81 -2.31 180) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CB9EC)
    (at 99.06 71.12 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 3.81 -2.31 180) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -12V))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CB9F7)
    (at 91.44 77.47 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 75K (at 3.81 2.31 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(Q2-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R11-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBA80)
    (at 91.44 90.17 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 100K (at 3.81 2.31 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R11-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A7CBA70)
    (at 99.06 90.17)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 20K (at 3.81 2.31) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R11-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 110.49 138.43 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference RV1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value 10K (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 110.49 123.19 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference RV2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value 10K (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Teensy_Footprints:Teensy30_31_32_LC (layer F.Cu) (tedit 5A29202F)
    (at 127 123.19 90)
    (fp_text reference U1 (at 0 -10.16 90) (layer F.SilkS))
    (fp_text value Teensy3.2 (at 0 10.16 90) (layer F.Fab))
    (fp_text user T3.2 (at -10.16 -2.54 180) (layer F.SilkS))
    (fp_text user T3.1 (at -6.35 -2.54 180) (layer F.SilkS))
    (pad 17 thru_hole circle (at 16.51 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 16.51 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad20)"))
    (pad 16 thru_hole circle (at 16.51 2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad16)"))
    (pad 15 thru_hole circle (at 16.51 5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad15)"))
    (pad 14 thru_hole circle (at 16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U1-Pad14)"))
    (pad 21 thru_hole circle (at 13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at 1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at -1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(RV1-Pad2)"))
    (pad 28 thru_hole circle (at -3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U1-Pad28)"))
    (pad 29 thru_hole circle (at -6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at -8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R2-Pad2)"))
    (pad 31 thru_hole circle (at -11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at -13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U1-Pad32)"))
    (pad 33 thru_hole circle (at -16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 +3V3))
    (pad 34 thru_hole circle (at -13.97 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U1-Pad34)"))
    (pad 35 thru_hole circle (at -8.89 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U1-Pad35)"))
    (pad 36 thru_hole circle (at -6.35 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U1-Pad36)"))
    (pad 37 thru_hole circle (at -3.81 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U1-Pad37)"))
    (pad 13 thru_hole circle (at 13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U1-Pad13)"))
    (pad 12 thru_hole circle (at 11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U1-Pad12)"))
    (pad 11 thru_hole circle (at 8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U1-Pad11)"))
    (pad 10 thru_hole circle (at 6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U1-Pad10)"))
    (pad 9 thru_hole circle (at 3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(U1-Pad9)"))
    (pad 8 thru_hole circle (at 1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at -1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(U1-Pad7)"))
    (pad 6 thru_hole circle (at -3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at -6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at -8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at -11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at -13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at -16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 38 thru_hole circle (at -1.27 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(U1-Pad38)"))
    (pad 39 thru_hole circle (at 1.27 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(U1-Pad39)"))
    (pad 40 thru_hole circle (at 3.81 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(U1-Pad40)"))
    (pad 41 thru_hole circle (at 6.35 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(U1-Pad41)"))
    (pad 42 thru_hole circle (at 8.89 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "Net-(U1-Pad42)"))
    (pad 43 thru_hole circle (at 11.43 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 "Net-(U1-Pad43)"))
    (pad 44 thru_hole circle (at 13.97 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "Net-(U1-Pad44)"))
    (pad 45 thru_hole circle (at 13.97 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "Net-(U1-Pad45)"))
    (pad 46 thru_hole circle (at 11.43 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "Net-(U1-Pad46)"))
    (pad 47 thru_hole circle (at 8.89 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "Net-(U1-Pad47)"))
    (pad 48 thru_hole circle (at 6.35 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(U1-Pad48)"))
    (pad 49 thru_hole circle (at 3.81 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 "Net-(U1-Pad49)"))
    (pad 50 thru_hole circle (at 1.27 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(U1-Pad50)"))
    (pad 51 thru_hole circle (at -1.27 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 "Net-(U1-Pad51)"))
    (pad 52 thru_hole circle (at -6.35 0 90) (size 1.9 1.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(U1-Pad52)"))
    (pad 52 thru_hole circle (at -10.16 0 90) (size 1.9 1.9) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(U1-Pad52)"))
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5A7CB9C4)
    (at 115.57 91.44)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS) hide)
    (fp_text value TL072 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(R1-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R12-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R2-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R12-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 -12VA))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINHEAD1-2 (layer F.Cu) (tedit 0)
    (at 146.05 125.73 180)
    (fp_text reference J2 (at 1.27 -3.9 180) (layer F.SilkS))
    (fp_text value Audio-Jack-2 (at 1.27 3.81 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.51 3.01) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 143.51 138.43)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 92.71 139.7)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 90.17 66.04)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 140.97 66.04)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 88.9 63.5) (end 149.86 63.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.9 144.78) (end 149.86 144.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.86 63.5) (end 149.86 144.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87.63 144.78) (end 88.9 144.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87.63 63.5) (end 87.63 144.78) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.9 63.5) (end 87.63 63.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.59 143.51) (xy 88.9 143.51) (xy 88.9 64.77) (xy 148.59 64.77)
      )
    )
  )
)
