(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 136)
    (no_connects 0)
    (area 12.649999 12.649999 203.250001 63.550001)
    (thickness 1.6)
    (drawings 145)
    (tracks 565)
    (zones 0)
    (modules 67)
    (nets 73)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.8128)
    (user_trace_width 0.254)
    (user_trace_width 0.4572)
    (user_trace_width 0.8128)
    (user_trace_width 2.032)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2032)
    (edge_width 0.1016)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.9398 0.5842)
    (user_via 1.27 0.8382)
    (uvia_size 0.3302)
    (uvia_drill 0.1778)
    (uvias_allowed no)
    (uvia_min_size 0.03302)
    (uvia_min_drill 0.1778)
    (pcb_text_width 0.254)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF6F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory C:/temp/))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 +12P)
  (net 4 +3V3)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 /TTL_DATA)
  (net 10 "Net-(P1-Pad1)")
  (net 11 "Net-(P2-Pad2)")
  (net 12 "Net-(P2-Pad3)")
  (net 13 /UTIL1)
  (net 14 /UTIL2)
  (net 15 /SDA1)
  (net 16 /SCL1)
  (net 17 /TX2)
  (net 18 /RX2)
  (net 19 /TX3)
  (net 20 /RX3)
  (net 21 "Net-(Q2-Pad2)")
  (net 22 "Net-(R2-Pad1)")
  (net 23 /PWRON)
  (net 24 /SCORE)
  (net 25 "Net-(U2-Pad4)")
  (net 26 "Net-(U2-Pad5)")
  (net 27 "Net-(U2-Pad7)")
  (net 28 "Net-(U2-Pad8)")
  (net 29 "Net-(U2-Pad9)")
  (net 30 "Net-(U2-Pad11)")
  (net 31 "Net-(U2-Pad12)")
  (net 32 "Net-(U2-Pad14)")
  (net 33 "Net-(U2-Pad16)")
  (net 34 "Net-(U2-Pad17)")
  (net 35 "Net-(U2-Pad18)")
  (net 36 "Net-(U2-Pad19)")
  (net 37 "Net-(U2-Pad20)")
  (net 38 "Net-(U3-Pad1)")
  (net 39 "Net-(U3-Pad2)")
  (net 40 "Net-(U3-Pad3)")
  (net 41 "Net-(U3-Pad6)")
  (net 42 "Net-(U3-Pad7)")
  (net 43 "Net-(U3-Pad8)")
  (net 44 "Net-(U3-Pad11)")
  (net 45 "Net-(U3-Pad12)")
  (net 46 "Net-(U3-Pad13)")
  (net 47 "Net-(U3-Pad17)")
  (net 48 "Net-(U3-Pad21)")
  (net 49 "Net-(U3-Pad22)")
  (net 50 "Net-(U3-Pad25)")
  (net 51 "Net-(U3-Pad29)")
  (net 52 "Net-(U3-Pad30)")
  (net 53 "Net-(U3-Pad33)")
  (net 54 "Net-(U3-Pad34)")
  (net 55 "Net-(U3-Pad35)")
  (net 56 "Net-(P6-Pad2)")
  (net 57 /F_MAIN)
  (net 58 /F_ALT)
  (net 59 /Xbee/RSSI)
  (net 60 /Xbee/ASSOC)
  (net 61 "/Fire Ctl/Detect_LED")
  (net 62 /SHOT)
  (net 63 /V_SENSE)
  (net 64 "Net-(P9-Pad2)")
  (net 65 /Xbee/ONSLEEP)
  (net 66 "Net-(U3-Pad39)")
  (net 67 "Net-(U4-Pad1)")
  (net 68 "Net-(D6-Pad2)")
  (net 69 "Net-(D7-Pad2)")
  (net 70 "Net-(D8-Pad2)")
  (net 71 "Net-(R18-Pad1)")
  (net 72 "Net-(R19-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3302)
    (uvia_drill 0.1778)
    (add_net +12P)
    (add_net +12V)
    (add_net +3V3)
    (add_net /F_ALT)
    (add_net /F_MAIN)
    (add_net "/Fire Ctl/Detect_LED")
    (add_net /PWRON)
    (add_net /RX2)
    (add_net /RX3)
    (add_net /SCL1)
    (add_net /SCORE)
    (add_net /SDA1)
    (add_net /SHOT)
    (add_net /TTL_DATA)
    (add_net /TX2)
    (add_net /TX3)
    (add_net /UTIL1)
    (add_net /UTIL2)
    (add_net /V_SENSE)
    (add_net /Xbee/ASSOC)
    (add_net /Xbee/ONSLEEP)
    (add_net /Xbee/RSSI)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad21)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad25)")
    (add_net "Net-(U3-Pad29)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad30)")
    (add_net "Net-(U3-Pad33)")
    (add_net "Net-(U3-Pad34)")
    (add_net "Net-(U3-Pad35)")
    (add_net "Net-(U3-Pad39)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad1)")
  )
  (module OpenCM:OpenCM (layer F.Cu) (tedit 589F9C6F)
    (at 171.069 37.846 90)
    (fp_text reference U3 (at -11.557 30.099 90) (layer F.SilkS))
    (fp_text value OpenCM-9.04 (at 0 0 90) (layer F.Fab))
    (fp_text user 5 (at 9.25 24.25 90) (layer F.SilkS))
    (fp_text user - (at -9.5 -16.5 90) (layer F.SilkS))
    (fp_text user 3 (at -9.5 -19.25 90) (layer F.SilkS))
    (fp_text user 5 (at -9.5 -21.75 90) (layer F.SilkS))
    (fp_text user R (at -9.5 -24.25 90) (layer F.SilkS))
    (fp_text user - (at 9.75 -16.5 90) (layer F.SilkS))
    (fp_text user - (at 9.75 -19 90) (layer F.SilkS))
    (fp_text user + (at 9.75 -21.5 90) (layer F.SilkS))
    (fp_text user + (at 9.75 -24.25 90) (layer F.SilkS))
    (fp_text user USB (at 0 30.75 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -11.43 -24.13 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad1)"))
    (pad 2 thru_hole circle (at -11.43 -21.59 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 "Net-(U3-Pad2)"))
    (pad 3 thru_hole circle (at -11.43 -19.05 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 "Net-(U3-Pad3)"))
    (pad 4 thru_hole circle (at -11.43 -16.51 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -11.43 -13.97 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 62 /SHOT))
    (pad 6 thru_hole circle (at -11.43 -11.43 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "Net-(U3-Pad6)"))
    (pad 7 thru_hole circle (at -11.43 -8.89 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 "Net-(U3-Pad7)"))
    (pad 8 thru_hole circle (at -11.43 -6.35 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(U3-Pad8)"))
    (pad 9 thru_hole circle (at -11.43 -3.81 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 /TX2))
    (pad 10 thru_hole circle (at -11.43 -1.27 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /RX2))
    (pad 11 thru_hole circle (at -11.43 1.27 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(U3-Pad11)"))
    (pad 12 thru_hole circle (at -11.43 3.81 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 "Net-(U3-Pad12)"))
    (pad 13 thru_hole circle (at -11.43 6.35 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 "Net-(U3-Pad13)"))
    (pad 14 thru_hole circle (at -11.43 8.89 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 63 /V_SENSE))
    (pad 15 thru_hole circle (at -11.43 11.43 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 57 /F_MAIN))
    (pad 16 thru_hole circle (at -11.43 13.97 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 /F_ALT))
    (pad 17 thru_hole circle (at -11.43 16.51 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 "Net-(U3-Pad17)"))
    (pad 18 thru_hole circle (at -11.43 19.05 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 /SCL1))
    (pad 19 thru_hole circle (at -11.43 21.59 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /SDA1))
    (pad 20 thru_hole circle (at -11.43 24.13 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 /UTIL1))
    (pad 21 thru_hole circle (at 11.43 24.13 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "Net-(U3-Pad21)"))
    (pad 22 thru_hole circle (at 11.43 21.59 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 "Net-(U3-Pad22)"))
    (pad 23 thru_hole circle (at 11.43 19.05 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 /RX3))
    (pad 24 thru_hole circle (at 11.43 16.51 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /TX3))
    (pad 25 thru_hole circle (at 11.43 13.97 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 50 "Net-(U3-Pad25)"))
    (pad 26 thru_hole circle (at 11.43 11.43 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 72 "Net-(R19-Pad1)"))
    (pad 27 thru_hole circle (at 11.43 8.89 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 71 "Net-(R18-Pad1)"))
    (pad 28 thru_hole circle (at 11.43 6.35 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 /SCORE))
    (pad 29 thru_hole circle (at 11.43 3.81 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 51 "Net-(U3-Pad29)"))
    (pad 30 thru_hole circle (at 11.43 1.27 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 52 "Net-(U3-Pad30)"))
    (pad 31 thru_hole circle (at 11.43 -1.27 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /PWRON))
    (pad 32 thru_hole circle (at 11.43 -3.81 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 /UTIL2))
    (pad 33 thru_hole circle (at 11.43 -6.35 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 53 "Net-(U3-Pad33)"))
    (pad 34 thru_hole circle (at 11.43 -8.89 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 54 "Net-(U3-Pad34)"))
    (pad 35 thru_hole circle (at 11.43 -11.43 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 55 "Net-(U3-Pad35)"))
    (pad 36 thru_hole circle (at 11.43 -13.97 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 37 thru_hole circle (at 11.43 -16.51 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 38 thru_hole circle (at 11.43 -19.05 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 39 thru_hole circle (at 11.43 -21.59 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 "Net-(U3-Pad39)"))
    (pad 40 thru_hole circle (at 11.43 -24.13 90) (size 1.6256 1.6256) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 "Net-(U3-Pad39)"))
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 58765D06)
    (at 67.183 46.355)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.21) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.21) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 589F9C20)
    (at 72.263 15.621 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 5.588 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.21 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 58A0C110)
    (at 33.782 56.642 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C6 (at 5.334 0.127 540) (layer F.SilkS))
    (fp_text value 10uF (at -2.54 2.286 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 589E824B)
    (at 41.275 16.51 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 3.175 -2.54 180) (layer F.SilkS))
    (fp_text value PowerOK (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 589E824F)
    (at 36.195 16.51 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 3.175 -2.54 180) (layer F.SilkS))
    (fp_text value RSSI (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 589E8255)
    (at 31.115 16.51 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 3.175 -2.54 180) (layer F.SilkS))
    (fp_text value Assoc (at 1.27 2.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight (layer F.Cu) (tedit 589F7BC5)
    (at 187.452 15.875 270)
    (descr "Connector Headers with Friction Lock, 22-03-5035, http://www.molex.com/pdm_docs/ps/PS-5264-001-001.pdf")
    (tags "connector molex SPOX 5267 22-03-5035")
    (fp_text reference J2 (at -0.254 2.794 270) (layer F.SilkS))
    (fp_text value SPOX (at 2.54 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight.wrl
      (at (xyz 0.1 0.023622 0.114173))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connectors_Molex:Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight (layer F.Cu) (tedit 589F7C6B)
    (at 165.1 54.61 270)
    (descr "Connector Headers with Friction Lock, 22-03-5035, http://www.molex.com/pdm_docs/ps/PS-5264-001-001.pdf")
    (tags "connector molex SPOX 5267 22-03-5035")
    (fp_text reference J3 (at 5.461 -4.318 360) (layer F.SilkS))
    (fp_text value SPOX (at 2.54 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight.wrl
      (at (xyz 0.1 0.023622 0.114173))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connectors_Molex:Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight (layer F.Cu) (tedit 589E826B)
    (at 47.625 16.51 270)
    (descr "Connector Headers with Friction Lock, 22-03-5035, http://www.molex.com/pdm_docs/ps/PS-5264-001-001.pdf")
    (tags "connector molex SPOX 5267 22-03-5035")
    (fp_text reference J4 (at 8.255 0 360) (layer F.SilkS))
    (fp_text value SPOX (at 2.54 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight.wrl
      (at (xyz 0.1 0.023622 0.114173))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connectors_Molex:Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight (layer F.Cu) (tedit 589F7C75)
    (at 124.587 54.61 270)
    (descr "Connector Headers with Friction Lock, 22-03-5035, http://www.molex.com/pdm_docs/ps/PS-5264-001-001.pdf")
    (tags "connector molex SPOX 5267 22-03-5035")
    (fp_text reference J5 (at 5.461 -4.445 360) (layer F.SilkS))
    (fp_text value SPOX (at 2.54 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight.wrl
      (at (xyz 0.1 0.023622 0.114173))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connectors_Molex:Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight (layer F.Cu) (tedit 589F9C1B)
    (at 64.389 16.51 270)
    (descr "Connector Headers with Friction Lock, 22-03-5035, http://www.molex.com/pdm_docs/ps/PS-5264-001-001.pdf")
    (tags "connector molex SPOX 5267 22-03-5035")
    (fp_text reference J6 (at 2.794 2.921 360) (layer F.SilkS))
    (fp_text value SPOX (at 2.54 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight.wrl
      (at (xyz 0.1 0.023622 0.114173))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connectors_Molex:Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight (layer F.Cu) (tedit 589F7C66)
    (at 187.325 54.61 270)
    (descr "Connector Headers with Friction Lock, 22-03-5035, http://www.molex.com/pdm_docs/ps/PS-5264-001-001.pdf")
    (tags "connector molex SPOX 5267 22-03-5035")
    (fp_text reference J7 (at 5.461 -4.445 360) (layer F.SilkS))
    (fp_text value SPOX (at 2.54 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight.wrl
      (at (xyz 0.1 0.023622 0.114173))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connectors_Molex:Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight (layer F.Cu) (tedit 589F7C71)
    (at 149.86 54.61 270)
    (descr "Connector Headers with Friction Lock, 22-03-5035, http://www.molex.com/pdm_docs/ps/PS-5264-001-001.pdf")
    (tags "connector molex SPOX 5267 22-03-5035")
    (fp_text reference J8 (at 5.461 -4.191 360) (layer F.SilkS))
    (fp_text value SPOX (at 2.54 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 /TTL_DATA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_SPOX-5267_22-03-5035_03x2.54mm_Straight.wrl
      (at (xyz 0.1 0.023622 0.114173))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 589F9C2E)
    (at 79.883 28.448 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J9 (at 0.127 5.334 90) (layer F.SilkS))
    (fp_text value Switch (at 1.905 3.175 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 589F9E61)
    (at 78.486 15.875)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J10 (at -2.54 -1.524 90) (layer F.SilkS))
    (fp_text value Video (at 1.75 6) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 589F9C46)
    (at 72.263 35.56 180)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference Q1 (at -0.127 -3.937 180) (layer F.SilkS))
    (fp_text value SUP75_PWR (at 0 3.175 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 589E82D7)
    (at 87.249 43.942 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 5.08 -1.27 180) (layer F.SilkS))
    (fp_text value BS170_DGS (at 1.27 1.905 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589E81F7)
    (at 82.55 39.37)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at -1.905 0) (layer F.SilkS))
    (fp_text value 470R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589F9C3A)
    (at 88.9 48.26 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 2.413 -1.905 180) (layer F.SilkS))
    (fp_text value 4k7 (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589E82D0)
    (at 91.44 48.26)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 6.985 0) (layer F.SilkS))
    (fp_text value 220R (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 /PWRON))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589E82ED)
    (at 40.005 25.4 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 470R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589E82F1)
    (at 34.925 25.4 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 470R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 "Net-(P9-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589F9C86)
    (at 176.149 34.925 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at -2.159 0 270) (layer F.SilkS))
    (fp_text value 1k (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 /SCORE))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589E82BE)
    (at 178.435 29.845 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at 6.985 0 270) (layer F.SilkS))
    (fp_text value 4k7 (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 /SCORE))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589FA518)
    (at 29.845 25.4 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R9 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 470R (at 2.54 0.127 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /Xbee/ASSOC))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589F8AA1)
    (at 177.8 57.15 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 47k (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /V_SENSE))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589F9C79)
    (at 175.26 53.975 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R11 (at 2.413 -1.905 180) (layer F.SilkS))
    (fp_text value 10k (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /V_SENSE))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_Micro_SPST (layer F.Cu) (tedit 589F9C41)
    (at 83.82 34.29)
    (tags "Switch Micro SPST")
    (fp_text reference SW1 (at -1.905 -2.159) (layer F.SilkS))
    (fp_text value Safe (at 0 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "Net-(R2-Pad1)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Buttons_Switches_ThroughHole.3dshapes/SW_Micro_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.33 0.33 0.33))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58A1175A)
    (at 59.436 36.195 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U1 (at 6.35 -0.381 360) (layer F.SilkS))
    (fp_text value OKI-78SR-3.3 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 3 +12P))
  )
  (module OpenCM:XBeePro (layer F.Cu) (tedit 589D58B9)
    (at 27.94 40.64 90)
    (fp_text reference U2 (at -11 -13 90) (layer F.SilkS))
    (fp_text value XBee (at 0 -11.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -11 -8 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at -11 -6 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 /RX2))
    (pad 3 thru_hole circle (at -11 -4 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 /TX2))
    (pad 4 thru_hole circle (at -11 -2 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at -11 0 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at -11 2 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 /Xbee/RSSI))
    (pad 7 thru_hole circle (at -11 4 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 27 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at -11 6 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 28 "Net-(U2-Pad8)"))
    (pad 9 thru_hole circle (at -11 8 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad9)"))
    (pad 10 thru_hole circle (at -11 10 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole circle (at 11 10 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad11)"))
    (pad 12 thru_hole circle (at 11 8 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad12)"))
    (pad 13 thru_hole circle (at 11 6 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 /Xbee/ONSLEEP))
    (pad 14 thru_hole circle (at 11 4 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad14)"))
    (pad 15 thru_hole circle (at 11 2 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /Xbee/ASSOC))
    (pad 16 thru_hole circle (at 11 0 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad16)"))
    (pad 17 thru_hole circle (at 11 -2 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad17)"))
    (pad 18 thru_hole circle (at 11 -4 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-Pad18)"))
    (pad 19 thru_hole circle (at 11 -6 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad19)"))
    (pad 20 thru_hole circle (at 11 -8 90) (size 1.524 1.524) (drill 0.7) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad20)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380 (layer F.Cu) (tedit 589E7824)
    (at 19.05 16.51)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380 (at 0 3.85) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380 (layer F.Cu) (tedit 589E781C)
    (at 19.05 59.69)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380 (at 0 3.85) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380 (layer F.Cu) (tedit 589E7807)
    (at 196.85 59.69)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380 (at 0 3.85) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380 (layer F.Cu) (tedit 589E7800)
    (at 196.85 16.51)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380 (at 0 3.85) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380 (layer F.Cu) (tedit 589E7814)
    (at 107.95 59.69)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380 (at 0 3.85) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 589E7A66)
    (at 80.01 57.15 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58A0B088)
    (at 113.919 33.528 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R12 (at 7.747 0.254 270) (layer F.SilkS))
    (fp_text value 1k5 (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 /SDA1))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58A0B083)
    (at 111.125 36.068 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R13 (at 8.382 0 270) (layer F.SilkS))
    (fp_text value 1k5 (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 /SCL1))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 58BFA942)
    (at 136.779 19.685 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J11 (at -2.667 1.905 180) (layer F.SilkS))
    (fp_text value F_Main (at 1.905 -5.7658 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 68 "Net-(D6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +12P))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 58BFA90A)
    (at 150.876 17.78 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference Q3 (at -4.3688 2.7432 90) (layer F.SilkS))
    (fp_text value 8721_M (at 0.4064 2.7432 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 68 "Net-(D6-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 57 /F_MAIN))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58BFAA82)
    (at 158.75 19.05)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 1.27 -3.556) (layer F.SilkS))
    (fp_text value BS170_A (at 1.8796 2.794) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 58 /F_ALT))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 56 "Net-(P6-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58C0E2EB)
    (at 168.148 15.367)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R15 (at 2.54 2.159) (layer F.SilkS))
    (fp_text value 1k (at 2.54 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 57 /F_MAIN))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 589FA434)
    (at 166.116 14.986 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R17 (at 2.54 -1.86 180) (layer F.SilkS))
    (fp_text value 2k2 (at 2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 /F_ALT))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58A0B31D)
    (at 125.349 30.988)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P5 (at -0.127 -2.286) (layer F.SilkS))
    (fp_text value AuxSerial (at 0 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /TX3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /RX3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 53.594 42.418 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at 0 -2.39 180) (layer F.SilkS))
    (fp_text value XbeeIn (at 0 10.01 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /TX2))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /RX2))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58A0B318)
    (at 132.715 35.814)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P2 (at 0.127 -2.54) (layer F.SilkS))
    (fp_text value ScoreSystem (at 0 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 58A0B330)
    (at 118.364 28.448)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P3 (at 0 -2.286) (layer F.SilkS))
    (fp_text value I2C (at 0 17.63) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /UTIL2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /UTIL1))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SDA1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /SCL1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 58A0C120)
    (at 26.416 55.372 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C4 (at -1.905 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 1.27 -0.254 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 58765D06)
    (at 134.747 57.15 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.25 -4.21 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.21 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58BFAA73)
    (at 134.366 27.559 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P6 (at 0 -2.39 180) (layer F.SilkS))
    (fp_text value F_Alt (at -2.4384 1.0414 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(P6-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 93.98 34.29 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 270) (layer F.SilkS))
    (fp_text value On (at 0 4.93 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 589F9C7C)
    (at 180.975 53.975)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C5 (at 1.27 2.159) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /V_SENSE))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 100.965 36.83)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P7 (at 0 -2.39) (layer F.SilkS))
    (fp_text value Gun_Sense (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "/Fire Ctl/Detect_LED"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /SHOT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58A004BB)
    (at 104.14 40.005 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R14 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 10k (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 /SHOT))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58A004B5)
    (at 107.315 37.465 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R16 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 47R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 "/Fire Ctl/Detect_LED"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A0B109)
    (at 111.252 30.48)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P8 (at 0 -2.39) (layer F.SilkS))
    (fp_text value 3V (at 0 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module OpenCM:SMD_Cuttable_Jumper_Patch_3 (layer B.Cu) (tedit 58A7C9E9)
    (at 34.925 23.114 180)
    (fp_text reference P9 (at -3.429 -0.127 270) (layer B.SilkS))
    (fp_text value JLED (at 0 -3.81 180) (layer B.Fab))
    (pad 1 smd rect (at -1.5748 0 180) (size 1.27 2.032) (layers B.Cu B.Paste B.Mask)
      (net 59 /Xbee/RSSI))
    (pad 2 smd rect (at 0 0 180) (size 1.27 2.032) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(P9-Pad2)"))
    (pad 3 smd rect (at 1.5748 0 180) (size 1.27 2.032) (layers B.Cu B.Paste B.Mask)
      (net 65 /Xbee/ONSLEEP))
  )
  (module OpenCM:200mil_Screw_Terminal (layer F.Cu) (tedit 58BE3D11)
    (at 67.31 56.769 270)
    (fp_text reference J1 (at 0 5.08 270) (layer F.SilkS))
    (fp_text value Battery (at 0 -5.588 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.286 2.794) (drill 1.3716) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.3716) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Diodes_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 58BE400C)
    (at 76.2 57.15 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.08 -2.06 90) (layer F.SilkS))
    (fp_text value 12V (at 5.207 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 58C1AFF4)
    (at 146.304 24.1808 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D5 (at 8.1788 -1.0668 180) (layer F.SilkS))
    (fp_text value 17V (at 5.2578 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module OpenCM:Pololu_Vreg_04_05 (layer F.Cu) (tedit 58BFAA67)
    (at 147.828 34.925 270)
    (fp_text reference U4 (at 5.0038 -6.35 270) (layer F.SilkS))
    (fp_text value 6V (at 4.8006 -2.9464 360) (layer F.Fab))
    (fp_text user VOUT (at -1.397 3.81 270) (layer F.SilkS))
    (fp_text user GND (at -1.905 1.27 270) (layer F.SilkS))
    (fp_text user VIN (at -2.032 -1.27 270) (layer F.SilkS))
    (fp_text user ~SHDN (at -1.27 -3.81 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 -3.81 270) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 67 "Net-(U4-Pad1)"))
    (pad 2 thru_hole circle (at -5.08 -1.27 270) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 3 thru_hole circle (at -5.08 1.27 270) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -5.08 3.81 270) (size 2.032 2.032) (drill 1.27) (layers *.Cu *.Mask)
      (net 66 "Net-(U3-Pad39)"))
  )
  (module Discret:DO-35 (layer F.Cu) (tedit 58BFA914)
    (at 143.0528 20.0152 270)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D6 (at -5.588 0 360) (layer F.SilkS))
    (fp_text value "500 mA" (at -11.8364 0.0508 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 3.81 0 270) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask)
      (net 3 +12P))
    (pad 2 thru_hole circle (at -3.81 0 270) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask)
      (net 68 "Net-(D6-Pad2)"))
    (model Discret.3dshapes/DO-35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 58C0E720)
    (at 178.562 16.002 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D7 (at 2.921 2.032 180) (layer F.SilkS))
    (fp_text value INFO_GRN (at -0.381 -3.048 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 58C0E725)
    (at 183.515 16.002 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D8 (at 2.794 2.032 180) (layer F.SilkS))
    (fp_text value ALRT_BLU (at -0.635 -3.048 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 "Net-(D8-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58C0E609)
    (at 182.118 34.925 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R18 (at -2.413 0 90) (layer F.SilkS))
    (fp_text value 47R (at 2.54 0.127 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 "Net-(R18-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "Net-(D7-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 58C0E60E)
    (at 185.928 34.925 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R19 (at -2.413 0.127 90) (layer F.SilkS))
    (fp_text value 47R (at 2.54 0.127 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 72 "Net-(R19-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 "Net-(D8-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text ALRT (at 182.499 19.05) (layer F.SilkS))
  (gr_text "INFO\n" (at 177.292 19.05) (layer F.SilkS))
  (gr_text "47R\n" (at 186.055 32.385 90) (layer F.SilkS))
  (gr_text 47R (at 182.245 32.385 90) (layer F.SilkS))
  (gr_text 6V (at 150.7744 39.624) (layer F.SilkS))
  (gr_text 470R (at 40.005 22.86 90) (layer F.SilkS))
  (gr_text + (at 148.082 24.638) (layer B.SilkS))
  (gr_text - (at 153.289 24.892) (layer B.SilkS))
  (gr_text G (at 154.559 47.498) (layer B.SilkS))
  (gr_text En (at 81.153 36.83) (layer B.SilkS))
  (gr_text G (at 86.233 36.83) (layer B.SilkS))
  (gr_text G (at 91.44 36.703) (layer B.SilkS))
  (gr_text S (at 98.552 41.783) (layer B.SilkS))
  (gr_text L (at 98.679 36.83) (layer B.SilkS))
  (gr_text G (at 98.552 39.37) (layer B.SilkS))
  (gr_text + (at 109.22 30.353) (layer B.SilkS))
  (gr_text G (at 109.347 33.147) (layer B.SilkS))
  (gr_text G (at 127.762 38.608) (layer B.SilkS))
  (gr_text G (at 120.904 43.688) (layer B.SilkS))
  (gr_text G (at 135.382 43.434) (layer B.SilkS))
  (gr_text T (at 189.865 15.875) (layer B.SilkS))
  (gr_text + (at 189.738 18.415) (layer B.SilkS))
  (gr_text - (at 189.992 20.828) (layer B.SilkS))
  (gr_text M (at 137.541 25.019) (layer B.SilkS))
  (gr_text + (at 137.668 27.559) (layer B.SilkS))
  (gr_text M (at 139.319 16.256) (layer B.SilkS))
  (gr_text + (at 139.319 19.685) (layer B.SilkS))
  (gr_text T (at 162.306 54.61) (layer B.SilkS))
  (gr_text + (at 162.306 57.15) (layer B.SilkS))
  (gr_text - (at 162.306 59.436) (layer B.SilkS))
  (gr_text T (at 50.292 16.51) (layer B.SilkS))
  (gr_text - (at 50.165 21.717) (layer B.SilkS))
  (gr_text + (at 50.419 19.05) (layer B.SilkS))
  (gr_text ON (at 33.401 20.701 90) (layer B.SilkS))
  (gr_text RSSI (at 36.576 20.066 90) (layer B.SilkS))
  (gr_text GLHF! (at 93.091 58.166) (layer F.SilkS))
  (gr_text "\"Freedom is worth awakening for.\"\n                           -- SkyNet" (at 33.909 34.29) (layer B.SilkS))
  (gr_text 3.3V (at 59.944 44.45) (layer F.SilkS))
  (gr_text Out (at 56.515 38.735) (layer F.SilkS))
  (gr_text In (at 56.642 33.528) (layer F.SilkS))
  (gr_text 10uF (at 31.496 54.102) (layer F.SilkS))
  (gr_text 100nF (at 25.4 57.404) (layer F.SilkS))
  (gr_text Cycle (at 100.838 44.831) (layer F.SilkS))
  (gr_text I2C (at 118.364 48.006) (layer F.SilkS))
  (gr_text Aux (at 125.222 48.006) (layer F.SilkS))
  (gr_text Score (at 133.096 48.006) (layer F.SilkS))
  (gr_text "F_Main\n" (at 131.0132 17.8308 90) (layer F.SilkS))
  (gr_text F_Alt (at 136.652 26.416 90) (layer F.SilkS))
  (gr_text Gnd (at 109.22 33.147 90) (layer F.SilkS))
  (gr_text +3 (at 109.093 29.972 90) (layer F.SilkS))
  (gr_text 10k (at 104.14 37.465 90) (layer F.SilkS))
  (gr_text 47R (at 107.315 34.925 90) (layer F.SilkS))
  (gr_text GND (at 97.282 39.37) (layer F.SilkS))
  (gr_text SENS (at 96.774 41.91) (layer F.SilkS))
  (gr_text LED (at 97.536 36.83) (layer F.SilkS))
  (gr_text 470R (at 35.052 22.86 90) (layer F.SilkS))
  (gr_text 470R (at 29.972 22.86 90) (layer F.SilkS))
  (gr_text "470R\n" (at 85.09 39.37) (layer F.SilkS))
  (gr_text 12V (at 76.2 51.943 90) (layer F.SilkS))
  (gr_text 4k7 (at 80.01 52.07 90) (layer F.SilkS))
  (gr_text 4k7 (at 86.36 48.26) (layer F.SilkS))
  (gr_text "220R\n" (at 93.98 48.26) (layer F.SilkS))
  (gr_text 1k5 (at 110.998 38.608 90) (layer F.SilkS))
  (gr_text 1k5 (at 113.792 36.068 90) (layer F.SilkS))
  (gr_text 10k (at 172.72 53.848) (layer F.SilkS))
  (gr_text 47k (at 177.8 54.61 90) (layer F.SilkS))
  (gr_text 100nF (at 182.118 52.578) (layer F.SilkS))
  (gr_text 1k (at 176.149 32.385 90) (layer F.SilkS))
  (gr_text 4k7 (at 178.435 32.385 90) (layer F.SilkS))
  (gr_text 1k (at 170.688 15.367) (layer F.SilkS))
  (gr_text "2k2\n" (at 163.576 14.986) (layer F.SilkS))
  (gr_text BS170 (at 160.02 21.844) (layer F.SilkS))
  (gr_text 8721 (at 153.67 18.288 90) (layer F.SilkS))
  (gr_text "17V\n" (at 146.2532 18.8976 90) (layer F.SilkS))
  (gr_text 3V (at 39.878 13.716) (layer F.SilkS))
  (gr_text RSS (at 35.052 13.716) (layer F.SilkS))
  (gr_text Ass (at 29.718 13.716) (layer F.SilkS))
  (gr_text Assoc (at 29.845 34.29 270) (layer F.SilkS))
  (gr_text +3V (at 19.685 48.26 90) (layer F.SilkS))
  (gr_text Gnd (at 38.1 48.26 90) (layer F.SilkS))
  (gr_text Rssi (at 29.845 47.625 90) (layer F.SilkS))
  (gr_text Tx2 (at 23.495 48.26 90) (layer F.SilkS))
  (gr_text Rx2 (at 21.59 48.26 90) (layer F.SilkS))
  (gr_text - (at 62.23 59.055) (layer F.SilkS))
  (gr_text + (at 62.23 53.975) (layer F.SilkS))
  (gr_text Util1 (at 194.945 45.085 90) (layer F.SilkS))
  (gr_text SDA (at 192.405 45.72 90) (layer F.SilkS))
  (gr_text SCL (at 189.865 45.72 90) (layer F.SilkS))
  (gr_text Alt (at 184.785 45.72 90) (layer F.SilkS))
  (gr_text "Main\n" (at 182.245 45.085 90) (layer F.SilkS))
  (gr_text Vsens (at 179.705 44.45 90) (layer F.SilkS))
  (gr_text Rx2 (at 169.545 45.72 90) (layer F.SilkS))
  (gr_text Tx2 (at 167.005 45.72 90) (layer F.SilkS))
  (gr_text "TTL\n" (at 157.226 29.464 90) (layer F.SilkS))
  (gr_text Util2 (at 167.132 30.353 90) (layer F.SilkS))
  (gr_text Score (at 173.99 31.623 90) (layer F.SilkS))
  (gr_text M (at 132.4864 15.24) (layer F.SilkS))
  (gr_text + (at 132.5372 20.4216) (layer F.SilkS))
  (gr_text A (at 131.445 25.4) (layer F.SilkS))
  (gr_text + (at 131.445 27.94) (layer F.SilkS))
  (gr_text Gnd (at 136.525 43.18) (layer F.SilkS))
  (gr_text S_IN (at 136.906 40.894) (layer F.SilkS))
  (gr_text "+12\n" (at 136.144 35.814) (layer F.SilkS))
  (gr_text +3 (at 128.27 31.115) (layer F.SilkS))
  (gr_text Tx3 (at 128.905 33.655) (layer F.SilkS))
  (gr_text "Rx3\n" (at 128.905 36.195) (layer F.SilkS))
  (gr_text Gnd (at 128.905 38.735) (layer F.SilkS))
  (gr_text "Gnd\n" (at 121.92 43.815) (layer F.SilkS))
  (gr_text SCL (at 121.92 41.275) (layer F.SilkS))
  (gr_text SDA (at 121.92 38.735) (layer F.SilkS))
  (gr_text "U1\n" (at 121.285 36.195) (layer F.SilkS))
  (gr_text "U2\n" (at 121.285 33.655) (layer F.SilkS))
  (gr_text "+3\n" (at 121.285 31.115) (layer F.SilkS))
  (gr_text "+12\n" (at 121.285 28.575) (layer F.SilkS))
  (gr_text "On\n" (at 92.71 36.83) (layer F.SilkS))
  (gr_text En (at 81.28 36.83) (layer F.SilkS))
  (gr_text Gnd (at 50.165 34.925) (layer F.SilkS))
  (gr_text Rx2 (at 50.165 37.465) (layer F.SilkS))
  (gr_text Tx2 (at 50.165 40.005) (layer F.SilkS))
  (gr_text "+3\n" (at 50.165 42.545) (layer F.SilkS))
  (gr_text + (at 74.93 27.94) (layer F.SilkS))
  (gr_text - (at 74.93 24.13) (layer F.SilkS))
  (gr_text - (at 82.042 18.669) (layer B.SilkS))
  (gr_text + (at 77.47 21.59) (layer F.SilkS))
  (gr_text + (at 76.454 28.321) (layer B.SilkS))
  (gr_text - (at 76.708 24.892) (layer B.SilkS))
  (gr_text - (at 82.55 21.59) (layer F.SilkS))
  (gr_text + (at 78.486 18.669) (layer B.SilkS))
  (gr_text "Onyx X Power Board v2\n2017-03-09\nJon Watte" (at 171.958 36.83) (layer B.SilkS))
  (gr_arc (start 13.97 62.23) (end 13.97 63.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 13.97 13.97) (end 12.7 13.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 84.455 13.97) (end 84.455 12.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 86.995 24.13) (end 86.995 25.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 128.905 24.13) (end 130.175 24.13) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.445 13.97) (end 130.175 13.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 201.93 13.97) (end 201.93 12.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 201.93 62.23) (end 203.2 62.23) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.445 12.7) (end 201.93 12.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.175 24.13) (end 130.175 13.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 86.995 25.4) (end 128.905 25.4) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 85.725 13.97) (end 85.725 24.13) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 13.97 12.7) (end 84.455 12.7) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 203.2 62.23) (end 203.2 13.97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 13.97 63.5) (end 201.93 63.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 12.7 13.97) (end 12.7 62.23) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 29.21 12.7) (xy 29.21 63.5) (xy 203.2 63.5) (xy 203.2 12.7)
      )
    )
  )
  (zone (net 3) (net_name +12P) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 44.45 12.7) (xy 44.45 25.4) (xy 52.07 33.02) (xy 53.34 33.02) (xy 54.61 34.29)
        (xy 54.61 36.83) (xy 55.88 38.1) (xy 62.23 38.1) (xy 66.04 34.29) (xy 67.31 33.02)
        (xy 71.12 33.02) (xy 71.12 52.07) (xy 77.597 58.42) (xy 97.79 58.42) (xy 101.6 54.61)
        (xy 111.76 54.61) (xy 120.65 63.5) (xy 203.2 63.5) (xy 203.2 12.7) (xy 57.15 12.7)
      )
    )
  )
  (zone (net 1) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.381) (thermal_bridge_width 0.762) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 62.103 49.657) (xy 62.103 38.989) (xy 67.691 33.274) (xy 70.866 33.274) (xy 70.866 52.197)
        (xy 70.866 55.499) (xy 65.278 55.499) (xy 62.103 52.324)
      )
    )
  )
)
