(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 50)
    (no_connects 0)
    (area 55.100999 54.461 255.277714 200.232)
    (thickness 1.6)
    (drawings 33)
    (tracks 97)
    (zones 0)
    (modules 34)
    (nets 23)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (33 F.Adhes user hide)
    (35 F.Paste user hide)
    (37 F.SilkS user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (47 F.CrtYd user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 62.23 105.41)
    (grid_origin 62.23 105.41)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00020_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 /PulseOutput)
  (net 6 +5V)
  (net 7 "Net-(D1-Pad2)")
  (net 8 "Net-(D2-Pad2)")
  (net 9 "Net-(J1-Pad3)")
  (net 10 "Net-(J1-Pad2)")
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J3-Pad1)")
  (net 13 "Net-(Q1-Pad1)")
  (net 14 "Net-(RV1-Pad3)")
  (net 15 "Net-(RV2-Pad3)")
  (net 16 "Net-(U1-Pad5)")
  (net 17 "Net-(R4-Pad2)")
  (net 18 "Net-(R7-Pad1)")
  (net 19 "Net-(Q2-Pad3)")
  (net 20 "Net-(Q4-Pad2)")
  (net 21 "Net-(Q1-Pad3)")
  (net 22 "Net-(C5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PulseOutput)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(RV2-Pad3)")
    (add_net "Net-(U1-Pad5)")
  )
  (net_class Wide ""
    (clearance 0.254)
    (trace_width 1.016)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(R7-Pad1)")
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal (layer F.Cu) (tedit 59C53756)
    (at 149.352 64.77)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference FuseHolder1 (at 7.62 -2.66) (layer Cmts.User) hide)
    (fp_text value FuseHolder (at 7.62 2.66) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 15.24 0) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal (layer F.Cu) (tedit 59C5374B)
    (at 75.438 64.77)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=15.24mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 15.24mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (fp_text reference FuseHolder1 (at 7.62 -2.66) (layer Cmts.User) hide)
    (fp_text value FuseHolder (at 7.62 2.66) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 15.24 0) (size 4 4) (drill 2) (layers *.Cu *.Mask))
    (model Resistors_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59C1803B)
    (at 183.896 100.33)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 4.318 2.54) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 7.366 4.318) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59BAC180)
    (at 67.31 100.584)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Wire_Connections_Bridges:WireConnection_1.50mmDrill placed (layer F.Cu) (tedit 59C188C0)
    (at 129.54 72.136)
    (descr "WireConnection with 1.5mm drill")
    (fp_text reference J2 (at 0 3.302) (layer F.SilkS))
    (fp_text value GM_Tube (at 1.524 5.334) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 10.16 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 59C17F39)
    (at 112.776 77.47)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 10n (at 5.334 0) (layer F.SilkS))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 59C17D12)
    (at 77.216 94.742 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at 2.286 -2.54 180) (layer F.SilkS))
    (fp_text value 1n (at -1.778 -2.54 180) (layer F.SilkS))
    (fp_text user %R (at 2.286 -2.54 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 59C17FE7)
    (at 139.7 83.058 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at 2.54 3.048 270) (layer F.SilkS))
    (fp_text value 220pF (at -2.54 3.048 270) (layer F.SilkS))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering placed (layer F.Cu) (tedit 59C1802F)
    (at 165.354 92.71 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C4 (at -4.572 1.27 360) (layer F.SilkS))
    (fp_text value 20uF (at -4.572 -2.794 360) (layer F.SilkS))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /PulseOutput))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P12.70mm_Horizontal placed (layer F.Cu) (tedit 59C18802)
    (at 110.744 72.136 180)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 11.938 -2.54 180) (layer F.SilkS))
    (fp_text value 1N4937 (at 6.35 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 180) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P12.70mm_Horizontal placed (layer F.Cu) (tedit 59C17D06)
    (at 84.836 90.424 270)
    (descr "D, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 10.16 2.54 270) (layer F.SilkS))
    (fp_text value 1N914 (at 3.81 2.54 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (model Diodes_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_A placed (layer F.Cu) (tedit 59C17F67)
    (at 68.58 74.93 270)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J1 (at 12.954 4.572 360) (layer F.SilkS))
    (fp_text value USB_A (at 12.954 0.762 360) (layer F.SilkS))
    (pad 4 thru_hole circle (at 7.11 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 5 thru_hole circle (at 10.16 2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -3.56 2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol placed (layer F.Cu) (tedit 59C53EE2)
    (at 183.388 83.566 90)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J3 (at -3.81 -1.27 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x02 (at 2.286 -6.604 90) (layer Cmts.User) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal placed (layer F.Cu) (tedit 59C17CF5)
    (at 85.852 72.136)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference L1 (at 0 -2.032) (layer F.SilkS))
    (fp_text value 10mH (at 5.842 -2.032) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide placed (layer F.Cu) (tedit 59C17FAF)
    (at 96.012 78.994 180)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 5.08 2.794 360) (layer F.SilkS))
    (fp_text value JN3303 (at -2.286 2.794 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide placed (layer F.Cu) (tedit 59C17FA3)
    (at 113.538 99.568 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at -2.794 -2.54 360) (layer F.SilkS))
    (fp_text value 2N3904 (at -2.794 2.794 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(Q2-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal placed (layer F.Cu) (tedit 59BAB341)
    (at 150.876 94.996 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, http://www.Suntan.com/docs/51016/TSR-3386.pdf")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single")
    (fp_text reference RV1 (at 3.556 3.81 180) (layer F.SilkS))
    (fp_text value ">100k POT" (at -3.302 3.81 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(RV1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /PulseOutput))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal placed (layer F.Cu) (tedit 59C18016)
    (at 125.476 96.012 180)
    (descr "Potentiometer, horizontally mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, http://www.Suntan.com/docs/51016/TSR-3386.pdf")
    (tags "Potentiometer horizontal  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single")
    (fp_text reference RV2 (at -6.858 -3.048 180) (layer F.SilkS))
    (fp_text value "10Ω POT" (at -8.89 -4.826 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(RV2-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 -2.54 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R7-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Suntan_TSR-3386P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_Socket placed (layer F.Cu) (tedit 59C17F4C)
    (at 97.79 88.646)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), Socket")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil Socket")
    (fp_text reference U1 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LM555N (at 3.81 10.01) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(R4-Pad2)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(Q2-Pad3)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SC-59_Handsoldering (layer F.Cu) (tedit 59C17D3B)
    (at 175.006 91.694)
    (descr "SC-59, hand-soldering varaint, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
    (tags "SC-59 hand-soldering")
    (attr smd)
    (fp_text reference Q3 (at 0.254 3.048 90) (layer F.SilkS))
    (fp_text value DMN1019USN-13 (at 4.572 1.778 90) (layer F.SilkS))
    (fp_text user %R (at 0.254 3.048 90) (layer F.Fab))
    (pad 1 smd rect (at -1.65 -0.95) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /PulseOutput))
    (pad 2 smd rect (at -1.65 0.95) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.65 0) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J3-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes\SC-59_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F73)
    (at 80.518 80.01 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R1 (at -1.524 -3.048 90) (layer F.SilkS))
    (fp_text value 100k (at 1.778 -3.048 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 "Net-(Q2-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 +5V))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C1801A)
    (at 168.402 76.708)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R2 (at -0.254 -3.048) (layer F.SilkS))
    (fp_text value 15 (at -0.254 3.048) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F3E)
    (at 117.602 72.136)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R3 (at 2.54 -2.86) (layer F.SilkS))
    (fp_text value 4.7M (at 2.54 2.86) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F8C)
    (at 113.792 84.328 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R4 (at 4.572 -2.794 270) (layer F.SilkS))
    (fp_text value 330 (at 0.508 -2.794 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(R4-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F55)
    (at 90.424 95.25 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R5 (at 4.572 -3.048 270) (layer F.SilkS))
    (fp_text value 1k (at 1.778 -3.048 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(R4-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17FFC)
    (at 146.812 84.328 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R6 (at 2.54 -2.86 90) (layer F.SilkS))
    (fp_text value 22k (at 2.54 2.86 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(Q4-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F95)
    (at 122.682 88.9 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R7 (at -0.254 2.794 90) (layer F.SilkS))
    (fp_text value 15 (at 4.064 2.794 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(R7-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17F5C)
    (at 80.01 86.106 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R8 (at 6.604 -3.048 180) (layer F.SilkS))
    (fp_text value 220k (at 2.794 -3.048 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module KNEK-TEK_logo:KNEK-TEK_logo_small_INVERTED (layer F.Cu) (tedit 59BAB1C9)
    (at 178.054 66.04)
    (fp_text reference G*** (at -11.684 -7.366) (layer Cmts.User) hide)
    (fp_text value LOGO (at -13.208 4.572) (layer Cmts.User) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 59BAC180)
    (at 67.31 59.69)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer Cmts.User) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer Cmts.User) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Wide (layer F.Cu) (tedit 59C18007)
    (at 156.718 86.868 90)
    (descr "TO-92 leads in-line, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 0 -3.556 360) (layer F.SilkS))
    (fp_text value 2N3904 (at 2.794 5.588 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(Q4-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.524 1.524) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /PulseOutput))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical (layer F.Cu) (tedit 59C17FEF)
    (at 138.43 90.932)
    (descr "Resistor, Axial_DIN0411 series, Axial, Vertical, pin pitch=5.08mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Vertical pin pitch 5.08mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R9 (at -1.524 3.048) (layer F.SilkS))
    (fp_text value 100k (at 4.064 3.048) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 5.08 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(Q4-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 59C18020)
    (at 173.736 83.566 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C5 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value 20uF (at 0 2.5 270) (layer F.SilkS))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 59C17F80)
    (at 105.156 83.312)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C6 (at 4.826 -0.254) (layer F.SilkS))
    (fp_text value 1uF (at 2.794 2.794) (layer F.SilkS))
    (fp_text user %R (at 0 -2.25) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "K'NEK-TEK Star Jar v1.0\nSept 2017" (at 167.64 101.6) (layer B.Cu))
  (dimension 127 (width 0.3) (layer F.SilkS)
    (gr_text "5.0000 in" (at 125.73 111.078) (layer F.SilkS))
    (feature1 (pts (xy 62.23 108.966) (xy 62.23 112.428)))
    (feature2 (pts (xy 189.23 108.966) (xy 189.23 112.428)))
    (crossbar (pts (xy 189.23 109.728) (xy 62.23 109.728)))
    (arrow1a (pts (xy 62.23 109.728) (xy 63.356504 109.141579)))
    (arrow1b (pts (xy 62.23 109.728) (xy 63.356504 110.314421)))
    (arrow2a (pts (xy 189.23 109.728) (xy 188.103496 109.141579)))
    (arrow2b (pts (xy 189.23 109.728) (xy 188.103496 110.314421)))
  )
  (dimension 50.8 (width 0.3) (layer F.SilkS)
    (gr_text "2.0000 in" (at 193.882 80.01 270) (layer F.SilkS))
    (feature1 (pts (xy 191.008 105.41) (xy 195.232 105.41)))
    (feature2 (pts (xy 191.008 54.61) (xy 195.232 54.61)))
    (crossbar (pts (xy 192.532 54.61) (xy 192.532 105.41)))
    (arrow1a (pts (xy 192.532 105.41) (xy 191.945579 104.283496)))
    (arrow1b (pts (xy 192.532 105.41) (xy 193.118421 104.283496)))
    (arrow2a (pts (xy 192.532 54.61) (xy 191.945579 55.736504)))
    (arrow2b (pts (xy 192.532 54.61) (xy 193.118421 55.736504)))
  )
  (gr_text "HIGH VOLTAGE ZONE - 400V+" (at 89.916 57.658) (layer F.SilkS))
  (gr_text - (at 186.69 87.122) (layer F.SilkS))
  (gr_text + (at 186.944 74.422) (layer F.SilkS))
  (gr_text "K'NEK-TEK Star Jar v1.0\nSept 2017" (at 167.64 101.6) (layer F.Fab))
  (gr_text 1.0 (at 253.492 198.882) (layer F.Fab))
  (gr_text "September 2017" (at 200.152 198.882) (layer F.Fab))
  (gr_text "Star Jar" (at 175.514 195.326) (layer F.Fab))
  (gr_text "K'NEK-TEK Star Jar v1.0\nSept 2017" (at 167.64 101.6) (layer F.Cu))
  (gr_text "R2 is brightness control\n(5V - Vdrop) = 2.6V\n2.6V / R2 = I_limit" (at 158.496 76.708) (layer F.SilkS))
  (gr_text "HV Tuning" (at 134.62 102.87) (layer F.SilkS))
  (gr_text "Pulse Length Control" (at 150.876 103.378) (layer F.SilkS))
  (gr_line (start 62.23 54.61) (end 62.23 105.41) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.23 54.61) (end 62.23 54.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 189.23 105.41) (end 189.23 54.61) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 62.23 105.41) (end 189.23 105.41) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.214 104.648) (xy 62.992 104.648) (xy 62.992 55.626) (xy 188.214 55.626)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 188.214 104.648) (xy 62.992 104.648) (xy 62.992 55.626) (xy 188.214 55.626)
      )
    )
  )
)
