(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 29)
    (no_connects 0)
    (area 81.102654 78.924999 138.246429 121.598481)
    (thickness 1.6)
    (drawings 12)
    (tracks 119)
    (zones 0)
    (modules 12)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x0103c_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 /RST)
  (net 6 "Net-(IC1-Pad3)")
  (net 7 /MOSI)
  (net 8 /MISO)
  (net 9 /SCK)
  (net 10 "Net-(L1-Pad1)")
  (net 11 "Net-(L1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net VCC)
  )
  (module "theinventorhouse:1411(3528m)-B%2CM%2CH%2CT-TANTALUM" (layer F.Cu) (tedit 0)
    (at 111.1 102.8 270)
    (solder_paste_margin -0.127)
    (attr smd)
    (fp_text reference C1 (at -3.8 1.8 270) (layer F.SilkS))
    (fp_text value 100uF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.5 0 270) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.5 0 270) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module "theinventorhouse:1411(3528m)-B%2CM%2CH%2CT-TANTALUM" (layer F.Cu) (tedit 0)
    (at 120.9 84.5 270)
    (solder_paste_margin -0.127)
    (attr smd)
    (fp_text reference C2 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value 100uF (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.5 0 270) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.5 0 270) (size 1.6 2.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 131.95 92.8)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.35 -0.4) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.95 1.4) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 127.78 97.47)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at -0.88 -3.27) (layer F.SilkS))
    (fp_text value ATTINY85-P (at -2.48 3.53 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MOSI))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MISO))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCK))
    (pad 8 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 569FD137)
    (at 111.3 82.8 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference L1 (at -2.3 -2.2 180) (layer F.SilkS))
    (fp_text value Coil (at 0.1 2.7 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(L1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(L1-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 569FD1BD)
    (at 106.6 104 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 1 5.2 180) (layer F.SilkS))
    (fp_text value Battery (at 2.7 1.2 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 569FD1D0)
    (at 120.34 96.78 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 3.74 7.68 180) (layer F.SilkS))
    (fp_text value "AVR ICSP" (at 1.44 -2.92 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module open-project:SW_PUSH_SMD (layer F.Cu) (tedit 514E2F98)
    (at 109.30204 91.5479)
    (fp_text reference SW1 (at -0.05 -3.95) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0 3.85) (layer F.SilkS))
    (pad 1 smd rect (at -3.99796 -2.2479) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 1 smd rect (at 3.99796 -2.2479) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 2 smd rect (at 3.99796 2.2479) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.99796 2.2479) (size 1.5494 1.2954) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 134.39 81.53 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 8.37 10.99 270) (layer F.SilkS))
    (fp_text value L9110 (at 3.57 3.79 360) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(L1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(L1-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /MOSI))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MISO))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 116.05098 105.3 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.04902 0) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 121.25 105.3)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 569FDA3A)
    (at 110.4 93.4 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference Electroniccats (at 0.09906 4.38912 180) (layer B.SilkS))
    (fp_text value OSHW-Logo (at 0.30988 -6.56082 180) (layer B.Fab))
  )
  (gr_arc (start 104 107) (end 104 108) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 104 80) (end 103 80) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137 107) (end 138 107) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137 80) (end 137 79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138 80) (end 138 107) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104 79) (end 137 79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103 107) (end 103 80) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137 108) (end 104 108) (layer Edge.Cuts) (width 0.15))
  (dimension 30.000667 (width 0.3) (layer Margin)
    (gr_text "30.001 mm" (at 87.752653 93.997684 89.6180338) (layer Margin))
    (feature1 (pts (xy 103.2 79.1) (xy 86.502683 78.988684)))
    (feature2 (pts (xy 103 109.1) (xy 86.302683 108.988684)))
    (crossbar (pts (xy 89.002623 109.006684) (xy 89.202623 79.006684)))
    (arrow1a (pts (xy 89.202623 79.006684) (xy 89.781521 80.137072)))
    (arrow1b (pts (xy 89.202623 79.006684) (xy 88.608705 80.129253)))
    (arrow2a (pts (xy 89.002623 109.006684) (xy 89.596541 107.884115)))
    (arrow2b (pts (xy 89.002623 109.006684) (xy 88.423725 107.876296)))
  )
  (dimension 35.000143 (width 0.3) (layer Margin)
    (gr_text "35.000 mm" (at 120.467862 120.198485 359.8362982) (layer Margin))
    (feature1 (pts (xy 103 108.9) (xy 102.964005 121.49848)))
    (feature2 (pts (xy 138 109) (xy 137.964005 121.59848)))
    (crossbar (pts (xy 137.971719 118.898491) (xy 102.971719 118.798491)))
    (arrow1a (pts (xy 102.971719 118.798491) (xy 104.099894 118.215291)))
    (arrow1b (pts (xy 102.971719 118.798491) (xy 104.096543 119.388128)))
    (arrow2a (pts (xy 137.971719 118.898491) (xy 136.846895 118.308854)))
    (arrow2b (pts (xy 137.971719 118.898491) (xy 136.843544 119.481691)))
  )
  (dimension 37.900528 (width 0.3) (layer Margin)
    (gr_text "37.901 mm" (at 118.977187 114.251985 0.302349592) (layer Margin))
    (feature1 (pts (xy 137.9 109) (xy 137.934311 115.501966)))
    (feature2 (pts (xy 100 109.2) (xy 100.034311 115.701966)))
    (crossbar (pts (xy 100.020063 113.002004) (xy 137.920063 112.802004)))
    (arrow1a (pts (xy 137.920063 112.802004) (xy 136.796669 113.394361)))
    (arrow1b (pts (xy 137.920063 112.802004) (xy 136.79048 112.221536)))
    (arrow2a (pts (xy 100.020063 113.002004) (xy 101.149646 113.582472)))
    (arrow2b (pts (xy 100.020063 113.002004) (xy 101.143457 112.409647)))
  )
  (dimension 30.100166 (width 0.3) (layer Margin)
    (gr_text "30.100 mm" (at 93.299401 94.271763 270.1903507) (layer Margin))
    (feature1 (pts (xy 99.8 79.2) (xy 91.899409 79.226248)))
    (feature2 (pts (xy 99.9 109.3) (xy 91.999409 109.326248)))
    (crossbar (pts (xy 94.699394 109.317278) (xy 94.599394 79.217278)))
    (arrow1a (pts (xy 94.599394 79.217278) (xy 95.189554 80.341827)))
    (arrow1b (pts (xy 94.599394 79.217278) (xy 94.016719 80.345724)))
    (arrow2a (pts (xy 94.699394 109.317278) (xy 95.282069 108.188832)))
    (arrow2b (pts (xy 94.699394 109.317278) (xy 94.109234 108.192729)))
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103 79) (xy 137.9 79.1) (xy 138 108) (xy 103 107.8)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 103.1 79) (xy 137.9 79.1) (xy 138 108) (xy 103 107.9) (xy 103 79)
      )
    )
  )
)
