(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "2_14_P")
	(net 2 "4_16_P")
	(net 3 "5_17_P")
	(net 4 "6_18_P")
	(net 5 "7_19_P")
	(net 6 "8_20_P")
	(net 7 "9_21_P")
	(net 8 "10_22_P")
	(net 9 "11_23_P")
	(net 10 "12_24_P")
	(net 11 "13_25_P")
	(net 12 "3_15_P")
	(net 13 "2_14_N")
	(net 14 "3_15_N")
	(net 15 "4_16_N")
	(net 16 "5_17_N")
	(net 17 "6_18_N")
	(net 18 "7_19_N")
	(net 19 "8_20_N")
	(net 20 "9_21_N")
	(net 21 "10_22_N")
	(net 22 "11_23_N")
	(net 23 "12_24_N")
	(net 24 "13_25_N")
	(net 25 "CLAMP_POUR_TOP_1")
	(footprint "SMA"
		(layer "F.Cu")
		(at 158.6611 89.7636)
		(property "Reference" "U$3"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "3_15_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "3_15_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "3_15_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "3_15_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "3_15_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 148.5011 120.2436)
		(property "Reference" "U$11"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "11_23_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "11_23_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "11_23_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "11_23_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "11_23_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 168.8211 120.2436)
		(property "Reference" "U$13"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "13_25_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "13_25_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "13_25_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "13_25_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "13_25_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 168.8211 89.7636)
		(property "Reference" "U$4"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "4_16_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "4_16_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "4_16_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "4_16_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "4_16_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 168.8211 110.0836)
		(property "Reference" "U$10"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "10_22_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "10_22_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "10_22_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "10_22_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "10_22_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 158.6611 110.0836)
		(property "Reference" "U$9"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "9_21_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "9_21_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "9_21_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "9_21_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "9_21_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 148.5011 110.0836)
		(property "Reference" "U$8"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "8_20_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "8_20_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "8_20_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "8_20_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "8_20_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 158.6611 120.2436)
		(property "Reference" "U$12"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "12_24_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "12_24_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "12_24_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "12_24_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "12_24_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "MICRO-D-RIGHT-ANGLE"
		(layer "F.Cu")
		(at 128.9431 105.0036 90)
		(property "Reference" "U$1"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RIGHT-ANGLE-MICRO-D"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "7"
			(at -0.635 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at 5.715 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Glenair MWDM 2L 25S CBR P .110"
			(at 0 -3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "22"
			(at -5.715 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "12"
			(at -9.525 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "17"
			(at 4.445 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 8.255 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "16"
			(at 5.715 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 9.525 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "21"
			(at -4.445 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "11"
			(at -6.985 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at -9.525 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "6"
			(at 0.635 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "19"
			(at 0.635 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at 1.905 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "8"
			(at -1.905 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "14"
			(at 8.255 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "18"
			(at 3.175 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at -8.255 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at -1.905 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "13"
			(at -10.795 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4"
			(at 3.175 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "9"
			(at -3.175 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "15"
			(at 6.985 1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at -4.445 -1.27 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "23"
			(at -6.985 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "" np_thru_hole circle
			(at -12.2555 0.508 90)
			(size 2.4384 2.4384)
			(drill 2.4384)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 12.2555 0.508 90)
			(size 2.4384 2.4384)
			(drill 2.4384)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at 10.16 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "2_14_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 8.89 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "3_15_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 6.35 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "4_16_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 3.81 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "5_17_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 2.54 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "6_18_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 1.27 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "7_19_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 0 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "8_20_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -1.27 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "9_21_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -2.54 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "10_22_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at -3.81 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "11_23_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at -6.35 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "12_24_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at -8.89 -2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "13_25_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at -10.16 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at 8.89 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "2_14_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 7.62 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "3_15_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 6.35 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "4_16_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 5.08 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "5_17_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 3.81 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "6_18_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at 1.27 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "7_19_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at -1.27 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "8_20_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at -3.81 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "9_21_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at -5.08 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "10_22_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at -6.35 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "11_23_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at -7.62 0 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "12_24_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at -8.89 2.54 90)
			(size 1.016 1.016)
			(drill 0.635)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "13_25_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 158.6611 99.9236)
		(property "Reference" "U$6"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "6_18_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "6_18_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "6_18_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "6_18_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "6_18_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 148.5011 89.7636)
		(property "Reference" "U$2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "2_14_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "2_14_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "2_14_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "2_14_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "2_14_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 148.5011 99.9236)
		(property "Reference" "U$5"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "5_17_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "5_17_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "5_17_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "5_17_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "5_17_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "SMA"
		(layer "F.Cu")
		(at 168.8211 99.9236)
		(property "Reference" "U$7"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SMA-JACK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND1" thru_hole circle
			(at -2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "7_19_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "7_19_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "7_19_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "GND4" thru_hole circle
			(at -2.54 2.54)
			(size 2.1844 2.1844)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "7_19_N")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "PIN" thru_hole circle
			(at 0 0)
			(size 2.1844 2.1844)
			(drill 1.397)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "7_19_P")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 123.1011 127.8636)
		(end 124.3711 129.1336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.6311 80.8736)
		(end 173.9011 82.1436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.6311 80.8736)
		(end 124.3711 80.8736)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.1011 82.1436)
		(end 123.1011 127.8636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.6311 129.1336)
		(end 124.3711 129.1336)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.6311 129.1336)
		(end 173.9011 127.8636)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.9011 127.8636)
		(end 173.9011 82.1436)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.1011 82.1436)
		(end 124.3711 80.8736)
		(layer "Edge.Cuts")
	)
	(gr_text "8"
		(at 154.8511 105.6386 0)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 144.6911 116.4336 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 165.0111 96.1136 0)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 165.0111 116.4336 0)
		(layer "F.SilkS")
	)
	(gr_text "uD-SMA Breakout \nDesign by BS 01.18.21\nModified by JMA 07.09.25"
		(at 125.558046 88.191857 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 144.6911 105.6386 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 164.3761 86.5886 0)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 154.8511 116.4336 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 154.2161 86.5886 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 165.0111 105.6386 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 154.8511 96.1136 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 144.6911 86.5886 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 144.6911 96.1136 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.0381)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.1262)
			(thermal_bridge_width 0.1262)
		)
		(polygon
			(pts
				(xy 173.9392 127.879382) (xy 172.646882 129.1717) (xy 124.355318 129.1717) (xy 123.063 127.879382)
				(xy 123.063 125.2855) (xy 173.9392 125.2855)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.0635)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.177)
			(thermal_bridge_width 0.177)
		)
		(polygon
			(pts
				(xy 173.9646 82.117297) (xy 173.9646 84.7471) (xy 123.0376 84.7471) (xy 123.0376 80.8101) (xy 172.657403 80.8101)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.0635)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.177)
			(thermal_bridge_width 0.177)
		)
		(polygon
			(pts
				(xy 173.9646 127.889903) (xy 172.657403 129.1971) (xy 123.0376 129.1971) (xy 123.0376 125.2601)
				(xy 173.9646 125.2601)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.0381)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.1262)
			(thermal_bridge_width 0.1262)
		)
		(polygon
			(pts
				(xy 173.9392 127.879382) (xy 172.646882 129.1717) (xy 124.355318 129.1717) (xy 123.063 127.879382)
				(xy 123.063 125.2855) (xy 173.9392 125.2855)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.0635)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.177)
			(thermal_bridge_width 0.177)
		)
		(polygon
			(pts
				(xy 173.9646 82.117297) (xy 173.9646 84.7471) (xy 123.0376 84.7471) (xy 123.0376 80.8101) (xy 172.657403 80.8101)
			)
		)
	)
	(embedded_fonts no)
)
