(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 12)
    (no_connects 0)
    (area 161.214999 107.874999 171.525001 118.185001)
    (thickness 1.6)
    (drawings 8)
    (tracks 63)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VDD)
  (net 3 /MOSI)
  (net 4 /MISO)
  (net 5 /SCK)
  (net 6 /CS)
  (net 7 /INT2)
  (net 8 /INT1)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CS)
    (add_net /INT1)
    (add_net /INT2)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net GND)
    (add_net VDD)
  )
  (module Capacitors_SMD:C_0805 (layer Top) (tedit 5415D6EA)
    (at 166.37 115.824)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.6985 -1.5875) (layer F.SilkS))
    (fp_text value 100nF (at 0 5.5245) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer Top) (tedit 58673BB4)
    (at 162.56 109.22)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39) (layer F.Fab))
    (fp_text value CONN_01X04 (at 7.5565 -4.191) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /MOSI))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MISO))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SCK))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /CS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer Top) (tedit 58673B87)
    (at 170.18 116.84 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P2 (at 0 -2.39 180) (layer F.Fab))
    (fp_text value CONN_01X04 (at 0 10.287 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /INT2))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /INT1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VDD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module bmi160:BMI160 (layer Top) (tedit 58670696)
    (at 166.37 111.252)
    (fp_text reference U1 (at -1.905 -1.524) (layer F.SilkS))
    (fp_text value BMI160 (at 1.524 2.032) (layer Dwgs.User))
    (pad 1 smd rect (at -1.3 -0.5) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 4 /MISO))
    (pad 2 smd rect (at -1.3 0) (size 0.675 0.25) (layers Top F.Paste F.Mask))
    (pad 3 smd rect (at -1.3 0.5) (size 0.675 0.25) (layers Top F.Paste F.Mask))
    (pad 4 smd rect (at -1.3 1) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 8 /INT1))
    (pad 5 smd rect (at -0.5 1.3 90) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 2 VDD))
    (pad 6 smd rect (at 0 1.3 90) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.5 1.3 90) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.3 1 180) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 2 VDD))
    (pad 9 smd rect (at 1.3 0.5 180) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 7 /INT2))
    (pad 10 smd rect (at 1.3 0 180) (size 0.675 0.25) (layers Top F.Paste F.Mask))
    (pad 11 smd rect (at 1.3 -0.5 180) (size 0.675 0.25) (layers Top F.Paste F.Mask))
    (pad 12 smd rect (at 0.5 -0.8 270) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 6 /CS))
    (pad 13 smd rect (at 0 -0.8 270) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 5 /SCK))
    (pad 14 smd rect (at -0.5 -0.8 270) (size 0.675 0.25) (layers Top F.Paste F.Mask)
      (net 3 /MOSI))
  )
  (gr_text "BMI160 v1\nTelltale HRV" (at 166.37 113.0935 90) (layer B.SilkS))
  (dimension 7.62 (width 0.3) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 166.321968 125.048) (layer Dwgs.User))
    (feature1 (pts (xy 170.131968 109.22) (xy 170.131968 126.398)))
    (feature2 (pts (xy 162.511968 109.22) (xy 162.511968 126.398)))
    (crossbar (pts (xy 162.511968 123.698) (xy 170.131968 123.698)))
    (arrow1a (pts (xy 170.131968 123.698) (xy 169.005464 124.284421)))
    (arrow1b (pts (xy 170.131968 123.698) (xy 169.005464 123.111579)))
    (arrow2a (pts (xy 162.511968 123.698) (xy 163.638472 124.284421)))
    (arrow2b (pts (xy 162.511968 123.698) (xy 163.638472 123.111579)))
  )
  (dimension 10.16 (width 0.3) (layer Dwgs.User)
    (gr_text "10.160 mm" (at 166.37 99.996) (layer Dwgs.User))
    (feature1 (pts (xy 171.45 107.95) (xy 171.45 98.646)))
    (feature2 (pts (xy 161.29 107.95) (xy 161.29 98.646)))
    (crossbar (pts (xy 161.29 101.346) (xy 171.45 101.346)))
    (arrow1a (pts (xy 171.45 101.346) (xy 170.323496 101.932421)))
    (arrow1b (pts (xy 171.45 101.346) (xy 170.323496 100.759579)))
    (arrow2a (pts (xy 161.29 101.346) (xy 162.416504 101.932421)))
    (arrow2b (pts (xy 161.29 101.346) (xy 162.416504 100.759579)))
  )
  (dimension 10.16 (width 0.3) (layer Dwgs.User)
    (gr_text "10.160 mm" (at 154.4155 113.03 270) (layer Dwgs.User))
    (feature1 (pts (xy 161.29 118.11) (xy 153.0655 118.11)))
    (feature2 (pts (xy 161.29 107.95) (xy 153.0655 107.95)))
    (crossbar (pts (xy 155.7655 107.95) (xy 155.7655 118.11)))
    (arrow1a (pts (xy 155.7655 118.11) (xy 155.179079 116.983496)))
    (arrow1b (pts (xy 155.7655 118.11) (xy 156.351921 116.983496)))
    (arrow2a (pts (xy 155.7655 107.95) (xy 155.179079 109.076504)))
    (arrow2b (pts (xy 155.7655 107.95) (xy 156.351921 109.076504)))
  )
  (gr_line (start 161.29 107.95) (end 161.29 118.11) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 107.95) (end 161.29 107.95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.45 118.11) (end 171.45 107.95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.29 118.11) (end 171.45 118.11) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.45 107.95) (xy 161.29 107.95) (xy 161.29 118.11) (xy 171.45 118.11)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 107.95) (xy 171.45 107.95) (xy 171.45 118.11) (xy 161.29 118.11)
      )
    )
  )
)
