(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 263)
    (zones 0)
    (modules 22)
    (nets 48)
  )
  (page USLetter)
  (title_block
    (date 2019-03-11)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(S1-Pad1)")
  (net 4 "Net-(S1-Pad2)")
  (net 5 "Net-(S1-Pad3)")
  (net 6 "Net-(S2-Pad3)")
  (net 7 "Net-(S2-Pad2)")
  (net 8 "Net-(S2-Pad1)")
  (net 9 "Net-(S3-Pad1)")
  (net 10 "Net-(S3-Pad2)")
  (net 11 "Net-(S3-Pad3)")
  (net 12 "Net-(S4-Pad3)")
  (net 13 "Net-(S4-Pad2)")
  (net 14 "Net-(S4-Pad1)")
  (net 15 "Net-(S5-Pad1)")
  (net 16 "Net-(S5-Pad2)")
  (net 17 "Net-(S5-Pad3)")
  (net 18 "Net-(J0-Pad1)")
  (net 19 "Net-(J0-Pad2)")
  (net 20 "Net-(J0-Pad3)")
  (net 21 "Net-(J1-Pad1)")
  (net 22 "Net-(J1-Pad2)")
  (net 23 "Net-(J1-Pad3)")
  (net 24 "Net-(J2-Pad3)")
  (net 25 "Net-(J2-Pad2)")
  (net 26 "Net-(J2-Pad1)")
  (net 27 "Net-(S0-Pad1)")
  (net 28 "Net-(S0-Pad2)")
  (net 29 "Net-(S0-Pad3)")
  (net 30 "Net-(J3-Pad3)")
  (net 31 "Net-(J3-Pad2)")
  (net 32 "Net-(J3-Pad1)")
  (net 33 "Net-(J4-Pad1)")
  (net 34 "Net-(J4-Pad2)")
  (net 35 "Net-(J4-Pad3)")
  (net 36 "Net-(J5-Pad3)")
  (net 37 "Net-(J5-Pad2)")
  (net 38 "Net-(J5-Pad1)")
  (net 39 "Net-(Q30-Pad2)")
  (net 40 "Net-(Q31-Pad2)")
  (net 41 "Net-(Q32-Pad2)")
  (net 42 "Net-(Q40-Pad2)")
  (net 43 "Net-(Q41-Pad2)")
  (net 44 "Net-(Q42-Pad2)")
  (net 45 "Net-(Q50-Pad2)")
  (net 46 "Net-(Q51-Pad2)")
  (net 47 "Net-(Q52-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J0-Pad1)")
    (add_net "Net-(J0-Pad2)")
    (add_net "Net-(J0-Pad3)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(Q30-Pad2)")
    (add_net "Net-(Q31-Pad2)")
    (add_net "Net-(Q32-Pad2)")
    (add_net "Net-(Q40-Pad2)")
    (add_net "Net-(Q41-Pad2)")
    (add_net "Net-(Q42-Pad2)")
    (add_net "Net-(Q50-Pad2)")
    (add_net "Net-(Q51-Pad2)")
    (add_net "Net-(Q52-Pad2)")
    (add_net "Net-(S0-Pad1)")
    (add_net "Net-(S0-Pad2)")
    (add_net "Net-(S0-Pad3)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S1-Pad2)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(S2-Pad1)")
    (add_net "Net-(S2-Pad2)")
    (add_net "Net-(S2-Pad3)")
    (add_net "Net-(S3-Pad1)")
    (add_net "Net-(S3-Pad2)")
    (add_net "Net-(S3-Pad3)")
    (add_net "Net-(S4-Pad1)")
    (add_net "Net-(S4-Pad2)")
    (add_net "Net-(S4-Pad3)")
    (add_net "Net-(S5-Pad1)")
    (add_net "Net-(S5-Pad2)")
    (add_net "Net-(S5-Pad3)")
  )
  (module Arduino:Arduino_Mega2560_Shield (layer F.Cu) (tedit 5A8605D3)
    (at 110.565001 116.915001)
    (descr https://store.arduino.cc/arduino-mega-2560-rev3)
    (fp_text reference XA1 (at 2.54 -54.356) (layer F.SilkS))
    (fp_text value Arduino_Mega2560_Shield (at 15.494 -54.356) (layer F.Fab))
    (fp_text user . (at 62.484 -32.004) (layer F.SilkS))
    (pad RST2 thru_hole oval (at 63.627 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad GND4 thru_hole oval (at 66.167 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad MOSI thru_hole oval (at 66.167 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad SCK thru_hole oval (at 63.627 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5V2 thru_hole oval (at 66.167 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A0 thru_hole oval (at 50.8 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad VIN thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad GND3 thru_hole oval (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad GND2 thru_hole oval (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5V1 thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3V3 thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad RST1 thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad IORF thru_hole oval (at 30.48 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D21 thru_hole oval (at 86.36 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D20 thru_hole oval (at 83.82 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D19 thru_hole oval (at 81.28 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D18 thru_hole oval (at 78.74 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D17 thru_hole oval (at 76.2 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D16 thru_hole oval (at 73.66 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D15 thru_hole oval (at 71.12 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D14 thru_hole oval (at 68.58 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D0 thru_hole oval (at 63.5 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D1 thru_hole oval (at 60.96 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D2 thru_hole oval (at 58.42 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D3 thru_hole oval (at 55.88 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D4 thru_hole oval (at 53.34 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D5 thru_hole oval (at 50.8 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D6 thru_hole oval (at 48.26 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D7 thru_hole oval (at 45.72 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad GND1 thru_hole oval (at 26.416 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad D8 thru_hole oval (at 41.656 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D9 thru_hole oval (at 39.116 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D10 thru_hole oval (at 36.576 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(J0-Pad1)"))
    (pad "" np_thru_hole circle (at 66.04 -7.62) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 66.04 -35.56) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 90.17 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 15.24 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 96.52 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 13.97 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad SCL thru_hole oval (at 18.796 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad SDA thru_hole oval (at 21.336 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad AREF thru_hole oval (at 23.876 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad D13 thru_hole oval (at 28.956 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad1)"))
    (pad D12 thru_hole oval (at 31.496 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J0-Pad3)"))
    (pad D11 thru_hole oval (at 34.036 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(J0-Pad2)"))
    (pad "" thru_hole oval (at 27.94 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A1 thru_hole oval (at 53.34 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A2 thru_hole oval (at 55.88 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A3 thru_hole oval (at 58.42 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A4 thru_hole oval (at 60.96 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A5 thru_hole oval (at 63.5 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A6 thru_hole oval (at 66.04 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A7 thru_hole oval (at 68.58 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A8 thru_hole oval (at 73.66 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A9 thru_hole oval (at 76.2 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A10 thru_hole oval (at 78.74 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A11 thru_hole oval (at 81.28 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A12 thru_hole oval (at 83.82 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A13 thru_hole oval (at 86.36 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A14 thru_hole oval (at 88.9 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad A15 thru_hole oval (at 91.44 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 5V3 thru_hole oval (at 93.98 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5V4 thru_hole oval (at 96.52 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad D22 thru_hole oval (at 93.98 -48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad2)"))
    (pad D23 thru_hole oval (at 96.52 -48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (pad D24 thru_hole oval (at 93.98 -45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad1)"))
    (pad D25 thru_hole oval (at 96.52 -45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad2)"))
    (pad D26 thru_hole oval (at 93.98 -43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad3)"))
    (pad D27 thru_hole oval (at 96.52 -43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(Q30-Pad2)"))
    (pad D28 thru_hole oval (at 93.98 -40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(Q31-Pad2)"))
    (pad D29 thru_hole oval (at 96.52 -40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(Q32-Pad2)"))
    (pad D30 thru_hole oval (at 93.98 -38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(Q40-Pad2)"))
    (pad D31 thru_hole oval (at 96.52 -38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(Q41-Pad2)"))
    (pad D32 thru_hole oval (at 93.98 -35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "Net-(Q42-Pad2)"))
    (pad D33 thru_hole oval (at 96.52 -35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "Net-(Q50-Pad2)"))
    (pad D34 thru_hole oval (at 93.98 -33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "Net-(Q51-Pad2)"))
    (pad D35 thru_hole oval (at 96.52 -33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "Net-(Q52-Pad2)"))
    (pad D36 thru_hole oval (at 93.98 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(S0-Pad1)"))
    (pad D37 thru_hole oval (at 96.52 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(S0-Pad2)"))
    (pad D38 thru_hole oval (at 93.98 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(S0-Pad3)"))
    (pad D39 thru_hole oval (at 96.52 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(S1-Pad1)"))
    (pad D40 thru_hole oval (at 93.98 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(S1-Pad2)"))
    (pad D41 thru_hole oval (at 96.52 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(S1-Pad3)"))
    (pad D42 thru_hole oval (at 93.98 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(S2-Pad1)"))
    (pad D43 thru_hole oval (at 96.52 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(S2-Pad2)"))
    (pad D44 thru_hole oval (at 93.98 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(S2-Pad3)"))
    (pad D45 thru_hole oval (at 96.52 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(S3-Pad1)"))
    (pad D46 thru_hole oval (at 93.98 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(S3-Pad2)"))
    (pad D47 thru_hole oval (at 96.52 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(S3-Pad3)"))
    (pad D48 thru_hole oval (at 93.98 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(S4-Pad1)"))
    (pad D49 thru_hole oval (at 96.52 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(S4-Pad2)"))
    (pad D50 thru_hole oval (at 93.98 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(S4-Pad3)"))
    (pad D51 thru_hole oval (at 96.52 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(S5-Pad1)"))
    (pad D52 thru_hole oval (at 93.98 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(S5-Pad2)"))
    (pad D53 thru_hole oval (at 96.52 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(S5-Pad3)"))
    (pad GND5 thru_hole oval (at 93.98 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad GND6 thru_hole oval (at 96.52 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad MISO thru_hole oval (at 63.627 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
  )
  (module Connect_JST:JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 130.81 73.7 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference J0 (at -4.485 0 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.75 3.4 270) (layer F.Fab))
    (fp_text user %R (at 3.75 1.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 18 "Net-(J0-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 "Net-(J0-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 20 "Net-(J0-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 139.065 73.7 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference J1 (at -4.485 0 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.75 3.4 270) (layer F.Fab))
    (fp_text user %R (at 3.75 1.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 21 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 147.32 73.66 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference J2 (at -4.445 0 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.75 3.4 270) (layer F.Fab))
    (fp_text user %R (at 3.75 1.5 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 26 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 163.83 73.66 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference J3 (at -4.445 0 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.75 3.4 270) (layer F.Fab))
    (fp_text user %R (at 3.75 1.5 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 32 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 182.88 73.66 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference J4 (at -4.445 0 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.75 3.4 270) (layer F.Fab))
    (fp_text user %R (at 3.75 1.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 33 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 194.945 73.7 270)
    (descr "JST EH series connector, B4B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference J5 (at -4.485 0 270) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.75 3.4 270) (layer F.Fab))
    (fp_text user %R (at 3.75 1.5 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 38 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B4B-EH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 153.035 93.345 270)
    (descr "JST EH series connector, B5B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference S1 (at 5 -2.8 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 3.4 270) (layer F.Fab))
    (fp_text user %R (at 5 1.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 3 "Net-(S1-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 "Net-(S1-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 "Net-(S1-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 161.29 93.345 270)
    (descr "JST EH series connector, B5B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference S2 (at 5 -2.8 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 3.4 270) (layer F.Fab))
    (fp_text user %R (at 5 1.5 270) (layer F.Fab))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 "Net-(S2-Pad3)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(S2-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 8 "Net-(S2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 169.545 93.345 270)
    (descr "JST EH series connector, B5B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference S3 (at 5 -2.8 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 3.4 270) (layer F.Fab))
    (fp_text user %R (at 5 1.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 9 "Net-(S3-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 "Net-(S3-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 "Net-(S3-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 182.88 93.345 270)
    (descr "JST EH series connector, B5B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference S4 (at 5 -2.8 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 3.4 270) (layer F.Fab))
    (fp_text user %R (at 5 1.5 270) (layer F.Fab))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 "Net-(S4-Pad3)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 "Net-(S4-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 14 "Net-(S4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 191.135 93.345 270)
    (descr "JST EH series connector, B5B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference S5 (at 5 -2.8 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 3.4 270) (layer F.Fab))
    (fp_text user %R (at 5 1.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 15 "Net-(S5-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 "Net-(S5-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 17 "Net-(S5-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect_JST:JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical (layer F.Cu) (tedit 5C28142C)
    (at 144.78 93.345 270)
    (descr "JST EH series connector, B5B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST EH vertical")
    (fp_text reference S0 (at 5 -2.8 270) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 5 3.4 270) (layer F.Fab))
    (fp_text user %R (at 5 1.5 270) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 27 "Net-(S0-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 28 "Net-(S0-Pad2)"))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 29 "Net-(S0-Pad3)"))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_EH_B5B-EH-A_1x05_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 167.64 72.39)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q30 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 39 "Net-(Q30-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 167.64 77.47)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q31 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 40 "Net-(Q31-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 167.64 82.55)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q32 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 41 "Net-(Q32-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 186.69 72.39)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q40 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 42 "Net-(Q40-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 186.700001 77.47)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q41 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 43 "Net-(Q41-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 186.69 82.55)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q42 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad3)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 44 "Net-(Q42-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 198.755 72.39)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q50 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 45 "Net-(Q50-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 38 "Net-(J5-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 198.755 77.47)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q51 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 46 "Net-(Q51-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 198.755 82.55)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q52 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 47 "Net-(Q52-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "marginallyclever.com\nSixi 2 mega shield v1\nDan Royer 2019-03-11" (at 131.445 99.695 90) (layer B.SilkS))
  (gr_line (start 208.28 116.84) (end 207.645 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.55 115.57) (end 208.28 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.55 114.935) (end 209.55 115.57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.825 63.5) (end 125.095 63.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 65.405) (end 123.825 63.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 115.57) (end 121.92 65.405) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.19 116.84) (end 121.92 115.57) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.825 116.84) (end 123.19 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.645 116.84) (end 123.825 116.84) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 209.55 64.77) (end 209.55 114.935) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 208.28 63.5) (end 209.55 64.77) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.095 63.5) (end 208.28 63.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.49 63.5) (xy 208.28 63.5) (xy 210.185 65.405) (xy 210.185 76.2) (xy 212.725 78.74)
        (xy 212.725 113.03) (xy 209.55 117.475) (xy 110.49 116.84)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.49 63.5) (xy 208.28 63.5) (xy 210.185 65.405) (xy 210.185 76.2) (xy 212.725 78.74)
        (xy 212.725 113.03) (xy 209.55 117.475) (xy 110.49 116.84)
      )
    )
  )
)
