(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Quad ESL-63 Zener Clamp Board")
    (date "12/3/2016")
    (company "SDS Labs")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-K)")
  (net 2 "Net-(D1-A)")
  (net 3 "Net-(D15-A)")
  (net 4 "Net-(D16-A)")
  (net 5 "Net-(D5-A)")
  (net 6 "Net-(D6-A)")
  (net 7 "Net-(D7-A)")
  (net 8 "Net-(D8-A)")
  (net 9 "Net-(D10-K)")
  (net 10 "Net-(D10-A)")
  (net 11 "Net-(D11-A)")
  (net 12 "Net-(D12-A)")
  (net 13 "Net-(D13-A)")
  (net 14 "Net-(D14-A)")
  (net 15 "Net-(D16-K)")
  (net 16 "Net-(D17-A)")
  (net 17 "Net-(D18-A)")
  (net 18 "Net-(D20-A)")
  (net 19 "Net-(D21-A)")
  (net 20 "Net-(D22-A)")
  (net 21 "Net-(D23-A)")
  (net 22 "Net-(D24-A)")
  (net 23 "Net-(D25-K)")
  (net 24 "Net-(D26-A)")
  (net 25 "Net-(D27-A)")
  (net 26 "Net-(D28-A)")
  (net 27 "Net-(D29-A)")
  (net 28 "Net-(D31-K)")
  (net 29 "Net-(D32-A)")
  (net 30 "Net-(D33-A)")
  (net 31 "Net-(D35-A)")
  (net 32 "Net-(D36-A)")
  (net 33 "Net-(D37-A)")
  (net 34 "Net-(D38-A)")
  (net 35 "Net-(D39-A)")
  (net 36 "Net-(D40-A)")
  (net 37 "Net-(D41-A)")
  (net 38 "Net-(D42-A)")
  (net 39 "Net-(D43-A)")
  (net 40 "Net-(D44-A)")
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 104.14 73.66)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 5.08 -2.47) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 146.05 73.66)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at 5.08 -2.47) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D1-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D15-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 99.314 75.184 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at 5.08 -2.47 -90) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D16-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 160.02 85.725 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at 5.08 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D16-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D15-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 99.314 99.314 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D16" (at 5.08 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D16-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D16-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 160.02 90.424 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D17" (at 5.08 -2.47 -90) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D16-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D17-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 99.314 102.997 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D18" (at 5.08 -2.47 -90) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D16-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(D18-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 159.893 114.554 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D19" (at 5.08 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(D18-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(D17-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (at 131.318 101.092 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D25" (at 1.27 -3.96 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 23 "Net-(D25-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 22 "Net-(D24-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 99.314 127.254 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D31" (at 5.08 -2.47 90) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 5.47 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(D31-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(D18-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 159.766 120.65 180)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D32" (at 5.08 -2.47 180) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47 180) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 180) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(D18-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D32-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 99.314 142.494)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D33" (at 5.08 -2.47) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 28 "Net-(D31-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(D33-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (layer "F.Cu")
    (at 125.984 142.621)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D34" (at 5.08 -2.47) (layer "F.SilkS"))
    (fp_text value "D" (at 5.08 2.47) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(D33-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D32-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connect:1pin" (layer "F.Cu")
    (at 125.984 73.66)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at -2.921 1.651) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 2.794) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at 0 0) (size 6.35 3.81) (drill 1.5875) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D1-A)") (pinfunction "P1") (pintype "passive"))
  )
  (footprint "Connect:1pin" (layer "F.Cu")
    (at 116.205 142.621)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags "DEV")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P2" (at -2.794 -2.921) (layer "F.SilkS"))
    (fp_text value "CONN_01X01" (at 0 2.794) (layer "F.Fab") hide)
    (pad "1" thru_hole oval (at 0 0) (size 6.35 3.81) (drill 1.5875) (layers "*.Cu" "*.Mask")
      (net 30 "Net-(D33-A)") (pinfunction "P1") (pintype "passive"))
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 105.41 83.775 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at -4.405 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 1 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 5 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 110.236 83.82 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 4.445 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 5 "Net-(D5-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 6 "Net-(D6-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 115.062 83.775 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D7" (at -4.54 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 6 "Net-(D6-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 7 "Net-(D7-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 119.888 83.82 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D8" (at 4.445 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 7 "Net-(D7-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 8 "Net-(D8-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 124.714 83.775 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D9" (at -4.445 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 8 "Net-(D8-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 9 "Net-(D10-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 129.54 83.82 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D10" (at 4.35 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 9 "Net-(D10-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 10 "Net-(D10-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 134.366 83.775 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D11" (at -4.445 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 10 "Net-(D10-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 11 "Net-(D11-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 139.192 83.82 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D12" (at 4.445 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 11 "Net-(D11-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 12 "Net-(D12-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 144.018 83.775 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D13" (at -4.445 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 12 "Net-(D12-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 13 "Net-(D13-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 148.844 83.82 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D14" (at 4.35 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 13 "Net-(D13-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 14 "Net-(D14-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 153.67 83.775 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D15" (at -4.35 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 14 "Net-(D14-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 3 "Net-(D15-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 104.775 103.41 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D20" (at -4.54 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 15 "Net-(D16-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 18 "Net-(D20-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 109.5375 103.455 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D21" (at 4.495 -0.3175 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 18 "Net-(D20-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 19 "Net-(D21-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 114.3 103.41 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D22" (at -4.54 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 19 "Net-(D21-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 20 "Net-(D22-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 119.0625 103.455 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D23" (at 4.495 -0.3175 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 20 "Net-(D22-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 21 "Net-(D23-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 123.825 103.41 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D24" (at -4.54 0 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 21 "Net-(D23-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 22 "Net-(D24-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 135.89 103.455 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D26" (at 4.495 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 23 "Net-(D25-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 24 "Net-(D26-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 140.6525 103.41 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D27" (at -4.54 0.3175 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 24 "Net-(D26-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 25 "Net-(D27-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 145.415 103.455 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D28" (at 4.495 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 25 "Net-(D27-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 26 "Net-(D28-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 150.1775 103.41 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D29" (at -4.54 0.3175 180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 26 "Net-(D28-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 90) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 27 "Net-(D29-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 154.94 103.455 -90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D30" (at 4.495 0 -180) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 27 "Net-(D29-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 270) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 16 "Net-(D17-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 107.455 132.715)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D35" (at -0.14 2.54) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.485) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 28 "Net-(D31-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 31 "Net-(D35-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 107.41 127.3175 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D36" (at 0.095 -2.8575) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 31 "Net-(D35-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 32 "Net-(D36-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 107.455 121.92)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D37" (at 0 2.54) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 4.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 32 "Net-(D36-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 33 "Net-(D37-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 116.885 121.92)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D38" (at -0.045 2.54) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 4.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 33 "Net-(D37-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 34 "Net-(D38-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 116.84 127.3175 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D39" (at 0 -2.8575) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 34 "Net-(D38-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 35 "Net-(D39-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 116.885 132.715)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D40" (at -0.045 2.54) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.485) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 35 "Net-(D39-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 36 "Net-(D40-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 126.555 132.715)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D41" (at 0.445 2.54) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0.19 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.485) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 36 "Net-(D40-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 37 "Net-(D41-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 126.51 127.3175 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D42" (at 0 -2.8575) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at -0.19 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 37 "Net-(D41-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 38 "Net-(D42-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 126.555 121.92)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D43" (at 0 2.54) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0.19 4.31) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 38 "Net-(D42-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 39 "Net-(D43-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 135.935 127.3175)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D44" (at 0 2.8575) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 39 "Net-(D43-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 40 "Net-(D44-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMA" (layer "F.Cu")
    (at 135.89 132.715 180)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (property "Sheetfile" "C:/Users/stokessd/Documents/Circuit Boards/esl63_zener_board/esl63_zener_boards.sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D45" (at 0 -2.54) (layer "F.SilkS"))
    (fp_text value "ZENERsmall" (at 0 6.485) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.5) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 40 "Net-(D44-A)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 2 0 180) (size 2.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1388888889)
      (net 29 "Net-(D32-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Mounting_Holes:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 172.212 89.408)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Mounting_Holes:MountingHole_4.3mm_M4" (layer "F.Cu")
    (at 172.212 140.208)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (attr through_hole)
    (fp_text reference "REF**" (at 0 -5.3) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_4.3mm_M4" (at 0 5.3) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Symbol:Symbol_HighVoltage_Type2_CopperTop_VerySmall" (layer "F.Cu")
    (at 157.48 139.065 90)
    (descr "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (tags "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at -0.127 -5.715 90) (layer "F.SilkS") hide)
    (fp_text value "Symbol_HighVoltage_Type2_CopperTop_VerySmall" (at -0.381 4.572 90) (layer "F.Fab"))
  )
  (footprint "sdsLogos:sdsLabs-large-fSilk" (layer "F.Cu")
    (at 168.29 113.57 90)
    (attr through_hole)
    (fp_text reference "G***" (at 0 -7.62 90) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0 -5.08 90) (layer "F.SilkS") hide)
  )
  (gr_line (start 176.149 70.231) (end 176.149 141.351)
    (layer "Edge.Cuts"))
  (gr_line (start 94.869 70.231) (end 94.869 146.431)
    (layer "Edge.Cuts"))
  (gr_line (start 144.399 123.571) (end 144.399 146.431)
    (layer "Edge.Cuts"))
  (gr_circle (center 172.339 89.281) (end 173.609 89.281)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 171.069 146.431) (end 150.749 146.431)
    (layer "Edge.Cuts"))
  (gr_line (start 150.749 123.571) (end 144.399 123.571)
    (layer "Edge.Cuts"))
  (gr_line (start 144.399 146.431) (end 94.869 146.431)
    (layer "Edge.Cuts"))
  (gr_line (start 94.869 70.231) (end 176.149 70.231)
    (layer "Edge.Cuts"))
  (gr_line (start 176.149 141.351) (end 171.069 146.431)
    (layer "Edge.Cuts"))
  (gr_circle (center 172.339 140.081) (end 173.609 140.081)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 150.749 146.431) (end 150.749 123.571)
    (layer "Edge.Cuts"))
  (gr_text "ESL63 Zener Board" (at 173.99 114.173 90) (layer "F.SilkS"))
)
