<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="50.995078125" y1="37.084" x2="12.297221875" y2="37.084" width="0" layer="20"/>
<wire x1="12.297221875" y1="37.084" x2="11.43" y2="36.216778125" width="0" layer="20" curve="90"/>
<wire x1="11.43" y1="36.216778125" x2="11.43" y2="8.487221875" width="0" layer="20"/>
<wire x1="11.43" y1="8.487221875" x2="12.297221875" y2="7.62" width="0" layer="20" curve="90"/>
<wire x1="12.297221875" y1="7.62" x2="50.995078125" y2="7.62" width="0" layer="20"/>
<wire x1="50.995078125" y1="7.62" x2="52.07" y2="8.694921875" width="0" layer="20" curve="90"/>
<wire x1="52.07" y1="8.694921875" x2="52.07" y2="36.009078125" width="0" layer="20"/>
<wire x1="52.07" y1="36.009078125" x2="50.995078125" y2="37.084" width="0" layer="20" curve="90"/>
<text>Output</text>
<text>12V</text>
<text>GND</text>
<text>LED</text>
<text>RV-Project.Com</text>
<text>3/5/2019 Rev D</text>
<text>2A Max</text>
<text>RX Adapter Board</text>
<text>A=Light On/Relay Off</text>
<text>B=Light On/Relay On</text>
<text>PGM</text>
<text>Use 2 Oz Copper!</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="KEYSTONE3578">
</package>
<package name="1X01_HEADER">
<description>Drill: 0.039" dia</description>
</package>
<package name="1206-RES">
</package>
<package name="BIGFOOT_MEDIUM">
</package>
<package name="SOD-123(LARGE)">
<description>Suitable for LL4148, FDLL4148, etc/&lt;br&gt;Pad Size:  0.25"x0.7"</description>
</package>
<package name="DO214AC_JBEND">
<description>Pad Size: 0.3"x0.1"</description>
</package>
<package name="FUSE476">
<description>Pad Size: 0.38"x0.15"</description>
</package>
<package name="KEYSTONE_4919">
</package>
<package name="SMA-DIODE_ALT">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;SMA diode.&lt;br&gt;
Pad Size: 0.25"x0.09"</description>
</package>
<package name="ACJ11XX_RELAY">
</package>
<package name="SMD-JUMPER_3">
<description>Pad Size: 0.18"x0.06"&lt;br&gt;Resist remoted between pads for ease of solder bridge.</description>
</package>
<package name="MICRO_RECEIVER_PGM">
<description>Pitch: 0.1" (2.54mm)</description>
</package>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP3" library="a-lib" package="KEYSTONE3578" value="">
<attribute name="CLASSIFICATION" value="Low Insertion"/>
<attribute name="ORENTATION" value="vertical"/>
<attribute name="TAB" value="0.187"/>
<attribute name="THICKNESS" value="0.020"/>
</element>
<element name="JP4" library="a-lib" package="KEYSTONE3578" value="">
<attribute name="CLASSIFICATION" value="Low Insertion"/>
<attribute name="ORENTATION" value="vertical"/>
<attribute name="TAB" value="0.187"/>
<attribute name="THICKNESS" value="0.020"/>
</element>
<element name="JP5" library="a-lib" package="KEYSTONE3578" value="">
<attribute name="CLASSIFICATION" value="Low Insertion"/>
<attribute name="ORENTATION" value="vertical"/>
<attribute name="TAB" value="0.187"/>
<attribute name="THICKNESS" value="0.020"/>
</element>
<element name="JP2" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="a-lib" package="1X01_HEADER" value="">
<attribute name="DIAMETER" value=".0315"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE" value="1.5k"/>
</element>
<element name="U$2" library="a-lib" package="BIGFOOT_MEDIUM" value=""/>
<element name="D2" library="a-lib" package="SOD-123(LARGE)" value="TVS-SEASY_SOD-123">
<attribute name="NAME"/>
</element>
<element name="D1" library="a-lib" package="DO214AC_JBEND" value="1N400x">
<attribute name="MARKING" value="M1-M7"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="1N400x"/>
</element>
<element name="F1" library="a-lib" package="FUSE476" value="2.5A">
<attribute name="NAME"/>
<attribute name="VALUE" value="2.5A"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="a-lib" package="KEYSTONE_4919" value=""/>
<element name="JP6" library="a-lib" package="KEYSTONE_4919" value=""/>
<element name="JP7" library="a-lib" package="KEYSTONE_4919" value=""/>
<element name="D3" library="a-lib" package="SMA-DIODE_ALT" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="a-lib" package="ACJ11XX_RELAY" value="SPDT_RELAYACJ11XX">
<attribute name="CURRENT" value="20A"/>
</element>
<element name="J1" library="a-lib" package="SMD-JUMPER_3" value="SMD-JUMPER"/>
<element name="RX1" library="a-lib" package="MICRO_RECEIVER_PGM" value=""/>
<element name="S1" library="a-lib" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-08247"/>
</element>
</elements>
<signals>
<signal name="N$5">
<contactref element="JP1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="D2" pad="A"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP7" pad="T1"/>
<contactref element="JP7" pad="T3"/>
<contactref element="JP7" pad="T2"/>
<contactref element="RX1" pad="GND"/>
</signal>
<signal name="N$9">
<contactref element="JP4" pad="P$1"/>
<contactref element="JP4" pad="P$2"/>
<contactref element="F1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="JP5" pad="P$1"/>
<contactref element="JP5" pad="P$2"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="RX1" pad="12V"/>
</signal>
<signal name="N$3">
<contactref element="JP3" pad="P$1"/>
<contactref element="JP3" pad="P$2"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="JP8" pad="T3"/>
<contactref element="JP8" pad="T1"/>
<contactref element="JP8" pad="T2"/>
</signal>
<signal name="N$6">
<contactref element="F1" pad="P$2"/>
<contactref element="JP6" pad="T1"/>
<contactref element="JP6" pad="T3"/>
<contactref element="JP6" pad="T2"/>
</signal>
<signal name="N$4">
<contactref element="D1" pad="A"/>
<contactref element="K1" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="D3" pad="A"/>
<contactref element="K1" pad="L1"/>
<contactref element="RX1" pad="OUTGND"/>
</signal>
<signal name="N$8">
<contactref element="D3" pad="C"/>
<contactref element="K1" pad="L2"/>
<contactref element="RX1" pad="OUT12V"/>
</signal>
<signal name="N$1">
<contactref element="K1" pad="NC"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="K1" pad="NO"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="S1" pad="3"/>
<contactref element="RX1" pad="S1"/>
</signal>
<signal name="N$13">
<contactref element="S1" pad="1"/>
<contactref element="RX1" pad="S2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
