(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 62)
    (tracks 444)
    (zones 0)
    (modules 41)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.05)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 USB1_FPGA_PULL_D+)
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 USB1_FPGA_PULL_D-)
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D4-Pad2)")
  (net 7 USB1_FPGA_D+)
  (net 8 GND)
  (net 9 /US1VBUS)
  (net 10 +5V)
  (net 11 USB1_FPGA_D-)
  (net 12 "Net-(D8-Pad1)")
  (net 13 USB2_FPGA_PULL_D+)
  (net 14 "Net-(D9-Pad2)")
  (net 15 USB2_FPGA_PULL_D-)
  (net 16 "Net-(D10-Pad1)")
  (net 17 "Net-(D11-Pad2)")
  (net 18 USB2_FPGA_D+)
  (net 19 /US2VBUS)
  (net 20 USB2_FPGA_D-)
  (net 21 GP27)
  (net 22 GN27)
  (net 23 GP26)
  (net 24 GN26)
  (net 25 +3V3)
  (net 26 /FPD1-)
  (net 27 /FPD1+)
  (net 28 /FPD2-)
  (net 29 /FPD2+)
  (net 30 "Net-(D15-Pad1)")
  (net 31 "Net-(D15-Pad2)")
  (net 32 "Net-(D16-Pad1)")
  (net 33 "Net-(D17-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /FPD1+)
    (add_net /FPD1-)
    (add_net /FPD2+)
    (add_net /FPD2-)
    (add_net /US1VBUS)
    (add_net /US2VBUS)
    (add_net GN26)
    (add_net GN27)
    (add_net GND)
    (add_net GP26)
    (add_net GP27)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D17-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net USB1_FPGA_D+)
    (add_net USB1_FPGA_D-)
    (add_net USB1_FPGA_PULL_D+)
    (add_net USB1_FPGA_PULL_D-)
    (add_net USB2_FPGA_D+)
    (add_net USB2_FPGA_D-)
    (add_net USB2_FPGA_PULL_D+)
    (add_net USB2_FPGA_PULL_D-)
  )
  (module parts:radiona-10mm (layer B.Cu) (tedit 0)
    (at 149.4 100.4 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module parts:OSH_10x10 (layer B.Cu) (tedit 0)
    (at 137 85.2 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 142.4 98.05)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.54 0 -90) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 -0.254 -180) (layer F.Fab))
    (fp_text user %R (at 0 0 -90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 GN26))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D17-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_A_Stewart_SS-52100-001_Horizontal (layer F.Cu) (tedit 5CB49A87)
    (at 166.624 91.186 180)
    (descr "USB A connector https://belfuse.com/resources/drawings/stewartconnector/dr-stw-ss-52100-001.pdf")
    (tags "USB_A Female Connector receptacle")
    (fp_text reference US4 (at -6.096 2.667 270) (layer F.SilkS))
    (fp_text value USB_A (at 3.5 14.49) (layer F.Fab))
    (fp_text user %R (at 3.5 5.99) (layer F.Fab))
    (pad 5 thru_hole circle (at 10.07 2.71 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5 thru_hole circle (at -3.07 2.71 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 19 /US2VBUS))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 28 /FPD2-))
    (pad 3 thru_hole circle (at 4.5 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 29 /FPD2+))
    (pad 4 thru_hole circle (at 7 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ../parts/USB_A/usb_A.wrl
      (offset (xyz 3.5 -6 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 157.099 94.996 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D12 (at -0.127 -1.778) (layer F.SilkS))
    (fp_text value 3.6V (at -0.127 0) (layer F.Fab))
    (fp_text user %R (at 0.127 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 USB2_FPGA_D+))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x12_P2.54mm_Horizontal (layer F.Cu) (tedit 59FED5CB)
    (at 126.238 107.95 180)
    (descr "Through hole angled pin header, 2x12, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x12 2.54mm double row")
    (fp_text reference J1 (at 1.27 -1.016) (layer F.SilkS))
    (fp_text value Conn_02x12_Odd_Even (at -1.143 13.843 90) (layer F.Fab))
    (fp_text user %R (at 5.31 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 USB2_FPGA_D-))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 USB2_FPGA_D+))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 +3V3))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 USB1_FPGA_D-))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 USB1_FPGA_D+))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 USB1_FPGA_PULL_D-))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 USB1_FPGA_PULL_D+))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 USB2_FPGA_PULL_D-))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 USB2_FPGA_PULL_D+))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 USB2_FPGA_D-))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 USB2_FPGA_D+))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 USB1_FPGA_D-))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 USB1_FPGA_D+))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 GN26))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 GP26))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 GN27))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 GP27))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 22 thru_hole oval (at 2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 24 thru_hole oval (at 2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x12_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 129.54 106.299 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at -1.143 -4.064 90) (layer F.SilkS))
    (fp_text value 1N914 (at -0.107 0.127 90) (layer F.Fab))
    (fp_text user %R (at -0.234 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 USB1_FPGA_PULL_D+))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 131.826 106.299 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D2 (at -0.889 1.778 90) (layer F.SilkS))
    (fp_text value 1N914 (at 0.1 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 USB1_FPGA_PULL_D+))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 136.652 108.204)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 3.048 0) (layer F.SilkS))
    (fp_text value 1N914 (at 0.127 0) (layer F.Fab))
    (fp_text user %R (at 0.127 -0.127) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 USB1_FPGA_PULL_D-))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 142.748 108.204 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D4 (at -3.048 0) (layer F.SilkS))
    (fp_text value 1N914 (at -0.127 0) (layer F.Fab))
    (fp_text user %R (at 0.127 0.127) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 USB1_FPGA_PULL_D-))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 147.8 94.95)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at 0 1.6) (layer F.SilkS))
    (fp_text value 3.6V (at 0.1 -0.127) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 USB1_FPGA_D+))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module jumper:D_SMA_Jumper_NC (layer F.Cu) (tedit 5DEA313B)
    (at 148.336 83.058 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr virtual)
    (fp_text reference D6 (at -0.095 0 270) (layer F.SilkS))
    (fp_text value 0 (at 0 -0.127 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 0 90) (layer Eco2.User) hide)
    (pad 1 smd roundrect (at -2 0 90) (size 2.5 1.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 9 /US1VBUS))
    (pad 2 smd roundrect (at 2 0 90) (size 2.5 1.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 10 +5V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl_disabled
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 147.8 91.65)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D7 (at 0 1.7) (layer F.SilkS))
    (fp_text value 3.6V (at -0.02 -0.127) (layer F.Fab))
    (fp_text user %R (at 0 -0.127) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 11 USB1_FPGA_D-))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 151.968 88.365 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D8 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 1N914 (at 0.127 0.127) (layer F.Fab))
    (fp_text user %R (at 0.254 0.127) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 13 USB2_FPGA_PULL_D+))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 151.968 91.667)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D9 (at -0.127 1.651) (layer F.SilkS))
    (fp_text value 1N914 (at 0.127 0) (layer F.Fab))
    (fp_text user %R (at -0.254 0.127) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 13 USB2_FPGA_PULL_D+))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 151.968 94.969 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D10 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 1N914 (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0.127 0.127) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 USB2_FPGA_PULL_D-))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 151.968 98.271)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D11 (at -0.127 1.778) (layer F.SilkS))
    (fp_text value 1N914 (at 0 0.127) (layer F.Fab))
    (fp_text user %R (at 0.127 0) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 USB2_FPGA_PULL_D-))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module jumper:D_SMA_Jumper_NC (layer F.Cu) (tedit 5DEA313B)
    (at 152.4 83.058 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr virtual)
    (fp_text reference D13 (at 0 0 90) (layer F.SilkS))
    (fp_text value 0 (at -0.095 0 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.095 0 90) (layer Eco2.User) hide)
    (pad 2 smd roundrect (at 2 0 90) (size 2.5 1.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 10 +5V))
    (pad 1 smd roundrect (at -2 0 90) (size 2.5 1.8) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 19 /US2VBUS))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl_disabled
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 58641869)
    (at 157.099 98.298 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D14 (at -0.127 -1.651) (layer F.SilkS))
    (fp_text value 3.6V (at 0 -0.127) (layer F.Fab))
    (fp_text user %R (at 0.127 0.127) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 20 USB2_FPGA_D-))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 129.286 100.584 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.413 0 90) (layer F.SilkS))
    (fp_text value 1.1k (at -0.1525 -0.127 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 USB1_FPGA_D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.191 100.584 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.413 0 90) (layer F.SilkS))
    (fp_text value 15k (at 0.127 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 USB1_FPGA_D+))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 135.001 100.584 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 1.1k (at 0 -0.127 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 USB1_FPGA_D-))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133.096 100.584 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.413 0.127 90) (layer F.SilkS))
    (fp_text value 15k (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(D4-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 USB1_FPGA_D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.2 93.436 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.413 0 180) (layer F.SilkS))
    (fp_text value 27 (at -0.127 0.127 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /FPD1-))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 USB1_FPGA_D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.177 95.341 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.5145 0 180) (layer F.SilkS))
    (fp_text value 27 (at -0.1015 0.127 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /FPD1+))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 USB1_FPGA_D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 169.5 101 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 1.1k (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 USB2_FPGA_D+))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 164.4 101 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.667 0 90) (layer F.SilkS))
    (fp_text value 15k (at 0 -0.127 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 USB2_FPGA_D+))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 167.829 101.011 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.667 -0.127 90) (layer F.SilkS))
    (fp_text value 1.1k (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 USB2_FPGA_D-))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166.1 101 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -3.048 0 90) (layer F.SilkS))
    (fp_text value 15k (at 0.127 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D11-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 USB2_FPGA_D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166 95.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -2.921 0 180) (layer F.SilkS))
    (fp_text value 27 (at 0 0.127 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 USB2_FPGA_D-))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /FPD2-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 166 97.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -2.921 0 180) (layer F.SilkS))
    (fp_text value 27 (at -0.127 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /FPD2+))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 USB2_FPGA_D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_A_Stewart_SS-52100-001_Horizontal (layer F.Cu) (tedit 5CB49A87)
    (at 140.6 91.1 180)
    (descr "USB A connector https://belfuse.com/resources/drawings/stewartconnector/dr-stw-ss-52100-001.pdf")
    (tags "USB_A Female Connector receptacle")
    (fp_text reference US3 (at -5.969 2.667 90) (layer F.SilkS))
    (fp_text value USB_A (at 3.5 14.49) (layer F.Fab))
    (fp_text user %R (at 3.5 5.99) (layer F.Fab))
    (pad 4 thru_hole circle (at 7 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 3 thru_hole circle (at 4.5 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 27 /FPD1+))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 26 /FPD1-))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.92) (layers *.Cu *.Mask)
      (net 9 /US1VBUS))
    (pad 5 thru_hole circle (at -3.07 2.71 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 8 GND))
    (pad 5 thru_hole circle (at 10.07 2.71 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ../parts/USB_A/usb_A.wrl
      (offset (xyz 3.5 -6 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_IRBlack (layer F.Cu) (tedit 5A6C9BB8)
    (at 145.9 103.5 180)
    (descr "IR-ED, diameter 3.0mm, 2 pins, color: black")
    (tags "IR infrared LED diameter 3.0mm 2 pins black")
    (fp_text reference D15 (at 1.2 -3) (layer F.SilkS))
    (fp_text value LED (at 1.27 0 180) (layer F.Fab))
    (fp_text user %R (at 1.47 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(D15-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_IRBlack.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_IRBlack (layer F.Cu) (tedit 5A6C9BB8)
    (at 150.8 103.5 180)
    (descr "IR-ED, diameter 3.0mm, 2 pins, color: black")
    (tags "IR infrared LED diameter 3.0mm 2 pins black")
    (fp_text reference D16 (at 1.5 -3) (layer F.SilkS))
    (fp_text value LED (at 1.016 0 180) (layer F.Fab))
    (fp_text user %R (at 1.47 0 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(D15-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(D16-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_IRBlack.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm_IRBlack (layer F.Cu) (tedit 5A6C9BB8)
    (at 155.7 103.5 180)
    (descr "IR-ED, diameter 3.0mm, 2 pins, color: black")
    (tags "IR infrared LED diameter 3.0mm 2 pins black")
    (fp_text reference D17 (at 1.3 -3) (layer F.SilkS))
    (fp_text value LED (at 1.27 0 180) (layer F.Fab))
    (fp_text user %R (at 1.47 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(D17-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(D16-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm_IRBlack.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 172.212 96.52)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 +3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 GN27))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 GP27))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 148.4 108.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -3.1 -0.1) (layer F.SilkS))
    (fp_text value 27 (at -0.0255 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +5V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module OptoDevice:Vishay_CAST-3Pin (layer F.Cu) (tedit 5B88841D)
    (at 137.4 97 180)
    (descr "IR Receiver Vishay TSOP-xxxx, CAST package, see https://www.vishay.com/docs/82493/tsop311.pdf")
    (tags "IRReceiverVishayTSOP-xxxx CAST")
    (fp_text reference U1 (at 8.128 3.302) (layer F.SilkS))
    (fp_text value TSOP17xx (at 3.4 4.8 180) (layer F.Fab))
    (fp_text user %R (at 3.8 1.017) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask) (roundrect_rratio 0.178)
      (net 8 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 +3V3))
    (pad 3 thru_hole circle (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 GP26))
    (model ${KISYS3DMOD}/OptoDevice.3dshapes/Vishay_CAST-3Pin.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module parts:radiona-10mm (layer F.Cu) (tedit 0)
    (at 166.025 107.375)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module parts:OSH_5x5 (layer F.Cu) (tedit 0)
    (at 147.15 99.875)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module parts:OSH_10x10 (layer B.Cu) (tedit 0)
    (at 163 85.4 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text +5V (at 121.8 80) (layer B.SilkS))
  (gr_circle (center 139.617563 103.632) (end 140.125563 105.156) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 159.536607 103.632) (end 160.552607 104.902) (layer Edge.Cuts) (width 0.05))
  (gr_text GP20 (at 121.6 108) (layer B.SilkS))
  (gr_text 3V3 (at 121.8 105.4) (layer B.SilkS))
  (gr_text GP26 (at 121.6 87.6) (layer B.SilkS))
  (gr_text GP25 (at 121.6 90.2) (layer B.SilkS))
  (gr_text GP21 (at 121.6 100.4) (layer B.SilkS))
  (gr_text GP27 (at 121.6 85.2) (layer B.SilkS))
  (gr_text GP24 (at 121.6 92.6) (layer B.SilkS))
  (gr_text +5V (at 128.25 80) (layer B.SilkS))
  (gr_text GP22 (at 121.6 97.8) (layer B.SilkS))
  (gr_text GP23 (at 121.6 95.2) (layer B.SilkS))
  (gr_text GND (at 128.2 82.6) (layer B.SilkS))
  (gr_text GND (at 121.8 102.8) (layer B.SilkS))
  (gr_text GN20 (at 128.4 108) (layer B.SilkS))
  (gr_text GND (at 128.2 102.8) (layer B.SilkS))
  (gr_text GN26 (at 128.2 87.8) (layer B.SilkS))
  (gr_text GN25 (at 128.2 90.2) (layer B.SilkS))
  (gr_text GN22 (at 128.4 97.8) (layer B.SilkS))
  (gr_text GN23 (at 128.4 95.4) (layer B.SilkS))
  (gr_text GN24 (at 128.4 92.6) (layer B.SilkS))
  (gr_text 3V3 (at 128.2 105.4) (layer B.SilkS))
  (gr_text GN21 (at 128.2 100.4) (layer B.SilkS))
  (gr_text GN27 (at 128.2 85.2) (layer B.SilkS))
  (gr_text GND (at 121.8 82.6) (layer B.SilkS))
  (gr_line (start 174.244 78.74) (end 119.634 78.74) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.244 109.728) (end 174.244 78.74) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.634 109.728) (end 174.244 109.728) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.634 78.74) (end 119.634 109.728) (layer Edge.Cuts) (width 0.05))
  (gr_text GP20 (at 123.825 106.68) (layer F.SilkS))
  (gr_text GN20 (at 126.238 106.68) (layer F.SilkS))
  (gr_text 3V3 (at 123.825 104.14) (layer F.SilkS))
  (gr_text 3V3 (at 126.238 104.14) (layer F.SilkS))
  (gr_text GND (at 123.825 101.6) (layer F.SilkS))
  (gr_text GND (at 126.238 101.6) (layer F.SilkS))
  (gr_text GN21 (at 126.238 99.06) (layer F.SilkS))
  (gr_text GP21 (at 123.825 99.06) (layer F.SilkS))
  (gr_text GP22 (at 123.825 96.52) (layer F.SilkS))
  (gr_text GN22 (at 126.238 96.52) (layer F.SilkS))
  (gr_text GP23 (at 123.825 93.98) (layer F.SilkS))
  (gr_text GN23 (at 126.238 93.98) (layer F.SilkS))
  (gr_text GP24 (at 123.825 91.44) (layer F.SilkS))
  (gr_text GN24 (at 126.238 91.44) (layer F.SilkS))
  (gr_text GN25 (at 126.238 88.9) (layer F.SilkS))
  (gr_text GP25 (at 123.825 88.9) (layer F.SilkS))
  (gr_text GN26 (at 126.365 86.36) (layer F.SilkS))
  (gr_text GP26 (at 123.825 86.36) (layer F.SilkS))
  (gr_text GN27 (at 126.238 83.82) (layer F.SilkS))
  (gr_text GP27 (at 123.698 83.82) (layer F.SilkS))
  (gr_text GND (at 123.698 81.28) (layer F.SilkS))
  (gr_text GND (at 126.111 81.28) (layer F.SilkS))
  (gr_text +5V (at 128.27 80.01) (layer F.SilkS))
  (zone (net 8) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.625 78.75) (xy 174.25 78.75) (xy 174.25 109.725) (xy 119.625 109.725)
      )
    )
  )
  (zone (net 8) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.65 78.75) (xy 174.25 78.75) (xy 174.25 109.725) (xy 119.65 109.725)
      )
    )
  )
)
