(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/Kick 2")
	(net 2 "GND")
	(net 3 "/Punch 1")
	(net 4 "/Kick 3")
	(net 5 "/Punch 3")
	(net 6 "/Punch 2")
	(net 7 "/Kick 1")
	(net 8 "/Left")
	(net 9 "/Right")
	(net 10 "/Down")
	(net 11 "/Up")
	(net 12 "/Punch 4")
	(net 13 "/Kick 4")
	(net 14 "/Home")
	(net 15 "/Start")
	(net 16 "/Select")
	(net 17 "unconnected-(U1-D7-PadJP7_3)")
	(net 18 "unconnected-(U1-D9-PadJP7_1)")
	(net 19 "unconnected-(U1-~{RESET}-PadJP6_3)")
	(net 20 "unconnected-(U1-D5-PadJP7_5)")
	(net 21 "unconnected-(U1-VCC-PadJP6_4)")
	(net 22 "unconnected-(U1-RAW-PadJP6_1)")
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 108.625 64.897)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Punch 1"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 3 "/Punch 1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 108.752 54.991)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Kick 1"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Kick 1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B5B-XH-A_1x05_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 141.986 81.922 90)
		(descr "JST XH series connector, B5B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Up/Down/Right/Left/GND"
			(at 5 -3.55 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05_Socket"
			(at 5 4.6 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B5B-XH-A_1x05_P2.50mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5 2.7 -90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 11 "/Up")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Down")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Right")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.5 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Left")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10 0 90)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B5B-XH-A_1x05_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 109.006 101.964)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Home"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.103 4.445 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Home")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 130.85 102.108)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Select"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.123 4.462 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Select")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 108.879 92.837)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Punch 4"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Punch 4")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 108.752 74.295)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Kick 2"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Kick 2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 108.879 83.693)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Kick 4"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Kick 4")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:Arduino Pro Micro"
		(layer "F.Cu")
		(at 126.111 80.518)
		(property "Reference" "Arduino Pro Micro"
			(at -1.778 -17.399 0)
			(layer "F.SilkS")
		)
		(property "Value" "Arduino Pro Micro"
			(at 1.27 17.907 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Module:Arduino Pro Micro"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/DEV-12587/SparkFun/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "N/A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/DEV-12587/SparkFun/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "2/12/2015"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "SparkFun Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "DEV-12587"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "\n                        \n                            ATmega32U4 Pro Micro AVR® ATmega AVR MCU 8-Bit Embedded Evaluation Board\n                        \n"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "SparkFun Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(pad "JP6_1" thru_hole circle
			(at 7.62 -12.7)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(U1-RAW-PadJP6_1)")
			(pinfunction "RAW")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_2" thru_hole circle
			(at 7.62 -10.16)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_3" thru_hole circle
			(at 7.62 -7.62)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U1-~{RESET}-PadJP6_3)")
			(pinfunction "~{RESET}")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_4" thru_hole circle
			(at 7.62 -5.08)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(U1-VCC-PadJP6_4)")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_5" thru_hole circle
			(at 7.62 -2.54)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Right")
			(pinfunction "A3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_6" thru_hole circle
			(at 7.62 0)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Left")
			(pinfunction "A2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_7" thru_hole circle
			(at 7.62 2.54)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Down")
			(pinfunction "A1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_8" thru_hole circle
			(at 7.62 5.08)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Up")
			(pinfunction "A0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_9" thru_hole circle
			(at 7.62 7.62)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Punch 3")
			(pinfunction "SCK")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_10" thru_hole circle
			(at 7.62 10.16)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Start")
			(pinfunction "MISO")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_11" thru_hole circle
			(at 7.62 12.7)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Select")
			(pinfunction "MOSI")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "JP6_12" thru_hole circle
			(at 7.62 15.24)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/Kick 3")
			(pinfunction "D10")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_1" thru_hole circle
			(at -7.62 15.24)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(U1-D9-PadJP7_1)")
			(pinfunction "D9")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_2" thru_hole circle
			(at -7.62 12.7)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Home")
			(pinfunction "D8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_3" thru_hole circle
			(at -7.62 10.16)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U1-D7-PadJP7_3)")
			(pinfunction "D7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_4" thru_hole circle
			(at -7.62 7.62)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Kick 4")
			(pinfunction "D6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_5" thru_hole circle
			(at -7.62 5.08)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(U1-D5-PadJP7_5)")
			(pinfunction "D5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_6" thru_hole circle
			(at -7.62 2.54)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Punch 4")
			(pinfunction "D4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_7" thru_hole circle
			(at -7.62 0)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Kick 1")
			(pinfunction "D3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_8" thru_hole circle
			(at -7.62 -2.54)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Kick 2")
			(pinfunction "D2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_9" thru_hole circle
			(at -7.62 -5.08)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_10" thru_hole circle
			(at -7.62 -7.62)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_11" thru_hole circle
			(at -7.62 -10.16)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/Punch 1")
			(pinfunction "RXI")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "JP7_12" thru_hole circle
			(at -7.62 -12.7)
			(size 1.8796 1.8796)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Punch 2")
			(pinfunction "TXO")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(model "${KICAD8_3DMODEL_DIR}/Module.3dshapes/ARDUINO PRO MICRO.STEP"
			(offset
				(xyz -7.5 12.5 4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 119.928 101.964)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Kick3"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/Kick 3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 141.097 62.23)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Punch 2"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 6 "/Punch 2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 141.391 102.108)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Start"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.357 4.699 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.23 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Start")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 141.371 90.788)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "Punch 3"
			(at 1.25 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.25 4.6 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Arcade Encoder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 2.7 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 5 "/Punch 3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 148.336 49.276)
		(end 102.616 49.276)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.616 49.276)
		(end 102.616 107.569)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 148.336 107.569)
		(end 148.336 49.276)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.616 107.569)
		(end 148.336 107.569)
		(layer "Edge.Cuts")
	)
	(gr_text "DaemonBite Arcade Encoder Breakout Board "
		(at 113.411 51.562 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.368 46.863) (xy 100.965 46.863) (xy 100.965 109.093) (xy 150.368 109.22)
			)
		)
	)
)