(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 15)
    (no_connects 0)
    (area 144.407143 94.7 155.575 104.575)
    (thickness 0.8)
    (drawings 12)
    (tracks 57)
    (zones 0)
    (modules 7)
    (nets 11)
  )
  (page A4)
  (title_block
    (title "TOF Sensor")
    (date 2017-03-22)
    (rev 1.0)
    (company "ECE 445")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 +2V8)
  (net 2 GND)
  (net 3 /SDA)
  (net 4 /SCL)
  (net 5 "Net-(R1-Pad2)")
  (net 6 /INT)
  (net 7 "Net-(U1-Pad2)")
  (net 8 "Net-(U1-Pad3)")
  (net 9 "Net-(U1-Pad7)")
  (net 10 "Net-(U1-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net /INT)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad7)")
  )
  (module Connectors_JST:JST_GH_BM04B-GHS-TBT_04x1.25mm_Straight (layer B.Cu) (tedit 58D2A224)
    (at 150 100.25)
    (descr "JST GH series connector, BM04B-GHS-TBT, top entry type")
    (tags "connector jst GH SMT top vertical entry 1.25mm pitch")
    (attr smd)
    (fp_text reference J1 (at 0 -1) (layer B.SilkS))
    (fp_text value TOF (at 0 -4.575) (layer B.Fab))
    (fp_text user %R (at 0 -1.825) (layer B.Fab))
    (pad 1 smd rect (at -1.875 1.675) (size 0.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +2V8))
    (pad 2 smd rect (at -0.625 1.675) (size 0.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 /SDA))
    (pad 3 smd rect (at 0.625 1.675) (size 0.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 4 /SCL))
    (pad 4 smd rect (at 1.875 1.675) (size 0.6 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad "" smd rect (at 3.6 -1.675) (size 1 2.8) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at -3.6 -1.675) (size 1 2.8) (layers B.Cu B.Paste B.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D1A24D)
    (at 153 98.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58D1A259)
    (at 153 101.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D1A267)
    (at 147 101.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58D1A262)
    (at 147 98.5 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 47k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /INT))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module bcan:VL6180X (layer F.Cu) (tedit 58D1A289)
    (at 150 100)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value VL6180X (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -1.875) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /INT))
    (pad 2 smd rect (at -1.25 -1.125) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -1.25 -0.375) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -1.25 0.375) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at -1.25 1.125) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 6 smd rect (at -1.25 1.875) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /SDA))
    (pad 7 smd rect (at 1.25 1.875) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 1.25 1.125) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 9 smd rect (at 1.25 0.375) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 1.25 -0.375) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +2V8))
    (pad 11 smd rect (at 1.25 -1.125) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 1.25 -1.875) (size 1.1 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Measurement_Points:Measurement_Point_Square-SMD-Pad_Small (layer F.Cu) (tedit 58D2AA3D)
    (at 145.75 98)
    (descr "Mesurement Point, Square, SMD Pad,  1.5mm x 1.5mm,")
    (tags "Mesurement Point Square SMD Pad 1.5x1.5mm")
    (attr virtual)
    (fp_text reference J2 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value INT (at 0 2) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 6 /INT))
  )
  (gr_text "Rev 1.0" (at 150 100.25) (layer B.SilkS))
  (gr_text JST-GH (at 150 98.25) (layer B.SilkS))
  (gr_text "bcan TOF" (at 154.5 100 90) (layer F.SilkS))
  (gr_text INT (at 145.75 100 90) (layer F.SilkS))
  (gr_line (start 145 103.2) (end 145 96.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155 103.2) (end 145 103.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155 96.8) (end 155 103.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 96.8) (end 155 96.8) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 97) (xy 155 97) (xy 155 103) (xy 145 103)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.25) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 97) (xy 155 97) (xy 155 103) (xy 145 103)
      )
    )
  )
)
