(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 0)
    (no_connects 0)
    (area 91.8671 30.6298 161.7138 105.7536)
    (thickness 1.6)
    (drawings 29)
    (tracks 73)
    (zones 0)
    (modules 8)
    (nets 40)
  )
  (page A4)
  (title_block
    (title "Extending Tepmachcha")
    (date 2017-04-12)
    (rev 0.1)
    (company "STEM Phnom Penh/Theorent")
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.25)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 97.7138 86.2076)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/Users/leo/Documents/STEMPP repos/Tepmachcha_mod/Production/"))
  )
  (net 0 "")
  (net 1 /MISO)
  (net 2 VCC)
  (net 3 /SCK)
  (net 4 /MOSI)
  (net 5 /RST)
  (net 6 GND)
  (net 7 "Net-(P2-Pad1)")
  (net 8 "Net-(P2-Pad2)")
  (net 9 "Net-(SHIELD1-PadAD5)")
  (net 10 "Net-(SHIELD1-PadAD4)")
  (net 11 "Net-(SHIELD1-PadAD3)")
  (net 12 "Net-(SHIELD1-PadAD0)")
  (net 13 "Net-(SHIELD1-PadAD1)")
  (net 14 "Net-(SHIELD1-PadAD2)")
  (net 15 "Net-(SHIELD1-PadV_IN)")
  (net 16 "Net-(SHIELD1-PadGND2)")
  (net 17 "Net-(SHIELD1-Pad3V3)")
  (net 18 "Net-(SHIELD1-Pad0)")
  (net 19 "Net-(SHIELD1-Pad1)")
  (net 20 "Net-(SHIELD1-Pad2)")
  (net 21 "Net-(SHIELD1-Pad3)")
  (net 22 "Net-(SHIELD1-Pad4)")
  (net 23 "Net-(SHIELD1-Pad5)")
  (net 24 "Net-(SHIELD1-Pad6)")
  (net 25 "Net-(SHIELD1-Pad9)")
  (net 26 "Net-(SHIELD1-Pad10)")
  (net 27 "Net-(SHIELD1-PadGND3)")
  (net 28 "Net-(SHIELD1-PadAREF)")
  (net 29 "Net-(SHIELD1-PadSDA)")
  (net 30 "Net-(SHIELD1-PadSCL)")
  (net 31 "Net-(SHIELD1-PadIO_R)")
  (net 32 "Net-(SHIELD1-PadNC)")
  (net 33 "Net-(U1-Pad1)")
  (net 34 "Net-(U1-Pad10)")
  (net 35 "Net-(U1-Pad12)")
  (net 36 "Net-(U1-Pad13)")
  (net 37 "Net-(U1-Pad14)")
  (net 38 "Net-(U1-Pad15)")
  (net 39 "Net-(U1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(SHIELD1-Pad0)")
    (add_net "Net-(SHIELD1-Pad1)")
    (add_net "Net-(SHIELD1-Pad10)")
    (add_net "Net-(SHIELD1-Pad2)")
    (add_net "Net-(SHIELD1-Pad3)")
    (add_net "Net-(SHIELD1-Pad3V3)")
    (add_net "Net-(SHIELD1-Pad4)")
    (add_net "Net-(SHIELD1-Pad5)")
    (add_net "Net-(SHIELD1-Pad6)")
    (add_net "Net-(SHIELD1-Pad9)")
    (add_net "Net-(SHIELD1-PadAD0)")
    (add_net "Net-(SHIELD1-PadAD1)")
    (add_net "Net-(SHIELD1-PadAD2)")
    (add_net "Net-(SHIELD1-PadAD3)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadGND2)")
    (add_net "Net-(SHIELD1-PadGND3)")
    (add_net "Net-(SHIELD1-PadIO_R)")
    (add_net "Net-(SHIELD1-PadNC)")
    (add_net "Net-(SHIELD1-PadSCL)")
    (add_net "Net-(SHIELD1-PadSDA)")
    (add_net "Net-(SHIELD1-PadV_IN)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
  )
  (net_class pow_lines ""
    (clearance 0.5)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module freetronics_footprints:ARDUINO_SHIELD (layer F.Cu) (tedit 58EB0895)
    (at 148.5011 105.0036 90)
    (descr http://www.thingiverse.com/thing:9630)
    (fp_text reference SHIELD1 (at 8.3566 -23.7617 180) (layer F.SilkS))
    (fp_text value ARDUINO_SHIELD (at 10.16 -54.61 90) (layer F.SilkS) hide)
    (pad AD5 thru_hole circle (at 63.5 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole circle (at 60.96 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole circle (at 58.42 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SHIELD1-PadAD3)"))
    (pad AD0 thru_hole circle (at 50.8 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SHIELD1-PadAD0)"))
    (pad AD1 thru_hole circle (at 53.34 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SHIELD1-PadAD1)"))
    (pad AD2 thru_hole circle (at 55.88 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-PadAD2)"))
    (pad V_IN thru_hole circle (at 45.72 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SHIELD1-PadV_IN)"))
    (pad GND2 thru_hole circle (at 43.18 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SHIELD1-PadGND2)"))
    (pad GND1 thru_hole circle (at 40.64 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3V3 thru_hole circle (at 35.56 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(SHIELD1-Pad3V3)"))
    (pad RST thru_hole circle (at 33.02 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (pad 0 thru_hole circle (at 63.5 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(SHIELD1-Pad0)"))
    (pad 1 thru_hole circle (at 60.96 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SHIELD1-Pad1)"))
    (pad 2 thru_hole circle (at 58.42 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(SHIELD1-Pad2)"))
    (pad 3 thru_hole circle (at 55.88 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SHIELD1-Pad3)"))
    (pad 4 thru_hole circle (at 53.34 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(SHIELD1-Pad4)"))
    (pad 5 thru_hole circle (at 50.8 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(SHIELD1-Pad5)"))
    (pad 6 thru_hole circle (at 48.26 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad6)"))
    (pad 7 thru_hole circle (at 45.72 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P2-Pad1)"))
    (pad 8 thru_hole circle (at 41.656 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad2)"))
    (pad 9 thru_hole circle (at 39.116 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-Pad9)"))
    (pad 10 thru_hole circle (at 36.576 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(SHIELD1-Pad10)"))
    (pad 11 thru_hole circle (at 34.036 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /MOSI))
    (pad 12 thru_hole circle (at 31.496 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /MISO))
    (pad 13 thru_hole circle (at 28.956 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SCK))
    (pad GND3 thru_hole circle (at 26.416 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(SHIELD1-PadGND3)"))
    (pad AREF thru_hole circle (at 23.876 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole circle (at 38.1 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad SDA thru_hole circle (at 21.336 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(SHIELD1-PadSDA)"))
    (pad SCL thru_hole circle (at 18.796 -50.8 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(SHIELD1-PadSCL)"))
    (pad IO_R thru_hole circle (at 30.48 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(SHIELD1-PadIO_R)"))
    (pad NC thru_hole circle (at 27.94 -2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(SHIELD1-PadNC)"))
  )
  (module Connectors:Grove_1x04 (layer F.Cu) (tedit 587F9C9D)
    (at 101.8418 43.2816 90)
    (descr https://statics3.seeedstudio.com/images/opl/datasheet/3470130P1.pdf)
    (tags Grove-1x04)
    (fp_text reference P2 (at -1.9304 2.6792 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 11.2268 1.333 180) (layer F.Fab))
    (fp_text user 1 (at -1.775 0.075 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at 0 2 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at 0 4 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 4 thru_hole circle (at 0 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Connectors.3dshapes/Grove_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 -90))
    )
  )
  (module freetronics_footprints:Adafruit_FONA_808_Theorent (layer F.Cu) (tedit 58EB0AF6)
    (at 99.0796 87.2476 180)
    (fp_text reference U1 (at -8.6342 16.54 180) (layer F.SilkS))
    (fp_text value FONA_808 (at -13.6342 16.54 180) (layer F.Fab))
    (fp_text user Audio (at -35 -1.94 180) (layer F.SilkS))
    (fp_text user USB (at -24 -1.94 180) (layer F.SilkS))
    (fp_text user "Batt Conn" (at -10 -1.94 180) (layer F.SilkS))
    (fp_text user SIM (at -21.164 27.4052 180) (layer F.SilkS))
    (fp_text user S- (at -39.65 39.14 180) (layer F.SilkS))
    (fp_text user S+ (at -39.65 36.6 180) (layer F.SilkS))
    (fp_text user M- (at -39.65 34.06 180) (layer F.SilkS))
    (fp_text user M+ (at -39.65 31.5 180) (layer F.SilkS))
    (fp_text user NS (at -40 28.98 180) (layer F.SilkS))
    (fp_text user PSt (at -39.96 26.46 180) (layer F.SilkS))
    (fp_text user RI (at -40 23.92 180) (layer F.SilkS))
    (fp_text user Key (at -40 21.36 180) (layer F.SilkS))
    (fp_text user RTS (at -40 18.82 180) (layer F.SilkS))
    (fp_text user TX (at -39.96 16.3 180) (layer F.SilkS))
    (fp_text user RX (at -39.96 13.76 180) (layer F.SilkS))
    (fp_text user Rst (at -39.96 11.2 180) (layer F.SilkS))
    (fp_text user Vio (at -39.96 8.68 180) (layer F.SilkS))
    (fp_text user GND (at -39.96 6.12 180) (layer F.SilkS))
    (fp_text user Vcc (at -39.96 3.6 180) (layer F.SilkS))
    (fp_text user 5V (at -39.96 1.04 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -42.5 1.04 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -42.5 3.58 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -42.5 6.12 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 4 thru_hole circle (at -42.5 8.66 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(SHIELD1-PadIO_R)"))
    (pad 5 thru_hole circle (at -42.5 11.2 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(SHIELD1-Pad3)"))
    (pad 6 thru_hole circle (at -42.5 13.74 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad6)"))
    (pad 7 thru_hole circle (at -42.5 16.28 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(SHIELD1-Pad9)"))
    (pad 8 thru_hole circle (at -42.5 18.82 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(SHIELD1-PadAD1)"))
    (pad 9 thru_hole circle (at -42.5 21.36 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-PadAD2)"))
    (pad 10 thru_hole circle (at -42.5 23.9 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at -42.5 26.44 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SHIELD1-PadAD3)"))
    (pad 12 thru_hole circle (at -42.5 28.98 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -42.5 31.52 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at -42.5 34.06 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at -42.5 36.6 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at -42.5 39.14 180) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U1-Pad16)"))
    (pad "" np_thru_hole circle (at -2.5 2.54 180) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -2.5 37.66 180) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
  )
  (module Graphics:makerlab-logo (layer B.Cu) (tedit 0)
    (at 133.7138 76.2076 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Graphics:PIN-Logo (layer B.Cu) (tedit 0)
    (at 106.7138 76.2076 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Graphics:STEMPP-logo (layer B.Cu) (tedit 0)
    (at 120.2138 76.2076 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module freetronics_footprints:LOGO_OSHW_silkscreen_5mm (layer F.Cu) (tedit 0)
    (at 102.7138 75.7076)
    (fp_text reference LOGO_OSHW_silkscreen_5mm (at 0 2.65176) (layer F.SilkS) hide)
    (fp_text value val** (at 0 -2.65176) (layer F.SilkS) hide)
  )
  (module Graphics:tepmachcha (layer F.Cu) (tedit 0)
    (at 121.7138 77.2076)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text github.com/theorent/tepmachcha (at 121.2138 83.7076) (layer B.SilkS))
  (gr_text github.com/theorent/tepmachcha (at 121.2138 83.7076) (layer F.SilkS))
  (dimension 48.5 (width 0.3) (layer Cmts.User)
    (gr_text "48.500 mm" (at 155.0638 63.9576 270) (layer Cmts.User))
    (feature1 (pts (xy 148.7138 88.2076) (xy 156.4138 88.2076)))
    (feature2 (pts (xy 148.7138 39.7076) (xy 156.4138 39.7076)))
    (crossbar (pts (xy 153.7138 39.7076) (xy 153.7138 88.2076)))
    (arrow1a (pts (xy 153.7138 88.2076) (xy 153.127379 87.081096)))
    (arrow1b (pts (xy 153.7138 88.2076) (xy 154.300221 87.081096)))
    (arrow2a (pts (xy 153.7138 39.7076) (xy 153.127379 40.834104)))
    (arrow2b (pts (xy 153.7138 39.7076) (xy 154.300221 40.834104)))
  )
  (dimension 53.5 (width 0.3) (layer Cmts.User)
    (gr_text "53.500 mm" (at 121.9638 32.3576) (layer Cmts.User))
    (feature1 (pts (xy 148.7138 39.7076) (xy 148.7138 31.0076)))
    (feature2 (pts (xy 95.2138 39.7076) (xy 95.2138 31.0076)))
    (crossbar (pts (xy 95.2138 33.7076) (xy 148.7138 33.7076)))
    (arrow1a (pts (xy 148.7138 33.7076) (xy 147.587296 34.294021)))
    (arrow1b (pts (xy 148.7138 33.7076) (xy 147.587296 33.121179)))
    (arrow2a (pts (xy 95.2138 33.7076) (xy 96.340304 34.294021)))
    (arrow2b (pts (xy 95.2138 33.7076) (xy 96.340304 33.121179)))
  )
  (gr_line (start 136.2138 85.2076) (end 139.2138 88.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.7138 85.2076) (end 136.2138 85.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.7138 88.2076) (end 106.7138 85.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.2138 88.2076) (end 143.7138 88.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.2138 79.7076) (end 144.2138 88.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.7138 79.7076) (end 144.2138 79.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.7138 66.2076) (end 148.7138 79.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.7138 39.7076) (end 148.2138 39.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.7138 66.2076) (end 148.7138 39.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.7138 49.2076) (end 111.2138 47.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.7138 49.2076) (end 106.7138 49.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.7138 49.7076) (end 104.7138 49.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.7138 39.7076) (end 148.2138 39.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.2138 39.7076) (end 147.7138 39.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.7138 49.2076) (end 144.2138 39.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.7138 69.2076) (end 135.7138 49.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.7138 69.2076) (end 135.7138 69.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.7138 49.7076) (end 104.7138 69.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.2138 39.7076) (end 111.2138 47.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.2138 39.7076) (end 111.2138 39.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.2138 88.2076) (end 95.2138 39.7076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.7138 88.2076) (end 95.2138 88.2076) (layer Edge.Cuts) (width 0.15))
  (gr_text "Adafruit FONA 808 GSM/GPS" (at 101.7138 61.7076 90) (layer F.SilkS))
  (gr_line (start 103.7138 88.2076) (end 95.7138 88.2076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.7138 88.2076) (end 139.2138 88.2076) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.7138 39.2076) (xy 149.2138 39.2076) (xy 149.2138 88.7076) (xy 94.7138 88.7076)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 94.7138 39.2076) (xy 149.2138 39.2076) (xy 149.2138 88.7076) (xy 94.7138 88.7076)
      )
    )
  )
)
